BrlAPI 0.8

Macros | Functions
Getting Terminal information

How to get information about the connected Terminal. More...

## Macros
#define | BRLAPI_MAXNAMELENGTH 31

## Functions
int BRLAPI_STDCALL | brlapi_getDriverName (char *buffer, size_t size)
int BRLAPI_STDCALL | brlapi__getDriverName (brlapi_handle_t *handle, char *buffer, size_t size)
int BRLAPI_STDCALL | brlapi_getModelIdentifier (char *buffer, size_t size)
int BRLAPI_STDCALL | brlapi__getModelIdentifier (brlapi_handle_t *handle, char *buffer, size_t size)
int BRLAPI_STDCALL | brlapi_getDisplaySize (unsigned int *x, unsigned int *y)
int BRLAPI_STDCALL | brlapi__getDisplaySize (brlapi_handle_t *handle, unsigned int *x, unsigned int *y)

## Detailed Description

Before using Raw mode or key codes, the application should always check the type of the connected terminal, to be sure it is really the one it expects.

One should also check for display size, so as to adjust further displaying on it.

## Macro Definition Documentation

## ◆ BRLAPI_MAXNAMELENGTH

#define BRLAPI_MAXNAMELENGTH 31

Maximum name length for driver names embeded in BrlAPI packets, not counting any termination \0 character

## Function Documentation

## ◆ brlapi__getDisplaySize()

int BRLAPI_STDCALL brlapi__getDisplaySize | ( | brlapi_handle_t * | handle,
|  | unsigned int * | x,
|  | unsigned int * | y
| ) |  |

## ◆ brlapi__getDriverName()

int BRLAPI_STDCALL brlapi__getDriverName | ( | brlapi_handle_t * | handle,
|  | char * | buffer,
|  | size_t | size
| ) |  |

## ◆ brlapi__getModelIdentifier()

int BRLAPI_STDCALL brlapi__getModelIdentifier | ( | brlapi_handle_t * | handle,
|  | char * | buffer,
|  | size_t | size
| ) |  |

## ◆ brlapi_getDisplaySize()

int BRLAPI_STDCALL brlapi_getDisplaySize | ( | unsigned int * | x,
|  | unsigned int * | y
| ) |  |

Return the size of the braille display

## ◆ brlapi_getDriverName()

int BRLAPI_STDCALL brlapi_getDriverName | ( | char * | buffer,
|  | size_t | size
| ) |  |

Return the complete name of the driver used by brltty

This function fills its argument with the whole name of the braille driver if available, terminated with a '\0'.

Parameters

  buffer | is the buffer provided by the application;
  size | is the maximum size for the name buffer.

Returns
  -1 on error, otherwise a positive value giving the size of the needed buffer (including '\0'). If that value is bigger than `size`, the value was truncated and the caller should retry with a bigger buffer accordingly.

## ◆ brlapi_getModelIdentifier()

int BRLAPI_STDCALL brlapi_getModelIdentifier | ( | char * | buffer,
|  | size_t | size
| ) |  |

Return an identifier for the device model used by brltty

This function fills its argument with the whole identifier of the braille device model if available, terminated with a '\0'.

Parameters

  buffer | is the buffer given by the application;
  size | is the maximum size for the identifier buffer.

Returns
  -1 on error, otherwise a positive value giving the size of the needed buffer (including '\0'). If that value is bigger than `size`, the value was truncated and the caller should retry with a bigger buffer accordingly.