# Class CIM_ReplicationService
extends CIM_Service

The ReplicationService class provides methods to allow a client to manage copy operations on storage objects, including management of replication groups, manipulation of replication operations, and retrieval of replication relationships.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_Service
|
+--CIM_ReplicationService

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | The ReplicationService class provides methods to allow a client to manage copy operations on storage objects, including management of replication groups, manipulation of replication operations, and retrieval of replication relationships.
Experimental | boolean | true
UMLPackagePath | string | CIM::Device::StorageServices
Version | string | 2.42.0

## Class Properties

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_Service
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
LoSID | string | CIM_Service
LoSOrgID | string | CIM_Service
Name | string | CIM_Service
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
PrimaryOwnerContact | string | CIM_Service
PrimaryOwnerName | string | CIM_Service
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedState | uint16 | CIM_EnabledLogicalElement
Started | boolean | CIM_Service
StartMode | string | CIM_Service
Status | string | CIM_ManagedSystemElement
SystemCreationClassName | string | CIM_Service
SystemName | string | CIM_Service
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
OperationalStatus | uint16[] | CIM_ManagedSystemElement
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Local Class Methods

#### CreateGroup (uint32)

#### Method Qualifiers (CreateGroup)

Name | Data Type | Value
--- | --- | ---
Description | string | Create a new replication group.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, .., 0x8000..
Values | string | Success, Not Supported, Unknown, Timeout, Failed, Invalid Parameter, In Use, Groups are not nameable, DMTF Reserved, Vendor Specific

#### Method Parameters (CreateGroup)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
DeleteOnEmptyElement | boolean
Description | string | If true and empty groups are allowed, the group will be deleted when the last element is removed from the group. If empty groups are not allowed, the group will be deleted automatically when the group becomes empty. If this parameter is not NULL, its value will be used to set the group's DeleteOnEmptyElement property. Use the intrinsic method ModifyInstance to change this property after the group is created.
IN | boolean | true
DeleteOnUnassociated | boolean
Description | string | If true, the group will be deleted when the group is no longer associated with another group. This can happen if all synchronization associations to the individual elements of the group are dissolved. If this parameter is not NULL, its value will be used to set the group's DeleteOnUnassociated property. Use the intrinsic method ModifyInstance to change this property after the group is created.
IN | boolean | true
GroupName | string
Description | string | If nameable, an end user relevant name for the group being created. If NULL or not nameable, then system assigns a name.
IN | boolean | true
Persistent | boolean
Description | string | If false, the group, not the elements associated with the group, may be deleted at the completion of a copy operation. Use the intrinsic method ModifyInstance to change Persistency of a group.
IN | boolean | true
ReplicationSettingData | string
Description | string | If supplied, it provides additional replication settings for the method. For example, to supply the "Description" for the created group.
EmbeddedInstance | string | CIM_ReplicationSettingData
IN | boolean | true
ReservedAs | uint16
Description | string | The created group is reserved to be the source or the target of a copy operation. If not supplied, the group can be either the source or the target (4).
IN | boolean | true
ValueMap | string | 2, 3, 4, .., 0x8000..
Values | string | Source Only, Target Only, Source or Target, DMTF Reserved, Vendor Specific
Members | CIM_LogicalElement[]
Description | string | List of elements to add to the group -- order is maintained. If NULL, the group will be empty -- if empty groups are supported.
IN | boolean | true
ReplicationGroup | REF CIM_ReplicationGroup
Description | string | Reference to the created group.
IN | boolean | false
OUT | boolean | true
ServiceAccessPoint | REF CIM_ServiceAccessPoint
Description | string | Reference to access point information to allow the service to create a group on a remote system. If NULL, the group is created on the local system.
IN | boolean | true

#### DeleteGroup (uint32)

#### Method Qualifiers (DeleteGroup)

Name | Data Type | Value
--- | --- | ---
Description | string | Delete a replication group.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, .., 0x8000..
Values | string | Success, Not Supported, Unknown, Timeout, Failed, Invalid Parameter, In Use, One or more elements in a replication relationship, DMTF Reserved, Vendor Specific

#### Method Parameters (DeleteGroup)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
RemoveElements | boolean
Description | string | Delete the group even if it is not empty. If one or more elements in the group are in a replication relationship, RemoveElements has no effect.
IN | boolean | true
ReplicationSettingData | string
Description | string | If supplied, it provides additional replication settings for the method. For example, what should happen OnGroupOrListError.
EmbeddedInstance | string | CIM_ReplicationSettingData
IN | boolean | true
ReplicationGroup | REF CIM_ReplicationGroup
Description | string | Reference to a replication group.
IN | boolean | true
Required | boolean | true
ServiceAccessPoint | REF CIM_ServiceAccessPoint
Description | string | Reference to access point information to allow the service to delete the group on a remote system.
IN | boolean | true

#### AddMembers (uint32)

#### Method Qualifiers (AddMembers)

Name | Data Type | Value
--- | --- | ---
Description | string | Add members to an existing replication group.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, .., 0x8000..
Values | string | Success, Not Supported, Unknown, Timeout, Failed, Invalid Parameter, In Use, Group does not exist, DMTF Reserved, Vendor Specific

#### Method Parameters (AddMembers)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
ReplicationSettingData | string
Description | string | If supplied, it provides additional replication settings for the method. For example, what should happen OnGroupOrListError.
EmbeddedInstance | string | CIM_ReplicationSettingData
IN | boolean | true
Members | CIM_LogicalElement[]
Description | string | List of elements to add to the group. New members are added, in the order supplied, to the end of the existing members of the group. It is not an error, if a new member is already in the group.
IN | boolean | true
ReplicationGroup | REF CIM_ReplicationGroup
Description | string | Reference to an existing replication group.
IN | boolean | true
Required | boolean | true
ServiceAccessPoint | REF CIM_ServiceAccessPoint
Description | string | Reference to access point information to allow the service to access the group on a remote system.
IN | boolean | true

#### RemoveMembers (uint32)

#### Method Qualifiers (RemoveMembers)

Name | Data Type | Value
--- | --- | ---
Description | string | Remove members from a replication group.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, .., 0x8000..
Values | string | Success, Not Supported, Unknown, Timeout, Failed, Invalid Parameter, In Use, Group does not exist, Member not in group, DMTF Reserved, Vendor Specific

#### Method Parameters (RemoveMembers)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
DeleteOnEmptyElement | boolean
Description | string | If true and removal of the members causes the group to become empty, the group will be deleted. Note, if empty groups are not allowed, the group will be deleted automatically when the group becomes empty. If this parameter is not NULL, it overrides the group's property DeleteOnEmptyElement.
IN | boolean | true
ReplicationSettingData | string
Description | string | If supplied, it provides additional replication settings for the method. For example, what should happen OnGroupOrListError.
EmbeddedInstance | string | CIM_ReplicationSettingData
IN | boolean | true
Members | CIM_LogicalElement[]
Description | string | List of elements to remove from a group. A member can not be removed if it is in a replication relationship. Deleting all members of a group is equivalent to deleting the group if empty groups are not supported by the implementation.
IN | boolean | true
ReplicationGroup | REF CIM_ReplicationGroup
Description | string | Reference to an existing replication group.
IN | boolean | true
Required | boolean | true
ServiceAccessPoint | REF CIM_ServiceAccessPoint
Description | string | Reference to access point information to allow the service to access the group on a remote system.
IN | boolean | true

#### CreateElementReplica (uint32)

#### Method Qualifiers (CreateElementReplica)

Name | Data Type | Value
--- | --- | ---
Description | string | Create (or start a job to create) a new storage object, which is a replica of the specified source storage object (SourceElement). Note that using the input parameter, SyncType, this function can be used to instantiate the replica, and to create an ongoing association between the source and replica. If 0 is returned, the function completed successfully and no ConcreteJob instance created. If 4096/0x1000 is returned, a ConcreteJob is started, a reference to which is returned in the Job output parameter.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 4096, 4097..32767, 0x8000..
Values | string | Completed with No Error, Not Supported, Unknown, Timeout, Failed, Invalid Parameter, In Use, DMTF Reserved, Method Parameters Checked - Job Started, Method Reserved, Vendor Specific

#### Method Parameters (CreateElementReplica)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
ElementName | string
Description | string | A end user relevant name for the element being created. If NULL, then a system supplied default name can be used. The value will be stored in the 'ElementName' property for the created element.
IN | boolean | true
Mode | uint16
Description | string | Mode describes whether the target elements will be updated synchronously or asynchronously. Adaptive: Allows implementation to dynamically switch between synchronous and asynchronous modes. If NULL, implementation decides the mode.
IN | boolean | true
ModelCorrespondence | string | CIM_Synchronized.Mode
ValueMap | string | 2, 3, 4, .., 0x8000..
Values | string | Synchronous, Asynchronous, Adaptive, DMTF Reserved, Vendor Specific
ReplicationSettingData | string
Description | string | If provided, it overrides the default replication setting data for the given SyncType. If not provided, the management server uses the default replication setting data.
EmbeddedInstance | string | CIM_ReplicationSettingData
IN | boolean | true
SyncType | uint16
Description | string | SyncType describes the type of copy that will be made.
IN | boolean | true
ModelCorrespondence | string | CIM_Synchronized.SyncType
Required | boolean | true
ValueMap | string | .., 6, 7, 8, 9, .., 0x8000..
Values | string | DMTF Reserved, Mirror, Snapshot, Clone, TokenizedClone, DMTF Reserved, Vendor Specific
WaitForCopyState | uint16
Description | string | Method must wait until this CopyState is reached before returning. Only a subset of valid CopyStates apply. For example, Initialized: Associations have been established, but there is no data flow. Inactive: Initialization is complete, but the data flow remains idle until it is activated. Synchronized: Replicas are an exact copy of the source. UnSynchronized: Copy operation is in progress.
IN | boolean | true
ModelCorrespondence | string | CIM_Synchronized.CopyState
Collections | CIM_Collection[]
Description | string | The target elements are added to each referenced collection, for example, DeviceMaskingGroups.
IN | boolean | true
ConnectivityCollection | REF CIM_ConnectivityCollection
Description | string | Reference to the ConnectivityCollection - for example, a RemoteReplicationCollection. Since a RemoteReplicationCollection aggregates the ProtocolEndpoints that provide the paths to a remote system, generally, it is not necessary to supply both the ConnectivityCollection and the ServiceAccessPoint.
IN | boolean | true
Job | REF CIM_ConcreteJob
Description | string | Reference to the job (may be NULL if job is completed).
IN | boolean | false
OUT | boolean | true
SourceAccessPoint | REF CIM_ServiceAccessPoint
Description | string | Reference to source access point information. If NULL, service does not need access information to access the source element.
IN | boolean | true
SourceElement | REF CIM_LogicalElement
Description | string | The source storage object which may be a StorageVolume or other storage objects.
IN | boolean | true
Required | boolean | true
Synchronization | REF CIM_Synchronized
Description | string | Reference to the created association between the source and the target element. If a job is created, this parameter may be NULL unless the association is actually formed.
IN | boolean | false
OUT | boolean | true
TargetAccessPoint | REF CIM_ServiceAccessPoint
Description | string | Reference to target access point information. If NULL, service does not need access information to access the target elements.
IN | boolean | true
TargetElement | REF CIM_LogicalElement
Description | string | Optionally, as an input, refers to a target element to use. As an output, refers to the created target storage element (i.e., the replica). If a job is created, the target element may not be available immediately.
IN | boolean | true
OUT | boolean | true
TargetPool | REF CIM_ResourcePool
Description | string | The underlying storage for the target element (the replica) will be drawn from TargetPool if specified, otherwise the allocation is implementation specific. If a target element is supplied, this parameter shall be NULL.
IN | boolean | true
TargetSettingGoal | REF CIM_SettingData
Description | string | The definition for the SettingData to be maintained by the target storage object (the replica). If a target element is supplied, this parameter shall be NULL.
IN | boolean | true

#### CreateGroupReplica (uint32)

#### Method Qualifiers (CreateGroupReplica)

Name | Data Type | Value
--- | --- | ---
Description | string | Create (or start a job to create) a new group of storage objects which are replicas of the specified source storage or a group of source storage objects (SourceElements). Note that using the input parameter, SyncType, this function can be used to instantiate the replicas, and to create an ongoing association between the source(s) and replicas. If 0 is returned, the function completed successfully and no ConcreteJob instance is created. If 4096/0x1000 is returned, a ConcreteJob is started, a reference to which is returned in the Job output parameter.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 4096, 4097..32767, 0x8000..
Values | string | Completed with No Error, Not Supported, Unknown, Timeout, Failed, Invalid Parameter, In Use, DMTF Reserved, Method Parameters Checked - Job Started, Method Reserved, Vendor Specific

#### Method Parameters (CreateGroupReplica)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
Consistency | uint16
Description | string | Overrides the default group consistency.
IN | boolean | true
ValueMap | string | 2, 3, .., 0x8000..
Values | string | No Consistency, Sequential Consistency, DMTF Reserved, Vendor Specific
Mode | uint16
Description | string | Mode describes whether the target elements will be updated synchronously or asynchronously. Adaptive: Allows implementation to dynamically switch between synchronous and asynchronous modes. If NULL, implementation decides the mode.
IN | boolean | true
ModelCorrespondence | string | CIM_Synchronized.Mode
ValueMap | string | 2, 3, 4, .., 0x8000..
Values | string | Synchronous, Asynchronous, Adaptive, DMTF Reserved, Vendor Specific
RelationshipName | string
Description | string | A user relevant name for the relationship between the source and target groups or between a source element and a target group (i.e. one-to-many). If NULL, the implementation assigns a name. If the individual target elements require an ElementName, the implementation constructs an appropriate ElementName using the RelationshipName. For example, RelationshipName as a prefix followed by "_n" sequence number, where n is a number beginning with 1.
IN | boolean | true
ReplicationSettingData | string
Description | string | If provided, it overrides the default replication setting data for the given SyncType. If not provided, the management server uses the default replication setting data.
EmbeddedInstance | string | CIM_ReplicationSettingData
IN | boolean | true
SyncType | uint16
Description | string | SyncType describes the type of copy that will be made.
IN | boolean | true
ModelCorrespondence | string | CIM_Synchronized.SyncType
Required | boolean | true
ValueMap | string | .., 6, 7, 8, 9, .., 0x8000..
Values | string | DMTF Reserved, Mirror, Snapshot, Clone, TokenizedClone, DMTF Reserved, Vendor Specific
TargetElementCount | uint64
Description | string | This parameter applies to one-source-to-many-target- elements. It is possible to create multiple copies of a source element. If TargetGroup is supplied, this parameter shall be NULL.
IN | boolean | true
WaitForCopyState | uint16
Description | string | Method must wait until this CopyState is reached before returning. Only a subset of valid CopyStates apply. For example, Initialized: Associations have been established, but there is no data flow. Inactive: Initialization is complete, but the data flow remains idle until it is activated. Synchronized: Replicas are an exact copy of the source. UnSynchronized: Copy operation is in progress.
IN | boolean | true
ModelCorrespondence | string | CIM_Synchronized.CopyState
Collections | CIM_Collection[]
Description | string | The target elements are added to each referenced collection, for example, DeviceMaskingGroups.
IN | boolean | true
ConnectivityCollection | REF CIM_ConnectivityCollection
Description | string | Reference to the ConnectivityCollection - for example, a RemoteReplicationCollection. Since a RemoteReplicationCollection aggregates the ProtocolEndpoints that provide the paths to a remote system, generally, it is not necessary to supply both the ConnectivityCollection and the ServiceAccessPoint.
IN | boolean | true
Job | REF CIM_ConcreteJob
Description | string | Reference to the job (may be NULL if job is completed).
IN | boolean | false
OUT | boolean | true
SourceAccessPoint | REF CIM_ServiceAccessPoint
Description | string | Reference to source access point information. If NULL, service does not need access information to access the source element.
IN | boolean | true
SourceElement | REF CIM_LogicalElement
Description | string | The source storage object which may be a StorageVolume or other storage objects. If this parameter is not supplied, SourceGroup is required. Both SourceGroup and SourceElement shall not be supplied.
IN | boolean | true
SourceGroup | REF CIM_ReplicationGroup
Description | string | A group of source storage objects which may be one or more StorageVolumes or other storage objects. If this parameter is not supplied, SourceElement is required. Both SourceGroup and SourceElement shall not be supplied.
IN | boolean | true
Synchronization | REF CIM_Synchronized
Description | string | Reference to the created group association between the source and the target elements. If a job is created, this parameter may be NULL until the association is actually formed.
IN | boolean | false
OUT | boolean | true
TargetAccessPoint | REF CIM_ServiceAccessPoint
Description | string | Reference to target access point information. If NULL, service does not need access information to access the target element/group.
IN | boolean | true
TargetGroup | REF CIM_ReplicationGroup
Description | string | Optionally, as an input, refers to a target group to use. As an output, refers to the created target group (i.e., the replica group). If a job is created, the target group may not be available immediately. If TargetGroup is supplied, TargetElementCount shall be NULL.
IN | boolean | true
OUT | boolean | true
TargetPool | REF CIM_ResourcePool
Description | string | The underlying storage for the target elements (the replicas) will be drawn from TargetPool if specified, otherwise the allocation is implementation specific. If target elements are supplied, this parameter shall be NULL.
IN | boolean | true
TargetSettingGoal | REF CIM_SettingData
Description | string | The definition for the SettingData to be maintained by the target storage objects (the replicas). If target elements are supplied, this parameter shall be NULL.
IN | boolean | true

#### CreateSynchronizationAspect (uint32)

#### Method Qualifiers (CreateSynchronizationAspect)

Name | Data Type | Value
--- | --- | ---
Description | string | Create (or start a job to create) a new point-in-time representation of a source element. This representation may be of a form of pointers that keep track of data at the time the point-in-time was created, or a series checkpoints that capture the view of data on the source elements at the time of point-in-time. This method does not include a target element, however, a target element can be added subsequently using the ModifySettingsDefineState method. If the method executes successfully, a SettingsDefineState association is created between the source element and the SynchronizationAspect, which will have the datetime of the point-in-time.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 4096, 4097..32767, 0x8000..
Values | string | Completed with No Error, Not Supported, Unknown, Timeout, Failed, Invalid Parameter, In Use, DMTF Reserved, Method Parameters Checked - Job Started, Method Reserved, Vendor Specific

#### Method Parameters (CreateSynchronizationAspect)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
Consistency | uint16
Description | string | Overrides the default group consistency.
IN | boolean | true
ValueMap | string | 2, 3, .., 0x8000..
Values | string | No Consistency, Sequential Consistency, DMTF Reserved, Vendor Specific
Mode | uint16
Description | string | Mode describes whether the target elements will be updated synchronously or asynchronously. Adaptive: Allows implementation to dynamically switch between synchronous and asynchronous modes. If NULL, implementation decides the mode.
IN | boolean | true
ModelCorrespondence | string | CIM_Synchronized.Mode
ValueMap | string | 2, 3, 4, .., 0x8000..
Values | string | Synchronous, Asynchronous, Adaptive, DMTF Reserved, Vendor Specific
Name | string
Description | string | A end user relevant name for the element or relationship being created. If NULL, then a system supplied default name can be used. The value will be stored in the ElementName or relationship name depending on whether an element is created or a group.
IN | boolean | true
ReplicationSettingData | string
Description | string | If provided, it overrides the default replication setting data for the given SyncType. If not provided, the management server uses the default replication setting data.
EmbeddedInstance | string | CIM_ReplicationSettingData
IN | boolean | true
SyncType | uint16
Description | string | SyncType describes the type of copy that will be made.
IN | boolean | true
ModelCorrespondence | string | CIM_Synchronized.SyncType
Required | boolean | true
ValueMap | string | .., 6, 7, 8, 9, .., 0x8000..
Values | string | DMTF Reserved, Mirror, Snapshot, Clone, TokenizedClone, DMTF Reserved, Vendor Specific
Job | REF CIM_ConcreteJob
Description | string | Reference to the job (may be NULL if job is completed).
IN | boolean | false
OUT | boolean | true
SettingsState | REF CIM_SettingsDefineState
Description | string | Reference to the created association between the source element or group and an instance of SynchronizationAspect. If a job is created, this parameter may be NULL unless the association is actually formed.
IN | boolean | false
OUT | boolean | true
SourceAccessPoint | REF CIM_ServiceAccessPoint
Description | string | Reference to source access point information. If NULL, service does not need access information to access the source element/group.
IN | boolean | true
SourceElement | REF CIM_ManagedElement
Description | string | The source storage object which may be a StorageVolume or other storage objects. If this parameter is not supplied, SourceGroup is required. Both SourceGroup and SourceElement shall not be supplied.
IN | boolean | true
SourceGroup | REF CIM_ReplicationGroup
Description | string | A group of source storage objects which may be one or more StorageVolumes or other storage objects. If this parameter is not supplied, SourceElement is required. Both SourceGroup and SourceElement shall not be supplied.
IN | boolean | true

#### ModifyReplicaSynchronization (uint32)

#### Method Qualifiers (ModifyReplicaSynchronization)

Name | Data Type | Value
--- | --- | ---
Description | string | Modify (or start a job to modify) the synchronization association between two storage objects or replication groups. If 0 is returned, the function completed successfully and no ConcreteJob instance was created. If 0x1000 is returned, a ConcreteJob was started and a reference to this Job is returned in the Job output parameter. A return value of 1 indicates the method is not supported. All other values indicate some type of error condition.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 4096, 4097..32767, 0x8000..
Values | string | Completed with No Error, Not Supported, Unspecified Error, Timeout, Failed, Invalid Parameter, In Use, DMTF Reserved, Method Parameters Checked - Job Started, Method Reserved, Vendor Specific

#### Method Parameters (ModifyReplicaSynchronization)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
Force | boolean
Description | string | Some operations may cause an inconsistency among the target elements. If true, the client is not warned and the operation is performed.
IN | boolean | true
Operation | uint16
Description | string | Operation describes the type of modification to be made to the replica and/or to the related associations. Abort: Abort the copy operation if it is possible. Activate Consistency: if consistency was not requested when CreateGroupReplica was called. If Consistency is already active, no modification is made. Activate: Activate an inactive or prepared Synchronized association. AddSyncPair: Add pairs of elements already in a relationship to source and target groups -- see SyncPair parameter. Deactivate Consistency: Deactivate consistency. If consistency was not enabled, this operation has no effect. Deactivate: Stop the data flow. Writes to source element are not copied to target. For Snapshots, writes to target are lost as the pointers to changed data are deleted. Detach: 'Forget' the synchronization between two storage objects. Start to treat the objects as independent. Dissolve: Dissolve the synchronization between two storage objects, however, the target element continues to exist. Failover: Use the target element as the source elements. Failback: Reverse the effect of failback. Fracture: Suspend the synchronization between two storage objects. The association and (typically) changes are remembered to allow a fast resynchronization. This may be used during a backup cycle to allow one of the objects to be copied while the other remains in production. RemoveSyncPair: Remove the pair associated via StorageSynchronized from the source and target groups. The pair continue to remain associated but not in the groups. Resync Replica: Re-establish the synchronization. This will negate the action of a previous Fracture/Split operation. Recreate a Point In Time image for a Snapshot or a Clone replication. Restart a Broken or Aborted synchronization relationship. Restore from Replica: Renew the contents of the original storage object from a replica. Resume: Continue the copy operation of a suspended association. Reset To Sync: Change the Mode of the copy operation to Synchronous (e.g., from the Asynchronous Mode). Reset To Async: Change the Mode of the copy operation to Asynchronous (e.g., from the Synchronous Mode). Return to ResourcePool: Dissolve a snapshot and free up its space back to the storage pool. Reverse Roles: Source element becomes the target element and vise versa. Split: Same as Fracture, however steps are taken to ensure the target elements are consistent. For example, stop I/O to source elements, wait for in-transit copy operations between source and target elements to stop, then instantly split source/target groups/elements. Suspend: Stop the background copy previously started. Unprepare: note, this operation has been deprecated. Use "Prepare" instead. Prepare: Causes the synchronization to be reinitialized. Reset To Adaptive: Change the Mode of the copy operation to Adaptive.
IN | boolean | true
Required | boolean | true
ValueMap | string | 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20, 21, 22, 23, 24, 25, .., 0x8000..0xFFFF
Values | string | Abort, Activate Consistency, Activate, AddSyncPair, Deactivate Consistency, Deactivate, Detach, Dissolve, Failover, Failback, Fracture, RemoveSyncPair, Resync Replica, Restore from Replica, Resume, Reset To Sync, Reset To Async, Return To ResourcePool, Reverse Roles, Split, Suspend, Unprepare, Prepare, Reset to Adaptive, DMTF Reserved, Vendor Specific
ReplicationSettingData | string
Description | string | If provided, it overrides the default replication setting data for the given SyncType. If not provided, the management server uses the default replication setting data.
EmbeddedInstance | string | CIM_ReplicationSettingData
IN | boolean | true
WaitForCopyState | uint16
Description | string | Method must wait until this CopyState is reached before returning. Only a subset of valid CopyStates apply. For example, Initialized: Associations have been established, but there is no data flow. Inactive: Initialization is complete, but the data flow remains idle until it is activated. Synchronized: Replicas are an exact copy of the source. UnSynchronized: Copy operation is in progress. Fractured/Split: Target elements are separated from the source elements. Etc.
IN | boolean | true
ModelCorrespondence | string | CIM_Synchronized.CopyState
SyncPair | CIM_Synchronized[]
Description | string | This parameter applies to AddSyncPair/RemoveSyncPair Operations.
IN | boolean | true
Job | REF CIM_ConcreteJob
Description | string | Reference to the job (may be NULL if the task completed).
IN | boolean | false
OUT | boolean | true
SettingsState | REF CIM_SettingsDefineState
Description | string | Reference to the association between the source element and an instance of SynchronizationAspect. This parameters applies to operations such as Dissolve, which dissolves the Synchronized relationship, but causes the SettingDefineState association to be created.
IN | boolean | false
OUT | boolean | true
Synchronization | REF CIM_Synchronized
Description | string | The reference to the replication association describing the elements/groups relationship.
IN | boolean | true
Required | boolean | true
UpdatedSynchronization | REF CIM_Synchronized
Description | string | If the operation updates the keys of the supplied Synchronization parameter, a reference to the updated Synchronization parameter is returned in this parameter.
IN | boolean | false
OUT | boolean | true

#### ModifyListSynchronization (uint32)

#### Method Qualifiers (ModifyListSynchronization)

Name | Data Type | Value
--- | --- | ---
Description | string | Modify (or start a job to modify) an array of synchronization associations between two storage objects or replication groups. If 0 is returned, the function completed successfully and no ConcreteJob instance was created. If 4096 is returned, a ConcreteJob was started and a reference to this Job is returned in the Job output parameter. A return value of 1 indicates the method is not supported. All other values indicate some type of error condition.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 4096, 4097..32767, 0x8000..
Values | string | Completed with No Error, Not Supported, Unspecified Error, Timeout, Failed, Invalid Parameter, In Use, DMTF Reserved, Method Parameters Checked - Job Started, Method Reserved, Vendor Specific

#### Method Parameters (ModifyListSynchronization)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
Force | boolean
Description | string | Some operations may cause an inconsistency among the target elements. If true, the client is not warned and the operation is performed.
IN | boolean | true
Operation | uint16
Description | string | Operation describes the type of modification to be made to the replica and/or to the related associations. Abort: Abort the copy operation if it is possible. Activate: Activate an inactive or prepared Synchronized association. Deactivate: Stop the data flow. Writes to source element are not copied to target. For Snapshots, writes to target are lost as the pointers to changed data are deleted. Detach: 'Forget' the synchronization between two storage objects. Start to treat the objects as independent. Dissolve: Dissolve the synchronization between two storage objects, however, the target element continues to exist. Failover: Use the target element as the source elements. Failback: Reverse the effect of failback. Fracture: Suspend the synchronization between two storage objects using Mirror or Snapshot replication. The association and (typically) changes are remembered to allow a fast resynchronization. This may be used during a backup cycle to allow one of the objects to be copied while the other remains in production. Resync Replica: Re-establish the synchronization. This will negate the action of a previous Fracture/Split operation. Recreate a Point In Time image for a Snapshot or a Clone replication. Restart a Broken or Aborted synchronization relationship. Restore from Replica: Renew the contents of the original storage object from a replica. Resume: Continue the copy operation of a suspended association. Reset To Sync: Change the Mode of the copy operations to Synchronous (e.g., from the Asynchronous Mode). Reset To Async: Change the Mode of the copy operations to Asynchronous (e.g., from the Synchronous Mode). Return to ResourcePool: Dissolve a snapshot and free up its space back to the storage pool. Reverse Roles: Source element becomes the target element and vise versa. Split: Same as Fracture, however steps are taken to ensure the target elements are consistent. For example, stop I/O to source elements, wait for in-transit copy operations between source and target elements to stop, then instantly split source/target groups/elements. Suspend: Stop the background copy previously started. Unprepare: note, this operation has been deprecated. Use "Prepare" instead. Prepare: Causes the synchronization to be reinitialized. Reset To Adaptive: Change the Mode of the copy operation to Adaptive.
IN | boolean | true
Required | boolean | true
ValueMap | string | 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20, 21, 22, 23, 24, 25, .., 0x8000..0xFFFF
Values | string | Abort, DMTF Reserved, Activate, DMTF Reserved, DMTF Reserved, Deactivate, Detach, Dissolve, Failover, Failback, Fracture, DMTF Reserved, Resync Replica, Restore from Replica, Resume, Reset To Sync, Reset To Async, Return To ResourcePool, Reverse Roles, Split, Suspend, Unprepare, Prepare, Reset to Adaptive, DMTF Reserved, Vendor Specific
ReplicationSettingData | string
Description | string | If provided, it overrides the default replication setting data for the given SyncType. If not provided, the management server uses the default replication setting data.
EmbeddedInstance | string | CIM_ReplicationSettingData
IN | boolean | true
WaitForCopyState | uint16
Description | string | Method must wait until this CopyState is reached before returning. Only a subset of valid CopyStates apply. For example, Initialized: Associations have been established, but there is no data flow. Inactive: Initialization is complete, but the data flow remains idle until it is activated. Synchronized: Replicas are an exact copy of the source. UnSynchronized: Copy operation is in progress. Fractured/Split: Target elements are separated from the source elements. Etc.
IN | boolean | true
ModelCorrespondence | string | CIM_Synchronized.CopyState
SettingsState | CIM_SettingsDefineState[]
Description | string | References to the associations between the source element and an instance of SynchronizationAspect. This parameters applies to operations such as Dissolve, which dissolves the Synchronized relationship, but causes the SettingDefineState association to be created..
IN | boolean | false
OUT | boolean | true
Synchronization | CIM_Synchronized[]
Description | string | Array of replication associations describing the elements/groups relationship. All elements of this array shall be the same concrete class, i.e. StorageSynchronized or GroupSynchronized, and shall have the same SyncType, the same Mode, and the Operation must be valid for the ReplicationType -- SyncType, Mode, Local/Remote.
IN | boolean | true
Required | boolean | true
UpdatedSynchronizations | CIM_Synchronized[]
Description | string | If the operation updates the keys of the supplied synchronizations in the Synchronization parameter, references to the updated synchronizations are returned in this parameter.
IN | boolean | false
OUT | boolean | true
Job | REF CIM_ConcreteJob
Description | string | Reference to the job (may be NULL if the task completed).
IN | boolean | false
OUT | boolean | true

#### ModifySettingsDefineState (uint32)

#### Method Qualifiers (ModifySettingsDefineState)

Name | Data Type | Value
--- | --- | ---
Description | string | Modify (or start a job to modify) the SettingsDefineState association between the storage objects and SynchronizationAspect. The modification could range from introducing the target elements, which creates a new StorageSynchronized association to dissolving the SettingsDefineState association. If 0 is returned, the function completed successfully and no ConcreteJob instance was created. If 4096/0x1000 is returned, a ConcreteJob was started and a reference to this Job is returned in the Job output parameter. A return value of 1 indicates the method is not supported. All other values indicate some type of error condition.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 4096, 4097..32767, 0x8000..
Values | string | Completed with No Error, Not Supported, Unspecified Error, Timeout, Failed, Invalid Parameter, In Use, DMTF Reserved, Method Parameters Checked - Job Started, Method Reserved, Vendor Specific

#### Method Parameters (ModifySettingsDefineState)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
ElementName | string
Description | string | A end user relevant name for the element being created. If NULL, then a system supplied default name can be used. The value will be stored in the 'ElementName' property for the created element.
IN | boolean | true
Operation | uint16
Description | string | Operation describes the type of modification to be made to the related associations. Activate Consistency: if consistency was not requested when CreateSynchronizationAspect was called. If Consistency is already active, no modification is made. Deactivate Consistency: Deactivate consistency. If consistency was not enabled, this operation has no effect. Delete: Remove the SettingsDefineState association and the associated SynchronizationAspect. Copy To Target: Introduces the target elements and forms the necessary associations between the source and the target elements i.e. StorageSynchronized and GroupSynchronized. Detach: Removes the association between the SynchronizationAspect and the target element. Restore: Restore the source element from the associated SynchronizationAspect. Attach To Target: Same as Copy To Target except no data is copied.
IN | boolean | true
Required | boolean | true
ValueMap | string | 2, 3, 4, 5, 6, 7, 8, .., 0x8000..0xFFFF
Values | string | Activate Consistency, Deactivate Consistency, Delete, Copy To Target, Detach, Restore, Attach To Target, DMTF Reserved, Vendor Specific
ReplicationSettingData | string
Description | string | If provided, it overrides the default replication setting data for the given SyncType. If not provided, the management server uses the default replication setting data.
EmbeddedInstance | string | CIM_ReplicationSettingData
IN | boolean | true
TargetElementCount | uint64
Description | string | This parameter applies to one-source-to-many-target- elements. It is possible to create multiple copies of a source element. If TargetCount is supplied, TargetElement and TargetGroup shall be NULL.
IN | boolean | true
WaitForCopyState | uint16
Description | string | Method must wait until this CopyState is reached before returning. Only a subset of valid CopyStates apply. For example, Initialized: Associations have been established, but there is no data flow. Inactive: Initialization is complete, but the data flow remains idle until it is activated. Synchronized: Replicas are an exact copy of the source. UnSynchronized: Copy operation is in progress. Fractured/Split: Target elements are separated from the source elements. Etc.
IN | boolean | true
ModelCorrespondence | string | CIM_Synchronized.CopyState
Collections | CIM_Collection[]
Description | string | The target elements are added to each referenced collection, for example, DeviceMaskingGroups.
IN | boolean | true
Job | REF CIM_ConcreteJob
Description | string | Reference to the job (may be NULL if the task completed).
IN | boolean | false
OUT | boolean | true
SettingsState | REF CIM_SettingsDefineState
Description | string | Reference to the association between the source element and an instance of SynchronizationAspect.
IN | boolean | true
Required | boolean | true
Synchronization | REF CIM_Synchronized
Description | string | The reference to the created replication association describing the elements/groups relationship.
IN | boolean | false
OUT | boolean | true
TargetAccessPoint | REF CIM_ServiceAccessPoint
Description | string | Reference to target access point information. If NULL, service does not need access information to access the target elements/group.
IN | boolean | true
TargetElement | REF CIM_LogicalElement
Description | string | Optionally, as an input, refers to a target element to use. If TargetElement is supplied, TargetGroup and TargetCount shall be NULL. As an output, refers to the created target storage element (i.e., the replica). If a job is created, the target element may not be available immediately.
IN | boolean | true
OUT | boolean | true
TargetGroup | REF CIM_ReplicationGroup
Description | string | Optionally, as an input, refers to a target group to use. If TargetGroup is supplied, TargetElement and TargetCount shall be NULL. As an output, refers to the created target group (i.e., the replica group). If a job is created, the target group may not be available immediately. If TargetGroup is supplied, TargetElementCount shall be NULL.
IN | boolean | true
OUT | boolean | true
TargetPool | REF CIM_ResourcePool
Description | string | The underlying storage for the target element (the replica) will be drawn from TargetPool if specified, otherwise the allocation is implementation specific. If a target element is supplied, this parameter shall be NULL.
IN | boolean | true
TargetSettingGoal | REF CIM_SettingData
Description | string | The definition for the SettingData to be maintained by the target storage object (the replica). If a target element is supplied, this parameter shall be NULL.
IN | boolean | true

#### GetAvailableTargetElements (uint32)

#### Method Qualifiers (GetAvailableTargetElements)

Name | Data Type | Value
--- | --- | ---
Description | string | Get (or start a job to get) all of the candidate target elements for the supplied source element. If a job is started, once the job completes, examine the AffectedJobElement associations for candidate targets.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 4096, 4097..32767, 0x8000..
Values | string | Completed with No Error, Not Supported, Unspecified Error, Timeout, Failed, Invalid Parameter, In Use, DMTF Reserved, Method Parameters Checked - Job Started, Method Reserved, Vendor Specific

#### Method Parameters (GetAvailableTargetElements)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
MaxElementCount | uint16
Description | string | Specifies the maximum number of elements to be returned by the method.
IN | boolean | true
Mode | uint16
Description | string | Mode describes whether the target elements will be updated synchronously or asynchronously. Adaptive: Allows implementation to dynamically switch between synchronous and asynchronous modes. If NULL, implementation decides the mode.
IN | boolean | true
ModelCorrespondence | string | CIM_Synchronized.Mode
ValueMap | string | 2, 3, 4, .., 0x8000..
Values | string | Synchronous, Asynchronous, Adaptive, DMTF Reserved, Vendor Specific
ReplicationSettingData | string
Description | string | If provided, it overrides the default replication setting data for the given SyncType. If not provided, the management server uses the default replication setting data.
EmbeddedInstance | string | CIM_ReplicationSettingData
IN | boolean | true
SyncType | uint16
Description | string | SyncType describes the type of copy.
IN | boolean | true
ModelCorrespondence | string | CIM_Synchronized.SyncType
Required | boolean | true
ValueMap | string | .., 6, 7, 8, 9, .., 0x8000..
Values | string | DMTF Reserved, Mirror, Snapshot, Clone, TokenizedClone, DMTF Reserved, Vendor Specific
Candidates | CIM_LogicalElement[]
Description | string | The list of the candidate target elements.
OUT | boolean | true
TargetPools | CIM_ResourcePool[]
Description | string | The storage pools for the target elements. If NULL, all storage pools (on the given system) will be examined.
IN | boolean | true
Job | REF CIM_ConcreteJob
Description | string | Reference to the job (may be NULL if the task completed).
IN | boolean | false
OUT | boolean | true
SourceElement | REF CIM_LogicalElement
Description | string | The source storage object which may be a StorageVolume or other storage objects.
IN | boolean | true
Required | boolean | true
TargetAccessPoint | REF CIM_ServiceAccessPoint
Description | string | Reference to access point information. If NULL, only local system is examined.
IN | boolean | true
TargetSettingGoal | REF CIM_SettingData
Description | string | Desired target SettingData. If NULL, settings of the source element will be used.
IN | boolean | true

#### GetPeerSystems (uint32)

#### Method Qualifiers (GetPeerSystems)

Name | Data Type | Value
--- | --- | ---
Description | string | Get (or start a job to get) all of the peer systems. A peer system is a system that is known and visible to the Replication Service. Peer systems are discovered through discovery services and/or implementation specific services.If a job is started, once the job completes, examine the AffectedJobElement associations for the peer systems.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 4096, 4097..32767, 0x8000..
Values | string | Completed with No Error, Not Supported, Unspecified Error, Timeout, Failed, Invalid Parameter, In Use, DMTF Reserved, Method Parameters Checked - Job Started, Method Reserved, Vendor Specific

#### Method Parameters (GetPeerSystems)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
Options | uint16
Description | string | This parameter specifies which peer systems to return. If NULL, all known systems are returned, whether those systems are currently reachable or not.
IN | boolean | true
ValueMap | string | 2, 3, .., 0x8000..
Values | string | Only systems currently reachable, Include access points for systems currently reachable, DMTF Reserved, Vendor Specific
LocalAccessPoints | CIM_ServiceAccessPoint[]
ArrayType | string | Indexed
Description | string | An array of references to local ServiceAccessPoints (for example, ProtocolEndpoints) that allow communication to the remote system.
ModelCorrespondence | string | CIM_ReplicationService.GetPeerSystems(Systems)
OUT | boolean | true
RemoteAccessPoints | CIM_ServiceAccessPoint[]
ArrayType | string | Indexed
Description | string | An array of references to remote ServiceAccessPoints (for example, ProtocolEndpoints) that allow communication to the remote system.
ModelCorrespondence | string | CIM_ReplicationService.GetPeerSystems(Systems)
OUT | boolean | true
Systems | CIM_ComputerSystem[]
ArrayType | string | Indexed
Description | string | List of peer ComputerSystems.
ModelCorrespondence | string | CIM_ReplicationService.GetPeerSystems(LocalAccessPoints), CIM_ReplicationService.GetPeerSystems(RemoteAccessPoints)
OUT | boolean | true
Job | REF CIM_ConcreteJob
Description | string | Reference to the job (may be NULL if the task completed).
IN | boolean | false
OUT | boolean | true

#### GetReplicationRelationships (uint32)

#### Method Qualifiers (GetReplicationRelationships)

Name | Data Type | Value
--- | --- | ---
Description | string | Get (or start a job to get) all of the synchronization relationships known to the processing replication service. If a job is started, once the job completes, examine the AffectedJobElement associations for the synchronization relationships.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 4096, 4097..32767, 0x8000..
Values | string | Completed with No Error, Not Supported, Unspecified Error, Timeout, Failed, Invalid Parameter, In Use, DMTF Reserved, Method Parameters Checked - Job Started, Method Reserved, Vendor Specific

#### Method Parameters (GetReplicationRelationships)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
CopyState | uint16
Description | string | Only retrieve synchronization relationships that are currently in this CopyState. If this parameter is not supplied, relationships are retrieved regardless of their current CopyState.
IN | boolean | true
ModelCorrespondence | string | CIM_Synchronized.CopyState
Locality | uint16
Description | string | Describes the desired locality. If this parameter is not supplied, all replication relationships are retrieved, regardless of the locality of elements. Local only: Source and target elements are contained in the same system. Remote only: Source and target elements are contained in two different systems.
IN | boolean | true
ValueMap | string | 2, 3, .., 0x8000..
Values | string | Local only, Remote only, DMTF Reserved, Vendor Specific
Mode | uint16
Description | string | Describes the desired mode. If this parameter is not supplied, both all modes are retrieved. Adaptive: Allows implementation to dynamically switch between synchronous and asynchronous modes.
IN | boolean | true
ModelCorrespondence | string | CIM_Synchronized.Mode
ValueMap | string | 2, 3, 4, .., 0x8000..
Values | string | Synchronous, Asynchronous, Adaptive, DMTF Reserved, Vendor Specific
ReplicationSettingData | string
Description | string | If supplied, it provides additional replication settings to consider in locating the replication relationships, for example, the CopyMethodology -- which indicates how the copy operation is carried out -- for example, full or incremental mirroring.
EmbeddedInstance | string | CIM_ReplicationSettingData
IN | boolean | true
SyncType | uint16
Description | string | Describes the desired synchronization type. If this parameter is not specified, all SyncType are retrieved.
IN | boolean | true
ModelCorrespondence | string | CIM_Synchronized.SyncType
ValueMap | string | .., 6, 7, 8, 9, .., 0x8000..
Values | string | DMTF Reserved, Mirror, Snapshot, Clone, TokenizedClone, DMTF Reserved, Vendor Specific
Type | uint16
Description | string | The type of synchronization relationships, for example, StorageSynchronized or GroupSynchronized. If this parameter is not supplied, all such relationships are retrieved.
IN | boolean | true
ValueMap | string | 2, 3, .., 0x8000..
Values | string | StorageSynchronized, GroupSynchronized, DMTF Reserved, Vendor Specific
Synchronizations | CIM_Synchronized[]
Description | string | An array of elements found.
OUT | boolean | true
Job | REF CIM_ConcreteJob
Description | string | Reference to the job (may be NULL if the task completed).
IN | boolean | false
OUT | boolean | true

#### GetServiceAccessPoints (uint32)

#### Method Qualifiers (GetServiceAccessPoints)

Name | Data Type | Value
--- | --- | ---
Description | string | Get (or start a job to get) ServiceAccessPoints associated with a peer system. If a job is started, once the job completes, examine the AffectedJobElement associations for the peer system's ServiceAccessPoints.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 4096, 4097..32767, 0x8000..
Values | string | Completed with No Error, Not Supported, Unspecified Error, Timeout, Failed, Invalid Parameter, In Use, DMTF Reserved, Method Parameters Checked - Job Started, Method Reserved, Vendor Specific

#### Method Parameters (GetServiceAccessPoints)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
ServiceAccessPoints | CIM_ServiceAccessPoint[]
Description | string | List of ServiceAccessPoints for the supplied System.
OUT | boolean | true
Job | REF CIM_ConcreteJob
Description | string | Reference to the job (may be NULL if the task completed).
IN | boolean | false
OUT | boolean | true
System | REF CIM_ComputerSystem
Description | string | This parameter specifies the peer system.
IN | boolean | true
Required | boolean | true

#### AddReplicationEntity (uint32)

#### Method Qualifiers (AddReplicationEntity)

Name | Data Type | Value
--- | --- | ---
Description | string | Introduces a new instance of ReplicationEntity in the specified Namespace.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 0x8000..
Values | string | Completed with No Error, Not Supported, Unspecified Error, Timeout, Failed, Invalid Parameter, In Use, DMTF Reserved, Vendor Specific

#### Method Parameters (AddReplicationEntity)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
InstanceNamespace | string
Description | string | Namespace of created instance. If null, created instance will be in the same namespace as the service.
IN | boolean | true
Persistent | boolean
Description | string | If true, the instance must persist across Management Server reboot. If NULL, the value will be based on the default value of the class in the MOF. Use the intrinsic method ModifyInstance to change the Persistency value.
IN | boolean | true
ReplicationEntity | string
EmbeddedInstance | string | CIM_ReplicationEntity
IN | boolean | true
Required | boolean | true
ReplicationEntityPath | REF CIM_ReplicationEntity
Description | string | Reference to the created instance.
OUT | boolean | true

#### AddServiceAccessPoint (uint32)

#### Method Qualifiers (AddServiceAccessPoint)

Name | Data Type | Value
--- | --- | ---
Description | string | Introduces a new instance of a ServiceAccessPoint, or one of its subclasses, for example, a RemoteServiceAccessPoint in the specified namespace.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 0x8000..
Values | string | Completed with No Error, Not Supported, Unspecified Error, Timeout, Failed, Invalid Parameter, In Use, DMTF Reserved, Vendor Specific

#### Method Parameters (AddServiceAccessPoint)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
InstanceNamespace | string
Description | string | Namespace of created instance. If null, created instance will be in the same namespace as the service.
IN | boolean | true
ServiceAccessPoint | string
EmbeddedInstance | string | CIM_ServiceAccessPoint
IN | boolean | true
Required | boolean | true
ServiceAccessPointPath | REF CIM_ServiceAccessPoint
Description | string | Reference to the created instance.
OUT | boolean | true

#### AddSharedSecret (uint32)

#### Method Qualifiers (AddSharedSecret)

Name | Data Type | Value
--- | --- | ---
Description | string | Introduces a new instance of SharedSecret in the specified namespace and optionally associates it to an instance of a ServiceAccessPoint.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 0x8000..
Values | string | Completed with No Error, Not Supported, Unspecified Error, Timeout, Failed, Invalid Parameter, In Use, DMTF Reserved, Vendor Specific

#### Method Parameters (AddSharedSecret)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
InstanceNamespace | string
Description | string | Namespace of created instance. If null, created instance will be in the same namespace as the the service.
IN | boolean | true
SharedSecret | string
EmbeddedInstance | string | CIM_SharedSecret
IN | boolean | true
Required | boolean | true
ServiceAccessPoint | REF CIM_ServiceAccessPoint
Description | string | Associate created instance to this ServiceAccessPoint. If null, no such association is established.
IN | boolean | true
SharedSecretPath | REF CIM_SharedSecret
Description | string | Reference to the created instance.
OUT | boolean | true

#### CreateListReplica (uint32)

#### Method Qualifiers (CreateListReplica)

Name | Data Type | Value
--- | --- | ---
Description | string | Create (or start a job to create) new storage objects, which are replicas of the specified source storage objects (SourceElements). Note that using the input parameter, SyncType, this function can be used to instantiate the replicas, and to create an ongoing association between the source and replica elements. If 0 is returned, the function completed successfully and no ConcreteJob instance created. If 4096/0x1000 is returned, a ConcreteJob is started, a reference to which is returned in the Job output parameter.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 4096, 4097..32767, 0x8000..
Values | string | Completed with No Error, Not Supported, Unknown, Timeout, Failed, Invalid Parameter, In Use, DMTF Reserved, Method Parameters Checked - Job Started, Method Reserved, Vendor Specific

#### Method Parameters (CreateListReplica)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
Consistency | uint16
Description | string | Specifies whether consistency is to be maintained across the list of created replication relationships.
IN | boolean | true
ValueMap | string | 2, 3, .., 0x8000..
Values | string | No Consistency, Sequential Consistency, DMTF Reserved, Vendor Specific
Mode | uint16
Description | string | Mode describes whether the target elements will be updated synchronously or asynchronously. Adaptive: Allows implementation to dynamically switch between synchronous and asynchronous modes. If NULL, implementation decides the mode.
IN | boolean | true
ModelCorrespondence | string | CIM_Synchronized.Mode
ValueMap | string | 2, 3, 4, .., 0x8000..
Values | string | Synchronous, Asynchronous, Adaptive, DMTF Reserved, Vendor Specific
ReplicationSettingData | string
Description | string | If provided, it overrides the default replication setting data for the given SyncType. If not provided, the provider uses the default replication setting data. The same ReplicationSettingData applies to all SourceElements entries.
EmbeddedInstance | string | CIM_ReplicationSettingData
IN | boolean | true
SyncType | uint16
Description | string | SyncType describes the type of copy that will be made. The same SyncType applies to all elements in the list.
IN | boolean | true
ModelCorrespondence | string | CIM_Synchronized.SyncType
Required | boolean | true
ValueMap | string | .., 6, 7, 8, 9, .., 0x8000..
Values | string | DMTF Reserved, Mirror, Snapshot, Clone, TokenizedClone, DMTF Reserved, Vendor Specific
WaitForCopyState | uint16
Description | string | Method must wait until this CopyState is reached before returning. Only a subset of valid CopyStates apply. For example, Initialized: Associations have been established, but there is no data flow. Inactive: Initialization is complete, but the copy operation remains idle until it is activated. Synchronized: Replicas are an exact copy of the sources. UnSynchronized: Copy operation is in progress. If this parameter is supplied, then all the created replication relationships shall have this supplied CopyState before the method returns.
IN | boolean | true
ModelCorrespondence | string | CIM_Synchronized.CopyState
ElementNames | string[]
Description | string | An array of end user relevant names for the elements being created. If NULL, then a system supplied name is used. The value will be stored in the 'ElementName' property for the created element. The first element of the array ElementNames is assigned to the first replica, the second element to the second replica and so on. If there are more SourceElements entries than ElementNames, the system supplied name is used.
IN | boolean | true
Collections | CIM_Collection[]
Description | string | The target elements are added to each referenced collection, for example, DeviceMaskingGroups.
IN | boolean | true
SourceElements | CIM_LogicalElement[]
Description | string | A list of source storage objects which may be StorageVolumes or other storage objects. All the source elements shall be of the same type -- for example, all StorageVolumes.
IN | boolean | true
Required | boolean | true
Synchronizations | CIM_Synchronized[]
Description | string | Reference to the created associations between the source and the target elements. If a job is created, this parameter may be NULL unless the associations are actually formed.
IN | boolean | false
OUT | boolean | true
TargetElements | CIM_LogicalElement[]
Description | string | Optionally, as an input, refers to the target elements to use. If specified, the elements will match one to one with SourceElements[]. As an output, refers to the created target storage elements (i.e., the replicas). If a job is created, the target elements may not be available immediately.
IN | boolean | true
OUT | boolean | true
ConnectivityCollection | REF CIM_ConnectivityCollection
Description | string | Reference to the ConnectivityCollection - for example, a RemoteReplicationCollection. Since a RemoteReplicationCollection aggregates the ProtocolEndpoints that provide the paths to a remote system, generally, it is not necessary to supply both the ConnectivityCollection and the ServiceAccessPoint.
IN | boolean | true
Job | REF CIM_ConcreteJob
Description | string | Reference to the job (may be NULL if job is completed).
IN | boolean | false
OUT | boolean | true
SourceAccessPoint | REF CIM_ServiceAccessPoint
Description | string | Reference to source access point information. If NULL, service does not need access information to access the source element. This parameter applies to all elements in the source list.
IN | boolean | true
TargetAccessPoint | REF CIM_ServiceAccessPoint
Description | string | Reference to target access point information. If NULL, service does not need access information to access the target elements. This parameter applies to all elements in the target list.
IN | boolean | true
TargetPool | REF CIM_ResourcePool
Description | string | The underlying storage for the target elements (the replicas) will be drawn from TargetPool if specified, otherwise the allocation is implementation specific. If the target elements are supplied, this parameter shall be NULL. This parameter applies to all elements in the target list.
IN | boolean | true
TargetSettingGoal | REF CIM_SettingData
Description | string | The definition for the SettingData to be maintained by the target storage objects (the replicas). If the target elements are supplied, this parameter shall be NULL. This parameter applies to all elements in the target list.
IN | boolean | true

#### CreateGroupReplicaFromElements (uint32)

#### Method Qualifiers (CreateGroupReplicaFromElements)

Name | Data Type | Value
--- | --- | ---
Description | string | Create (or start a job to create) new storage objects, which are replicas of the specified source storage objects (SourceElements). Note that using the input parameter, SyncType, this function can be used to instantiate the replicas, and to create an ongoing association between the source and replica elements. If 0 is returned, the function completed successfully and no ConcreteJob instance created. If 4096/0x1000 is returned, a ConcreteJob is started, a reference to which is returned in the Job output parameter. This method combines the functionality of CreateGroup and CreateGroupReplica, in one call.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 4096, 4097..32767, 0x8000..
Values | string | Completed with No Error, Not Supported, Unknown, Timeout, Failed, Invalid Parameter, In Use, DMTF Reserved, Method Parameters Checked - Job Started, Method Reserved, Vendor Specific

#### Method Parameters (CreateGroupReplicaFromElements)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
Consistency | uint16
Description | string | Overrides the default group consistency.
IN | boolean | true
ValueMap | string | 2, 3, .., 0x8000..
Values | string | No Consistency, Sequential Consistency, DMTF Reserved, Vendor Specific
Mode | uint16
Description | string | Mode describes whether the target elements will be updated synchronously or asynchronously. Adaptive: Allows implementation to dynamically switch between synchronous and asynchronous modes. If NULL, implementation decides the mode.
IN | boolean | true
ModelCorrespondence | string | CIM_Synchronized.Mode
ValueMap | string | 2, 3, 4, .., 0x8000..
Values | string | Synchronous, Asynchronous, Adaptive, DMTF Reserved, Vendor Specific
RelationshipName | string
Description | string | A user relevant name for the relationship between the source and target groups or between a source element and a target group (i.e. one-to-many). If NULL, the implementation assigns a name. If the individual target elements require an ElementName, the implementation constructs an appropriate ElementName using the RelationshipName. For example, RelationshipName as a prefix followed by "_n" sequence number, where n is a number beginning with 1.
IN | boolean | true
ReplicationSettingData | string
Description | string | If provided, it overrides the default replication setting data for the given SyncType. If not provided, the management server uses the default replication setting data.
EmbeddedInstance | string | CIM_ReplicationSettingData
IN | boolean | true
SourceGroupName | string
Description | string | As in parameter, the name of the group to be created. If the name is not supplied, the implementation may assign a group name and return it in this parameter.
IN | boolean | true
OUT | boolean | true
SyncType | uint16
Description | string | SyncType describes the type of copy that will be made.
IN | boolean | true
ModelCorrespondence | string | CIM_Synchronized.SyncType
Required | boolean | true
ValueMap | string | .., 6, 7, 8, 9, .., 0x8000..
Values | string | DMTF Reserved, Mirror, Snapshot, Clone, TokenizedClone, DMTF Reserved, Vendor Specific
TargetGroupName | string
Description | string | As in parameter, the name of the group to be created. If the name is not supplied, the implementation may assign a group name and return it in this parameter.
IN | boolean | true
OUT | boolean | true
WaitForCopyState | uint16
Description | string | Method must wait until this CopyState is reached before returning. Only a subset of valid CopyStates apply. For example, Initialized: Associations have been established, but there is no data flow. Inactive: Initialization is complete, but the data flow remains idle until it is activated. Synchronized: Replicas are an exact copy of the source. UnSynchronized: Copy operation is in progress.
IN | boolean | true
ModelCorrespondence | string | CIM_Synchronized.CopyState
TargetElementNames | string[]
Description | string | An array of end user relevant names for the elements being created. If NULL, then a system supplied name is used. The value will be stored in the 'ElementName' property for the created elements.
IN | boolean | true
Collections | CIM_Collection[]
Description | string | The target elements are added to each referenced collection, for example, DeviceMaskingGroups.
IN | boolean | true
SourceElements | CIM_LogicalElement[]
Description | string | A list of source storage objects which may be StorageVolumes or other storage objects. All the source elements shall be of the same type -- for example, all StorageVolumes.
IN | boolean | true
Required | boolean | true
TargetElements | CIM_LogicalElement[]
Description | string | A list of target storage objects which may be StorageVolumes or other storage objects. All the target elements shall be of the same type -- for example, all StorageVolumes.
IN | boolean | true
TargetPools | CIM_ResourcePool[]
Description | string | The underlying storage for the target elements (the replicas) will be drawn from TargetPools if specified, otherwise the allocation is implementation specific. If target elements are supplied, this parameter shall be NULL.supplied, this parameter shall be NULL. If TargetPools supplied, TargetPool shall be NULL.
IN | boolean | true
ConnectivityCollection | REF CIM_ConnectivityCollection
Description | string | Reference to the ConnectivityCollection - for example, a RemoteReplicationCollection. Since a RemoteReplicationCollection aggregates the ProtocolEndpoints that provide the paths to a remote system, generally, it is not necessary to supply both the ConnectivityCollection and the ServiceAccessPoint.
IN | boolean | true
Job | REF CIM_ConcreteJob
Description | string | Reference to the job (may be NULL if job is completed).
IN | boolean | false
OUT | boolean | true
SourceAccessPoint | REF CIM_ServiceAccessPoint
Description | string | Reference to source access point information. If NULL, service does not need access information to access the source elements.
IN | boolean | true
SourceGroup | REF CIM_ReplicationGroup
Description | string | Optionally, as an input, refers to a source group to use. As an output, refers to the created source group (i.e., the replica group). If a job is created, the source group may not be available immediately.
IN | boolean | true
OUT | boolean | true
Synchronization | REF CIM_Synchronized
Description | string | Reference to the created group association between the source and the target elements. If a job is created, this parameter may be NULL until the association is actually formed.
IN | boolean | false
OUT | boolean | true
TargetAccessPoint | REF CIM_ServiceAccessPoint
Description | string | Reference to target access point information. If NULL, service does not need access information to access the target element/group.
IN | boolean | true
TargetGroup | REF CIM_ReplicationGroup
Description | string | Optionally, as an input, refers to a target group to use. As an output, refers to the created target group (i.e., the replica group). If a job is created, the target group may not be available immediately.
IN | boolean | true
OUT | boolean | true
TargetPool | REF CIM_ResourcePool
Description | string | The underlying storage for the target elements (the replicas) will be drawn from TargetPool if specified, otherwise the allocation is implementation specific. If target elements are supplied, this parameter shall be NULL. If TargetPool supplied, TargetPools shall be NULL.
IN | boolean | true
TargetSettingGoal | REF CIM_SettingData
Description | string | The definition for the SettingData to be maintained by the target storage objects (the replicas). If target elements are supplied, this parameter shall be NULL.
IN | boolean | true

#### GetReplicationRelationshipInstances (uint32)

#### Method Qualifiers (GetReplicationRelationshipInstances)

Name | Data Type | Value
--- | --- | ---
Description | string | Get (or start a job to get) all of the synchronization relationships known to the processing replication service. If a job is started, once the job completes, examine the AffectedJobElement associations for the synchronization relationships. This method is similar to GetReplicationRelationships, except that this method returns the instances as opposed to object paths.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 4096, 4097..32767, 0x8000..
Values | string | Completed with No Error, Not Supported, Unspecified Error, Timeout, Failed, Invalid Parameter, In Use, DMTF Reserved, Method Parameters Checked - Job Started, Method Reserved, Vendor Specific

#### Method Parameters (GetReplicationRelationshipInstances)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
CopyState | uint16
Description | string | Only retrieve synchronization relationships that are currently in this CopyState. If this parameter is not supplied, relationships are retrieved regardless of their current CopyState.
IN | boolean | true
ModelCorrespondence | string | CIM_Synchronized.CopyState
Locality | uint16
Description | string | Describes the desired locality. If this parameter is not supplied, all replication relationships are retrieved, regardless of the locality of elements. Local only: Source and target elements are contained in the same system. Remote only: Source and target elements are contained in two different systems.
IN | boolean | true
ValueMap | string | 2, 3, .., 0x8000..
Values | string | Local only, Remote only, DMTF Reserved, Vendor Specific
Mode | uint16
Description | string | Describes the desired mode. If this parameter is not supplied, all modes are retrieved. Adaptive: Allows implementation to dynamically switch between synchronous and asynchronous modes.
IN | boolean | true
ModelCorrespondence | string | CIM_Synchronized.Mode
ValueMap | string | 2, 3, 4, .., 0x8000..
Values | string | Synchronous, Asynchronous, Adaptive, DMTF Reserved, Vendor Specific
ReplicationSettingData | string
Description | string | If supplied, it provides additional replication settings to consider in locating the replication relationships, for example, the CopyMethodology -- which indicates how the copy operation is carried out -- for example, full or incremental mirroring.
EmbeddedInstance | string | CIM_ReplicationSettingData
IN | boolean | true
SyncType | uint16
Description | string | Describes the desired synchronization type. If this parameter is not specified, all SyncType are retrieved.
IN | boolean | true
ModelCorrespondence | string | CIM_Synchronized.SyncType
ValueMap | string | .., 6, 7, 8, 9, .., 0x8000..
Values | string | DMTF Reserved, Mirror, Snapshot, Clone, TokenizedClone, DMTF Reserved, Vendor Specific
Type | uint16
Description | string | The type of synchronization relationships, for example, StorageSynchronized or GroupSynchronized. If this parameter is not supplied, all such relationships are retrieved.
IN | boolean | true
ValueMap | string | 2, 3, .., 0x8000..
Values | string | StorageSynchronized, GroupSynchronized, DMTF Reserved, Vendor Specific
Synchronizations | string[]
Description | string | An array of instances found.
EmbeddedInstance | string | CIM_Synchronized
OUT | boolean | true
Job | REF CIM_ConcreteJob
Description | string | Reference to the job (may be NULL if the task completed).
IN | boolean | false
OUT | boolean | true

#### ModifyListSettingsDefineState (uint32)

#### Method Qualifiers (ModifyListSettingsDefineState)

Name | Data Type | Value
--- | --- | ---
Description | string | Modify (or start a job to modify) the SettingsDefineState associations between the storage objects and instances of SynchronizationAspect. The modification could range from introducing the target elements, which creates new StorageSynchronized associations to dissolving the SettingsDefineState associations. If 0 is returned, the function completed successfully and no ConcreteJob instance was created. If 4096/0x1000 is returned, a ConcreteJob was started and a reference to this Job is returned in the Job output parameter. A return value of 1 indicates the method is not supported. All other values indicate some type of error condition.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 4096, 4097..32767, 0x8000..
Values | string | Completed with No Error, Not Supported, Unspecified Error, Timeout, Failed, Invalid Parameter, In Use, DMTF Reserved, Method Parameters Checked - Job Started, Method Reserved, Vendor Specific

#### Method Parameters (ModifyListSettingsDefineState)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
Operation | uint16
Description | string | Operation describes the type of modification to be made to the related associations. Activate Consistency: if consistency was not requested when CreateListSynchronizationAspect was called. If Consistency is already active, no modification is made. Deactivate Consistency: Deactivate consistency. If consistency was not enabled, this operation has no effect. Delete: Remove the SettingsDefineState association. Copy To Target: Introduces the target elements and forms the necessary associations between the source and the target elements i.e. StorageSynchronized and GroupSynchronized. Detach: Removes the association between the SynchronizationAspect and the target element. Restore: Restore the source element from the associated SynchronizationAspect. Attach To Target: Same as Copy To Target except no data is copied.
IN | boolean | true
Required | boolean | true
ValueMap | string | 2, 3, 4, 5, 6, 7, 8, .., 0x8000..0xFFFF
Values | string | Activate Consistency, Deactivate Consistency, Delete, Copy To Target, Detach, Restore, Attach To Target, DMTF Reserved, Vendor Specific
ReplicationSettingData | string
Description | string | If provided, it overrides the default replication setting data for the given SyncType. If not provided, the management server uses the default replication setting data.
EmbeddedInstance | string | CIM_ReplicationSettingData
IN | boolean | true
TargetElementCount | uint64
Description | string | This parameter applies to one-source-to-many-target- elements. It is possible to create multiple copies of the source elements. If TargetCount is supplied, TargetElements and TargetGroups shall be NULL.
IN | boolean | true
WaitForCopyState | uint16
Description | string | Method must wait until this CopyState is reached before returning. Only a subset of valid CopyStates apply. For example, Initialized: Associations have been established, but there is no data flow. Inactive: Initialization is complete, but the data flow remains idle until it is activated. Synchronized: Replicas are an exact copy of the source. UnSynchronized: Copy operation is in progress. Fractured/Split: Target elements are separated from the source elements. Etc.
IN | boolean | true
ModelCorrespondence | string | CIM_Synchronized.CopyState
ElementNames | string[]
Description | string | A end user relevant name for the elements being created. If NULL, then a system supplied default names can be used. The value will be stored in the 'ElementName' property for the created elements.
IN | boolean | true
Collections | CIM_Collection[]
Description | string | The target elements are added to each referenced collection, for example, DeviceMaskingGroups.
IN | boolean | true
SettingsStates | CIM_SettingsDefineState[]
Description | string | References to the associations between the source elements and instances of SynchronizationAspect.
IN | boolean | true
Required | boolean | true
Synchronizations | CIM_Synchronized[]
Description | string | References to the created replication associations describing the elements/groups relationships.
IN | boolean | false
OUT | boolean | true
TargetElements | CIM_LogicalElement[]
Description | string | Optionally, as an input, refers to target elements to use. If TargetElements are supplied, TargetGroups and TargetCount shall be NULL. As an output, refers to the created target storage elements (i.e., the replicas). If a job is created, the target elements may not be available immediately.
IN | boolean | true
OUT | boolean | true
TargetGroups | CIM_ReplicationGroup[]
Description | string | Optionally, as an input, refers to a target groups to use. If TargetGroups are supplied, TargetElements and TargetCount shall be NULL. As an output, refers to the created target groups (i.e., the replica groups). If a job is created, the target groups may not be available immediately. If TargetGroups are supplied, TargetElementCount shall be NULL.
IN | boolean | true
OUT | boolean | true
TargetPools | CIM_ResourcePool[]
Description | string | The underlying storage for the target elements (the replicas) will be drawn from TargetPools if specified, otherwise the allocation is implementation specific. If target elements are supplied, this parameter shall be NULL.
IN | boolean | true
TargetSettingGoals | CIM_SettingData[]
Description | string | The definition for the SettingData to be maintained by the target storage objects (the replicas). If the target elementsare supplied, this parameter shall be NULL.
IN | boolean | true
Job | REF CIM_ConcreteJob
Description | string | Reference to the job (may be NULL if the task completed).
IN | boolean | false
OUT | boolean | true
TargetAccessPoint | REF CIM_ServiceAccessPoint
Description | string | Reference to target access point information. If NULL, service does not need access information to access the target elements/groups.
IN | boolean | true

#### AddToRemoteReplicationCollection (uint32)

#### Method Qualifiers (AddToRemoteReplicationCollection)

Name | Data Type | Value
--- | --- | ---
Description | string | Add (or start a job to add) additional service access points (i.e. ProtocolEndpoints) and/or remote systems associations to an existing instance of RemoteReplicationCollection.If 0 is returned, the function completed successfully and no ConcreteJob instance created. If 4096/0x1000 is returned, a ConcreteJob is started, a reference to which is returned in the Job output parameter. If parameter AccessPoints is NULL, then only the RemoteComputerSystem is added for the existing AccessPoints associated to the RemoteReplicationCollection. If RemoteComputerSystem is NULL, then only AccessPoints are added for the existing remote ComputerSystems known to the RemoteReplicationCollection.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 4096, 4097..32767, 0x8000..
Values | string | Completed with No Error, Not Supported, Unknown, Timeout, Failed, Invalid Parameter, In Use, DMTF Reserved, Method Parameters Checked - Job Started, Method Reserved, Vendor Specific

#### Method Parameters (AddToRemoteReplicationCollection)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
LocalAccessPoints | CIM_ServiceAccessPoint[]
Description | string | An array of references to local ServiceAccessPoints (for example, ProtocolEndpoints) that allow communication to the remote system.
IN | boolean | true
RemoteAccessPoints | CIM_ServiceAccessPoint[]
Description | string | An array of references to remote ServiceAccessPoints (for example, ProtocolEndpoints) that allow communication to the remote system.
IN | boolean | true
ConnectivityCollection | REF CIM_ConnectivityCollection
Description | string | The reference to the RemoteReplicationCollection to be expanded.
IN | boolean | true
Required | boolean | true
Job | REF CIM_ConcreteJob
Description | string | Reference to the job (may be NULL if job is completed).
IN | boolean | false
OUT | boolean | true
RemoteComputerSystem | REF CIM_ComputerSystem
Description | string | A reference to the remote system.
IN | boolean | true

#### CreateRemoteReplicationCollection (uint32)

#### Method Qualifiers (CreateRemoteReplicationCollection)

Name | Data Type | Value
--- | --- | ---
Description | string | Create (or start a job to create) a new instance of RemoteReplicationCollection, and optionally supply the remote system and the paths (i.e. ProtocolEndpoints) that are used to perform replication operations to/from the remote system. If 0 is returned, the function completed successfully and no ConcreteJob instance created. If 4096/0x1000 is returned, a ConcreteJob is started, a reference to which is returned in the Job output parameter. Once the job completes, examine the AffectedJobElement associations for the created instance of RemoteReplicationCollection.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 4096, 4097..32767, 0x8000..
Values | string | Completed with No Error, Not Supported, Unknown, Timeout, Failed, Invalid Parameter, In Use, DMTF Reserved, Method Parameters Checked - Job Started, Method Reserved, Vendor Specific

#### Method Parameters (CreateRemoteReplicationCollection)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
Active | boolean
Description | string | If true, the instance of RemoteReplicationCollection will be enabled and allows replication operations to to the remote system. Use the intrinsic method ModifyInstance to change this property after the RemoteReplicationCollection is created.
IN | boolean | true
DeleteOnUnassociated | boolean
Description | string | If true, the instance of RemoteReplicationCollection will be deleted when it is no longer associated to a ServiceAccessPoint. Use the intrinsic method ModifyInstance to change this property after the RemoteReplicationCollection is created.
IN | boolean | true
ElementName | string
Description | string | A end user relevant name for the element being created. If NULL, then a system supplied default name can be used. The value will be stored in the 'ElementName' property for the created element.
IN | boolean | true
ReplicationSettingData | string
Description | string | If supplied, it provides additional replication settings for the method. For example, enable data compression.
EmbeddedInstance | string | CIM_ReplicationSettingData
IN | boolean | true
LocalAccessPoints | CIM_ServiceAccessPoint[]
Description | string | An array of references to local ServiceAccessPoints (for example, ProtocolEndpoints) that allow communication to the remote system.
IN | boolean | true
RemoteAccessPoints | CIM_ServiceAccessPoint[]
Description | string | An array of references to remote ServiceAccessPoints (for example, ProtocolEndpoints) that allow communication to the remote system.
IN | boolean | true
ConnectivityCollection | REF CIM_ConnectivityCollection
Description | string | Reference to the created instance of RemoteReplicationCollection.
IN | boolean | false
OUT | boolean | true
Job | REF CIM_ConcreteJob
Description | string | Reference to the job (may be NULL if job is completed).
IN | boolean | false
OUT | boolean | true
RemoteComputerSystem | REF CIM_ComputerSystem
Description | string | A reference to the remote system.
IN | boolean | true

#### RemoveFromRemoteReplicationCollection (uint32)

#### Method Qualifiers (RemoveFromRemoteReplicationCollection)

Name | Data Type | Value
--- | --- | ---
Description | string | Remove (or start a job to remove) service access points (i.e. ProtocolEndpoints) and/or remote systems associations from an existing instance of RemoteReplicationCollection.If 0 is returned, the function completed successfully and no ConcreteJob instance created. If 4096/0x1000 is returned, a ConcreteJob is started, a reference to which is returned in the Job output parameter. If parameter AccessPoints is NULL, then only the remote ComputerSystem is removed for the existing AccessPoints associated to the RemoteReplicationCollection. If ComputerSystem is NULL, then only AccessPoints are removed from the existing remote ComputerSystems known to the RemoteReplicationCollection.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 4096, 4097..32767, 0x8000..
Values | string | Completed with No Error, Not Supported, Unknown, Timeout, Failed, Invalid Parameter, In Use, DMTF Reserved, Method Parameters Checked - Job Started, Method Reserved, Vendor Specific

#### Method Parameters (RemoveFromRemoteReplicationCollection)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
LocalAccessPoints | CIM_ServiceAccessPoint[]
Description | string | An array of references to local ServiceAccessPoints (for example, ProtocolEndpoints) that allow communication to the remote system.
IN | boolean | true
RemoteAccessPoints | CIM_ServiceAccessPoint[]
Description | string | An array of references to remote ServiceAccessPoints (for example, ProtocolEndpoints) that allow communication to the remote system.
IN | boolean | true
ConnectivityCollection | REF CIM_ConnectivityCollection
Description | string | The reference to the RemoteReplicationCollection to affect.
IN | boolean | true
Required | boolean | true
Job | REF CIM_ConcreteJob
Description | string | Reference to the job (may be NULL if job is completed).
IN | boolean | false
OUT | boolean | true
RemoteComputerSystem | REF CIM_ComputerSystem
Description | string | A reference to the remote system to remove.
IN | boolean | true

#### AddElementsToGroupSynchronized (uint32)

#### Method Qualifiers (AddElementsToGroupSynchronized)

Name | Data Type | Value
--- | --- | ---
Description | string | Add elements (or start a job to add elements) to replication groups of a GroupSynchronized association. The implementation then creates StorageSynchronized associations between the matching added elements. If 4096/0x1000 is returned, a ConcreteJob is started, a reference to which is returned in the Job output parameter.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 4096, 4097..32767, 0x8000..
Values | string | Completed with No Error, Not Supported, Unknown, Timeout, Failed, Invalid Parameter, In Use, DMTF Reserved, Method Parameters Checked - Job Started, Method Reserved, Vendor Specific

#### Method Parameters (AddElementsToGroupSynchronized)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
Consistency | uint16
Description | string | Overrides the default group consistency.
IN | boolean | true
ValueMap | string | 2, 3, .., 0x8000..
Values | string | No Consistency, Sequential Consistency, DMTF Reserved, Vendor Specific
ReplicationSettingData | string
Description | string | If provided, it overrides the default replication setting data for the given SyncType. If not provided, the management server uses the default replication setting data.
EmbeddedInstance | string | CIM_ReplicationSettingData
IN | boolean | true
WaitForCopyState | uint16
Description | string | Method must wait until this CopyState is reached before returning. Only a subset of valid CopyStates apply. For example, Initialized: Associations have been established, but there is no data flow. Inactive: Initialization is complete, but the data flow remains idle until it is activated. Synchronized: Replicas are an exact copy of the source. UnSynchronized: Copy operation is in progress.
IN | boolean | true
ModelCorrespondence | string | CIM_Synchronized.CopyState
SourceElements | CIM_LogicalElement[]
ArrayType | string | Indexed
Description | string | Reference to the elements to add to the source group.
IN | boolean | true
ModelCorrespondence | string | CIM_ReplicationService.AddElementsToGroupSynchronized(TargetElements)
Synchronizations | CIM_Synchronized[]
Description | string | Reference to the created associations between the source and the target elements. If a job is created, this parameter may be NULL until the associations is actually formed.
IN | boolean | false
OUT | boolean | true
TargetElements | CIM_LogicalElement[]
ArrayType | string | Indexed
Description | string | Reference to the elements to add to the target group. Pairing of source and target elements is controlled by the Pairing property of ReplicationSettingData if supplied, otherwise, based on default ReplicationSettingData.
IN | boolean | true
ModelCorrespondence | string | CIM_ReplicationService.AddElementsToGroupSynchronized(SourceElements)
Job | REF CIM_ConcreteJob
Description | string | Reference to the job (may be NULL if job is completed).
IN | boolean | false
OUT | boolean | true
SourceAccessPoint | REF CIM_ServiceAccessPoint
Description | string | Reference to source access point information. If NULL, service does not need access information to access the source element/group.
IN | boolean | true
Synchronized | REF CIM_Synchronized
Description | string | Reference to the Synchronized association.
IN | boolean | true
TargetAccessPoint | REF CIM_ServiceAccessPoint
Description | string | Reference to target access point information. If NULL, service does not need access information to access the target element/group.
IN | boolean | true

#### ConfirmTargetData (uint32)

#### Method Qualifiers (ConfirmTargetData)

Name | Data Type | Value
--- | --- | ---
Description | string | Confirm data written to the source elements has been replicated to the target elements. This method is useful for asynchronous replication where data written to the source elements may not be replicated to the target elements right away. If 4096/0x1000 is returned, a ConcreteJob is started, a reference to which is returned in the Job output parameter.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, .., 4096, 4097..32767, 0x8000..
Values | string | Completed with No Error, Not Supported, Unknown, Timeout, Failed, Invalid Parameter, In Use, Unable to confirm target data, DMTF Reserved, Method Parameters Checked - Job Started, Method Reserved, Vendor Specific

#### Method Parameters (ConfirmTargetData)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
ReplicationSettingData | string
Description | string | If provided, it overrides the default replication setting data for the given SyncType. If not provided, the management server uses the default replication setting data.
EmbeddedInstance | string | CIM_ReplicationSettingData
IN | boolean | true
WaitTime | datetime
Description | string | It specifies the interval of time to wait to confirm data is written to the target elements. For example, to wait 5 minutes, the value would be 00000000000500.000000:000, using the CIM interval format. If NULL or 0, the implementation decides the interval. If the WaitTime expires before the target data is confirmed, the method will return "3" (Timeout).
IN | boolean | true
ConnectivityCollection | REF CIM_ConnectivityCollection
Description | string | Reference to the ConnectivityCollection - for example, a RemoteReplicationCollection. Since a RemoteReplicationCollection aggregates the ProtocolEndpoints that provide the paths to a remote system, generally, it is not necessary to supply both the ConnectivityCollection and the ServiceAccessPoint.
IN | boolean | true
Job | REF CIM_ConcreteJob
Description | string | Reference to the job (may be NULL if job is completed).
IN | boolean | false
OUT | boolean | true
SourceAccessPoint | REF CIM_ServiceAccessPoint
Description | string | Reference to source access point information. If NULL, service does not need access information to access the source element/group.
IN | boolean | true
Synchronized | REF CIM_Synchronized
Description | string | Reference to the Synchronized association. For example, a StorageSynchronized or a GroupSynchronized.
IN | boolean | true
TargetAccessPoint | REF CIM_ServiceAccessPoint
Description | string | Reference to target access point information. If NULL, service does not need access information to access the target element/group.
IN | boolean | true

#### CreateGroupReplicaFromElementSynchronizations (uint32)

#### Method Qualifiers (CreateGroupReplicaFromElementSynchronizations)

Name | Data Type | Value
--- | --- | ---
Description | string | Based on existing storage element synchronizations, create (or start a job to create) the source and target groups, add the elements into the groups and create an ongoing association between the groups. If 0 is returned, the function completed successfully and no ConcreteJob instance created. If 4096/0x1000 is returned, a ConcreteJob is started, a reference to which is returned in the Job output parameter.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 4096, 4097..32767, 0x8000..
Values | string | Completed with No Error, Not Supported, Unknown, Timeout, Failed, Invalid Parameter, In Use, DMTF Reserved, Method Parameters Checked - Job Started, Method Reserved, Vendor Specific

#### Method Parameters (CreateGroupReplicaFromElementSynchronizations)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
Consistency | uint16
Description | string | Overrides the default group consistency.
IN | boolean | true
ValueMap | string | 2, 3, .., 0x8000..
Values | string | No Consistency, Sequential Consistency, DMTF Reserved, Vendor Specific
RelationshipName | string
Description | string | A user relevant name for the relationship between the source and target group. If NULL, the implementation assigns a name. If the target group requires an ElementName, the implementation constructs an appropriate ElementName using the RelationshipName. For example, RelationshipName as a prefix followed by "_n" sequence number, where n is a number beginning with 1.
IN | boolean | true
ReplicationSettingData | string
Description | string | If provided, it overrides the default replication setting data for the given SyncType. If not provided, the management server uses the default replication setting data.
EmbeddedInstance | string | CIM_ReplicationSettingData
IN | boolean | true
SourceGroupName | string
Description | string | As in parameter, the name of the source group to be created. If the name is not supplied, the implementation may assign a group name and return it in this parameter.
IN | boolean | true
OUT | boolean | true
TargetGroupName | string
Description | string | As in parameter, the name of the target group to be created. If the name is not supplied, the implementation may assign a group name and return it in this parameter.
IN | boolean | true
OUT | boolean | true
WaitForCopyState | uint16
Description | string | Method must wait until this CopyState is reached before returning. Only a subset of valid CopyStates apply. For example, Initialized: Associations have been established, but there is no data flow. Inactive: Initialization is complete, but the data flow remains idle until it is activated. Synchronized: Replicas are an exact copy of the source. UnSynchronized: Copy operation is in progress.
IN | boolean | true
ModelCorrespondence | string | CIM_Synchronized.CopyState
ElementSynchronizations | CIM_Synchronized[]
Description | string | Reference to the associations between the source and the target elements.
IN | boolean | true
GroupSynchronization | REF CIM_Synchronized
Description | string | Reference to the created group association between the source and the target elements. If a job is created, this parameter may be NULL until the association is actually formed.
IN | boolean | false
OUT | boolean | true
Job | REF CIM_ConcreteJob
Description | string | Reference to the job (may be NULL if job is completed).
IN | boolean | false
OUT | boolean | true
SourceAccessPoint | REF CIM_ServiceAccessPoint
Description | string | Reference to source access point information. If NULL, service does not need access information to access the source elements.
IN | boolean | true
SourceGroup | REF CIM_ReplicationGroup
Description | string | Optionally, as an input, refers to a source group to use. As an output, refers to the created source group (i.e., the replica group). If a job is created, the source group may not be available immediately.
IN | boolean | true
OUT | boolean | true
TargetAccessPoint | REF CIM_ServiceAccessPoint
Description | string | Reference to target access point information. If NULL, service does not need access information to access the target element/group.
IN | boolean | true
TargetGroup | REF CIM_ReplicationGroup
Description | string | Optionally, as an input, refers to a target group to use. As an output, refers to the created target group (i.e., the replica group). If a job is created, the target group may not be available immediately.
IN | boolean | true
OUT | boolean | true

#### GetSynchronizationAspectInstances (uint32)

#### Method Qualifiers (GetSynchronizationAspectInstances)

Name | Data Type | Value
--- | --- | ---
Description | string | Get (or start a job to get) all of the instances of synchronization aspects known to the processing replication service. If a job is started, once the job completes, examine the AffectedJobElement associations for the synchronization aspects.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 4096, 4097..32767, 0x8000..
Values | string | Completed with No Error, Not Supported, Unspecified Error, Timeout, Failed, Invalid Parameter, In Use, DMTF Reserved, Method Parameters Checked - Job Started, Method Reserved, Vendor Specific

#### Method Parameters (GetSynchronizationAspectInstances)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
CachedData | boolean
Description | string | If true, for faster response, retrieve the data from the local cache. If false retrieve the most up-to-date data by examining each relationship's updated state. If not specified, the implementation decides.
IN | boolean | true
Locality | uint16
Description | string | Describes the desired locality. If this parameter is not supplied, all synchronization aspects are retrieved, regardless of the locality of elements. Local only: Source and aspect are contained in the same system. Remote only: Source and aspect elements are contained in two different systems.
IN | boolean | true
ValueMap | string | 2, 3, .., 0x8000..
Values | string | Local only, Remote only, DMTF Reserved, Vendor Specific
Mode | uint16
Description | string | Describes the desired mode. If this parameter is not supplied, all modes are retrieved. Adaptive: Allows implementation to dynamically switch between synchronous and asynchronous modes.
IN | boolean | true
ModelCorrespondence | string | CIM_Synchronized.Mode
ValueMap | string | 2, 3, 4, .., 0x8000..
Values | string | Synchronous, Asynchronous, Adaptive, DMTF Reserved, Vendor Specific
ReplicationSettingData | string
Description | string | If supplied, it provides additional replication settings to consider in locating the replication relationships, for example, the CopyMethodology.
EmbeddedInstance | string | CIM_ReplicationSettingData
IN | boolean | true
SyncState | uint16
Description | string | Only retrieve synchronization aspects that are currently in this SyncState. If this parameter is not supplied, synchronization aspects are retrieved regardless of their current SyncState.
IN | boolean | true
ModelCorrespondence | string | CIM_SynchronizationAspect.SyncState
SyncType | uint16
Description | string | Describes the desired synchronization type. If this parameter is not specified, all SyncType are retrieved.
IN | boolean | true
ModelCorrespondence | string | CIM_Synchronized.SyncType
ValueMap | string | .., 6, 7, 8, 9, .., 0x8000..
Values | string | DMTF Reserved, Mirror, Snapshot, Clone, TokenizedClone, DMTF Reserved, Vendor Specific
SynchronizationAspects | string[]
Description | string | An array of instances found.
EmbeddedInstance | string | CIM_SynchronizationAspect
OUT | boolean | true
Job | REF CIM_ConcreteJob
Description | string | Reference to the job (may be NULL if the task completed).
IN | boolean | false
OUT | boolean | true

#### GetSynchronizationAspects (uint32)

#### Method Qualifiers (GetSynchronizationAspects)

Name | Data Type | Value
--- | --- | ---
Description | string | Get (or start a job to get) all of the synchronization aspects known to the processing replication service. If a job is started, once the job completes, examine the AffectedJobElement associations for the synchronization aspects.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 4096, 4097..32767, 0x8000..
Values | string | Completed with No Error, Not Supported, Unspecified Error, Timeout, Failed, Invalid Parameter, In Use, DMTF Reserved, Method Parameters Checked - Job Started, Method Reserved, Vendor Specific

#### Method Parameters (GetSynchronizationAspects)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
CachedData | boolean
Description | string | If true, for faster response, retrieve the data from the local cache. If false retrieve the most up-to-date data by examining each relationship's updated state. If not specified, the implementation decides.
IN | boolean | true
Locality | uint16
Description | string | Describes the desired locality. If this parameter is not supplied, all synchronization aspects are retrieved, regardless of the locality of elements. Local only: Source and aspect are contained in the same system. Remote only: Source and aspect elements are contained in two different systems.
IN | boolean | true
ValueMap | string | 2, 3, .., 0x8000..
Values | string | Local only, Remote only, DMTF Reserved, Vendor Specific
Mode | uint16
Description | string | Describes the desired mode. If this parameter is not supplied, all modes are retrieved. Adaptive: Allows implementation to dynamically switch between synchronous and asynchronous modes.
IN | boolean | true
ModelCorrespondence | string | CIM_Synchronized.Mode
ValueMap | string | 2, 3, 4, .., 0x8000..
Values | string | Synchronous, Asynchronous, Adaptive, DMTF Reserved, Vendor Specific
ReplicationSettingData | string
Description | string | If supplied, it provides additional replication settings to consider in locating the replication relationships, for example, the CopyMethodology.
EmbeddedInstance | string | CIM_ReplicationSettingData
IN | boolean | true
SyncState | uint16
Description | string | Only retrieve synchronization aspects that are currently in this SyncState. If this parameter is not supplied, synchronization aspects are retrieved regardless of their current SyncState.
IN | boolean | true
ModelCorrespondence | string | CIM_SynchronizationAspect.SyncState
SyncType | uint16
Description | string | Describes the desired synchronization type. If this parameter is not specified, all SyncType are retrieved.
IN | boolean | true
ModelCorrespondence | string | CIM_Synchronized.SyncType
ValueMap | string | .., 6, 7, 8, 9, .., 0x8000..
Values | string | DMTF Reserved, Mirror, Snapshot, Clone, TokenizedClone, DMTF Reserved, Vendor Specific
SynchronizationAspects | CIM_SynchronizationAspect[]
Description | string | An array of elements found.
OUT | boolean | true
Job | REF CIM_ConcreteJob
Description | string | Reference to the job (may be NULL if the task completed).
IN | boolean | false
OUT | boolean | true

#### CreateListSynchronizationAspect (uint32)

#### Method Qualifiers (CreateListSynchronizationAspect)

Name | Data Type | Value
--- | --- | ---
Description | string | Create (or start a job to create) new point-in-time representations of source elements. These representations may be of a form of pointers that keep track of data at the time the point-in-time was created, or a series of checkpoints that capture the view of data on the source elements at the time of point-in-time. This method does not include target elements, however, target elements can be added subsequently using the ModifyListSettingsDefineState method. If the method executes successfully, SettingsDefineState associations are created between the source elements and the SynchronizationAspect instances, which will have the datetime of the point-in-time.
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, .., 4096, 4097..32767, 0x8000..
Values | string | Completed with No Error, Not Supported, Unknown, Timeout, Failed, Invalid Parameter, In Use, DMTF Reserved, Method Parameters Checked - Job Started, Method Reserved, Vendor Specific

#### Method Parameters (CreateListSynchronizationAspect)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
Consistency | uint16
Description | string | Specifies whether consistency is to be maintained across the list of created replication relationships.
IN | boolean | true
ValueMap | string | 2, 3, .., 0x8000..
Values | string | No Consistency, Sequential Consistency, DMTF Reserved, Vendor Specific
Mode | uint16
Description | string | Mode describes whether the target elements will be updated synchronously or asynchronously. Adaptive: Allows implementation to dynamically switch between synchronous and asynchronous modes. If NULL, implementation decides the mode.
IN | boolean | true
ModelCorrespondence | string | CIM_Synchronized.Mode
ValueMap | string | 2, 3, 4, .., 0x8000..
Values | string | Synchronous, Asynchronous, Adaptive, DMTF Reserved, Vendor Specific
ReplicationSettingData | string
Description | string | If provided, it overrides the default replication setting data for the given SyncType. If not provided, the management server uses the default replication setting data.
EmbeddedInstance | string | CIM_ReplicationSettingData
IN | boolean | true
SyncType | uint16
Description | string | SyncType describes the type of copy that will be made.
IN | boolean | true
ModelCorrespondence | string | CIM_Synchronized.SyncType
Required | boolean | true
ValueMap | string | .., 6, 7, 8, 9, .., 0x8000..
Values | string | DMTF Reserved, Mirror, Snapshot, Clone, TokenizedClone, DMTF Reserved, Vendor Specific
Names | string[]
Description | string | A end user relevant names for the elements created. If NULL, then system supplied default names can be used. The value will be stored in the elements' ElementName.
IN | boolean | true
SettingsStates | CIM_SettingsDefineState[]
Description | string | References to the created associations between the source elements and the instances of SynchronizationAspect. If a job is created, this parameter may be NULL unless the associations are actually formed.
IN | boolean | false
OUT | boolean | true
SourceElements | CIM_ManagedElement[]
Description | string | The source storage objects which may be StorageVolumes or other storage objects.
IN | boolean | true
Required | boolean | true
Job | REF CIM_ConcreteJob
Description | string | Reference to the job (may be NULL if job is completed).
IN | boolean | false
OUT | boolean | true
SourceAccessPoint | REF CIM_ServiceAccessPoint
Description | string | Reference to source access point information. If NULL, service does not need access information to access the source elements.
IN | boolean | true

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
ChangeAffectedElementsAssignedSequence | uint32 | CIM_Service
RequestStateChange | uint32 | CIM_EnabledLogicalElement
StartService | uint32 | CIM_Service
StopService | uint32 | CIM_Service