# Class CIM_FCHBADiagnosticTest
extends CIM_DiagnosticTest

The CIM_FCHBADiagnosticTest class represents the framework for running diagnostic tests. Specific diagnostic tests may be defined by subclassing and/or instantiating this object. To provide more detail for a type of test(s) (i.e, additional properties and methods), subclassing is appropriate. When a DiagnosticTest can be simultaneously executed against several elements, then DiagnosticTest may launch a ConcreteJob to represent each execution.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_Service
|
+--CIM_DiagnosticService
|
+--CIM_DiagnosticTest
|
+--CIM_FCHBADiagnosticTest

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | The CIM_FCHBADiagnosticTest class represents the framework for running diagnostic tests. Specific diagnostic tests may be defined by subclassing and/or instantiating this object. To provide more detail for a type of test(s) (i.e, additional properties and methods), subclassing is appropriate. When a DiagnosticTest can be simultaneously executed against several elements, then DiagnosticTest may launch a ConcreteJob to represent each execution.
Experimental | boolean | true
UMLPackagePath | string | CIM::System::Diagnostics
Version | string | 2.28.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
FCHBATestType | uint16 |
Description | string | The descriptions for each FC HBA test type is: * "Beacon" (value=2) is specified for the tests that cause at least one of the LEDs of a FC HBA to flash on and off. CIM_DiagnosticTest.TestTypes shall be set to "Functional" (value=2). * "Echo" (value=3) is specified for the tests that stress the pathways between the FC HBA and devices connected to the FC SAN. CIM_DiagnosticTest.TestTypes shall be set to "Functional" (value=2). * "External Loopback" (value=4) is specified for the tests that are used to verify that the entire data path through an FC HBA is working properly. CIM_DiagnosticTest.TestTypes shall be set to "Access Test" (value=5). * "Host Bus Loopback" (value=5) is specified for the tests that verify the functionality of a FC HBA's host bus interface. CIM_DiagnosticTest.TestTypes shall be set to "Functional" (value=2). * "Internal Loopback" (value=6) is specified for the tests that verify the data path from the host through most of the FC HBA. CIM_DiagnosticTest.TestTypes shall be set to "Functional" (value=2). * "Ping" (value=7) is specified for the tests that verify the existence and accessibility of devices on the SAN. CIM_DiagnosticTest.TestTypes shall be set to "Access Test" (value=5). * "Reset" (value=8) is specified for the tests that cause the FC HBA to reinitialize itself. CIM_DiagnosticTest.TestTypes shall be set to "Functional" (value=2). * "Self" (value=9) is specified for the tests that verify the functionality of all possible components of the FC HBA. CIM_DiagnosticTest.TestTypes shall be set to "Functional" (value=2). * "Status" (value=10) is specified for the tests that checks the health of the FC HBA. CIM_DiagnosticTest.TestTypes shall be set to "Health Check" (value=4).
ModelCorrespondence | string | CIM_FCHBADiagnosticTest.OtherFCHBATestTypeDescription
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, .., 0x8000..
Values | string | Unknown, Other, Beacon, Echo, External Loopback, Host Bus Loopback, Internal Loopback, Ping, Reset, Self, Status, DMTF Reserved, Vendor Reserved
OtherFCHBATestTypeDescription | string |
Description | string | A string that describes the test when the FCHBATestType property is set to 1 (Other). This property must be set to null when FCHBATestType is any value other than 1.
ModelCorrespondence | string | CIM_FCHBADiagnosticTest.FCHBATestType

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_Service
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
IsInUse | boolean | CIM_DiagnosticTest
LoSID | string | CIM_Service
LoSOrgID | string | CIM_Service
Name | string | CIM_Service
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherCharacteristicDescription | string | CIM_DiagnosticTest
OtherEnabledState | string | CIM_EnabledLogicalElement
PrimaryOwnerContact | string | CIM_Service
PrimaryOwnerName | string | CIM_Service
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedState | uint16 | CIM_EnabledLogicalElement
Started | boolean | CIM_Service
StartMode | string | CIM_Service
Status | string | CIM_ManagedSystemElement
SystemCreationClassName | string | CIM_Service
SystemName | string | CIM_Service
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
Characteristics | uint16[] | CIM_DiagnosticTest
OperationalStatus | uint16[] | CIM_ManagedSystemElement
OtherCharacteristicsDescriptions | string[] | CIM_DiagnosticTest
OtherTestTypesDescriptions | string[] | CIM_DiagnosticTest
ResourcesUsed | uint16[] | CIM_DiagnosticTest
StatusDescriptions | string[] | CIM_ManagedSystemElement
TestTypes | uint16[] | CIM_DiagnosticTest

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
ChangeAffectedElementsAssignedSequence | uint32 | CIM_Service
ClearResults | uint32 | CIM_DiagnosticTest
DiscontinueTest | uint32 | CIM_DiagnosticTest
RequestStateChange | uint32 | CIM_EnabledLogicalElement
RunDiagnostic | uint32 | CIM_DiagnosticService
RunDiagnosticService | uint32 | CIM_DiagnosticService
RunTest | uint32 | CIM_DiagnosticTest
StartService | uint32 | CIM_Service
StopService | uint32 | CIM_Service