# Class CIM_IEEE8021xSettings
extends CIM_SettingData

IEEE8021xSettings specifies a set of IEEE 802.1x Port-Based Network Access Control settings that can be applied to a ISO OSI layer 2 ProtocolEndpoint.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_SettingData
|
+--CIM_IEEE8021xSettings

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | IEEE8021xSettings specifies a set of IEEE 802.1x Port-Based Network Access Control settings that can be applied to a ISO OSI layer 2 ProtocolEndpoint.
Experimental | boolean | true
UMLPackagePath | string | CIM::Network::IEEE8021x
Version | string | 2.22.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
AuthenticationProtocol | uint16 |
Description | string | AuthenticationProtocol shall indicate the desired EAP (Extensible Authentication Protocol) type. * EAP-TLS (0): shall indicate that the desired EAP type is the Transport Layer Security EAP type specified in RFC 2716. If AuthenticationProtocol contains 0, Username should not be null, ServerCertificateName and ServerCertificateNameComparison may be null or not null, and RoamingIdentity, Password, Domain, ProtectedAccessCredential, PACPassword, and PSK should be null. * EAP-TTLS/MSCHAPv2 (1): shall indicate that the desired EAP type is the Tunneled TLS Authentication Protocol EAP type specified in draft-ietf-pppext-eap-ttls, with Microsoft PPP CHAP Extensions, Version 2 (MSCHAPv2) as the inner authentication method. If AuthenticationProtocol contains 1, Username and Password should not be null, RoamingIdentity, ServerCertificateName, ServerCertificateNameComparison, and Domain may be null or not null, and ProtectedAccessCredential, PACPassword, and PSK should be null. * PEAPv0/EAP-MSCHAPv2 (2): shall indicate that the desired EAP type is the Protected Extensible Authentication Protocol (PEAP) Version 0 EAP type specified in draft-kamath-pppext-peapv0, with Microsoft PPP CHAP Extensions, Version 2 (MSCHAPv2) as the inner authentication method. If AuthenticationProtocol contains2, Username and Password should not be null, RoamingIdentity, ServerCertificateName, ServerCertificateNameComparison, and Domain may be null or not null, and ProtectedAccessCredential, PACPassword, and PSK should be null. * PEAPv1/EAP-GTC (3): shall indicate that the desired EAP type is the Protected Extensible Authentication Protocol (PEAP) Version 1 EAP type specified in draft-josefsson-pppext-eap-tls-eap, with Generic Token Card (GTC) as the inner authentication method. If AuthenticationProtocol contains 3, Username and Password should not be null, RoamingIdentity, ServerCertificateName, ServerCertificateNameComparison, and Domain may be null or not null, and ProtectedAccessCredential, PACPassword, and PSK should be null. * EAP-FAST/MSCHAPv2 (4): shall indicate that the desired EAP type is the Flexible Authentication Extensible Authentication Protocol EAP type specified in IETF RFC 4851, with Microsoft PPP CHAP Extensions, Version 2 (MSCHAPv2) as the inner authentication method. If AuthenticationProtocol contains 4, Username and Password should not be null, RoamingIdentity, ServerCertificateName, ServerCertificateNameComparison, Domain, ProtectedAccessCredential, and PACPassword may be null or not null, and PSK should be null. * EAP-FAST/GTC (5): shall indicate that the desired EAP type is the Flexible Authentication Extensible Authentication Protocol EAP type specified in IETF RFC 4851, with Generic Token Card (GTC) as the inner authentication method. If AuthenticationProtocol contains 5, Username and Password should not be null, RoamingIdentity, ServerCertificateName, ServerCertificateNameComparison, Domain, ProtectedAccessCredential, and PACPassword may be null or not null, and PSK should be null. * EAP-MD5 (6): shall indicate that the desired EAP type is the EAP MD5 authentication method, specified in RFC 3748. If AuthenticationProtocol contains 6, Username and Password should not be null, Domain may be null or not null, and RoamingIdentity, ServerCertificateName, ServerCertificateNameComparison, ProtectedAccessCredential, PACPassword, and PSK should be null. * EAP-PSK (7): shall indicate that the desired EAP type is the EAP-PSK (Pre-Shared Key) EAP type specified in RFC 4764. If AuthenticationProtocol contains 7, Username and PSK should not be null, Domain and RoamingIdentity may be null or not null, and Password, ServerCertificateName, ServerCertificateNameComparison, ProtectedAccessCredential, and PACPassword should be null. * EAP-SIM (8): shall indicate that the desired EAP type is the Extensible Authentication Protocol Method for Global System for Mobile Communications (GSM) Subscriber Identity Modules (EAP-SIM), specified in RFC 4186. If AuthenticationProtocol contains 8, Username and PSK should not be null, Domain and RoamingIdentity may be null or not null, and Password, ServerCertificateName, ServerCertificateNameComparison, ProtectedAccessCredential, and PACPassword should be null. * EAP-AKA (9): shall indicate that the desired EAP type is the EAP Method for 3rd Generation Authentication and Key Agreement (EAP-AKA), specified in RFC 4187. If AuthenticationProtocol contains 9, Username and PSK should not be null, Domain and RoamingIdentity may be null or not null, and Password, ServerCertificateName, ServerCertificateNameComparison, ProtectedAccessCredential, and PACPassword should be null. * EAP-FAST/TLS (10): shall indicate that the desired EAP type is the Flexible Authentication EAP type specified in IETF RFC 4851, with TLS as the inner authentication method. If AuthenticationProtocol contains 10, Username and Password should not be null, RoamingIdentity, ServerCertificateName, ServerCertificateNameComparison, Domain, ProtectedAccessCredential, and PACPassword may be null or not null, and PSK should be null.
MappingStrings | string | RFC4017.IETF, RFC2716.IETF, draft-ietf-pppext-eap-ttls.IETF, draft-kamath-pppext-peapv0.IETF, draft-josefsson-pppext-eap-tls-eap, RFC4851.IETF, RFC3748.IETF, RFC4764.IETF, RFC4186.IETF, RFC4187.IETF
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, ..
Values | string | EAP-TLS, EAP-TTLS/MSCHAPv2, PEAPv0/EAP-MSCHAPv2, PEAPv1/EAP-GTC, EAP-FAST/MSCHAPv2, EAP-FAST/GTC, EAP-MD5, EAP-PSK, EAP-SIM, EAP-AKA, EAP-FAST/TLS, DMTF Reserved
Domain | string |
Description | string | The domain (also known as realm) within which Username is unique.
MappingStrings | string | draft-ietf-pppext-eap-ttls.IETF, draft-kamath-pppext-peapv0.IETF, draft-josefsson-pppext-eap-tls-eap, RFC4851.IETF, RFC3748.IETF, RFC4764.IETF, RFC4186.IETF, RFC4187.IETF
PACPassword | string |
Description | string | Optional password to extract the PAC (Protected Access Credential) information from the PAC data.
MappingStrings | string | RFC4851.IETF
Password | string |
Description | string | A password associated with the user identified by Username within Domain.
MappingStrings | string | draft-ietf-pppext-eap-ttls.IETF, draft-kamath-pppext-peapv0.IETF, draft-josefsson-pppext-eap-tls-eap, RFC4851.IETF, RFC3748.IETF
RoamingIdentity | string |
Description | string | A string presented to the authentication server in 802.1x protocol exchange. The AAA server determines the format of this string. Formats supported by AAA servers include: <domain>\<username>, <username>@<domain>.
ServerCertificateName | string |
Description | string | The name that shall be compared against the subject name field in the certificate provided by the AAA server. Shall contain either the fully qualified domain name of the AAA server, in which case ServerCertificateNameComparison shall contain "FullName", or the domain suffix of the AAA server, in which case ServerCertificateNameComparison shall contain "DomainSuffix".
ModelCorrespondence | string | CIM_IEEE8021xSettings.ServerCertificateNameComparison
ServerCertificateNameComparison | uint16 |
Description | string | The comparison algorithm that shall be used by the server to validate the subject name field of the certificate presented by the AAA server against the value of the ServerCertificateName property.
ModelCorrespondence | string | CIM_IEEE8021xSettings.ServerCertificateName
ValueMap | string | 1, 2, 3, ..
Values | string | Other, FullName, DomainSuffix, DMTF Reserved
Username | string |
Description | string | Identifies the user requesting access to the network.
MappingStrings | string | RFC2716.IETF, draft-ietf-pppext-eap-ttls.IETF, draft-kamath-pppext-peapv0.IETF, draft-josefsson-pppext-eap-tls-eap, RFC4851.IETF, RFC3748.IETF, RFC4764.IETF, RFC4186.IETF, RFC4187.IETF
ProtectedAccessCredential | uint8[] |
Description | string | A credential used by the supplicant and AAA server to establish a mutually authenticated encrypted tunnel for confidential user authentication.
MappingStrings | string | RFC4851.IETF
OctetString | boolean | true
PSK | uint8[] |
Description | string | A pre-shared key used for pre-shared key EAP types such as EAP-PSK, EAP-SIM, and EAP-AKA.
MappingStrings | string | RFC4764.IETF, RFC4186.IETF, RFC4187.IETF
OctetString | boolean | true

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
ChangeableType | uint16 | CIM_SettingData
ConfigurationName | string | CIM_SettingData
Description | string | CIM_ManagedElement
ElementName | string | CIM_SettingData
Generation | uint64 | CIM_ManagedElement
InstanceID | string | CIM_SettingData
SoID | string | CIM_SettingData
SoOrgID | string | CIM_SettingData
ComponentSetting | string[] | CIM_SettingData

## Class Methods