# Class CIM_EthernetNICDiagnosticServiceCapabilities
extends CIM_DiagnosticServiceCapabilities

This class defines the permissible settings that can be used for EthenetNIC diagnostic tests.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_Capabilities
|
+--CIM_DiagnosticServiceCapabilities
|
+--CIM_EthernetNICDiagnosticServiceCapabilities

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | This class defines the permissible settings that can be used for EthenetNIC diagnostic tests.
Experimental | boolean | true
UMLPackagePath | string | CIM::System::Diagnostics
Version | string | 2.31.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
LinkSpeedsSupported | uint64[] |
Description | string | This array property is used by a provider to specify the list of link speeds supported by some EthernetNIC tests. The client should only select one of these values.
ModelCorrespondence | string | CIM_EthernetNICDiagnosticSettingData.LinkSpeeds
PUnit | string | bit / second * 10^6
LoopbackLayersSupported | uint16[] |
Description | string | This array property is used by a provider to specify the list of of layers (e.g. PHY, MAC, etc) supported by some EthernetNIC tests. The client should only select one of these values.
ModelCorrespondence | string | CIM_EthernetNICDiagnosticSettingData.LoopbackLayers, CIM_EthernetNICDiagnosticServiceCapabilities.OtherLoopbackLayersSupported
ValueMap | string | 1, 2, 3
Values | string | Other, PHY Layer, MAC Layer
OtherLoopbackLayersSupported | string[] |
Description | string | This array property is used by a provider to specify the layers supported by the test when LoopbackLayers has value set to 1 ("Other"). The client should only select one of these values.
ModelCorrespondence | string | CIM_EthernetNICDiagnosticServiceCapabilities.LoopbackLayersSupported, CIM_EthernetNICDiagnosticSettingData.OtherLoopbackLayers
PacketSizesSupported | uint16[] |
Description | string | This array property is used by a provider to specify the list of packet sizes supported by some Ethernet NIC tests. The client should only select one of these values.
ModelCorrespondence | string | CIM_EthernetNICDiagnosticSettingData.PacketSizes
PUnit | string | Byte

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
Description | string | CIM_ManagedElement
ElementName | string | CIM_Capabilities
Generation | uint64 | CIM_ManagedElement
InstanceID | string | CIM_Capabilities
SupportedTestWarnings | uint16 | CIM_DiagnosticServiceCapabilities
OtherSupportedExecutionControlsDescriptions | string[] | CIM_DiagnosticServiceCapabilities
OtherSupportedLogOptionsDescriptions | string[] | CIM_DiagnosticServiceCapabilities
OtherSupportedLogStorageDescriptions | string[] | CIM_DiagnosticServiceCapabilities
OtherSupportedLoopControlDescriptions | string[] | CIM_DiagnosticServiceCapabilities
OtherSupportedServiceModesDescriptions | string[] | CIM_DiagnosticServiceCapabilities
SupportedExecutionControls | uint16[] | CIM_DiagnosticServiceCapabilities
SupportedLogOptions | uint16[] | CIM_DiagnosticServiceCapabilities
SupportedLogStorage | uint16[] | CIM_DiagnosticServiceCapabilities
SupportedLoopControl | uint16[] | CIM_DiagnosticServiceCapabilities
SupportedServiceModes | uint16[] | CIM_DiagnosticServiceCapabilities

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
CreateGoalSettings | uint16 | CIM_Capabilities