# Class CIM_MPLSSegmentStats
extends CIM_StatisticalData

The class represents the statistics for an In or Out MPLSSegment. The statistics are associated to the Segment using the relationship CIM_ElementStatisticalData.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_StatisticalData
|
+--CIM_MPLSSegmentStats

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | The class represents the statistics for an In or Out MPLSSegment. The statistics are associated to the Segment using the relationship CIM_ElementStatisticalData.
Experimental | boolean | true
UMLPackagePath | string | CIM::Network::MPLS
Version | string | 2.8.1000

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
NumberOfDiscards | uint32 |
Counter | boolean | true
Description | string | The number of labeled packets received/sent on this Segment, which were chosen to be discarded even though no errors had been detected to prevent their being transmitted. One possible reason for discarding such a labeled packet could be to free up buffer space. Whether this value denotes In or Out Segments depends on the instance associated with MPLSSegmentStats.
MappingStrings | string | MIB.IETF|MPLS-LSR-MIB.MPLSInSegmentDiscards, MIB.IETF|MPLS-LSR-MIB.MPLSIOutSegmentDiscards
NumberOfErrors | uint32 |
Counter | boolean | true
Description | string | The number of errored packets received/sent on this Segment. Whether this value denotes In or Out Segments depends on the instance associated with MPLSSegmentStats.
MappingStrings | string | MIB.IETF|MPLS-LSR-MIB.MPLSInSegmentErrors, MIB.IETF|MPLS-LSR-MIB.MPLSIOutSegmentErrors
NumberOfOctets | uint32 |
Counter | boolean | true
Description | string | This value represents the total number of octets received/sent by this Segment. Whether it denotes In or Out Segments depends on the instance associated with MPLSSegmentStats.
MappingStrings | string | MIB.IETF|MPLS-LSR-MIB.MPLSInSegmentOctets, MIB.IETF|MPLS-LSR-MIB.MPLSIOutSegmentOctets
NumberOfPackets | uint32 |
Counter | boolean | true
Description | string | Total number of packets received/sent by this Segment. Whether this value denotes In or Out Segments depends on the instance associated with MPLSSegmentStats.
MappingStrings | string | MIB.IETF|MPLS-LSR-MIB.MPLSInSegmentPackets, MIB.IETF|MPLS-LSR-MIB.MPLSOutSegmentPackets

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
Description | string | CIM_ManagedElement
ElementName | string | CIM_StatisticalData
Generation | uint64 | CIM_ManagedElement
InstanceID | string | CIM_StatisticalData
RateIntervalEndTime | datetime | CIM_StatisticalData
RateIntervalStartTime | datetime | CIM_StatisticalData
SampleInterval | datetime | CIM_StatisticalData
StartStatisticTime | datetime | CIM_StatisticalData
StatisticTime | datetime | CIM_StatisticalData

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
ResetSelectedStats | uint32 | CIM_StatisticalData