# Class CIM_ParallelPort
extends CIM_LogicalPort

ParallelPort is the logical representation of parallel communications interface. It includes the setup or operation of the parallel chips, at the lowest layers of a parallel stack.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_LogicalPort
|
+--CIM_ParallelPort

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | ParallelPort is the logical representation of parallel communications interface. It includes the setup or operation of the parallel chips, at the lowest layers of a parallel stack.
Experimental | boolean | true
UMLPackagePath | string | CIM::Device::Ports
Version | string | 2.26.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
BaseIOAddress | uint64 |
Description | string | An integer value that represents the base I/O address used by the parallel port.
ConnectorType | uint16 |
Description | string | ConnectorType is defined to force consistent naming of the 'connector type' property in subclasses and to guarantee unique enum values for all instances of ParallelPort. When set to 3 ("Proprietary"), the related property OtherConnectorType contains a string description of the type of port.
MappingStrings | string | SMBIOS.DMTF|Connector Type|DSP0134_2.6.1.pdf 3.3.9.2
ModelCorrespondence | string | CIM_ParallelPort.OtherConnectorType
ValueMap | string | 0, 1, 2, 3, 4, 5, .., 32768..
Values | string | Unknown, Centronics, Mini-Centronics, Proprietary, DB-25 Female, DB-25 Male, DMTF Reserved, Vendor Reserved
IRQLevel | uint32 |
Description | string | An integer value that represents the IRQ level used by the parallel port.
OtherConnectorType | string |
Description | string | Describes the connector type of the parallel port, when ConnectorType is set to 3 ("Proprietary").
ModelCorrespondence | string | CIM_ParallelPort.ConnectorType
Pinout | uint32 |
Description | string | The pinout used by the I/O device on this parallel port.
MappingStrings | string | SMBIOS.DMTF|Port Type|DSP0134_2.6.1.pdf 3.3.9.3
ValueMap | string | 0, 1, 2, 3, 4, 5, 25, 26, ..
Values | string | Unknown, XT/AT, PS/2, ECP, EPP, IEEE 1284, PC-98, PC-98-Hireso, DMTF Reserved
Security | uint16 |
Description | string | An enumeration indicating the operational security for the Controller. For example, information that the Device's external interface is locked out (valuemap=3) or "Boot Bypass" (valuemap=5) can be described using this property.
ModelCorrespondence | string | CIM_ParallelController.Security
ValueMap | string | 0, 1, 2, 3, 4, 5, .., 32768..
Values | string | Unknown, Other, None, External Interface Locked Out, External Interface Enabled, Boot Bypass, DMTF Reserved, Vendor Reserved
Capabilities | uint16[] |
ArrayType | string | Indexed
Description | string | An integer enumeration indicating the capabilities of the ParallelController.
ModelCorrespondence | string | CIM_ParallelController.Capabilities
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, .., 32768..
Values | string | Unknown, Other, XT/AT Compatible, PS/2 Compatible, ECP, EPP, PC-98, PC-98-Hireso, PC-H98, Device supports DMA, DMTF Reserved, Vendor Reserved

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
AllocationState | string | CIM_LogicalDevice
Availability | uint16 | CIM_LogicalDevice
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_LogicalDevice
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
DeviceID | string | CIM_LogicalDevice
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
ErrorCleared | boolean | CIM_LogicalDevice
ErrorDescription | string | CIM_LogicalDevice
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
LastErrorCode | uint32 | CIM_LogicalDevice
LocationIndicator | uint16 | CIM_LogicalDevice
MaxQuiesceTime | uint64 | CIM_LogicalDevice
MaxSpeed | uint64 | CIM_LogicalPort
Name | string | CIM_ManagedSystemElement
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
OtherPortType | string | CIM_LogicalPort
PortType | uint16 | CIM_LogicalPort
PowerManagementSupported | boolean | CIM_LogicalDevice
PowerOnHours | uint64 | CIM_LogicalDevice
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedSpeed | uint64 | CIM_LogicalPort
RequestedState | uint16 | CIM_EnabledLogicalElement
Speed | uint64 | CIM_LogicalPort
Status | string | CIM_ManagedSystemElement
StatusInfo | uint16 | CIM_LogicalDevice
SystemCreationClassName | string | CIM_LogicalDevice
SystemName | string | CIM_LogicalDevice
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TotalPowerOnHours | uint64 | CIM_LogicalDevice
TransitioningToState | uint16 | CIM_EnabledLogicalElement
UsageRestriction | uint16 | CIM_LogicalPort
AdditionalAvailability | uint16[] | CIM_LogicalDevice
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
IdentifyingDescriptions | string[] | CIM_LogicalDevice
OperationalStatus | uint16[] | CIM_ManagedSystemElement
OtherIdentifyingInfo | string[] | CIM_LogicalDevice
PowerManagementCapabilities | uint16[] | CIM_LogicalDevice
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
EnableDevice | uint32 | CIM_LogicalDevice
OnlineDevice | uint32 | CIM_LogicalDevice
QuiesceDevice | uint32 | CIM_LogicalDevice
RequestStateChange | uint32 | CIM_EnabledLogicalElement
Reset | uint32 | CIM_LogicalDevice
RestoreProperties | uint32 | CIM_LogicalDevice
SaveProperties | uint32 | CIM_LogicalDevice
SetPowerState | uint32 | CIM_LogicalDevice