# Class CIM_LAGControlCapabilities
extends CIM_Capabilities

This class establishes the control protocol support of the system. The Capabilities instance is associated to a network ComputerSystem via the ElementCapabilities relationship.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_Capabilities
|
+--CIM_LAGControlCapabilities

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | This class establishes the control protocol support of the system. The Capabilities instance is associated to a network ComputerSystem via the ElementCapabilities relationship.
Experimental | boolean | true
UMLPackagePath | string | CIM::Network::8023LAG
Version | string | 2.8.1000

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
LAGControlMode | uint16 | 2
Description | string | A LAG may be under manual control (i.e., amanagement station is responsible for the additon and removal of LAG members) or automatic (i.e., a control protocol is employed to establish LAG membership.
ValueMap | string | 2, 3
Values | string | Manual, Automatic
LAGControlProtocol | uint16 |
Description | string | When the LAGMode is automatic, this propertyidentifies the control protocol in use.
ValueMap | string | 2, 3, 4..32767, ..
Values | string | None, LACP, DMTF Reserved, Vendor Reserved

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
Description | string | CIM_ManagedElement
ElementName | string | CIM_Capabilities
Generation | uint64 | CIM_ManagedElement
InstanceID | string | CIM_Capabilities

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
CreateGoalSettings | uint16 | CIM_Capabilities