# Class CIM_MPLSProtocolEndpoint
extends CIM_ProtocolEndpoint

This is the representation of an MPLS interface on a Label Switch Router (LSR).

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_ServiceAccessPoint
|
+--CIM_ProtocolEndpoint
|
+--CIM_MPLSProtocolEndpoint

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | This is the representation of an MPLS interface on a Label Switch Router (LSR).
Experimental | boolean | true
UMLPackagePath | string | CIM::Network::ProtocolEndpoints
Version | string | 2.8.1000

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
AvailableBandwidth | uint32 |
Description | string | This property indicates the total amount of available bandwidth for the interface and is specified in kilobits per second (Kbps). This value is calculated as the difference between the amount of bandwidth currently in use and that specified in TotalBandwidth. Note that this is not statistical data, since change is not frequent, and the property can be regarded as the 'current state' of the network. It is intended that this data be used by applications doing centralized LSP provisioning.
MappingStrings | string | MIB.IETF|MPLS-LSR-MIB.MPLSInterfaceAvailableBandwidth
ModelCorrespondence | string | CIM_MPLSProtocolEndpoint.TotalBandwidth
PUnit | string | bit / second * 10^3
Units | string | KiloBits per Second
OverruleLSR | boolean |
Description | string | If this property is true, the Label Min/Max In/Out values of the ProtocolEndpoint's MPLSCapabilities overrule the values specified for the Label Switched Router as a whole (where the LSR is indicated by the existence of an MPLSService). Note that the min/max in/out labels are only defined in the MPLSCapabilities class, which is associated with either an MPLSService or an MPLSProtocolEndpoint via the CIM_ElementCapabilities relationship.
ResourceClasses | uint32 |
Description | string | The ResourceClasses property defines a 32-bit vector representing the classes associated with a link, where the link originates at this ProtocolEndpoint. A resource class is described in [RFC2702].
TotalBandwidth | uint32 |
Description | string | This property indicates the total amount of usable bandwidth on this interface and is specified in kilobits per second (Kbps).
MappingStrings | string | MIB.IETF|MPLS-LSR-MIB.MPLSInterfaceTotalBandwidth
PUnit | string | bit / second * 10^3
Units | string | KiloBits per Second

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
BroadcastResetSupported | boolean | CIM_ProtocolEndpoint
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_ServiceAccessPoint
Description | string | CIM_ProtocolEndpoint
DetailedStatus | uint16 | CIM_ManagedSystemElement
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_ProtocolEndpoint
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
Name | string | CIM_ProtocolEndpoint
NameFormat | string | CIM_ProtocolEndpoint
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
OtherTypeDescription | string | CIM_ProtocolEndpoint
PrimaryStatus | uint16 | CIM_ManagedSystemElement
ProtocolIFType | uint16 | CIM_ProtocolEndpoint
ProtocolType | uint16 | CIM_ProtocolEndpoint
RequestedState | uint16 | CIM_EnabledLogicalElement
Status | string | CIM_ManagedSystemElement
SystemCreationClassName | string | CIM_ServiceAccessPoint
SystemName | string | CIM_ServiceAccessPoint
TimeOfLastStateChange | datetime | CIM_ProtocolEndpoint
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
OperationalStatus | uint16[] | CIM_ProtocolEndpoint
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
BroadcastReset | uint32 | CIM_ProtocolEndpoint
RequestStateChange | uint32 | CIM_EnabledLogicalElement