# Class CIM_VLANMembershipSettingData
extends CIM_ConnectivityMembershipSettingData

For dynamic VLAN assignment, these rules define how incoming traffic is assigned to a VLAN. A typical set of assignment rules include assignment based on MAC address, IP address, or IP subnet. Many other criteria or combination of criteria may be used.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_SettingData
|
+--CIM_ConnectivityMembershipSettingData
|
+--CIM_VLANMembershipSettingData

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | For dynamic VLAN assignment, these rules define how incoming traffic is assigned to a VLAN. A typical set of assignment rules include assignment based on MAC address, IP address, or IP subnet. Many other criteria or combination of criteria may be used.
Experimental | boolean | true
UMLPackagePath | string | CIM::Network::VLAN
Version | string | 2.8.1000

## Class Properties

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
ChangeableType | uint16 | CIM_SettingData
ConfigurationName | string | CIM_SettingData
ConnectivityMemberID | string | CIM_ConnectivityMembershipSettingData
ConnectivityMemberType | uint16 | CIM_ConnectivityMembershipSettingData
Description | string | CIM_ManagedElement
ElementName | string | CIM_SettingData
Generation | uint64 | CIM_ManagedElement
InstanceID | string | CIM_SettingData
OtherConnectivityMemberType | string | CIM_ConnectivityMembershipSettingData
SoID | string | CIM_SettingData
SoOrgID | string | CIM_SettingData
ComponentSetting | string[] | CIM_SettingData

## Class Methods