# Class CIM_PrintMediaPath
extends CIM_PrinterElement

This class represents the PrintMediaPath component of a Printer (print device). It contains properties that describe the PrintMediaPath, including type, speed, and status. Note: A PrintMediaPath shall be associated with exactly one Printer via an instance of the PrinterComponent class. See: Model in section 2 of Printer MIB (RFC 3805).

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_PrinterElement
|
+--CIM_PrintMediaPath

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | This class represents the PrintMediaPath component of a Printer (print device). It contains properties that describe the PrintMediaPath, including type, speed, and status. Note: A PrintMediaPath shall be associated with exactly one Printer via an instance of the PrinterComponent class. See: Model in section 2 of Printer MIB (RFC 3805).
Experimental | boolean | true
MappingStrings | string | MIB.IETF|Printer-MIB.prtMediaPathEntry
UMLPackagePath | string | CIM::Device::Printing
Version | string | 2.17.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
AvailabilityStatus | uint32 |
Description | string | This property contains detailed availability information for this PrintMediaPath, as follows: 1 (Other) means other detailed availability information is present in the OtherAvailabilityStatus property. 2 (Unknown) means detailed availability information for this PrintMediaPath is unknown. 3 (AvailableIdle) means this PrintMediaPath is available and idle, i.e., not currently in use. 4 (AvailableStandy) means this PrintMediaPath is available but on standby, e.g., in a power saving mode. 5 (AvailableActive) means this PrintMediaPath is available and active, i.e., currently in use. 6 (AvailableBusy) means this PrintMediaPath is available but busy, i.e., not immediately available for its primary function. 7 (UnavailableOnRequest) means this PrintMediaPath is not available and is on request, i.e., needs human intervention. 8 (UnavailableBroken) means this PrintMediaPath is not available and is broken, e.g., needs repair/replacement.
MappingStrings | string | MIB.IETF|Printer-MIB.PrtSubUnitStatusTC
ModelCorrespondence | string | CIM_ManagedSystemElement.OperatingStatus, CIM_PrintMediaPath.OtherAvailabilityStatus
ValueMap | string | 1, 2, 3, 4, 5, 6, 7, 8, ..
Values | string | Other, Unknown, AvailableIdle, AvailableStandby, AvailableActive, AvailableBusy, UnavailableOnRequest, UnavailableBroken, DMTF Reserved
CriticalAlertsPresent | boolean |
Description | string | If true, there are currently critical alerts on this PrintMediaPath.
MappingStrings | string | MIB.IETF|Printer-MIB.PrtSubUnitStatusTC
ModelCorrespondence | string | CIM_ManagedSystemElement.DetailedStatus
IsDefault | boolean |
Description | string | Denotes whether or not this PrintMediaPath is the default PrintMediaPath for this Printer. If the default PrintMediaPath feature is not sPrintMediaPathupported for this Printer, then this property shall be null. If the default PrintMediaPath feature is supported for this Printer, then this property shall be true for at most one instance of CIM_PrintMediaPath on this Printer, i.e., the default may not be currently configured.
MappingStrings | string | MIB.IETF|Printer-MIB.prtMediaPathDefaultIndex
LocalizedDescription | string |
Description | string | A free-form text description of this PrintMediaPath PrintMediaPath in the localization specified by CIM_Printer.CurrentNaturalLanguage.
MappingStrings | string | MIB.IETF|Printer-MIB.prtMediaPathDescription, MIB.IETF|Printer-MIB.PrtLocalizedDescriptionStringTC
MaxLen | uint32 | 255
MinLen | uint32 | 0
MaxMediaSizeName | string |
Description | string | This property provides the value of the PWG standard or, custom media size name of the media that is the maximum media size supported by this PrintMediaPath. The values of this property shall conform to the requirements of the PWG Media Standardized Names specification [PWG5101.1], which defines the normative values for this property.
MappingStrings | string | PWG5101-1.PWG|Media Standardized Names, MIB.IETF|Printer-MIB.prtMediaPathMaxMediaFeedDir, MIB.IETF|Printer-MIB.prtMediaPathMaxMediaXFeedDir
MaxLen | uint32 | 63
MinLen | uint32 | 0
MaxMediaSizeNameBasis | uint16 |
Description | string | The basis for the limit property MaxMediaSizeName, that specifies whether a meaningful value is available. 1 (Other) means the PrintMediaPath places no restrictions on maximum size and MaxMediaSizeName shall be null. 2 (Unknown) means the PrintMediaPath does not have a meaningful value and MaxMediaSizeName shall be null. 3 (Actual) means the PrintMediaPath does have a meaningful value and MaxMediaSizeName shall be present.
MappingStrings | string | MIB.IETF|Printer-MIB.prtMediaPathMaxMediaFeedDir, MIB.IETF|Printer-MIB.prtMediaPathMaxMediaXFeedDir
ValueMap | string | 1, 2, 3, ..
Values | string | Other, Unknown, Actual, DMTF Reserved
MaxSpeed | uint32 |
Description | string | The maximum printing speed of this PrintMediaPath.
MappingStrings | string | MIB.IETF|Printer-MIB.prtMediaPathMaxSpeed, MIB.IETF|Printer-MIB.prtMediaPathMaxSpeedPrintUnit, MIB.IETF|Printer-MIB.PrtMediaPathMaxSpeedPrintUnitTC
MaxValue | sint64 | 2147483647
MinValue | sint64 | 0
MaxSpeedBasis | uint16 |
Description | string | The basis for the limit property MaxSpeed, that specifies whether a meaningful value is available. 1 (Other) means the PrintMediaPath places no restrictions on speed and MaxSpeed shall be null. 2 (Unknown) means the PrintMediaPath does not have a meaningful value and MaxSpeed shall be null. 3 (Actual) means the PrintMediaPath does have a meaningful value and MaxSpeed shall be present.
MappingStrings | string | MIB.IETF|Printer-MIB.prtMediaPathMaxSpeed
ValueMap | string | 1, 2, 3, ..
Values | string | Other, Unknown, Actual, DMTF Reserved
MaxSpeedUnit | uint32 |
Description | string | The unit of measure used in specifying the speed of this PrintMediaPath.
MappingStrings | string | MIB.IETF|Printer-MIB.prtMediaPathMaxSpeedPrintUnit, MIB.IETF|Printer-MIB.PrtMediaPathMaxSpeedPrintUnitTC
ValueMap | string | 3, 4, 5, 6, 7, 8, 9, 16, 17, ..
Values | string | TenThousandthsOfInchesPerHour, MicrometersPerHour, CharactersPerHour, LinesPerHour, ImpressionsPerHour, SheetsPerHour, DotRowPerHour, FeetPerHour, MetersPerHour, DMTF Reserved
MinMediaSizeName | string |
Description | string | This property provides the value of the PWG standard or, custom media size name of the media that is the maximum media size supported by this PrintMediaPath. The values of this property shall conform to the requirements of the PWG Media Standardized Names specification [PWG5101.1], which defines the normative values for this property.
MappingStrings | string | PWG5101-1.PWG|Media Standardized Names, MIB.IETF|Printer-MIB.prtMediaPathMinMediaFeedDir, MIB.IETF|Printer-MIB.prtMediaPathMinMediaXFeedDir
MaxLen | uint32 | 63
MinLen | uint32 | 0
MinMediaSizeNameBasis | uint16 |
Description | string | The basis for the limit property MinMediaSizeName, that specifies whether a meaningful value is available. 1 (Other) means the PrintMediaPath places no restrictions on minimum size and MinMediaSizeName shall be null. 2 (Unknown) means the PrintMediaPath does not have a meaningful value and MinMediaSizeName shall be null. 3 (Actual) means the PrintMediaPath does have a meaningful value and MinMediaSizeName shall be present.
MappingStrings | string | MIB.IETF|Printer-MIB.prtMediaPathMinMediaFeedDir, MIB.IETF|Printer-MIB.prtMediaPathMinMediaXFeedDir
ValueMap | string | 1, 2, 3, ..
Values | string | Other, Unknown, Actual, DMTF Reserved
NonCriticalAlertsPresent | boolean |
Description | string | If true, there are currently non-critical alerts on this PrintMediaPath.
MappingStrings | string | MIB.IETF|Printer-MIB.PrtSubUnitStatusTC
ModelCorrespondence | string | CIM_ManagedSystemElement.DetailedStatus
OtherAvailabilityStatus | string |
Description | string | A free-form string that describes the detailed availability of this PrintMediaPath when the value of the AvailabilityStatus property is equal to 1 (Other).
MaxLen | uint32 | 255
MinLen | uint32 | 0
ModelCorrespondence | string | CIM_PrintMediaPath.AvailabilityStatus
OtherTypeDescription | string |
Description | string | A free-form string that describes the type of PrintMediaPath when the value of the Type property is equal to 1 (Other).
MaxLen | uint32 | 255
MinLen | uint32 | 0
Type | uint32 |
Description | string | The type of this PrintMediaPath.
MappingStrings | string | MIB.IETF|Printer-MIB.prtMediaPathType, MIB.IETF|IANA-PRINTER-MIB.PrtMediaPathTypeTC
ValueMap | string | 1, 2, 3, 4, 5, ..
Values | string | Other, Unknown, LongEdgeBindingDuplex, ShortEdgeBindingDuplex, Simplex, DMTF Reserved

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
ElementName | string | CIM_ManagedElement
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_PrinterElement
Name | string | CIM_ManagedSystemElement
OperatingStatus | uint16 | CIM_ManagedSystemElement
PrimaryStatus | uint16 | CIM_ManagedSystemElement
SNMPRowId | uint32 | CIM_PrinterElement
Status | string | CIM_ManagedSystemElement
OperationalStatus | uint16[] | CIM_ManagedSystemElement
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods