# Class CIM_MPLSCrossConnectLSP
extends CIM_Dependency

Defines the LSP to which the CrossConnect belongs.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_Dependency
|
+--CIM_MPLSCrossConnectLSP

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Association | boolean | true
Description | string | Defines the LSP to which the CrossConnect belongs.
Experimental | boolean | true
UMLPackagePath | string | CIM::Network::MPLS
Version | string | 2.8.1000

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
XcOrder | uint16 |
Description | string | This property defines the order of the CrossConnects in an LSP. An incrementally higher number indicates the next Cross Connect in the ordered sequence. Note that the first CrossConnect must be of type 'Orig', and the last of type 'Term' (see the property, XcType).
XcType | uint16 |
Description | string | The XcType property defines whether a CrossConnect is at the terminating end ("Term", 1), or originating end ("Orig", 2) of an LSP. A value of 4, "Normal", indicates the CrossConnect is switching through an LSP on an intermediate node. A value of 3, "Special", implies a terminating LSP for special traffic, e.g. signaling neighbor discovery, etc. Reserved MPLS labels with values 0 through 15 are used.
ValueMap | string | 1, 2, 3, 4
Values | string | Term, Orig, Special, Normal

### Association References

Name | Class Origin | Reference Class
--- | --- | ---
Antecedent | CIM_MPLSCrossConnectLSP | CIM_MPLSLSP
Dependent | CIM_MPLSCrossConnectLSP | CIM_MPLSCrossConnect

## Class Methods