# Class CIM_PrintInterlock
extends CIM_PrinterElement

This class represents the PrintInterlock (cover, access panel, or other interlock) component of a Printer (print device). It contains properties that describe the PrintInterlock component and the component status. Note: A PrintInterlock shall be associated with exactly one Printer via an instance of the ConcreteComponent class. See: Model in section 2 of Printer MIB (RFC 3805).

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_PrinterElement
|
+--CIM_PrintInterlock

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | This class represents the PrintInterlock (cover, access panel, or other interlock) component of a Printer (print device). It contains properties that describe the PrintInterlock component and the component status. Note: A PrintInterlock shall be associated with exactly one Printer via an instance of the ConcreteComponent class. See: Model in section 2 of Printer MIB (RFC 3805).
Experimental | boolean | true
MappingStrings | string | MIB.IETF|Printer-MIB.prtCoverEntry
UMLPackagePath | string | CIM::Device::Printing
Version | string | 2.18.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
InterlockStatus | uint32 |
Description | string | This property contains detailed status information for this PrintInterlock (cover, access panel, or other interlock), as follows: 1 (Other) means other detailed status information for this PrintInterlock is present in the OtherInterlockStatus property. 2 (Unknown) means detailed status information for this PrintInterlock is unknown. 3 (CoverOpen) means this PrintInterlock is a cover that is open (typically an exception condition). 4 (CoverClosed) means this PrintInterlock is a cover that is closed (typically a normal condition). 5 (InterlockOpen) means this PrintInterlock is an access panel or other interlock that is open (typically an exception condition). 6 (InterlockClosed) means this PrintInterlock is an access panel or other interlock that is closed (typically a normal condition).
MappingStrings | string | MIB.IETF|Printer-MIB.prtCoverStatus, MIB.IETF|IANA-PRINTER-MIB.PrtCoverStatusTC
ModelCorrespondence | string | CIM_ManagedSystemElement.DetailedStatus, CIM_PrintInterlock.OtherInterlockStatus
ValueMap | string | 1, 2, 3, 4, 5, 6, ..
Values | string | Other, Unknown, CoverOpen, CoverClosed, InterlockOpen, InterlockClosed, DMTF Reserved
LocalizedDescription | string |
Description | string | A free-form text description of this PrintInterlock (cover, access panel, or other interlock) in the localization specified by CIM_Printer.CurrentNaturalLanguage.
MappingStrings | string | MIB.IETF|Printer-MIB.prtCoverDescription, MIB.IETF|Printer-MIB.PrtLocalizedDescriptionStringTC
MaxLen | uint32 | 255
MinLen | uint32 | 0
OtherInterlockStatus | string |
Description | string | A free-form string that describes the detailed status of this PrintInterlock (cover, access panel, or other interlock) when the value of the InterlockStatus property is equal to 1 (Other).
MaxLen | uint32 | 255
MinLen | uint32 | 0
ModelCorrespondence | string | CIM_PrintInterlock.InterlockStatus

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
ElementName | string | CIM_ManagedElement
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_PrinterElement
Name | string | CIM_ManagedSystemElement
OperatingStatus | uint16 | CIM_ManagedSystemElement
PrimaryStatus | uint16 | CIM_ManagedSystemElement
SNMPRowId | uint32 | CIM_PrinterElement
Status | string | CIM_ManagedSystemElement
OperationalStatus | uint16[] | CIM_ManagedSystemElement
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods