# Class CIM_PrintFinisher
extends CIM_PrinterElement

This class represents the PrintFinisher component of a Printer (print device). It contains properties that describe the PrintFinisher type, capabilities, and status. Note: A PrintFinisher shall be associated with exactly one Printer via an instance of the ConcreteComponent class. See: Model in section 2 of Printer MIB (RFC 3805) and section 3 of Finisher MIB (RFC 3806).

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_PrinterElement
|
+--CIM_PrintFinisher

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | This class represents the PrintFinisher component of a Printer (print device). It contains properties that describe the PrintFinisher type, capabilities, and status. Note: A PrintFinisher shall be associated with exactly one Printer via an instance of the ConcreteComponent class. See: Model in section 2 of Printer MIB (RFC 3805) and section 3 of Finisher MIB (RFC 3806).
Experimental | boolean | true
MappingStrings | string | MIB.IETF|Finisher-MIB.finDeviceEntry
UMLPackagePath | string | CIM::Device::Printing
Version | string | 2.19.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
AvailabilityStatus | uint32 |
Description | string | This property contains detailed availability information for this PrintFinisher, as follows: 1 (Other) means other detailed availability information is present in the OtherAvailabilityStatus property. 2 (Unknown) means detailed availability information for this PrintFinisher is unknown. 3 (AvailableIdle) means this PrintFinisher is available and idle, i.e., not currently in use. 4 (AvailableStandy) means this PrintFinisher is available but on standby, e.g., in a power saving mode. 5 (AvailableActive) means this PrintFinisher is available and active, i.e., currently in use. 6 (AvailableBusy) means this PrintFinisher is available but busy, i.e., not immediately available for its primary function. 7 (UnavailableOnRequest) means this PrintFinisher is not available and is on request, i.e., needs human intervention. 8 (UnavailableBroken) means this PrintFinisher is not available and is broken, e.g., needs repair/replacement.
MappingStrings | string | MIB.IETF|Printer-MIB.PrtSubUnitStatusTC
ModelCorrespondence | string | CIM_ManagedSystemElement.OperatingStatus, CIM_PrintFinisher.OtherAvailabilityStatus
ValueMap | string | 1, 2, 3, 4, 5, 6, 7, 8, ..
Values | string | Other, Unknown, AvailableIdle, AvailableStandby, AvailableActive, AvailableBusy, UnavailableOnRequest, UnavailableBroken, DMTF Reserved
CapacityUnit | uint32 |
Description | string | The unit of measure for specifying the capacity of this PrintFinisher.
MappingStrings | string | MIB.IETF|Finisher-MIB.finDeviceCapacityUnit, MIB.IETF|Printer-MIB.PrtCapacityUnitTC
ModelCorrespondence | string | CIM_PrintFinisher.OtherCapacityUnit
ValueMap | string | 1, 2, 3, 4, 8, 16, 17, 18, 19, ..
Values | string | Other, Unknown, TenThousandthsOfInches, Micrometers, Sheets, Feet, Meters, Items, Percent, DMTF Reserved
CriticalAlertsPresent | boolean |
Description | string | If true, there are currently critical alerts on this PrintFinisher.
MappingStrings | string | MIB.IETF|Printer-MIB.PrtSubUnitStatusTC
ModelCorrespondence | string | CIM_ManagedSystemElement.DetailedStatus
CurrentCapacity | uint32 |
Description | string | The current capacity of the PrintFinisher in units specified by CIM_PrintFinisher.CapacityUnit. If this PrintFinisher can reliably sense this value, the value is sensed by the PrintFinisher and cannot be changed by the system administrator; otherwise, the value may be changed out-of-band by the system administrator.
MappingStrings | string | MIB.IETF|Finisher-MIB.finDeviceCurrentCapacity, MIB.IETF|Finisher-MIB.finDeviceCapacityUnit, MIB.IETF|Printer-MIB.PrtCapacityUnitTC
MaxValue | sint64 | 2147483647
MinValue | sint64 | 0
ModelCorrespondence | string | CIM_PrintFinisher.CurrentCapacityBasis
CurrentCapacityBasis | uint16 |
Description | string | The basis for the gauge property CurrentCapacity, that specifies whether a meaningful value is available. 1 (Other) means the PrintFinisher places no restrictions on capacity and CurrentCapacity shall be null. 2 (Unknown) means the PrintFinisher cannot sense a meaningful value and CurrentCapacity shall be null. 3 (Actual) means the PrintFinisher can sense a meaningful value and CurrentCapacity shall be present. 4 (AtLeastOne) means that the PrintFinisher can only sense that at least one capacity unit remains (i.e., not full) and CurrentCapacity shall be present and shall contain the value zero or one.
MappingStrings | string | MIB.IETF|Finisher-MIB.finDeviceCurrentCapacity
ModelCorrespondence | string | CIM_PrintFinisher.CurrentCapacity
ValueMap | string | 1, 2, 3, 4, ..
Values | string | Other, Unknown, Actual, AtLeastOne, DMTF Reserved
LocalizedDescription | string |
Description | string | A free-form text description of this PrintFinisher in the localization specified by CIM_Printer.CurrentNaturalLanguage.
MappingStrings | string | MIB.IETF|Finisher-MIB.finDeviceDescription, MIB.IETF|Printer-MIB.PrtLocalizedDescriptionStringTC
MaxLen | uint32 | 255
MinLen | uint32 | 0
ModelCorrespondence | string | CIM_Printer.CurrentNaturalLanguage
MaxCapacity | uint32 |
Description | string | The maximum capacity of the PrintFinisher in units specified by CIM_PrintFinisher.CapacityUnit. If this PrintFinisher can reliably sense this value, the value is sensed by the PrintFinisher and cannot be changed by the system administrator; otherwise, the value may be changed out-of-band by the system administrator.
MappingStrings | string | MIB.IETF|Finisher-MIB.finDeviceMaxCapacity, MIB.IETF|Finisher-MIB.finDeviceCapacityUnit, MIB.IETF|Printer-MIB.PrtCapacityUnitTC
MaxValue | sint64 | 2147483647
MinValue | sint64 | 0
ModelCorrespondence | string | CIM_PrintFinisher.MaxCapacityBasis
MaxCapacityBasis | uint16 |
Description | string | The basis for the limit property MaxCapacity, that specifies whether a meaningful value is available. 1 (Other) means the PrintFinisher places no restrictions on capacity and MaxCapacity shall be null. 2 (Unknown) means the PrintFinisher cannot sense a meaningful value and MaxCapacity shall be null. 3 (Actual) means the PrintFinisher can sense a meaningful value and MaxCapacity shall be present.
MappingStrings | string | MIB.IETF|Finisher-MIB.finDeviceMaxCapacity
ModelCorrespondence | string | CIM_PrintFinisher.MaxCapacity
ValueMap | string | 1, 2, 3, ..
Values | string | Other, Unknown, Actual, DMTF Reserved
NonCriticalAlertsPresent | boolean |
Description | string | If true, there are currently non-critical alerts on this PrintFinisher.
MappingStrings | string | MIB.IETF|Printer-MIB.PrtSubUnitStatusTC
ModelCorrespondence | string | CIM_ManagedSystemElement.DetailedStatus
OtherAvailabilityStatus | string |
Description | string | A free-form string that describes the detailed availability of this PrintFinisher when the value of the AvailabilityStatus property is equal to 1 (Other).
MaxLen | uint32 | 255
MinLen | uint32 | 0
ModelCorrespondence | string | CIM_PrintFinisher.AvailabilityStatus
OtherCapacityUnit | string |
Description | string | A free-form string that describes the capacity unit when the value of the CapacityUnit property is equal to 1 (Other).
MaxLen | uint32 | 255
MinLen | uint32 | 0
ModelCorrespondence | string | CIM_PrintFinisher.CapacityUnit
OtherTypeDescription | string |
Description | string | A free-form string that describes the type of PrintFinisher when the value of the Type property is equal to 1 (Other).
MaxLen | uint32 | 255
MinLen | uint32 | 0
ModelCorrespondence | string | CIM_PrintFinisher.Type
PresentOnOff | uint32 |
Description | string | Denotes whether this PrintFinisher is present (configured) and whether the PrintFinisher is enabled.
MappingStrings | string | MIB.IETF|Finisher-MIB.finDevicePresentOnOff, MIB.IETF|Printer-MIB.PresentOnOff
ValueMap | string | 1, 2, 3, 4, 5, ..
Values | string | Other, Unknown, On, Off, NotPresent, DMTF Reserved
Type | uint32 |
Description | string | Defines the type of finishing process associated with this PrintFinisher.
MappingStrings | string | MIB.IETF|Finisher-MIB.finDeviceType, MIB.IETF|IANA-PRINTER-MIB.PrtMarkerMarkTechTC
ModelCorrespondence | string | CIM_PrintFinisher.OtherTypeDescription
ValueMap | string | 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, ..
Values | string | Other, Unknown, Stitcher, Folder, Binder, Trimmer, DieCutter, Puncher, Perforater, Slitter, SeparationCutter, Imprinter, Wrapper, Bander, MakeEnvelope, Stacker, SheetRotator, Inserter, DMTF Reserved

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
ElementName | string | CIM_ManagedElement
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_PrinterElement
Name | string | CIM_ManagedSystemElement
OperatingStatus | uint16 | CIM_ManagedSystemElement
PrimaryStatus | uint16 | CIM_ManagedSystemElement
SNMPRowId | uint32 | CIM_PrinterElement
Status | string | CIM_ManagedSystemElement
OperationalStatus | uint16[] | CIM_ManagedSystemElement
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods