# Class CIM_ImagingStatisticalData
extends CIM_StatisticalData

This class extends StatisticalData to abstract the concept of ImagingStatisticalData associated with an imaging system (e.g., ComputerSystem), imaging service (e.g., PrintService), imaging device (e.g., Printer), imaging job (e.g., PrintJob), or any other imaging element. This abstract class defines common properties for: (a) persistence (PersistenceType and OtherPersistenceType); (b) correlation of ImagingStatisticalData information between CIM and SNMP interfaces (SNMPKeyId). Note: An instance of any concrete class derived from this abstract class shall be associated with exactly one instance of a scoping imaging element (e.g., Printer) via an instance of the ElementStatisticalData association class. See: Model and diagram in section 4 of PWG Imaging System State and Counter MIB (PWG 5106.3-2008, or successor).

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_StatisticalData
|
+--CIM_ImagingStatisticalData

## Direct Known Subclasses

CIM_ImagingMediaUsedStatisticalData
CIM_ImagingMonitorStatisticalData
CIM_ImagingWorkStatisticalData

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Abstract | boolean | true
Description | string | This class extends StatisticalData to abstract the concept of ImagingStatisticalData associated with an imaging system (e.g., ComputerSystem), imaging service (e.g., PrintService), imaging device (e.g., Printer), imaging job (e.g., PrintJob), or any other imaging element. This abstract class defines common properties for: (a) persistence (PersistenceType and OtherPersistenceType); (b) correlation of ImagingStatisticalData information between CIM and SNMP interfaces (SNMPKeyId). Note: An instance of any concrete class derived from this abstract class shall be associated with exactly one instance of a scoping imaging element (e.g., Printer) via an instance of the ElementStatisticalData association class. See: Model and diagram in section 4 of PWG Imaging System State and Counter MIB (PWG 5106.3-2008, or successor).
Experimental | boolean | true
UMLPackagePath | string | CIM::Core::Statistics
Version | string | 2.20.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
OtherPersistenceType | string |
Description | string | A free-form string that describes the persistence when the the value of the PersistenceType property is equal to 1 (Other).
MaxLen | uint32 | 255
MinLen | uint32 | 0
ModelCorrespondence | string | CIM_ImagingStatisticalData.PersistenceType, CIM_FileSystemSetting.OtherPersistenceTypes
PersistenceType | uint16 |
Description | string | Persistence of this instance of ImagingStatisticalData. 1 (Other) means vendor-specific persistence and should not be used (to avoid interoperability problems). 2 (Unknown) means unknown persistence and should not be be used (to avoid amgiguity in accounting applications). 3 (Lifetime) means since install of the scoping imaging element (e.g., PrintService). 4 (PowerOn) means since last power on of the scoping imaging element (e.g., Printer). 5 (Reset) means since the last reset of this instance of ImagingStatisticalData.
MappingStrings | string | MIB.PWG|PWG-IMAGING-COUNTER-MIB.icMonitorPersistence, MIB.PWG|PWG-IMAGING-COUNTER-MIB.icTimePersistence, MIB.PWG|PWG-IMAGING-COUNTER-MIB.icMediaUsedPersistence, MIB.PWG|PWG-IMAGING-COUNTER-MIB.icTrafficPersistence, MIB.PWG|PWG-IMAGING-COUNTER-MIB.icImagePersistence, MIB.PWG|PWG-IMAGING-COUNTER-MIB.icImpressionPersistence, MIB.PWG|PWG-IMAGING-COUNTER-MIB.icTwoSidedPersistence, MIB.PWG|PWG-IMAGING-COUNTER-MIB.icSheetPersistence
ModelCorrespondence | string | CIM_ImagingStatisticalData.OtherPersistenceType, CIM_StatisticalData.ResetSelectedStats, CIM_FileSystemSetting.PersistenceTypes
ValueMap | string | 1, 2, 3, 4, 5, ..
Values | string | Other, Unknown, Lifetime, PowerOn, Reset, DMTF Reserved
SNMPKeyId | uint32 |
Description | string | A unique value used by the scoping imaging element (e.g., PrintService) to identify this ImagingStatisticalData. Note: This property is necessary to correlate counter and event information between CIM and SNMP interfaces.
MappingStrings | string | MIB.PWG|PWG-IMAGING-COUNTER-MIB.icMonitorKeyIndex, MIB.PWG|PWG-IMAGING-COUNTER-MIB.icTimeKeyIndex, MIB.PWG|PWG-IMAGING-COUNTER-MIB.icMediaUsedKeyIndex, MIB.PWG|PWG-IMAGING-COUNTER-MIB.icTrafficKeyIndex, MIB.PWG|PWG-IMAGING-COUNTER-MIB.icImageKeyIndex, MIB.PWG|PWG-IMAGING-COUNTER-MIB.icImpressionKeyIndex, MIB.PWG|PWG-IMAGING-COUNTER-MIB.icTwoSidedKeyIndex, MIB.PWG|PWG-IMAGING-COUNTER-MIB.icSheetKeyIndex
MaxValue | sint64 | 2147483647
MinValue | sint64 | 1

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
Description | string | CIM_ManagedElement
ElementName | string | CIM_StatisticalData
Generation | uint64 | CIM_ManagedElement
InstanceID | string | CIM_StatisticalData
RateIntervalEndTime | datetime | CIM_StatisticalData
RateIntervalStartTime | datetime | CIM_StatisticalData
SampleInterval | datetime | CIM_StatisticalData
StartStatisticTime | datetime | CIM_StatisticalData
StatisticTime | datetime | CIM_StatisticalData

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
ResetSelectedStats | uint32 | CIM_StatisticalData