# Class CIM_PrintOutputTray
extends CIM_PrinterElement

This class represents the PrintOutputTray component of a Printer (print device). It contains properties that describe a device capable of receiving media delivered from the printing process. Note: A PrintOutputTray shall be associated with exactly one Printer via an instance of the PrinterComponent class. See: Model in section 2 of Printer MIB (RFC 3805).

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_PrinterElement
|
+--CIM_PrintOutputTray

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | This class represents the PrintOutputTray component of a Printer (print device). It contains properties that describe a device capable of receiving media delivered from the printing process. Note: A PrintOutputTray shall be associated with exactly one Printer via an instance of the PrinterComponent class. See: Model in section 2 of Printer MIB (RFC 3805).
Experimental | boolean | true
MappingStrings | string | MIB.IETF|Printer-MIB.prtOutputEntry
UMLPackagePath | string | CIM::Device::Printing
Version | string | 2.19.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
AvailabilityStatus | uint32 |
Description | string | This property contains detailed availability information for this PrintOutputTray, as follows: 1 (Other) means other detailed availability information is present in the OtherAvailabilityStatus property. 2 (Unknown) means detailed availability information for this PrintOutputTray is unknown. 3 (AvailableIdle) means this PrintOutputTray is available and idle, i.e., not currently in use. 4 (AvailableStandy) means this PrintOutputTray is available but on standby, e.g., in a power saving mode. 5 (AvailableActive) means this PrintOutputTray is available and active, i.e., currently in use. 6 (AvailableBusy) means this PrintOutputTray is available but busy, i.e., not immediately available for its primary function. 7 (UnavailableOnRequest) means this PrintOutputTray is not available and is on request, i.e., needs human intervention. 8 (UnavailableBroken) means this PrintOutputTray is not available and is broken, e.g., needs repair/replacement.
MappingStrings | string | MIB.IETF|Printer-MIB.PrtSubUnitStatusTC
ModelCorrespondence | string | CIM_ManagedSystemElement.OperatingStatus, CIM_PrintOutputTray.OtherAvailabilityStatus
ValueMap | string | 1, 2, 3, 4, 5, 6, 7, 8, ..
Values | string | Other, Unknown, AvailableIdle, AvailableStandby, AvailableActive, AvailableBusy, UnavailableOnRequest, UnavailableBroken, DMTF Reserved
CapacityUnit | uint32 |
Description | string | The unit of measurement for use in calculating and relaying capacity values for this PrintOutputTray.
MappingStrings | string | MIB.IETF|Printer-MIB.prtOutputCapacityUnit, MIB.IETF|Printer-MIB.PrtCapacityUnitTC
ValueMap | string | 1, 2, 3, 4, 8, 16, 17, 18, 19, ..
Values | string | Other, Unknown, TenThousandthsOfInches, Micrometers, Sheets, Feet, Meters, Items, Percent, DMTF Reserved
CriticalAlertsPresent | boolean |
Description | string | If true, there are currently critical alerts on this PrintOutputTray.
MappingStrings | string | MIB.IETF|Printer-MIB.PrtSubUnitStatusTC
ModelCorrespondence | string | CIM_ManagedSystemElement.DetailedStatus
ElementName | string |
Description | string | The user-friendly name for this instance of PrintOutputTray. In addition, the user-friendly name can be used as an index property for a search or query. (Note: The name does not have to be unique within a namespace.) This name shall be generated as a factory default by the manufacturer and may be changed out-of-band to a site-specific name by the system administrator.
MappingStrings | string | MIB.IETF|Printer-MIB.prtOutputName
ModelCorrespondence | string | CIM_ManagedElement.ElementName
Override | string | ElementName
Required | boolean | true
IsDefault | boolean |
Description | string | Denotes whether or not this PrintOutputTray is the default PrintOutputTray for this printer. If the default PrintOutputTray feature is not supported for this printer, then this property shall be null. If the default PrintOutputTray feature is supported for this printer, then this property shall be true for at most one instance of CIM_PrintOutputTray on this printer, i.e., the default may not be currently configured.
MappingStrings | string | MIB.IETF|Printer-MIB.prtOutputDefaultIndex
LocalizedDescription | string |
Description | string | A free-form text description of this PrintOutputTray in the localization specified by CIM_Printer.CurrentNaturalLanguage.
MappingStrings | string | MIB.IETF|Printer-MIB.prtOutputDescription, MIB.IETF|Printer-MIB.PrtLocalizedDescriptionStringTC
MaxLen | uint32 | 255
MinLen | uint32 | 0
ModelCorrespondence | string | CIM_Printer.CurrentNaturalLanguage
MaxCapacity | uint32 |
Description | string | The maximum capacity of this PrintOutputTray. There is no convention associated with the media itself so this value essentially reflects claimed capacity. If this PrintOutputTray can reliably sense this value, the value is sensed by the Printer and cannot be changed by the system administrator; otherwise, the value may be changed out-of-band by the system administrator.
MappingStrings | string | MIB.IETF|Printer-MIB.prtOutputMaxCapacity, MIB.IETF|Printer-MIB.prtOutputCapacityUnit, MIB.IETF|Printer-MIB.PrtCapacityUnitTC
MaxValue | sint64 | 2147483647
MinValue | sint64 | 0
MaxCapacityBasis | uint16 |
Description | string | The basis for the limit property MaxCapacity, that specifies whether a meaningful value is available. 1 (Other) means the PrintOutputTray places no restrictions on capacity and MaxCapacity shall be null. 2 (Unknown) means the PrintOutputTray cannot sense a meaningful value and MaxCapacity shall be null. 3 (Actual) means the PrintOutputTray can sense a meaningful value and MaxCapacity shall be present.
MappingStrings | string | MIB.IETF|Printer-MIB.prtOutputMaxCapacity
ModelCorrespondence | string | CIM_PrintOutputTray.MaxCapacity
ValueMap | string | 1, 2, 3, ..
Values | string | Other, Unknown, Actual, DMTF Reserved
NonCriticalAlertsPresent | boolean |
Description | string | If true, there are currently non-critical alerts on this PrintOutputTray.
MappingStrings | string | MIB.IETF|Printer-MIB.PrtSubUnitStatusTC
ModelCorrespondence | string | CIM_ManagedSystemElement.DetailedStatus
OtherAvailabilityStatus | string |
Description | string | A free-form string that describes the detailed availability of this PrintOutputTray when the value of the AvailabilityStatus property is equal to 1 (Other).
MaxLen | uint32 | 255
MinLen | uint32 | 0
ModelCorrespondence | string | CIM_PrintOutputTray.AvailabilityStatus
OtherCapacityUnit | string |
Description | string | A free-form string that describes the capacity unit when the value of the CapacityUnit property is equal to 1 (Other).
MaxLen | uint32 | 255
MinLen | uint32 | 0
OtherTypeDescription | string |
Description | string | A free-form string that describes the type of technology when the value of the Type property is equal to 1 (Other).
MaxLen | uint32 | 255
MinLen | uint32 | 0
RemainingCapacity | uint32 |
Description | string | The remaining capacity of this PrintOutputTray. If this PrintOutputTray can reliably sense this value, the value is sensed by the Printer and cannot be changed by the system administrator; otherwise, the value may be changed out-of-band by the system administrator.
MappingStrings | string | MIB.IETF|Printer-MIB.prtOutputRemainingCapacity, MIB.IETF|Printer-MIB.prtOutputCapacityUnit, MIB.IETF|Printer-MIB.PrtCapacityUnitTC
MaxValue | sint64 | 2147483647
MinValue | sint64 | 0
RemainingCapacityBasis | uint16 |
Description | string | The basis for the gauge property RemainingCapacity, that specifies whether a meaningful value is available. 1 (Other) means the Printer places no restrictions on capacity and RemainingCapacity shall be null. 2 (Unknown) means the Printer cannot sense a meaningful value and RemainingCapacity shall be null. 3 (Actual) means the Printer can sense a meaningful value and RemainingCapacity shall be present. 4 (AtLeastOne) means that the Printer can only sense that at least one capacity unit remains and RemainingCapacity shall be present and shall contain the value zero or one.
MappingStrings | string | MIB.IETF|Printer-MIB.prtOutputRemainingCapacity
ValueMap | string | 1, 2, 3, 4, ..
Values | string | Other, Unknown, Actual, AtLeastOne, DMTF Reserved
Type | uint32 |
Description | string | The type of technology supported by this PrintOutputTray.
MappingStrings | string | MIB.IETF|Printer-MIB.prtOutputType, MIB.IETF|IANA-PRINTER-MIB.PrtOutputTypeTC
ValueMap | string | 1, 2, 3, 4, 5, 6, 7, ..
Values | string | Other, Unknown, RemovableBin, UnRemovableBin, ContinuousRollDevice, MailBox, ContinuousFanFold, DMTF Reserved

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_PrinterElement
Name | string | CIM_ManagedSystemElement
OperatingStatus | uint16 | CIM_ManagedSystemElement
PrimaryStatus | uint16 | CIM_ManagedSystemElement
SNMPRowId | uint32 | CIM_PrinterElement
Status | string | CIM_ManagedSystemElement
OperationalStatus | uint16[] | CIM_ManagedSystemElement
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods