# Class CIM_PhysicalComputerSystemView
extends CIM_View

This class defines a view class for a physical computer system.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_View
|
+--CIM_PhysicalComputerSystemView

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | This class defines a view class for a physical computer system.
UMLPackagePath | string | CIM::Core::CoreElements
Version | string | 2.36.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
CurrentBIOSBuildNumber | uint16 |
Description | string | The build number component of the current BIOS version information.
ModelCorrespondence | string | CIM_SoftwareIdentity.BuildNumber
CurrentBIOSMajorVersion | uint16 |
Description | string | The major number component of the current BIOS version information.
ModelCorrespondence | string | CIM_SoftwareIdentity.MajorVersion
CurrentBIOSMinorVersion | uint16 |
Description | string | The minor number component of the current BIOS version information.
ModelCorrespondence | string | CIM_SoftwareIdentity.MinorVersion
CurrentBIOSRevisionNumber | uint16 |
Description | string | The revision number component of the current BIOS version information.
ModelCorrespondence | string | CIM_SoftwareIdentity.RevisionNumber
CurrentBIOSVersionString | string |
Description | string | The BIOS version information in string format.
ModelCorrespondence | string | CIM_SoftwareIdentity.VersionString
CurrentManagementFirmwareBuildNumber | uint16 |
Description | string | The build number component of the version information for the current management firmware on this physical computer system.
ModelCorrespondence | string | CIM_SoftwareIdentity.BuildNumber
CurrentManagementFirmwareElementName | string |
Description | string | The user-friendly name for the current management firmware on this physical computer system.
ModelCorrespondence | string | CIM_SoftwareIdentity.ElementName
CurrentManagementFirmwareMajorVersion | uint16 |
Description | string | The major number component of the version information for the current management firmware on this physical computer system.
ModelCorrespondence | string | CIM_SoftwareIdentity.MajorVersion
CurrentManagementFirmwareMinorVersion | uint16 |
Description | string | The minor number component of the version information for the current management firmware on this physical computer system.
ModelCorrespondence | string | CIM_SoftwareIdentity.MinorVersion
CurrentManagementFirmwareRevisionNumber | uint16 |
Description | string | The revision number component of the version information for the current management firmware on this physical computer system.
ModelCorrespondence | string | CIM_SoftwareIdentity.RevisionNumber
CurrentManagementFirmwareVersionString | string |
Description | string | The version string for the current management firmware on this physical computer system.
ModelCorrespondence | string | CIM_SoftwareIdentity.VersionString
EnabledState | uint16 |
Description | string | This property corresponds to the EnabledState property of the logical computer system represented by CIM_ComputerSystem. See CIM_EnabledLogicalElement.EnabledState for details on EnabledState.
ModelCorrespondence | string | CIM_ComputerSystem.EnabledState
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11..32767, 32768..65535
Values | string | Unknown, Other, Enabled, Disabled, Shutting Down, Not Applicable, Enabled but Offline, In Test, Deferred, Quiesce, Starting, DMTF Reserved, Vendor Reserved
FRUInfoSupported | boolean |
Description | string | This property indicates the availability of the FRU Information on this physical computer system. See CIM_PhysicalAssetCapabilities.FRUInfoSupported for details.
ModelCorrespondence | string | CIM_PhysicalAssetCapabilities.FRUInfoSupported
HealthState | uint16 |
Description | string | This property corresponds to the HealthState property of the logical computer system represented by CIM_ComputerSystem. See CIM_ManagedSystemElement.HealthState for details.
ModelCorrespondence | string | CIM_ComputerSystem.HealthState
ValueMap | string | 0, 5, 10, 15, 20, 25, 30, .., 32768..65535
Values | string | Unknown, OK, Degraded/Warning, Minor failure, Major failure, Critical failure, Non-recoverable error, DMTF Reserved, Vendor Specific
InstanceID | string |
Description | string | InstanceID is the property that may be used to opaquely and uniquely identify an instance of this class within the scope of the instantiating Namespace.
Key | boolean | true
Override | string | InstanceID
Manufacturer | string |
Description | string | This property corresponds to CIM_PhysicalFrame.Manufacturer. See CIM_PhysicalFrame.Manufacturer for details.
ModelCorrespondence | string | CIM_PhysicalFrame.Manufacturer
MemoryBlockSize | uint64 |
Description | string | See CIM_Memory.BlockSize for details.
ModelCorrespondence | string | CIM_Memory.BlockSize
MemoryConsumableBlocks | uint64 |
Description | string | See CIM_Memory.ConsumableBlocks for details.
ModelCorrespondence | string | CIM_Memory.ConsumableBlocks
MemoryNumberOfBlocks | uint64 |
Description | string | See CIM_Memory.NumberOfBlocks for details.
ModelCorrespondence | string | CIM_Memory.NumberOfBlocks
Model | string |
Description | string | This property corresponds to CIM_PhysicalFrame.Model. See CIM_PhysicalFrame.Model for details.
ModelCorrespondence | string | CIM_PhysicalFrame.Model
NumberOfProcessorCores | uint16 |
Description | string | See CIM_ProcessorCapabilities.NumberOfProcessorCores for details.
ModelCorrespondence | string | CIM_ProcessorCapabilities.NumberOfProcessorCores
NumberOfProcessors | uint16 |
Description | string | This property identifies the number of processors on this physical computer system.
NumberOfProcessorThreads | uint16 |
Description | string | See CIM_ProcessorCapabilities.NumberOfProcessorThreads for details.
ModelCorrespondence | string | CIM_ProcessorCapabilities.NumberOfHardwareThreads
OneTimeBootSource | uint8 |
Description | string | This property identifies the boot source that is used for the next one-time boot. The value of this property is an index referencing an element in the array of StructuredBootString.
OSEnabledState | uint16 |
Description | string | EnabledState of the current or last running operating system on this physcial computer system.
ModelCorrespondence | string | CIM_OperatingSystem.EnabledState
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11..32767, 32768..65535
Values | string | Unknown, Other, Enabled, Disabled, Shutting Down, Not Applicable, Enabled but Offline, In Test, Deferred, Quiesce, Starting, DMTF Reserved, Vendor Reserved
OSType | uint16 |
Description | string | Type information of the current or last running operating system on this physical computer system. See CIM_OperatingSystem.OSType for details.
ModelCorrespondence | string | CIM_OperatingSystem.OSType
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20, 21, 22, 23, 24, 25, 26, 27, 28, 29, 30, 31, 32, 33, 34, 35, 36, 37, 38, 39, 40, 41, 42, 43, 44, 45, 46, 47, 48, 49, 50, 51, 52, 53, 54, 55, 56, 57, 58, 59, 60, 61, 62, 63, 64, 65, 66, 67, 68, 69, 70, 71, 72, 73, 74, 75, 76, 77, 78, 79, 80, 81, 82, 83, 84, 85, 86, 87, 88, 89, 90, 91, 92, 93, 94, 95, 96, 97, 98, 99, 100, 101, 102, 103, 104, 105, 106, 107, 108, 109, 110, 111, 113, 114, 115, 116
Values | string | Unknown, Other, MACOS, ATTUNIX, DGUX, DECNT, Tru64 UNIX, OpenVMS, HPUX, AIX, MVS, OS400, OS/2, JavaVM, MSDOS, WIN3x, WIN95, WIN98, WINNT, WINCE, NCR3000, NetWare, OSF, DC/OS, Reliant UNIX, SCO UnixWare, SCO OpenServer, Sequent, IRIX, Solaris, SunOS, U6000, ASERIES, HP NonStop OS, HP NonStop OSS, BS2000, LINUX, Lynx, XENIX, VM, Interactive UNIX, BSDUNIX, FreeBSD, NetBSD, GNU Hurd, OS9, MACH Kernel, Inferno, QNX, EPOC, IxWorks, VxWorks, MiNT, BeOS, HP MPE, NextStep, PalmPilot, Rhapsody, Windows 2000, Dedicated, OS/390, VSE, TPF, Windows (R) Me, Caldera Open UNIX, OpenBSD, Not Applicable, Windows XP, z/OS, Microsoft Windows Server 2003, Microsoft Windows Server 2003 64-Bit, Windows XP 64-Bit, Windows XP Embedded, Windows Vista, Windows Vista 64-Bit, Windows Embedded for Point of Service, Microsoft Windows Server 2008, Microsoft Windows Server 2008 64-Bit, FreeBSD 64-Bit, RedHat Enterprise Linux, RedHat Enterprise Linux 64-Bit, Solaris 64-Bit, SUSE, SUSE 64-Bit, SLES, SLES 64-Bit, Novell OES, Novell Linux Desktop, Sun Java Desktop System, Mandriva, Mandriva 64-Bit, TurboLinux, TurboLinux 64-Bit, Ubuntu, Ubuntu 64-Bit, Debian, Debian 64-Bit, Linux 2.4.x, Linux 2.4.x 64-Bit, Linux 2.6.x, Linux 2.6.x 64-Bit, Linux 64-Bit, Other 64-Bit, Microsoft Windows Server 2008 R2, VMware ESXi, Microsoft Windows 7, CentOS 32-bit, CentOS 64-bit, Oracle Linux 32-bit, Oracle Linux 64-bit, eComStation 32-bitx, Microsoft Windows Server 2011, Microsoft Windows Server 2012, Microsoft Windows 8, Microsoft Windows 8 64-bit, Microsoft Windows Server 2012 R2
OSVersion | string |
Description | string | Version information of the current or last running operating system on this physical computer system. See CIM_OperatingSystem.Version for details.
ModelCorrespondence | string | CIM_OperatingSystem.Version
PartNumber | string |
Description | string | This property corresponds to CIM_PhysicalFrame.PartNumber. See CIM_PhysicalFrame.PartNumber for details.
ModelCorrespondence | string | CIM_PhysicalFrame.PartNumber
PowerAllocationLimit | uint64 |
Description | string | This property corresponds to CIM_PowerAllocationSettingData.Limit. See CIM_PowerAllocationSettingData.Limit for details.
ModelCorrespondence | string | CIM_PowerAllocationSettingData.Limit
PUnit | string | watt * 10^-3
PowerUtilizationMode | uint16 |
Description | string | This property corresponds to the PowerUtilizationMode of the CIM_PowerUtilizationManagementService. See CIM_PowerUtilizationManagementService.PowerUtilizationMode for details.
ModelCorrespondence | string | CIM_PowerUtilizationManagementService.PowerUtilizationMode
ValueMap | string | 2, 3, 4, .., 32768..65535
Values | string | None, Dynamic, Static, DMTF Reserved, Vendor Reserved
ProcessorCurrentClockSpeed | uint32 |
Description | string | See CIM_Processor.CurrentClockSpeed for details.
ModelCorrespondence | string | CIM_Processor.CurrentClockSpeed
PUnit | string | hertz * 10^6
ProcessorFamily | uint16 |
Description | string | See CIM_Processor.Family for details.
ModelCorrespondence | string | CIM_Processor.Family
ValueMap | string | 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20, 21, 24, 25, 26, 27, 28, 29, 30, 31, 32, 33, 34, 35, 36, 37, 38, 39, 40, 41, 42, 43, 44, 48, 49, 50, 51, 52, 53, 54, 55, 56, 57, 58, 59, 60, 61, 62, 63, 64, 65, 66, 67, 68, 69, 70, 71, 72, 73, 74, 75, 76, 77, 78, 79, 80, 81, 82, 83, 84, 85, 86, 87, 88, 96, 97, 98, 99, 100, 101, 102, 103, 104, 112, 120, 121, 122, 128, 130, 131, 132, 133, 134, 135, 136, 137, 138, 139, 140, 141, 142, 143, 144, 145, 146, 147, 148, 149, 150, 160, 161, 162, 163, 164, 165, 166, 167, 168, 169, 170, 171, 172, 173, 174, 175, 176, 177, 178, 179, 180, 181, 182, 183, 184, 185, 186, 187, 188, 189, 190, 191, 192, 193, 194, 195, 196, 197, 198, 199, 200, 201, 202, 203, 204, 205, 206, 210, 211, 212, 213, 214, 215, 216, 217, 218, 219, 221, 222, 223, 224, 228, 229, 230, 231, 232, 233, 234, 235, 236, 237, 238, 239, 250, 251, 254, 255, 260, 261, 280, 281, 300, 301, 302, 320, 350, 500, 65534, 65535
Values | string | Other, Unknown, 8086, 80286, 80386, 80486, 8087, 80287, 80387, 80487, Pentium(R) brand, Pentium(R) Pro, Pentium(R) II, Pentium(R) processor with MMX(TM) technology, Celeron(TM), Pentium(R) II Xeon(TM), Pentium(R) III, M1 Family, M2 Family, Intel(R) Celeron(R) M processor, Intel(R) Pentium(R) 4 HT processor, K5 Family, K6 Family, K6-2, K6-3, AMD Athlon(TM) Processor Family, AMD(R) Duron(TM) Processor, AMD29000 Family, K6-2+, Power PC Family, Power PC 601, Power PC 603, Power PC 603+, Power PC 604, Power PC 620, Power PC X704, Power PC 750, Intel(R) Core(TM) Duo processor, Intel(R) Core(TM) Duo mobile processor, Intel(R) Core(TM) Solo mobile processor, Intel(R) Atom(TM) processor, Intel(R) Core(TM) M processor, Alpha Family, Alpha 21064, Alpha 21066, Alpha 21164, Alpha 21164PC, Alpha 21164a, Alpha 21264, Alpha 21364, AMD Turion(TM) II Ultra Dual-Core Mobile M Processor Family, AMD Turion(TM) II Dual-Core Mobile M Processor Family, AMD Athlon(TM) II Dual-Core Mobile M Processor Family, AMD Opteron(TM) 6100 Series Processor, AMD Opteron(TM) 4100 Series Processor, AMD Opteron(TM) 6200 Series Processor, AMD Opteron(TM) 4200 Series Processor, AMD FX(TM) Series Processor, MIPS Family, MIPS R4000, MIPS R4200, MIPS R4400, MIPS R4600, MIPS R10000, AMD C-Series Processor, AMD E-Series Processor, AMD A-Series Processor, AMD G-Series Processor, AMD Z-Series Processor, AMD R-Series Processor, AMD Opteron(TM) 4300 Series Processor, AMD Opteron(TM) 6300 Series Processor, AMD Opteron(TM) 3300 Series Processor, AMD FirePro(TM) Series Processor, SPARC Family, SuperSPARC, microSPARC II, microSPARC IIep, UltraSPARC, UltraSPARC II, UltraSPARC IIi, UltraSPARC III, UltraSPARC IIIi, 68040, 68xxx Family, 68000, 68010, 68020, 68030, AMD Athlon(TM) X4 Quad-Core Processor Family, AMD Opteron(TM) X1000 Series Processor, AMD Opteron(TM) X2000 Series APU, Hobbit Family, Crusoe(TM) TM5000 Family, Crusoe(TM) TM3000 Family, Efficeon(TM) TM8000 Family, Weitek, Itanium(TM) Processor, AMD Athlon(TM) 64 Processor Family, AMD Opteron(TM) Processor Family, AMD Sempron(TM) Processor Family, AMD Turion(TM) 64 Mobile Technology, Dual-Core AMD Opteron(TM) Processor Family, AMD Athlon(TM) 64 X2 Dual-Core Processor Family, AMD Turion(TM) 64 X2 Mobile Technology, Quad-Core AMD Opteron(TM) Processor Family, Third-Generation AMD Opteron(TM) Processor Family, AMD Phenom(TM) FX Quad-Core Processor Family, AMD Phenom(TM) X4 Quad-Core Processor Family, AMD Phenom(TM) X2 Dual-Core Processor Family, AMD Athlon(TM) X2 Dual-Core Processor Family, PA-RISC Family, PA-RISC 8500, PA-RISC 8000, PA-RISC 7300LC, PA-RISC 7200, PA-RISC 7100LC, PA-RISC 7100, V30 Family, Quad-Core Intel(R) Xeon(R) processor 3200 Series, Dual-Core Intel(R) Xeon(R) processor 3000 Series, Quad-Core Intel(R) Xeon(R) processor 5300 Series, Dual-Core Intel(R) Xeon(R) processor 5100 Series, Dual-Core Intel(R) Xeon(R) processor 5000 Series, Dual-Core Intel(R) Xeon(R) processor LV, Dual-Core Intel(R) Xeon(R) processor ULV, Dual-Core Intel(R) Xeon(R) processor 7100 Series, Quad-Core Intel(R) Xeon(R) processor 5400 Series, Quad-Core Intel(R) Xeon(R) processor, Dual-Core Intel(R) Xeon(R) processor 5200 Series, Dual-Core Intel(R) Xeon(R) processor 7200 Series, Quad-Core Intel(R) Xeon(R) processor 7300 Series, Quad-Core Intel(R) Xeon(R) processor 7400 Series, Multi-Core Intel(R) Xeon(R) processor 7400 Series, Pentium(R) III Xeon(TM), Pentium(R) III Processor with Intel(R) SpeedStep(TM) Technology, Pentium(R) 4, Intel(R) Xeon(TM), AS400 Family, Intel(R) Xeon(TM) processor MP, AMD Athlon(TM) XP Family, AMD Athlon(TM) MP Family, Intel(R) Itanium(R) 2, Intel(R) Pentium(R) M processor, Intel(R) Celeron(R) D processor, Intel(R) Pentium(R) D processor, Intel(R) Pentium(R) Processor Extreme Edition, Intel(R) Core(TM) Solo Processor, K7, Intel(R) Core(TM)2 Duo Processor, Intel(R) Core(TM)2 Solo processor, Intel(R) Core(TM)2 Extreme processor, Intel(R) Core(TM)2 Quad processor, Intel(R) Core(TM)2 Extreme mobile processor, Intel(R) Core(TM)2 Duo mobile processor, Intel(R) Core(TM)2 Solo mobile processor, Intel(R) Core(TM) i7 processor, Dual-Core Intel(R) Celeron(R) Processor, S/390 and zSeries Family, ESA/390 G4, ESA/390 G5, ESA/390 G6, z/Architectur base, Intel(R) Core(TM) i5 processor, Intel(R) Core(TM) i3 processor, VIA C7(TM)-M Processor Family, VIA C7(TM)-D Processor Family, VIA C7(TM) Processor Family, VIA Eden(TM) Processor Family, Multi-Core Intel(R) Xeon(R) processor, Dual-Core Intel(R) Xeon(R) processor 3xxx Series, Quad-Core Intel(R) Xeon(R) processor 3xxx Series, VIA Nano(TM) Processor Family, Dual-Core Intel(R) Xeon(R) processor 5xxx Series, Quad-Core Intel(R) Xeon(R) processor 5xxx Series, Dual-Core Intel(R) Xeon(R) processor 7xxx Series, Quad-Core Intel(R) Xeon(R) processor 7xxx Series, Multi-Core Intel(R) Xeon(R) processor 7xxx Series, Multi-Core Intel(R) Xeon(R) processor 3400 Series, AMD Opteron(TM) 3000 Series Processor, AMD Sempron(TM) II Processor Family, Embedded AMD Opteron(TM) Quad-Core Processor Family, AMD Phenom(TM) Triple-Core Processor Family, AMD Turion(TM) Ultra Dual-Core Mobile Processor Family, AMD Turion(TM) Dual-Core Mobile Processor Family, AMD Athlon(TM) Dual-Core Processor Family, AMD Sempron(TM) SI Processor Family, AMD Phenom(TM) II Processor Family, AMD Athlon(TM) II Processor Family, Six-Core AMD Opteron(TM) Processor Family, AMD Sempron(TM) M Processor Family, i860, i960, Reserved (SMBIOS Extension), Reserved (Un-initialized Flash Content - Lo), SH-3, SH-4, ARM, StrongARM, 6x86, MediaGX, MII, WinChip, DSP, Video Processor, Reserved (For Future Special Purpose Assignment), Reserved (Un-initialized Flash Content - Hi)
ProcessorMaxClockSpeed | uint32 |
Description | string | See CIM_Processor.MaxClockSpeed for details.
ModelCorrespondence | string | CIM_Processor.MaxClockSpeed
PUnit | string | hertz * 10^6
RequestedState | uint16 |
Description | string | This property corresponds to the RequestedState property of the logical computer system represented by CIM_ComputerSystem. See CIM_EnabledLogicalElement.RequestedState for details on RequestedState.
ModelCorrespondence | string | CIM_ComputerSystem.RequestedState
ValueMap | string | 0, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, .., 32768..65535
Values | string | Unknown, Enabled, Disabled, Shut Down, No Change, Offline, Test, Deferred, Quiesce, Reboot, Reset, Not Applicable, DMTF Reserved, Vendor Reserved
SerialNumber | string |
Description | string | This property corresponds to CIM_PhysicalFrame.SerialNumber. See CIM_PhysicalFrame.SerialNumber for details.
ModelCorrespondence | string | CIM_PhysicalFrame.SerialNumber
SKU | string |
Description | string | This property corresponds to CIM_PhysicalFrame.SKU. See CIM_PhysicalFrame.SKU for details.
ModelCorrespondence | string | CIM_PhysicalFrame.SKU
Tag | string |
Description | string | This property corresponds to CIM_PhysicalFrame.Tag. See CIM_PhysicalFrame.Tag for details.
ModelCorrespondence | string | CIM_PhysicalFrame.Tag
Version | string |
Description | string | This property corresponds to CIM_PhysicalFrame.Version. See CIM_PhysicalFrame.Version for details.
ModelCorrespondence | string | CIM_PhysicalFrame.Version
Dedicated | uint16[] |
ArrayType | string | Indexed
Description | string | See CIM_ComputerSystem.Dedicated for details.
ModelCorrespondence | string | CIM_ComputerSystem.Dedicated, CIM_PhysicalComputerSystemView.OtherDedicatedDescriptions
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20, 21, 22, 23, 24, 25, 26, 27, 28, 29, 30, 31, 32, 33, 34, 35, 36, 37, 38, .., 32568..65535
Values | string | Not Dedicated, Unknown, Other, Storage, Router, Switch, Layer 3 Switch, Central Office Switch, Hub, Access Server, Firewall, Print, I/O, Web Caching, Management, Block Server, File Server, Mobile User Device, Repeater, Bridge/Extender, Gateway, Storage Virtualizer, Media Library, ExtenderNode, NAS Head, Self-contained NAS, UPS, IP Phone, Management Controller, Chassis Manager, Host-based RAID controller, Storage Device Enclosure, Desktop, Laptop, Virtual Tape Library, Virtual Library System, Network PC/Thin Client, FC Switch, Ethernet Switch, DMTF Reserved, Vendor Reserved
IdentifyingDescriptions | string[] |
ArrayType | string | Indexed
Description | string | See CIM_System.IdentifyingDescriptions for details.
ModelCorrespondence | string | CIM_ComputerSystem.IdentifyingDescriptions, CIM_PhysicalComputerSystemView.OtherIdentifyingInfo
LogCurrentNumberOfRecords | uint64[] |
ArrayType | string | Indexed
Description | string | See CIM_RecordLog.CurrentNumberOfRecords for details.
ModelCorrespondence | string | CIM_RecordLog.CurrentNumberOfRecords, CIM_PhysicalComputerSystemView.LogInstanceID, CIM_PhysicalComputerSystemView.LogMaxNumberOfRecords
LogInstanceID | string[] |
ArrayType | string | Indexed
Description | string | This property represents the identifiers for the underlying logs on this physical computer system. See CIM_RecordLog.InstanceID for details.
ModelCorrespondence | string | CIM_RecordLog.InstanceID
LogMaxNumberOfRecords | uint64[] |
ArrayType | string | Indexed
Description | string | See CIM_RecordLog.MaxNumberOfRecords for details.
ModelCorrespondence | string | CIM_RecordLog.MaxNumberOfRecords, CIM_PhysicalComputerSystemView.LogInstanceID
LogOverWritePolicy | uint16[] |
ArrayType | string | Indexed
Description | string | See CIM_RecordLog.OverWritePolicy for details.
ModelCorrespondence | string | CIM_RecordLog.OverwritePolicy, CIM_PhysicalComputerSystemView.LogInstanceID, CIM_PhysicalComputerSystemView.LogMaxNumberOfRecords, CIM_PhysicalComputerSystemView.LogCurrentNumberOfRecords
ValueMap | string | 0, 2, 7, .., 32768..65535
Values | string | Unknown, Wraps When Full, Never Overwrites, DMTF Reserved, Vendor Reserved
LogState | uint16[] |
ArrayType | string | Indexed
Description | string | See CIM_RecordLog.LogState for details.
ModelCorrespondence | string | CIM_RecordLog.LogState, CIM_PhysicalComputerSystemView.LogInstanceID, CIM_PhysicalComputerSystemView.LogMaxNumberOfRecords, CIM_PhysicalComputerSystemView.LogCurrentNumberOfRecords, CIM_PhysicalComputerSystemView.LogOverwritePolicy
ValueMap | string | 0, 2, 3, 4, .., 32768..65535
Values | string | Unknown, Normal, Erasing, Not Applicable, DMTF Reserved, Vendor Reserved
NumericSensorBaseUnits | uint16[] |
ArrayType | string | Indexed
Description | string | Base units of the values returned by the numeric sensors. See CIM_NumericSensor.BaseUnits for details.
ModelCorrespondence | string | CIM_NumericSensor.BaseUnits, CIM_PhysicalComputerSystemView.NumericSensorElementName, CIM_PhysicalComputerSystemView.NumericSensorEnabledState, CIM_PhysicalComputerSystemView.NumericSensorHealthState, CIM_PhysicalComputerSystemView.NumericSensorCurrentState, CIM_PhysicalComputerSystemView.NumericSensorPrimaryStatus
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20, 21, 22, 23, 24, 25, 26, 27, 28, 29, 30, 31, 32, 33, 34, 35, 36, 37, 38, 39, 40, 41, 42, 43, 44, 45, 46, 47, 48, 49, 50, 51, 52, 53, 54, 55, 56, 57, 58, 59, 60, 61, 62, 63, 64, 65, 66
Values | string | Unknown, Other, Degrees C, Degrees F, Degrees K, Volts, Amps, Watts, Joules, Coulombs, VA, Nits, Lumens, Lux, Candelas, kPa, PSI, Newtons, CFM, RPM, Hertz, Seconds, Minutes, Hours, Days, Weeks, Mils, Inches, Feet, Cubic Inches, Cubic Feet, Meters, Cubic Centimeters, Cubic Meters, Liters, Fluid Ounces, Radians, Steradians, Revolutions, Cycles, Gravities, Ounces, Pounds, Foot-Pounds, Ounce-Inches, Gauss, Gilberts, Henries, Farads, Ohms, Siemens, Moles, Becquerels, PPM (parts/million), Decibels, DbA, DbC, Grays, Sieverts, Color Temperature Degrees K, Bits, Bytes, Words (data), DoubleWords, QuadWords, Percentage, Pascals
NumericSensorContext | string[] |
ArrayType | string | Indexed
Description | string | See CIM_Sensor.SensorContext for details.
ModelCorrespondence | string | CIM_NumericSensor.SensorContext, CIM_PhysicalComputerSystemView.NumericSensorElementName, CIM_PhysicalComputerSystemView.NumericSensorEnabledState, CIM_PhysicalComputerSystemView.NumericSensorHealthState, CIM_PhysicalComputerSystemView.NumericSensorCurrentState, CIM_PhysicalComputerSystemView.NumericSensorPrimaryStatus, CIM_PhysicalComputerSystemView.NumericSensorBaseUnits, CIM_PhysicalComputerSystemView.NumericSensorUnitModifier, CIM_PhysicalComputerSystemView.NumericSensorRateUnits, CIM_PhysicalComputerSystemView.NumericSensorCurrentReading, CIM_PhysicalComputerSystemView.NumericSensorSensorType, CIM_PhysicalComputerSystemView.NumericSensorOtherSensorTypeDescription, CIM_PhysicalComputerSystemView.NumericSensorUpperThresholdNonCritical, CIM_PhysicalComputerSystemView.NumericSensorUpperThresholdCritical, CIM_PhysicalComputerSystemView.NumericSensorUpperThresholdFatal
NumericSensorCurrentReading | sint32[] |
ArrayType | string | Indexed
Description | string | See CIM_NumericSensor.CurrentReading for details.
ModelCorrespondence | string | CIM_NumericSensor.CurrentReading, CIM_PhysicalComputerSystemView.NumericSensorElementName, CIM_PhysicalComputerSystemView.NumericSensorEnabledState, CIM_PhysicalComputerSystemView.NumericSensorHealthState, CIM_PhysicalComputerSystemView.NumericSensorCurrentState, CIM_PhysicalComputerSystemView.NumericSensorPrimaryStatus, CIM_PhysicalComputerSystemView.NumericSensorBaseUnits, CIM_PhysicalComputerSystemView.NumericSensorUnitModifier, CIM_PhysicalComputerSystemView.NumericSensorRateUnits
NumericSensorCurrentState | string[] |
ArrayType | string | Indexed
Description | string | Current states of numeric sensors. See CIM_NumericSensor.CurrentState for details.
ModelCorrespondence | string | CIM_NumericSensor.CurrentState, CIM_PhysicalComputerSystemView.NumericSensorElementName, CIM_PhysicalComputerSystemView.NumericSensorEnabledState, CIM_PhysicalComputerSystemView.NumericSensorHealthState
NumericSensorElementName | string[] |
ArrayType | string | Indexed
Description | string | User-friendly names of the numeric sensors on the computer system. See CIM_NumericSensor.ElementName for details.
ModelCorrespondence | string | CIM_NumericSensor.ElementName
NumericSensorEnabledState | uint16[] |
ArrayType | string | Indexed
Description | string | States of numeric sensors. See CIM_NumericSensor.EnabledState for details.
ModelCorrespondence | string | CIM_NumericSensor.EnabledState, CIM_PhysicalComputerSystemView.NumericSensorElementName
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11..32767, 32768..65535
Values | string | Unknown, Other, Enabled, Disabled, Shutting Down, Not Applicable, Enabled but Offline, In Test, Deferred, Quiesce, Starting, DMTF Reserved, Vendor Reserved
NumericSensorHealthState | uint16[] |
ArrayType | string | Indexed
Description | string | Health states of numeric sensors. See CIM_NumericSensor.HealthState for details.
ModelCorrespondence | string | CIM_NumericSensor.HealthState, CIM_PhysicalComputerSystemView.NumericSensorElementName, CIM_PhysicalComputerSystemView.NumericSensorEnabledState
ValueMap | string | 0, 5, 10, 15, 20, 25, 30, .., 32768..65535
Values | string | Unknown, OK, Degraded/Warning, Minor failure, Major failure, Critical failure, Non-recoverable error, DMTF Reserved, Vendor Specific
NumericSensorLowerThresholdCritical | sint32[] |
ArrayType | string | Indexed
Description | string | See CIM_NumericSensor.LowerThresholdCritical description for details.
ModelCorrespondence | string | CIM_NumericSensor.LowerThresholdCritical, CIM_PhysicalComputerSystemView.NumericSensorElementName, CIM_PhysicalComputerSystemView.NumericSensorEnabledState, CIM_PhysicalComputerSystemView.NumericSensorHealthState, CIM_PhysicalComputerSystemView.NumericSensorCurrentState, CIM_PhysicalComputerSystemView.NumericSensorPrimaryStatus, CIM_PhysicalComputerSystemView.NumericSensorBaseUnits, CIM_PhysicalComputerSystemView.NumericSensorUnitModifier, CIM_PhysicalComputerSystemView.NumericSensorRateUnits, CIM_PhysicalComputerSystemView.NumericSensorCurrentReading, CIM_PhysicalComputerSystemView.NumericSensorSensorType, CIM_PhysicalComputerSystemView.NumericSensorOtherSensorTypeDescription, CIM_PhysicalComputerSystemView.NumericSensorUpperThresholdNonCritical, CIM_PhysicalComputerSystemView.NumericSensorUpperThresholdCritical, CIM_PhysicalComputerSystemView.NumericSensorUpperThresholdFatal
NumericSensorLowerThresholdFatal | sint32[] |
ArrayType | string | Indexed
Description | string | See CIM_NumericSensor.LowerThresholdFatal description for details.
ModelCorrespondence | string | CIM_NumericSensor.LowerThresholdFatal, CIM_PhysicalComputerSystemView.NumericSensorElementName, CIM_PhysicalComputerSystemView.NumericSensorEnabledState, CIM_PhysicalComputerSystemView.NumericSensorHealthState, CIM_PhysicalComputerSystemView.NumericSensorCurrentState, CIM_PhysicalComputerSystemView.NumericSensorPrimaryStatus, CIM_PhysicalComputerSystemView.NumericSensorBaseUnits, CIM_PhysicalComputerSystemView.NumericSensorUnitModifier, CIM_PhysicalComputerSystemView.NumericSensorRateUnits, CIM_PhysicalComputerSystemView.NumericSensorCurrentReading, CIM_PhysicalComputerSystemView.NumericSensorSensorType, CIM_PhysicalComputerSystemView.NumericSensorOtherSensorTypeDescription, CIM_PhysicalComputerSystemView.NumericSensorUpperThresholdNonCritical, CIM_PhysicalComputerSystemView.NumericSensorUpperThresholdCritical, CIM_PhysicalComputerSystemView.NumericSensorUpperThresholdFatal
NumericSensorLowerThresholdNonCritical | sint32[] |
ArrayType | string | Indexed
Description | string | See CIM_NumericSensor.LowerThresholdNonCritical for details.
ModelCorrespondence | string | CIM_NumericSensor.LowerThresholdNonCritical, CIM_PhysicalComputerSystemView.NumericSensorElementName, CIM_PhysicalComputerSystemView.NumericSensorEnabledState, CIM_PhysicalComputerSystemView.NumericSensorHealthState, CIM_PhysicalComputerSystemView.NumericSensorCurrentState, CIM_PhysicalComputerSystemView.NumericSensorPrimaryStatus, CIM_PhysicalComputerSystemView.NumericSensorBaseUnits, CIM_PhysicalComputerSystemView.NumericSensorUnitModifier, CIM_PhysicalComputerSystemView.NumericSensorRateUnits, CIM_PhysicalComputerSystemView.NumericSensorCurrentReading, CIM_PhysicalComputerSystemView.NumericSensorSensorType, CIM_PhysicalComputerSystemView.NumericSensorOtherSensorTypeDescription, CIM_PhysicalComputerSystemView.NumericSensorUpperThresholdNonCritical, CIM_PhysicalComputerSystemView.NumericSensorUpperThresholdCritical, CIM_PhysicalComputerSystemView.NumericSensorUpperThresholdFatal
NumericSensorOtherSensorTypeDescription | string[] |
ArrayType | string | Indexed
Description | string | See CIM_NumericSensor.OtherSensorTypeDescription for details.
ModelCorrespondence | string | CIM_NumericSensor.OtherSensorTypeDescription, CIM_PhysicalComputerSystemView.NumericSensorElementName, CIM_PhysicalComputerSystemView.NumericSensorEnabledState, CIM_PhysicalComputerSystemView.NumericSensorHealthState, CIM_PhysicalComputerSystemView.NumericSensorCurrentState, CIM_PhysicalComputerSystemView.NumericSensorPrimaryStatus, CIM_PhysicalComputerSystemView.NumericSensorBaseUnits, CIM_PhysicalComputerSystemView.NumericSensorUnitModifier, CIM_PhysicalComputerSystemView.NumericSensorRateUnits, CIM_PhysicalComputerSystemView.NumericSensorCurrentReading, CIM_PhysicalComputerSystemView.NumericSensorSensorType
NumericSensorPrimaryStatus | uint16[] |
ArrayType | string | Indexed
Description | string | Primary statuses of numeric sensors. See CIM_NumericSensor.PrimaryStatus for details.
ModelCorrespondence | string | CIM_NumericSensor.PrimaryStatus, CIM_PhysicalComputerSystemView.NumericSensorElementName, CIM_PhysicalComputerSystemView.NumericSensorEnabledState, CIM_PhysicalComputerSystemView.NumericSensorHealthState, CIM_PhysicalComputerSystemView.NumericSensorCurrentState
ValueMap | string | 0, 1, 2, 3, .., 0x8000..
Values | string | Unknown, OK, Degraded, Error, DMTF Reserved, Vendor Reserved
NumericSensorRateUnits | uint16[] |
ArrayType | string | Indexed
Description | string | See CIM_NumericSensor.RateUnits for details.
ModelCorrespondence | string | CIM_NumericSensor.RateUnits, CIM_PhysicalComputerSystemView.NumericSensorElementName, CIM_PhysicalComputerSystemView.NumericSensorEnabledState, CIM_PhysicalComputerSystemView.NumericSensorHealthState, CIM_PhysicalComputerSystemView.NumericSensorCurrentState, CIM_PhysicalComputerSystemView.NumericSensorPrimaryStatus, CIM_PhysicalComputerSystemView.NumericSensorBaseUnits, CIM_PhysicalComputerSystemView.NumericSensorUnitModifier
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9
Values | string | None, Per MicroSecond, Per MilliSecond, Per Second, Per Minute, Per Hour, Per Day, Per Week, Per Month, Per Year
NumericSensorSensorType | uint16[] |
ArrayType | string | Indexed
Description | string | See CIM_NumericSensor.SensorType for details.
ModelCorrespondence | string | CIM_NumericSensor.SensorType, CIM_PhysicalComputerSystemView.NumericSensorElementName, CIM_PhysicalComputerSystemView.NumericSensorEnabledState, CIM_PhysicalComputerSystemView.NumericSensorHealthState, CIM_PhysicalComputerSystemView.NumericSensorCurrentState, CIM_PhysicalComputerSystemView.NumericSensorPrimaryStatus, CIM_PhysicalComputerSystemView.NumericSensorBaseUnits, CIM_PhysicalComputerSystemView.NumericSensorUnitModifier, CIM_PhysicalComputerSystemView.NumericSensorRateUnits, CIM_PhysicalComputerSystemView.NumericSensorCurrentReading
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, .., 32768..65535
Values | string | Unknown, Other, Temperature, Voltage, Current, Tachometer, Counter, Switch, Lock, Humidity, Smoke Detection, Presence, Air Flow, Power Consumption, Power Production, Pressure, DMTF Reserved, Vendor Reserved
NumericSensorUnitModifier | sint32[] |
ArrayType | string | Indexed
Description | string | Unit modifiers for the values returned by the numeric sensors. See CIM_NumericSensor.UnitModifier description for details.
ModelCorrespondence | string | CIM_NumericSensor.UnitModifier, CIM_PhysicalComputerSystemView.NumericSensorElementName, CIM_PhysicalComputerSystemView.NumericSensorEnabledState, CIM_PhysicalComputerSystemView.NumericSensorHealthState, CIM_PhysicalComputerSystemView.NumericSensorCurrentState, CIM_PhysicalComputerSystemView.NumericSensorPrimaryStatus, CIM_PhysicalComputerSystemView.NumericSensorBaseUnits
NumericSensorUpperThresholdCritical | sint32[] |
ArrayType | string | Indexed
Description | string | See CIM_NumericSensor.UpperThresholdCritical description for details.
ModelCorrespondence | string | CIM_NumericSensor.UpperThresholdCritical, CIM_PhysicalComputerSystemView.NumericSensorElementName, CIM_PhysicalComputerSystemView.NumericSensorEnabledState, CIM_PhysicalComputerSystemView.NumericSensorHealthState, CIM_PhysicalComputerSystemView.NumericSensorCurrentState, CIM_PhysicalComputerSystemView.NumericSensorPrimaryStatus, CIM_PhysicalComputerSystemView.NumericSensorBaseUnits, CIM_PhysicalComputerSystemView.NumericSensorUnitModifier, CIM_PhysicalComputerSystemView.NumericSensorRateUnits, CIM_PhysicalComputerSystemView.NumericSensorCurrentReading, CIM_PhysicalComputerSystemView.NumericSensorSensorType, CIM_PhysicalComputerSystemView.NumericSensorOtherSensorTypeDescription, CIM_PhysicalComputerSystemView.NumericSensorUpperThresholdNonCritical
NumericSensorUpperThresholdFatal | sint32[] |
ArrayType | string | Indexed
Description | string | See CIM_NumericSensor.UpperThresholdFatal for details.
ModelCorrespondence | string | CIM_NumericSensor.UpperThresholdFatal, CIM_PhysicalComputerSystemView.NumericSensorElementName, CIM_PhysicalComputerSystemView.NumericSensorEnabledState, CIM_PhysicalComputerSystemView.NumericSensorHealthState, CIM_PhysicalComputerSystemView.NumericSensorCurrentState, CIM_PhysicalComputerSystemView.NumericSensorPrimaryStatus, CIM_PhysicalComputerSystemView.NumericSensorBaseUnits, CIM_PhysicalComputerSystemView.NumericSensorUnitModifier, CIM_PhysicalComputerSystemView.NumericSensorRateUnits, CIM_PhysicalComputerSystemView.NumericSensorCurrentReading, CIM_PhysicalComputerSystemView.NumericSensorSensorType, CIM_PhysicalComputerSystemView.NumericSensorOtherSensorTypeDescription, CIM_PhysicalComputerSystemView.NumericSensorUpperThresholdNonCritical, CIM_PhysicalComputerSystemView.NumericSensorUpperThresholdCritical
NumericSensorUpperThresholdNonCritical | sint32[] |
ArrayType | string | Indexed
Description | string | See CIM_NumericSensor.UpperThresholdNonCritical for details.
ModelCorrespondence | string | CIM_NumericSensor.UpperThresholdNonCritical, CIM_PhysicalComputerSystemView.NumericSensorElementName, CIM_PhysicalComputerSystemView.NumericSensorEnabledState, CIM_PhysicalComputerSystemView.NumericSensorHealthState, CIM_PhysicalComputerSystemView.NumericSensorCurrentState, CIM_PhysicalComputerSystemView.NumericSensorPrimaryStatus, CIM_PhysicalComputerSystemView.NumericSensorBaseUnits, CIM_PhysicalComputerSystemView.NumericSensorUnitModifier, CIM_PhysicalComputerSystemView.NumericSensorRateUnits, CIM_PhysicalComputerSystemView.NumericSensorCurrentReading, CIM_PhysicalComputerSystemView.NumericSensorSensorType, CIM_PhysicalComputerSystemView.NumericSensorOtherSensorTypeDescription
OperationalStatus | uint16[] |
Description | string | This property corresponds to the OperationalStatus property of the logical computer system represented by CIM_ComputerSystem. See CIM_ManagedSystemElement.OperationalStatus Description for details.
ModelCorrespondence | string | CIM_ComputerSystem.OperationalStatus
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, .., 0x8000..
Values | string | Unknown, Other, OK, Degraded, Stressed, Predictive Failure, Error, Non-Recoverable Error, Starting, Stopping, Stopped, In Service, No Contact, Lost Communication, Aborted, Dormant, Supporting Entity in Error, Completed, Power Mode, Relocating, DMTF Reserved, Vendor Reserved
OtherDedicatedDescriptions | string[] |
ArrayType | string | Indexed
Description | string | See CIM_ComputerSystem.OtherDedicatedDescriptions for details.
ModelCorrespondence | string | CIM_ComputerSystem.OtherDedicatedDescriptions, CIM_PhysicalComputerSystemView.Dedicated
OtherIdentifyingInfo | string[] |
ArrayType | string | Indexed
Description | string | See CIM_System.OtherIdentifyingInfo for details.
MaxLen | uint32 | 256
ModelCorrespondence | string | CIM_ComputerSystem.OtherIdentifyingInfo, CIM_PhysicalComputerSystemView.IdentifyingDescriptions
PersistentBootConfigOrder | uint8[] |
ArrayType | string | Ordered
Description | string | An array of elements identifying the boot order of the persistent boot configuration that shall be used during the next boot of the computer system, unless the OneTimeBootSource for the next boot is specified. The value of each element in this array is an index referencing an element in the array of StructuredBootString.
PowerUtilizationModesSupported | uint16[] |
Description | string | This property corresponds to PowerUtilizationModesSupported property of CIM_PowerUtilizationManagementCapabilities. See CIM_PowerUtilizationManagementCapabilities.PowerUtilizationModesSupported for details.
ModelCorrespondence | string | CIM_PowerUtilizationManagementCapabilities.PowerUtilizationModesSupported
ValueMap | string | 3, 4, .., 32768..65535
Values | string | Dynamic, Static, DMTF Reserved, Vendor Reserved
StructuredBootString | string[] |
Description | string | Strings identifying the boot sources on this physical computer system. See CIM_BootSourceSetting.StructuredBootString description for details.
ModelCorrespondence | string | CIM_BootSourceSetting.StructuredBootString

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
Description | string | CIM_ManagedElement
ElementName | string | CIM_ManagedElement
Generation | uint64 | CIM_ManagedElement

## Class Methods

### Local Class Methods

#### RequestStateChange (uint32)

#### Method Qualifiers (RequestStateChange)

Name | Data Type | Value
--- | --- | ---
Description | string | An extrinsic method for changing the state of this physical computer system. Requests that the state of the element be changed to the value specified in the RequestedState parameter. When the requested state change takes place, the EnabledState and RequestedState will be the same. Invoking the RequestStateChange method multiple times could result in earlier requests being overwritten or lost. A return code of 0 shall indicate the state change was successfully initiated. A return code of 1 shall indicate that the method is not supported. A return code of 2 shall indicate that the method failed. A return code of 4096 shall indicate the state change was successfully initiated, a ConcreteJob has been created, and its reference returned in the output parameter Job.
ModelCorrespondence | string | CIM_ComputerSystem.RequestStateChange
ValueMap | string | 0, 1, 2, 4096, .., 32768..65535
Values | string | Completed with No Error, Not Supported, Failed, Job Started, DMTF Reserved, Vendor Reserved

#### Method Parameters (RequestStateChange)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
RequestedState | uint16
Description | string | See CIM_ComputerSystem.RequestedStateChange.RequestedState for details.
ModelCorrespondence | string | CIM_ComputerSystem.RequestStateChange(RequestedState)
ValueMap | string | 2, 3, 4, 6, 7, 8, 9, 10, 11, .., 32768..65535
Values | string | Enabled, Disabled, Shut Down, Offline, Test, Defer, Quiesce, Reboot, Reset, DMTF Reserved, Vendor Reserved
TimeoutPeriod | datetime
Description | string | See CIM_ComputerSystem.TimeoutPeriod for details.
ModelCorrespondence | string | CIM_ComputerSystem.RequestStateChange(TimeoutPeriod)
Job | REF CIM_ConcreteJob
Description | string | May contain a reference to the ConcreteJob created to track the state transition initiated by the method invocation.
In | boolean | false
Out | boolean | true

#### ClearLog (uint32)

#### Method Qualifiers (ClearLog)

Name | Data Type | Value
--- | --- | ---
Description | string | An extrinsic method for clearing a log on this physical computer system. Requests that the Log be cleared of all entries. The return value shall be 0 if the request was successfully executed, 1 if the request is not supported, and 2 if an error occurred. A return code of 4096 shall indicate the request to clear log was successfully initiated, a ConcreteJob has been created, and its reference returned in the output parameter Job.
ValueMap | string | 0, 1, 2, .., 32768..65535
Values | string | Completed with No Error, Not Supported, Failed, DMTF Reserved, Vendor Reserved

#### Method Parameters (ClearLog)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
LogInstanceID | string
Description | string | Idenfier for the log that is requested to be cleared.
ModelCorrespondence | string | CIM_RecordLog.InstanceID, CIM_PhysicalComputerSystemView.LogInstanceID

#### InstallSoftwareFromURI (uint32)

#### Method Qualifiers (InstallSoftwareFromURI)

Name | Data Type | Value
--- | --- | ---
Description | string | An extrinsic method for installing software on this physical computer system. If 0 is returned, the function completed successfully and no ConcreteJob instance was required. The return value shall be 1 if the request is not supported, and 2 if an error occurred. If 4096 is returned, a ConcreteJob will be started to to perform the install. The Job's reference will be returned in the output parameter Job.
ModelCorrespondence | string | CIM_SoftwareInstallationService.InstallFromURI
ValueMap | string | 0, 1, 2, 4096, .., 32768..65535
Values | string | Completed with No Error, Not Supported, Failed, Job Started, DMTF Reserved, Vendor Reserved

#### Method Parameters (InstallSoftwareFromURI)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
URI | string
Description | string | See CIM_SoftwareInstallationService.InstallFromURI.URI for details.
ModelCorrespondence | string | CIM_SoftwareInstallationService.InstallFromURI
Classifications | uint16[]
ArrayType | string | Indexed
Description | string | See CIM_SoftwareIdentity.Classifications for details.
ModelCorrespondence | string | CIM_SoftwareIdentity.Classifications
ValueMap | string | 10, 11, 13, 14, .., 0x8000..0xFFFF
Values | string | Firmware, BIOS/FCode, Software Bundle, Management Firmware, DMTF Reserved, Vendor Reserved
InstallOptions | uint16[]
ArrayType | string | Indexed
Description | string | See CIM_SoftwareInstallationService.InstallFromURI.InstallOptions for details.
ModelCorrespondence | string | CIM_SoftwareInstallationService.InstallFromURI(InstallOptions), CIM_PhysicalComputerSystemView.InstallSoftwareFromURI(InstallOptionsValues)
ValueMap | string | 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, .., 32768..65535
Values | string | Defer target/system reset, Force installation, Install, Update, Repair, Reboot, Password, Uninstall, Log, SilentMode, AdministrativeMode, ScheduleInstallAt, DMTF Reserved, Vendor Specific
InstallOptionsValues | string[]
ArrayType | string | Indexed
Description | string | See CIM_SoftwareInstallationService.InstallFromURI.InstallOptionsValues for details.
ModelCorrespondence | string | CIM_SoftwareInstallationService.InstallFromURI(InstallOptionsValues), CIM_PhysicalComputerSystemView.InstallSoftwareFromURI(InstallOptions)
Job | REF CIM_ConcreteJob
Description | string | Reference to the job (may be null if job completed).
In | boolean | false
Out | boolean | true

#### ModifyPersistentBootConfigOrder (uint32)

#### Method Qualifiers (ModifyPersistentBootConfigOrder)

Name | Data Type | Value
--- | --- | ---
Description | string | This method is used to change the order of boot sources for the persistent boot configuration specified by the property CIM_PhysicalComputerSystemView.PersistentBootConfigOrder.
ValueMap | string | 0, 1, 2, 4096, .., 32768..65535
Values | string | Completed with No Error, Not Supported, Failed, Job Started, DMTF Reserved, Vendor Reserved

#### Method Parameters (ModifyPersistentBootConfigOrder)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
StructuredBootString | string[]
Description | string | An ordered array of strings representing the order of boot sources.
ModelCorrespondence | string | CIM_PhysicalComputerSystemView.StructuredBootString
Job | REF CIM_ConcreteJob
Description | string | Reference to the job spawned if the operation continues after the method returns. (May be null if the task is completed).
In | boolean | false
Out | boolean | true

#### SetOneTimeBootSource (uint32)

#### Method Qualifiers (SetOneTimeBootSource)

Name | Data Type | Value
--- | --- | ---
Description | string | This method is used to set the one time boot source for the next boot on this computer system.
ValueMap | string | 0, 1, 2, 4096, .., 32768..65535
Values | string | Completed with No Error, Not Supported, Failed, Job Started, DMTF Reserved, Vendor Reserved

#### Method Parameters (SetOneTimeBootSource)

Name | Type | Qualifiers
--- | --- | ---
Name | Data Type | Value
StructuredBootString | string
Description | string | A string representing the boot source for next boot.
ModelCorrespondence | string | CIM_PhysicalComputerSystemView.StructuredBootString
Job | REF CIM_ConcreteJob
Description | string | Reference to the job spawned if the operation continues after the method returns. (May be null if the task is completed).
In | boolean | false
Out | boolean | true