# Class CIM_PhysicalMemory
extends CIM_Chip

PhysicalMemory is a subclass of CIM_Chip, representing low level memory devices - SIMMS, DIMMs, raw memory chips, etc.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_PhysicalElement
|
+--CIM_PhysicalComponent
|
+--CIM_Chip
|
+--CIM_PhysicalMemory

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
ClassConstraint | string | inv:self.IsSpeedInMhz=true implies self.Speed = 0 and self.MaxMemorySpeed > 0, inv:self.IsSpeedInMhz=false implies self.MaxMemorySpeed=null
Description | string | PhysicalMemory is a subclass of CIM_Chip, representing low level memory devices - SIMMS, DIMMs, raw memory chips, etc.
UMLPackagePath | string | CIM::Physical::Component
Version | string | 2.33.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
BankLabel | string |
Description | string | A string identifying the physically labeled bank where the Memory is located - for example, 'Bank 0' or 'Bank A'.
MappingStrings | string | MIF.DMTF|Memory Device|005.4
MaxLen | uint32 | 64
Capacity | uint64 |
Description | string | The total capacity of this PhysicalMemory, in bytes.
MappingStrings | string | MIF.DMTF|Memory Device|005.5
Units | string | Bytes
ConfiguredMemoryClockSpeed | uint32 |
Description | string | The configured clock speed (in MHz) of PhysicalMemory.
Units | string | MegaHertz
DataWidth | uint16 |
Description | string | Data width of the PhysicalMemory, in bits. A data width of 0 and a TotalWidth of 8 would indicate that the Memory is solely used to provide error correction bits.
MappingStrings | string | MIF.DMTF|Memory Device|005.8
Units | string | Bits
FormFactor | uint16 |
Description | string | The implementation form factor for the Chip. For example, values such as SIMM (7), TSOP (9) or PGA (10) can be specified.
MappingStrings | string | MIF.DMTF|Memory Device|005.6
Override | string | FormFactor
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20, 21, 22, 23
Values | string | Unknown, Other, SIP, DIP, ZIP, SOJ, Proprietary, SIMM, DIMM, TSOP, PGA, RIMM, SODIMM, SRIMM, SMD, SSMP, QFP, TQFP, SOIC, LCC, PLCC, BGA, FPBGA, LGA
InterleavePosition | uint32 |
Description | string | The position of this PhysicalMemory in an interleave. 0 indicates non-interleaved. 1 indicates the first position, 2 the second position and so on. For example, in a 2:1 interleave, a value of '1' would indicate that the Memory is in the 'even' position.
MappingStrings | string | MIF.DMTF|Memory Device Mapped Addresses|001.7
IsSpeedInMhz | boolean | false
Description | string | The IsSpeedInMHz property is used to indicate if the Speed property or the MaxMemorySpeed contains the value of the memory speed. A value of TRUE shall indicate that the speed is represented by the MaxMemorySpeed property. A value of FALSE shall indicate that the speed is represented by the Speed property.
ModelCorrespondence | string | CIM_PhysicalMemory.Speed, CIM_PhysicalMemory.MaxMemorySpeed
MaxMemorySpeed | uint32 |
Description | string | The maximum speed (in MHz) of PhysicalMemory.
ModelCorrespondence | string | CIM_PhysicalMemory.Speed, CIM_PhysicalMemory.IsSpeedInMHz
Units | string | MegaHertz
MemoryType | uint16 |
Description | string | The type of PhysicalMemory. Synchronous DRAM is also known as SDRAM Cache DRAM is also known as CDRAM CDRAM is also known as Cache DRAM SDRAM is also known as Synchronous DRAM BRAM is also known as Block RAM
MappingStrings | string | MIF.DMTF|Memory Device|005.9
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 19, 20, 21, 22, 23, 24, 25, 26, 27, 28, 29, 30, 31..32567, 32568..65535
Values | string | Unknown, Other, DRAM, Synchronous DRAM, Cache DRAM, EDO, EDRAM, VRAM, SRAM, RAM, ROM, Flash, EEPROM, FEPROM, EPROM, CDRAM, 3DRAM, SDRAM, SGRAM, RDRAM, DDR, DDR-2, BRAM, FB-DIMM, DDR3, FBD2, DDR4, LPDDR, LPDDR2, LPDDR3, LPDDR4, DMTF Reserved, Vendor Reserved
PositionInRow | uint32 |
Description | string | Specifies the position of the PhysicalMemory in a 'row'. For example, if it takes two 8-bit memory devices to form a 16- bit row, then a value of '2'means that this Memory is the second device. 0 is an invalid value for this property.
MappingStrings | string | MIF.DMTF|Memory Device Mapped Addresses|001.6
Speed | uint32 |
Description | string | The speed of the PhysicalMemory, in nanoseconds.
MappingStrings | string | MIF.DMTF|Memory Device|005.24
ModelCorrespondence | string | CIM_PhysicalMemory.MaxMemorySpeed, CIM_PhysicalMemory.IsSpeedInMHz
Units | string | NanoSeconds
TotalWidth | uint16 |
Description | string | Total width, in bits, of the PhysicalMemory, including check or error correction bits. If there are no error correction bits, the value in this property should match that specified for DataWidth.
MappingStrings | string | MIF.DMTF|Memory Device|005.7
Units | string | Bits

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
CanBeFRUed | boolean | CIM_PhysicalElement
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_PhysicalElement
Description | string | CIM_PhysicalElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
ElementName | string | CIM_PhysicalElement
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
HotSwappable | boolean | CIM_PhysicalComponent
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
ManufactureDate | datetime | CIM_PhysicalElement
Manufacturer | string | CIM_PhysicalElement
Model | string | CIM_PhysicalElement
Name | string | CIM_ManagedSystemElement
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherIdentifyingInfo | string | CIM_PhysicalElement
PartNumber | string | CIM_PhysicalElement
PoweredOn | boolean | CIM_PhysicalElement
PrimaryStatus | uint16 | CIM_ManagedSystemElement
Removable | boolean | CIM_PhysicalComponent
RemovalConditions | uint16 | CIM_PhysicalComponent
Replaceable | boolean | CIM_PhysicalComponent
SerialNumber | string | CIM_PhysicalElement
SKU | string | CIM_PhysicalElement
Status | string | CIM_ManagedSystemElement
Tag | string | CIM_PhysicalElement
UserTracking | string | CIM_PhysicalElement
VendorEquipmentType | string | CIM_PhysicalElement
Version | string | CIM_PhysicalElement
OperationalStatus | uint16[] | CIM_ManagedSystemElement
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods