# Class CIM_PartitionedLibrarySetting
extends CIM_SettingData

PartitionedLibrarySetting is the partition parameters.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_SettingData
|
+--CIM_PartitionedLibrarySetting

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | PartitionedLibrarySetting is the partition parameters.
Experimental | boolean | true
UMLPackagePath | string | CIM::Device::Tape
Version | string | 2.42.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
DriveCount | uint32 |
Description | string | Number of tape drives assigned to this partiion. This value can be null or zero if setting this property is not applicable to the chosen PartitionMethod. This property is applicable to Simple partitioning method.
LibraryName | string |
Description | string | The name assigned to this library partition.
LibraryType | string |
Description | string | The type of the physical library this partition is emulating. This is given as input when creating this partition. This string is vendor specific. A vendor may support emulating multiple physical library types as listed in the capabilities.
ModelCorrespondence | string | CIM_PartitionedLibrarySystemCapabilities.LibraryTypesSupported
PartitionMethod | uint16 |
Description | string | The method to use to create a partition. An array of allowed methods supported by the Partitioned Library can be obtained in the capabilities.
ModelCorrespondence | string | CIM_PartitionedLibrarySystemCapabilities.PartitionMethodsSupported
ValueMap | string | 2, 3, 4, 5, 6..32767, 32768..65535
Values | string | Auto, Simple, Slot, VolSer, DMTF Reserved, Vendor Reserved
SlotCount | uint32 |
Description | string | The capacity of this library partition in number of slots. The number specified here should not exceed the maximum number of slots specified in capabilities. This value can be null or zero if setting this property is not applicable to the chosen PartitionMethod. This is a partition slot count and may not be the physical slot count. This property is applicable to Simple and VolSer partitioning method.
RangeEndAddresses | string[] |
ArrayType | string | Indexed
Description | string | In Slot-based or VolSer-based partitioning, a range of addresses are given as input for creating a partition. For Slot-based partitioning a range of storage media location element addresses are given. For VolSer-based partitioning, a range of cartridge volume serial numbers are given. This property array gives the ending addresses of the ranges. These values coupled with the RangeStartAddresses a the same index provide the ranges necessary to create a partition. For other types of PartitionMethod, this property can be null.
ModelCorrespondence | string | CIM_PartitionedLibrarySetting.RangeStartAddresses
RangeStartAddresses | string[] |
ArrayType | string | Indexed
Description | string | In Slot-based or VolSer-based partitioning, a range of addresses are given as input for creating a partition. For Slot-based partitioning a range of storage media location addresses are given. For VolSer-based partitioning, a range of cartridge volume serial numbers are given to assign to a partition. Also for VolSer-based partitioning, a rane of storage media locations that contain the drive are given for assigning drives to a partition. This property array gives the starting addresses of the ranges. These values coupled with the RangeEndAddress values at the same index provide the ranges necessary to create a partition. For other types of PartitionMethod, this property can be null.
ModelCorrespondence | string | CIM_PartitionedLibrarySetting.RangeEndAddresses
RangeType | uint16[] |
ArrayType | string | Indexed
Description | string | Enumeration indicating the range type for each of the given ranges. For Slot-based partitioning, only storage media location addresses are give. For VolSer based partitioning a combination of storage media location address ranges and VolSer ranges can be given.
ValueMap | string | 2, 3, 4..32767, 32768..65535
Values | string | Slot, VolSer, DMTF Reserved, Vendor Reserved
SupportedMediaTypes | string[] |
Description | string | Supported Types of media within a single Partition.

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
ChangeableType | uint16 | CIM_SettingData
ConfigurationName | string | CIM_SettingData
Description | string | CIM_ManagedElement
ElementName | string | CIM_SettingData
Generation | uint64 | CIM_ManagedElement
InstanceID | string | CIM_SettingData
SoID | string | CIM_SettingData
SoOrgID | string | CIM_SettingData
ComponentSetting | string[] | CIM_SettingData

## Class Methods