# Class CIM_IPEndpointStatistics
extends CIM_ProtocolEndpointStatistics

CIM_IPEndpointStatistics records the statistics for an associated CIM_IPProtocolEndpoint.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_StatisticalData
|
+--CIM_ProtocolEndpointStatistics
|
+--CIM_IPEndpointStatistics

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | CIM_IPEndpointStatistics records the statistics for an associated CIM_IPProtocolEndpoint.
Experimental | boolean | true
UMLPackagePath | string | CIM::Network::ChannelExtender
Version | string | 2.8.1000

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
Fragmentation | uint32 |
Counter | boolean | true
Description | string | The number of IP datagrams that have been successfully fragmented at this entity.
MappingStrings | string | MIB.IETF|IP-MIB.ipFragOKs
FragmentationFails | uint32 |
Counter | boolean | true
Description | string | The number of IP datagrams that have been discarded because they needed to be fragmented at this entity but could not be, e.g., because their Don't Fragment flag was set.
MappingStrings | string | MIB.IETF|IP-MIB.ipFragFails
FragmentedPDUsCreates | uint32 |
Counter | boolean | true
Description | string | The number of IP datagram fragments that have been generated as a result of fragmentation at this entity.
MappingStrings | string | MIB.IETF|IP-MIB.ipFragCreates
PDUDelivers | uint32 |
Counter | boolean | true
Description | string | The total number of input datagrams successfully delivered to IP user-protocols (including ICMP).
MappingStrings | string | MIB.IETF|IP-MIB.ipInDelivers
ReassembledPackets | uint32 |
Counter | boolean | true
Description | string | The number of IP datagrams successfully re-assembled.
MappingStrings | string | MIB.IETF|IP-MIB.ipReasmOKs
ReassemblyFailed | uint32 |
Counter | boolean | true
Description | string | The number of failures detected by the IP re-assembly algorithm (for whatever reason: timed out, errors, etc). Note that this is not necessarily a count of discarded IP fragments since some algorithms (notably the algorithm in RFC 815) can lose track of the number of fragments by combining them as they are received.
MappingStrings | string | MIB.IETF|IP-MIB.ipReasmFails
ReassemblyRequired | uint32 |
Counter | boolean | true
Description | string | The number of IP fragments received which needed to be reassembled at this entity.
MappingStrings | string | MIB.IETF|IP-MIB.ipReasmReqds
ReceivedPDUAddressErrors | uint32 |
Counter | boolean | true
Description | string | The number of input datagrams discarded because the IP address in their IP header's destination field was not a valid address to be received at this entity. This count includes invalid addresses (e.g., 0.0.0.0) and addresses of unsupported Classes (e.g., Class E). For entities which are not IP routers and therefore do not forward datagrams, this counter includes datagrams discarded because the destination address was not a local address.
MappingStrings | string | MIB.IETF|IP-MIB.ipInAddrErrors
Override | string | ReceivedPDUAddressErrors
ReceivedPDUDiscards | uint32 |
Counter | boolean | true
Description | string | The number of input IP datagrams for which no problems were encountered to prevent their continued processing, but which were discarded (e.g., for lack of buffer space). Note that this counter does not include any datagrams discarded while awaiting re-assembly.
MappingStrings | string | MIB.IETF|IP-MIB.ipInDiscards
ReceivedPDUForwards | uint32 |
Counter | boolean | true
Description | string | The number of input datagrams for which this entity was not their final IP destination, as a result of which an attempt was made to find a route to forward them to that final destination. In entities which do not act as IP routers, this counter will include only those packets which were Source-Routed via this entity, and the Source-Route option processing was successful.
MappingStrings | string | MIB.IETF|IP-MIB.ipForwDatagrams
ReceivedPDUHeaderErrors | uint32 |
Counter | boolean | true
Description | string | The number of input datagrams discarded due to errors in their IP headers, including bad checksums, version number mismatch, other format errors, time-to-live exceeded, errors discovered in processing their IP options, etc.
MappingStrings | string | MIB.IETF|IP-MIB.ipInHdrErrors
Override | string | ReceivedPDUHeaderErrors
ReceivedPDUs | uint32 |
Counter | boolean | true
Description | string | The total number of input datagrams received from interfaces, including those received in error.
MappingStrings | string | MIB.IETF|IP-MIB.ipInReceives
Override | string | ReceivedPDUs
ReceivedPDUUnknownProtocolErrors | uint32 |
Counter | boolean | true
Description | string | The number of locally-addressed datagrams received successfully but discarded because of an unknown or unsupported protocol.
MappingStrings | string | MIB.IETF|IP-MIB.ipInUnknownProtos
RouteEntriesDiscards | uint32 |
Counter | boolean | true
Description | string | The number of routing entries which were chosen to be discarded even though they are valid. One possible reason for discarding such an entry could be to free-up buffer space for other routing entries.
MappingStrings | string | MIB.IETF|IP-MIB.ipRoutingDiscards
SentPDUDiscards | uint32 |
Counter | boolean | true
Description | string | The number of output IP datagrams for which no problem was encountered to prevent their transmission to their destination, but which were discarded (e.g., for lack of buffer space). Note that this counter would include datagrams counted in ipForwDatagrams if any such packets met this (discretionary) discard criterion.
MappingStrings | string | MIB.IETF|IP-MIB.ipOutDiscards
SentPDUNoRouteErrors | uint32 |
Counter | boolean | true
Description | string | The number of IP datagrams discarded because no route could be found to transmit them to their destination. Note that this counter includes any packets counted in ipForwDatagrams which meet this 'no-route' criterion. Note that this includes any datagrams which a host cannot route because all of its default routers are down.
MappingStrings | string | MIB.IETF|IP-MIB.ipOutNoRoutes
SentPDUs | uint32 |
Counter | boolean | true
Description | string | The total number of IP datagrams which local IP user-protocols (including ICMP) supplied to IP in requests for transmission. Note that this counter does not include any datagrams counted in ipForwDatagrams.
MappingStrings | string | MIB.IETF|IP-MIB.ipOutRequests
Override | string | SentPDUs

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
Description | string | CIM_ManagedElement
ElementName | string | CIM_StatisticalData
Generation | uint64 | CIM_ManagedElement
InstanceID | string | CIM_StatisticalData
RateIntervalEndTime | datetime | CIM_StatisticalData
RateIntervalStartTime | datetime | CIM_StatisticalData
SampleInterval | datetime | CIM_StatisticalData
StartStatisticTime | datetime | CIM_StatisticalData
StatisticTime | datetime | CIM_StatisticalData

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
ResetSelectedStats | uint32 | CIM_StatisticalData