# Class CIM_IPsecAction
extends CIM_SANegotiationAction

IPsecAction specifies the parameters to use for an IPsec phase 2 negotiation.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_Policy
|
+--CIM_PolicyAction
|
+--CIM_SAAction
|
+--CIM_SANegotiationAction
|
+--CIM_IPsecAction

## Direct Known Subclasses

CIM_IPsecTransportAction
CIM_IPsecTunnelAction

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | IPsecAction specifies the parameters to use for an IPsec phase 2 negotiation.
MappingStrings | string | IPSP Policy Model.IETF|IPsecAction
UMLPackagePath | string | CIM::IPsecPolicy
Version | string | 2.8.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
Granularity | uint16 |
Description | string | The property Granularity is an enumeration that specifies how the selector for the SA should be derived from the traffic that triggered the negotiation. Its values are: 1=Other; See the OtherGranularity property for more information 2=Subnet; The source and destination subnet masks are used 3=Address; The source and destination IP addresses of the triggering packet are used 4=Protocol; The source and destination IP addresses and the IP protocol of the triggering packet are used 5=Port; The source and destination IP addresses, IP protocol and the source and destination layer 4 ports of the triggering packet are used.
MappingStrings | string | IPSP Policy Model.IETF|IPsecAction.Granularity
ModelCorrespondence | string | CIM_IPsecAction.OtherGranularity
ValueMap | string | 1, 2, 3, 4, 5
Values | string | Other, Subnet, Address, Protocol, Port
GroupId | uint16 |
Description | string | GroupId specifies the PFS group ID to use. This value is only used if PFS is True and UsePhase1Group is False. If the GroupID number is from the vendor-specific range (32768-65535), the VendorID qualifies the group number. Well-known group identifiers from RFC2412, Appendix E, are: Group 1='768 bit prime', Group 2='1024 bit prime', Group 3='Elliptic Curve Group with 155 bit field element', Group 4='Large Elliptic Curve Group with 185 bit field element', and Group 5='1536 bit prime'.
MappingStrings | string | IPSP Policy Model.IETF|IPsecAction.GroupID, RFC2412.IETF|Appendix E
ModelCorrespondence | string | CIM_IPsecAction.VendorID, CIM_IKESAEndpoint.GroupID
ValueMap | string | 0, 1, 2, 3, 4, 5, .., 0x8000..
Values | string | No Group/Non-Diffie-Hellman Exchange, DH-768 bit prime, DH-1024 bit prime, EC2N-155 bit field element, EC2N-185 bit field element, DH-1536 bit prime, Standard Group - Reserved, Vendor Reserved
OtherGranularity | string |
Description | string | Description of the granularity when the value 1 ("Other") is specified for the property, Granularity.
ModelCorrespondence | string | CIM_IPsecAction.Granularity
UsePFS | boolean |
Description | string | UsePFS indicates whether perfect forward secrecy is required when refreshing keys.
MappingStrings | string | IPSP Policy Model.IETF|IPsecAction.UsePFS
ModelCorrespondence | string | CIM_IPsecSAEndpoint.PFSInUse
UsePhase1Group | boolean |
Description | string | UsePhase1Group indicates that the phase 2 GroupId should be the same as that used in the phase 1 key exchange. If UsePFS is False, then this property is ignored. Note that a value of False indicates that the property GroupId will contain the key exchange group to use for phase 2.
MappingStrings | string | IPSP Policy Model.IETF|IPsecAction.UseIKEGroup
VendorID | string |
Description | string | The property VendorID is used together with the property GroupID (when it is in the vendor-specific range) to identify the key exchange group. VendorID is ignored unless UsePFS is true, AND UsePhase1Group is False, AND GroupID is in the vendor-specific range (32768-65535).
MappingStrings | string | IPSP Policy Model.IETF|IPsecAction.VendorID
ModelCorrespondence | string | CIM_IPsecAction.GroupId, CIM_IKESAEndpoint.VendorID

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
CommonName | string | CIM_Policy
CreationClassName | string | CIM_PolicyAction
Description | string | CIM_ManagedElement
DoActionLogging | boolean | CIM_PolicyAction
DoPacketLogging | boolean | CIM_SAAction
ElementName | string | CIM_ManagedElement
Generation | uint64 | CIM_ManagedElement
IdleDurationSeconds | uint64 | CIM_SANegotiationAction
InstanceID | string | CIM_ManagedElement
MinLifetimeKilobytes | uint64 | CIM_SANegotiationAction
MinLifetimeSeconds | uint64 | CIM_SANegotiationAction
PolicyActionName | string | CIM_PolicyAction
PolicyRuleCreationClassName | string | CIM_PolicyAction
PolicyRuleName | string | CIM_PolicyAction
SystemCreationClassName | string | CIM_PolicyAction
SystemName | string | CIM_PolicyAction
PolicyKeywords | string[] | CIM_Policy

## Class Methods