# Class CIM_PowerManagementCapabilities
extends CIM_Capabilities

A class derived from Capabilities that describes the power management aspects of an element (typically a system or device). The element's power management capabilities are decoupled from a PowerManagementService, since a single service could apply to multiple elements, each with specific capabilities.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_Capabilities
|
+--CIM_PowerManagementCapabilities

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | A class derived from Capabilities that describes the power management aspects of an element (typically a system or device). The element's power management capabilities are decoupled from a PowerManagementService, since a single service could apply to multiple elements, each with specific capabilities.
UMLPackagePath | string | CIM::Core::PowerMgmt
Version | string | 2.23.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
OtherPowerChangeCapabilities | string |
Description | string | A string describing the additional power management capabilities of the element, used when the PowerChangeCapabilities is set to the value 1, "Other".
ModelCorrespondence | string | CIM_PowerManagementCapabilities.PowerChangeCapabilities
OtherPowerCapabilitiesDescriptions | string[] |
Description | string | An array of strings describing an element's additional power management capabilities, used when the PowerCapabilities array includes the value 1, "Other".
ModelCorrespondence | string | CIM_PowerManagementCapabilities.PowerCapabilities
PowerCapabilities | uint16[] |
Description | string | An enumeration indicating the specific power-related capabilities of a managed element. Since this is an array, multiple values may be specified. The current values in the enumeration are: 0 = Unknown 1 = Other 2 = Power Saving Modes Entered Automatically, describing that a managed element can change its power state based on usage or other criteria 3 = Power State Settable, indicating that the SetPowerState method is supported 4 = Power Cycling Supported, indicating that the SetPowerState method can be invoked with the PowerState input variable set to 'Power Cycle' 5 = Timed Power On Supported, indicating that the SetPowerState method can be invoked with the PowerState input variable set to 'Power Cycle' and the Time parameter set to a specific date and time, or interval, for power-on.
MappingStrings | string | MIF.DMTF|System Power Controls|001.2
ModelCorrespondence | string | CIM_PowerManagementCapabilities.OtherPowerCapabilitiesDescriptions, CIM_PowerManagementService.SetPowerState
ValueMap | string | 0, 1, 2, 3, 4, 5
Values | string | Unknown, Other, Power Saving Modes Entered Automatically, Power State Settable, Power Cycling Supported, Timed Power On Supported
PowerChangeCapabilities | uint16[] |
Description | string | An enumeration indicating the specific power-related capabilities of a managed element. Since this is an array, multiple values may be specified. The current values in the enumeration are: 0 = Unknown 1 = Other 2 = Power Saving Modes Entered Automatically, describing that a managed element can change its power state based on usage or other criteria 3 = Power State Settable, indicating that the RequestPowerStateChange method is supported 4 = Power Cycling Supported, indicating that the RequestPowerStateChange method can be invoked with the PowerState input variable set to 'Power Cycle (Off Soft)' 5 = Timed Power On Supported, indicating that the RequestPowerStateChange method can be invoked with the PowerState input variable set to 'Power On' and the Time parameter set to a specific date and time, or interval, for power-on.8 = Graceful Shutdown Supported, indicating that the managed element can be sent a hardware signal requesting an orderly shutdown prior to the requested power state change.
ModelCorrespondence | string | CIM_PowerManagementService.RequestPowerStateChange, CIM_PowerManagementCapabilities.OtherPowerChangeCapabilities
ValueMap | string | 0, 1, 2, 3, 4, 5, 6, 7, 8
Values | string | Unknown, Other, Power Saving Modes Entered Automatically, Power State Settable, Power Cycling Supported, Timed Power On Supported, Off Hard Power Cycling Supported, HW Reset Supported, Graceful Shutdown Supported
PowerStatesSupported | uint16[] |
Description | string | An enumeration that indicates the power states supported by a managed element. Because this is an array, multiple values can be specified. The current values in the enumeration are: 2=On, corresponding to ACPI state G0 or S0 or D0. 3=Sleep - Light, corresponding to ACPI state G1, S1/S2, or D1. 4=Sleep - Deep, corresponding to ACPI state G1, S3, or D2. 5=Power Cycle (Off - Soft), corresponding to ACPI state G2, S5, or D3, but where the managed element is set to return to power state "On" at a pre-determined time. 6=Off - Hard, corresponding to ACPI state G3, S5, or D3. 7=Hibernate (Off - Soft), corresponding to ACPI state S4, where the state of the managed element is preserved and will be recovered upon powering on. 8=Off - Soft, corresponding to ACPI state G2, S5, or D3. 9= Power Cycle (Off-Hard), corresponds to the managed element reaching the ACPI state G3 followed by ACPI state S0. 10=Master Bus Reset, corresponds to the system reaching ACPI state S5 followed by ACPI state S0. This is used to represent system master bus reset. 11=Diagnostic Interrupt (NMI), corresponding to the system reaching ACPI state S5 followed by ACPI state S0. This is used to represent system non-maskable interrupt. 12=Off - Soft Graceful, equivalent to Off Soft but preceded by a request to the managed element to perform an orderlyshutdown. 13=Off - Hard Graceful, equivalent to Off Hard but preceded by a request to the managed element to perform an orderly shutdown. 14=Master Bus Rest Graceful, equivalent to Master Bus Reset but preceded by a request to the managed element to perform an orderly shutdown. 15=Power Cycle (Off - Soft Graceful), equivalent to Power Cycle (Off - Soft) but preceded by a request to the managed element to perform an orderly shutdown. 16=Power Cycle (Off - Hard Graceful), equivalent to Power Cycle (Off - Hard) but preceded by a request to the managed element to perform an orderly shutdown. ..=DMTF Reserved. 0x7FFF..0xFFFF = Vendor Specific.
MappingStrings | string | IEEE P1621 | 3.2
ModelCorrespondence | string | CIM_PowerManagementService.RequestPowerStateChange, CIM_AssociatedPowerManagementService.PowerState
ValueMap | string | 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, .., 0x7FFF..0xFFFF
Values | string | Other, On, Sleep - Light, Sleep -Deep, Power Cycle (Off - Soft), Off - Hard, Hibernate (Off - Soft), Off - Soft, Power Cycle (Off-Hard), Master Bus Reset, Diagnostic Interrupt (NMI), Off - Soft Graceful, Off - Hard Graceful, Master Bus Reset Graceful, Power Cycle (Off - Soft Graceful), Power Cycle (Off - Hard Graceful), DMTF Reserved, Vendor Specific
RequestedPowerStatesSupported | uint16[] |
Description | string | An enumeration that indicates the requested power states supported by the power management service. Because this is an array, multiple values can be specified. The current values in the enumeration are: 2=On, corresponding to ACPI state G0 or S0 or D0. 3=Sleep - Light, corresponding to ACPI state G1, S1/S2, or D1. 4=Sleep - Deep, corresponding to ACPI state G1, S3, or D2. 5=Power Cycle (Off - Soft), corresponding to ACPI state G2, S5, or D3, but where the managed element is set to return to power state "On" at a pre-determined time. 6=Off - Hard, corresponding to ACPI state G3, S5, or D3. 7=Hibernate (Off - Soft), corresponding to ACPI state S4, where the state of the managed element is preserved and will be recovered upon powering on. 8=Off - Soft, corresponding to ACPI state G2, S5, or D3. 9= Power Cycle (Off-Hard), corresponds to the managed element reaching the ACPI state G3 followed by ACPI state S0. 10=Master Bus Reset, corresponds to the system reaching ACPI state S5 followed by ACPI state S0. This is used to represent system master bus reset. 11=Diagnostic Interrupt (NMI), corresponding to the system reaching ACPI state S5 followed by ACPI state S0. This is used to represent system non-maskable interrupt. 12=Off - Soft Graceful, equivalent to Off Soft but preceded by a request to the managed element to perform an orderlyshutdown. 13=Off - Hard Graceful, equivalent to Off Hard but preceded by a request to the managed element to perform an orderly shutdown. 14=Master Bus Rest Graceful, equivalent to Master Bus Reset but preceded by a request to the managed element to perform an orderly shutdown. 15=Power Cycle (Off - Soft Graceful), equivalent to Power Cycle (Off - Soft) but preceded by a request to the managed element to perform an orderly shutdown. 16=Power Cycle (Off - Hard Graceful), equivalent to Power Cycle (Off - Hard) but preceded by a request to the managed element to perform an orderly shutdown. 17=Diagnostic Interrupt (INIT), equivalent to Diagnostic Interrupt (NMI) but performed by an INIT switch instead because the NMI signal is masked. ..=DMTF Reserved. 0x7FFF..0xFFFF = Vendor Specific.
MappingStrings | string | IEEE P1621 | 3.2
ModelCorrespondence | string | CIM_PowerManagementCapabilities.PowerStatesSupported, CIM_PowerManagementService.RequestPowerStateChange, CIM_AssociatedPowerManagementService.PowerState
ValueMap | string | 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, .., 0x7FFF..0xFFFF
Values | string | Other, On, Sleep - Light, Sleep -Deep, Power Cycle (Off - Soft), Off - Hard, Hibernate (Off - Soft), Off - Soft, Power Cycle (Off-Hard), Master Bus Reset, Diagnostic Interrupt (NMI), Off - Soft Graceful, Off - Hard Graceful, Master Bus Reset Graceful, Power Cycle (Off - Soft Graceful), Power Cycle (Off - Hard Graceful), Diagnostic Interrupt (INIT), DMTF Reserved, Vendor Specific

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
Description | string | CIM_ManagedElement
ElementName | string | CIM_Capabilities
Generation | uint64 | CIM_ManagedElement
InstanceID | string | CIM_Capabilities

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
CreateGoalSettings | uint16 | CIM_Capabilities