# Class CIM_ATAProtocolEndpoint
extends CIM_ProtocolEndpoint

An ATAProtocolEndpoint represents the protocol (command) aspects of a logical ATA port, independent of the connection/transport. ATAProtocolEndpoint is either directly or indirectly associated to one or more instances of LogicalPort depending on the underlying transport.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_ServiceAccessPoint
|
+--CIM_ProtocolEndpoint
|
+--CIM_ATAProtocolEndpoint

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | An ATAProtocolEndpoint represents the protocol (command) aspects of a logical ATA port, independent of the connection/transport. ATAProtocolEndpoint is either directly or indirectly associated to one or more instances of LogicalPort depending on the underlying transport.
Experimental | boolean | true
UMLPackagePath | string | CIM::Network::ProtocolEndpoints
Version | string | 2.13.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
ConnectionType | uint16 |
Description | string | The supported connection type for this endpoint. The connection type may be needed before the port(s) are associated and also is used in some ATA commands.
ValueMap | string | 1, 2, 3
Values | string | Other, ATA, SATA
Name | string |
Description | string | The ATA identifier for the target or initiator device, in the format appropriate for the ConnectionType. If a ConnectionType specific subclass is defined, the subclass may override Name to define the format. For other ConnectionTypes, the format (and content) should match that of PermanentAddress of the corresponding port if the port is is subclassed from NetworkPort.
Key | boolean | true
MaxLen | uint32 | 256
Override | string | Name
OtherConnectionType | string |
Description | string | The connection type, if ConnectionType is "Other".
Role | uint16 |
Description | string | This property indicates which role this ProtocolEndpoint implements.
ValueMap | string | 0, 2, 3, 4
Values | string | Unknown, Initiator, Target, Both Initiator and Target

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
BroadcastResetSupported | boolean | CIM_ProtocolEndpoint
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_ServiceAccessPoint
Description | string | CIM_ProtocolEndpoint
DetailedStatus | uint16 | CIM_ManagedSystemElement
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_ProtocolEndpoint
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
NameFormat | string | CIM_ProtocolEndpoint
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
OtherTypeDescription | string | CIM_ProtocolEndpoint
PrimaryStatus | uint16 | CIM_ManagedSystemElement
ProtocolIFType | uint16 | CIM_ProtocolEndpoint
ProtocolType | uint16 | CIM_ProtocolEndpoint
RequestedState | uint16 | CIM_EnabledLogicalElement
Status | string | CIM_ManagedSystemElement
SystemCreationClassName | string | CIM_ServiceAccessPoint
SystemName | string | CIM_ServiceAccessPoint
TimeOfLastStateChange | datetime | CIM_ProtocolEndpoint
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
OperationalStatus | uint16[] | CIM_ProtocolEndpoint
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
BroadcastReset | uint32 | CIM_ProtocolEndpoint
RequestStateChange | uint32 | CIM_EnabledLogicalElement