# Class CIM_LAGPortPartnerConnection
extends CIM_ActiveConnection

LAGPortPartnerConnection contains the configuration information for an instance of a LAGPort8023ad's partner. The partner is defined as a RemoteServiceAccessPoint and it represents the actor's view of the connection. If there is no known partner, then this association will not be defined for an instance of LAGPort8023ad.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_Dependency
|
+--CIM_SAPSAPDependency
|
+--CIM_ActiveConnection
|
+--CIM_LAGPortPartnerConnection

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Association | boolean | true
Description | string | LAGPortPartnerConnection contains the configuration information for an instance of a LAGPort8023ad's partner. The partner is defined as a RemoteServiceAccessPoint and it represents the actor's view of the connection. If there is no known partner, then this association will not be defined for an instance of LAGPort8023ad.
Experimental | boolean | true
UMLPackagePath | string | CIM::Network::8023LAG
Version | string | 2.8.1000

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
PortPartnerAdminState | uint16 |
Description | string | An enumerated array allowing administrator control of the Actor_State for the protocol Partner. For more information, refer to the IEEE 802.3ad document, Subclause 30.7.2.1.22.
MappingStrings | string | MIB.IEEE|IEEE8023-LAG-MIB.dot3adAggPortPartnerAdminState
ModelCorrespondence | string | CIM_LAGPortPartnerConnection.PortPartnerOperState
ValueMap | string | 0, 2, 3, 4, 5, 6, 7, 8, 9
Values | string | Unknown/Undefined, LACP_Activity, LACP_Timeout, Aggregation, Synchronization, Collecting, Distributing, Defaulted, Expired
Write | boolean | true
PortPartnerOperKey | uint16 |
Description | string | The current operational value of the 16-bit Keyfor the protocol Partner. For more information, refer to the IEEE 802.3ad document, Subclause 30.7.2.1.11.
MappingStrings | string | MIB.IEEE|IEEE8023-LAG-MIB.dot3adAggPortPartnerOperKey
ModelCorrespondence | string | CIM_LAGPortPartnerSettings.PortPartnerAdminKey
PortPartnerOperPort | uint16 |
Description | string | The operational port number assigned to the Aggregation Port's protocol Partner. For more information, refer to the IEEE 802.3ad document, Subclause 30.7.2.1.17.
MappingStrings | string | MIB.IEEE|IEEE8023-LAG-MIB.dot3adAggPortPartnerOperPort
ModelCorrespondence | string | CIM_LAGPortPartnerSettings.PortPartnerAdminPort
PortPartnerOperPortPriority | uint16 |
Description | string | The priority value assigned to the AggregationPort's protocol Partner. For more information, refer to the IEEE 802.3ad document, Subclause 30.7.2.1.19.
MappingStrings | string | MIB.IEEE|IEEE8023-LAG-MIB.dot3adAggPortPartnerOperPortPriority
ModelCorrespondence | string | CIM_LAGPortPartnerSettings.PortPartnerAdminPortPriority
PortPartnerOperState | uint16 |
Description | string | An enumerated array defining the Actor_State for the protocol Partner, from the most recently received LACPDU transmitted by the partner. For more information, refer to the IEEE 802.3ad document, Subclause 30.7.2.1.23.
MappingStrings | string | MIB.IEEE|IEEE8023-LAG-MIB.dot3adAggPortPartnerOperState
ModelCorrespondence | string | CIM_LAGPortPartnerConnection.PortPartnerAdminState
ValueMap | string | 0, 2, 3, 4, 5, 6, 7, 8, 9
Values | string | Unknown/Undefined, LACP_Activity, LACP_Timeout, Aggregation, Synchronization, Collecting, Distributing, Defaulted, Expired
PortPartnerOperSystemID | string |
Description | string | A 6-octet MACAddress value representing the current value of the Aggregation Port's protocol Partner's System ID. For more information, refer to the IEEE 802.3ad document, Subclause 30.7.2.1.9. Note that the MAC address is formatted as twelve hexadecimal digits (e.g., "010203040506"), with each pair representing one of the six octets of the MAC address in "canonical" bit order according to RFC 2469.
MappingStrings | string | MIB.IEEE|IEEE8023-LAG-MIB.dot3adAggPortPartnerOperSystemID
MaxLen | uint32 | 12
ModelCorrespondence | string | CIM_LAGPortPartnerSettings.PortPartnerAdminSystemID
PortPartnerOperSystemPriority | uint16 |
Description | string | A 2-octet value indicating the operational value of priority associated with the Partner's System ID. For more information, refer to the IEEE 802.3ad document, Subclause 30.7.2.1.7.
MappingStrings | string | MIB.IEEE|IEEE8023-LAG-MIB.dot3adAggPortPartnerOperSystemPriority
ModelCorrespondence | string | CIM_LAGPortPartnerSettings.PortPartnerAdminSystemPriority

### Association References

Name | Class Origin | Reference Class
--- | --- | ---
Antecedent | CIM_LAGPortPartnerConnection | CIM_LAGPort8023ad
Dependent | CIM_LAGPortPartnerConnection | CIM_RemoteServiceAccessPoint

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
IsUnidirectional | boolean | CIM_ActiveConnection
OtherTrafficDescription | string | CIM_ActiveConnection
TrafficType | uint16 | CIM_ActiveConnection

## Class Methods