# Class CIM_IPNetworkSecurityIndication
extends CIM_SecurityIndication

IPNetworkSecurityIndication is a class that represents events that have a network context, i.e. a source or destination address is a necessary property of the indication. More specific Indication subclasses that can derive from this class are for example, firewall or intrusion detection subclasses. This class is not limited to use on IPv4 networks but has numerical property support for IPv4 networks that can be used for efficient implementations of search and analysis.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_Indication
|
+--CIM_ProcessIndication
|
+--CIM_AlertIndication
|
+--CIM_SecurityIndication
|
+--CIM_IPNetworkSecurityIndication

## Direct Known Subclasses

CIM_IPPacketFilterIndication

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | IPNetworkSecurityIndication is a class that represents events that have a network context, i.e. a source or destination address is a necessary property of the indication. More specific Indication subclasses that can derive from this class are for example, firewall or intrusion detection subclasses. This class is not limited to use on IPv4 networks but has numerical property support for IPv4 networks that can be used for efficient implementations of search and analysis.
Experimental | boolean | true
Indication | boolean | true
UMLPackagePath | string | CIM::Event
Version | string | 2.10.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
DestAddress | string |
Description | string | The address for the destination of the network traffic associated with this Indication from the Detector's point of view. This address MUST be identical to the IPv4NumericDestAddress if both property values are not NULL and the IPVersionSupport property is "IPv4".
ModelCorrespondence | string | CIM_IPNetworkSecurityIndication.IPv4NumericDestAddress, CIM_IPNetworkSecurityIndication.IPVersionSupport
DestMACAddress | string |
Description | string | The MAC address for the destination address for this message from the Detector's point of view.
ModelCorrespondence | string | CIM_IPNetworkSecurityIndication.DestAddress, CIM_IPNetworkSecurityIndication.IPv4NumericDestAddress
DestPort | uint32 |
Description | string | The port for the destination address for this message from the Detector's point of view.
ModelCorrespondence | string | CIM_IPNetworkSecurityIndication.DestAddress, CIM_IPNetworkSecurityIndication.IPv4NumericDestAddress
DestPrefixLength | uint8 |
Description | string | The prefix length for the IPv6 address for the destination of the network traffic associated with this Indication from the Detector's point of view.
ModelCorrespondence | string | CIM_IPNetworkSecurityIndication.DestAddress, CIM_IPNetworkSecurityIndication.IPVersionSupport
IPv4NumericDestAddress | uint32 |
Description | string | The IPv4 destination address in numeric form. This address MUST be identical to the DestAddress property if both property values are not NULL and the IPVersionSupport property is "IPv4".
ModelCorrespondence | string | CIM_IPNetworkSecurityIndication.DestAddress, CIM_IPNetworkSecurityIndication.IPVersionSupport
IPv4NumericSourceAddress | uint32 |
Description | string | The IPv4 source address in numeric form. This address MUST be identical to the SourceAddress property if both property values are not NULL and the IPVersionSupport property is "IPv4".
ModelCorrespondence | string | CIM_IPNetworkSecurityIndication.SourceAddress, CIM_IPNetworkSecurityIndication.IPVersionSupport
IPVersionSupport | uint16 |
Description | string | This property explicitly defines support for different versions of the IP protocol for the traffic associated with this Indication.
Required | boolean | true
ValueMap | string | 0, 2, 3
Values | string | Unknown, IPv4, IPv6
MessageType | uint16 |
Description | string | An integer indicating the type of message to which the Indication applies. Generic indications of this class SHOULD set the value to Unknown. DMTF subclasses will define specific values from the DMTF Class Reserved range.
Override | string | MessageType
Required | boolean | true
ValueMap | string | 0, .., 2, 3..500, 16000..
Values | string | Unknown, DMTF Reserved, Not Applicable, DMTF Class Reserved, Vendor Reserved
Protocol | uint16 |
Description | string | An integer indicating the type of network protocol for the traffic associated with this Indication.
Required | boolean | true
ValueMap | string | 0, 2, 3, 4, 5, 6
Values | string | Unknown, ARP, TCP, UDP, ICMP, IGMP
SourceAddress | string |
Description | string | The address for the originator of the network traffic associated with this Indication from the Detector's point of view. This address MUST be identical to the IPv4NumericSourceAddress if both property values are not NULL and the IPVersionSupport property is "IPv4" .
ModelCorrespondence | string | CIM_IPNetworkSecurityIndication.IPv4NumericSourceAddress, CIM_IPNetworkSecurityIndication.IPVersionSupport
SourceMACAddress | string |
Description | string | The MAC address for the source address for this message from the Detector's point of view.
ModelCorrespondence | string | CIM_IPNetworkSecurityIndication.SourceAddress, CIM_IPNetworkSecurityIndication.IPv4NumericSourceAddress
SourcePort | uint32 |
Description | string | The port for the source address for this message from the Detector's point of view.
ModelCorrespondence | string | CIM_IPNetworkSecurityIndication.SourceAddress, CIM_IPNetworkSecurityIndication.IPv4NumericSourceAddress
SourcePrefixLength | uint8 |
Description | string | The prefix length for the IPv6 address for the originator of the network traffic associated with this Indication from the Detector's point of view.
ModelCorrespondence | string | CIM_IPNetworkSecurityIndication.SourceAddress, CIM_IPNetworkSecurityIndication.IPVersionSupport

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
AlertingElementFormat | uint16 | CIM_AlertIndication
AlertingManagedElement | string | CIM_AlertIndication
AlertType | uint16 | CIM_SecurityIndication
Description | string | CIM_AlertIndication
EventCount | uint16 | CIM_SecurityIndication
EventID | string | CIM_AlertIndication
EventTime | datetime | CIM_AlertIndication
IndicationFilterName | string | CIM_Indication
IndicationIdentifier | string | CIM_SecurityIndication
IndicationStartCountTime | datetime | CIM_SecurityIndication
IndicationTime | datetime | CIM_SecurityIndication
Message | string | CIM_AlertIndication
MessageID | string | CIM_AlertIndication
OtherAlertingElementFormat | string | CIM_AlertIndication
OtherAlertType | string | CIM_AlertIndication
OtherSeverity | string | CIM_Indication
OwningEntity | string | CIM_AlertIndication
PerceivedSeverity | uint16 | CIM_AlertIndication
ProbableCause | uint16 | CIM_AlertIndication
ProbableCauseDescription | string | CIM_AlertIndication
ProviderName | string | CIM_AlertIndication
SequenceContext | string | CIM_Indication
SequenceNumber | sint64 | CIM_Indication
SystemCreationClassName | string | CIM_AlertIndication
SystemName | string | CIM_AlertIndication
Trending | uint16 | CIM_AlertIndication
CorrelatedIndications | string[] | CIM_Indication
Effects | uint16[] | CIM_SecurityIndication
Mechanisms | uint16[] | CIM_SecurityIndication
MessageArguments | string[] | CIM_AlertIndication
MoreSpecificEffects | string[] | CIM_SecurityIndication
MoreSpecificMechanisms | string[] | CIM_SecurityIndication
MoreSpecificResources | string[] | CIM_SecurityIndication
RecommendedActions | string[] | CIM_AlertIndication
Resources | uint16[] | CIM_SecurityIndication

## Class Methods