# Class CIM_GARPMembershipSettingData
extends CIM_ConnectivityMembershipSettingData

Configuration for the Generic Attribute Registration Protocol (GARP). GARP is a protocol used by switches and end stations to register and de-register attribute values, such as VLAN Ids. The GVRP is an application of GARP for VLAN registration. The properties (timers) in this class are GARP control information about every ProtocolEndpoint supporting GARP & GVRP.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_SettingData
|
+--CIM_ConnectivityMembershipSettingData
|
+--CIM_GARPMembershipSettingData

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | Configuration for the Generic Attribute Registration Protocol (GARP). GARP is a protocol used by switches and end stations to register and de-register attribute values, such as VLAN Ids. The GVRP is an application of GARP for VLAN registration. The properties (timers) in this class are GARP control information about every ProtocolEndpoint supporting GARP & GVRP.
Experimental | boolean | true
UMLPackagePath | string | CIM::Network::VLAN
Version | string | 2.8.1000

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
Dot1dPortGarpJoinTime | uint32 |
Description | string | The GARP join time.
MappingStrings | string | MIB.IETF|Q-BRIDGE-MIB.dot1dPortGarpJoinTime
PUnit | string | second * 10^-3
Units | string | MilliSeconds
Dot1dPortGarpLeaveAllTime | uint32 |
Description | string | The GARP leave all time.
MappingStrings | string | MIB.IETF|Q-BRIDGE-MIB.dot1dPortGarpLeaveAllTime
PUnit | string | second * 10^-3
Units | string | MilliSeconds
Dot1dPortGarpLeaveTime | uint32 |
Description | string | The GARP leave time.
MappingStrings | string | MIB.IETF|Q-BRIDGE-MIB.dot1dPortGarpLeaveTime
PUnit | string | second * 10^-3
Units | string | MilliSeconds

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
ChangeableType | uint16 | CIM_SettingData
ConfigurationName | string | CIM_SettingData
ConnectivityMemberID | string | CIM_ConnectivityMembershipSettingData
ConnectivityMemberType | uint16 | CIM_ConnectivityMembershipSettingData
Description | string | CIM_ManagedElement
ElementName | string | CIM_SettingData
Generation | uint64 | CIM_ManagedElement
InstanceID | string | CIM_SettingData
OtherConnectivityMemberType | string | CIM_ConnectivityMembershipSettingData
SoID | string | CIM_SettingData
SoOrgID | string | CIM_SettingData
ComponentSetting | string[] | CIM_SettingData

## Class Methods