# Class CIM_FibrePortActiveLogin

Note: The use of FibrePortActiveLogin is deprecated because FibrePort is deprecated. Deprecated description: Information for FibrePortActiveLogin is found by examining the individual FCPorts, and an ActiveConnection between the FCProtocolEndpoints that are associated with the ports. FibrePortActiveLogin indicates that two FibrePorts are connected through a login and have negotiated their Class Of Service, frame size, and other link characteristics, as specified by an instance of this class.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_FibrePortActiveLogin

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Association | boolean | true
Deprecated | string | CIM_ActiveConnection, CIM_FCPort
Description | string | Note: The use of FibrePortActiveLogin is deprecated because FibrePort is deprecated. Deprecated description: Information for FibrePortActiveLogin is found by examining the individual FCPorts, and an ActiveConnection between the FCProtocolEndpoints that are associated with the ports. FibrePortActiveLogin indicates that two FibrePorts are connected through a login and have negotiated their Class Of Service, frame size, and other link characteristics, as specified by an instance of this class.
UMLPackagePath | string | CIM::Device::NetworkAdapter
Version | string | 2.10.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
ACKModel | uint16 |
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: Acknowledgement model that is negotiated during Port login. For example, ACK-1 indicates that each frame should be acknowledged.
MappingStrings | string | MIF.DMTF|Fibre Channel Bus PortExtensions|001.6
ValueMap | string | 0, 1, 2, 3
Values | string | Unknown, ACK-0, ACK-1, ACK-N
BufferToBufferModel | uint16 |
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: The buffer-to-buffer model that was negotiated during Port login. Either the model defined by the FC-PH standard is used (value=1, "Regular") or an "Alternate" model is negotiated.
ValueMap | string | 0, 1, 2
Values | string | Unknown, Regular, Alternate
NegotiatedCOS | uint16 |
Deprecated | string | CIM_FCPort.ActiveCOS
Description | string | Note: The use of this method has been deprecated. Deprecated description: The Fibre Channel Class of Service that is currently running between the Ports. Because two Ports can be simultaneously connected at different Classes of Service, this property had to be part of the key of the object and therefore, the identity of the instance.
Key | boolean | true
MappingStrings | string | MIF.DMTF|Fibre Channel Bus PortExtensions|001.5
ModelCorrespondence | string | CIM_FibreChannelAdapter.SupportedCOS
ValueMap | string | 0, 1, 2, 3, 4, 5, 6
Values | string | Unknown, 1, 2, 3, 4, 6, F
NegotiatedFrameSize | uint64 |
Deprecated | string | CIM_FCPort.ActiveMaximumTransmissionUnit
Description | string | Note: The use of this method has been deprecated. Deprecated description: The Fibre Channel frame size, in bytes, that is currently negotiated between the two Ports.
PUnit | string | byte
Units | string | Bytes
NegotiatedSpeed | uint64 |
Deprecated | string | CIM_FCPort.Speed
Description | string | Note: The use of this method has been deprecated. Deprecated description: The speed for communications that is currently negotiated between the two Ports. Speed is specified in Bits per Second. If this information is not available, the property should be set to 0.
PUnit | string | bit / second
Units | string | Bits per Second
OriginatorBufferCredit | uint64 |
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: OriginatorBufferCredit reflects the buffer credit of the Port that is defined as the LoginOriginator. This method is the number of frame buffers that were made available by the originating Port to the responder Port. Buffer credits are used in point-to- point connections, when an NL-Local Port is logged into another NL-Local Port, and when Nx Ports are logged into Fx Ports. In other scenarios, this value is undefined.
MappingStrings | string | MIF.DMTF|Fibre Channel Bus PortExtensions|001.3
OriginatorEndCredit | uint64 |
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: OriginatorEndCredit reflects the end credit of the Port that is defined as the LoginOriginator. This method is the number of frame buffers that were made available by the originating Port to the responder Port. End credits are used in point-to-point connections, when an NL-Local Port is logged into another NL-Local Port, and when Nx Ports are logged into remote Nx Ports. In other scenarios, this value is undefined.
MappingStrings | string | MIF.DMTF|Fibre Channel Bus PortExtensions|001.2
ResponderBufferCredit | uint64 |
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: ResponderBufferCredit reflects the buffer credit of the Port that is defined as the LoginResponder. This method is the number of frame buffers that were made available by the responder Port to the originating Port. Buffer credits are used in point-to-point connections, when an NL-Local Port is logged into another NL-Local Port, and when Nx Ports are logged into Fx Ports. In other scenarios, this value is undefined.
MappingStrings | string | MIF.DMTF|Fibre Channel Bus PortExtensions|001.3
ResponderEndCredit | uint64 |
Deprecated | string | No value
Description | string | Note: The use of this method has been deprecated. Deprecated description: ResponderEndCredit reflects the end credit of the Port that is defined as the LoginResponder. This method is the number of frame buffers that were made available by the responder Port to the originating Port. End credits are used in point-to-point connections, when an NL-Local Port is logged into another NL-Local Port, and when Nx Ports are logged into remote Nx Ports. In other scenarios, this value is undefined.
MappingStrings | string | MIF.DMTF|Fibre Channel Bus PortExtensions|001.2

### Association References

Name | Class Origin | Reference Class
--- | --- | ---
LoginOriginator | CIM_FibrePortActiveLogin | CIM_FibrePort
LoginResponder | CIM_FibrePortActiveLogin | CIM_FibrePort

## Class Methods