# Class CIM_LLDPEthernetPort
extends CIM_EthernetPort

This class describes the current LLDP configuration of an LLDP capable ethernet port.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_LogicalPort
|
+--CIM_NetworkPort
|
+--CIM_EthernetPort
|
+--CIM_LLDPEthernetPort

## Direct Known Subclasses

CIM_DataCenterEthernetPort

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | This class describes the current LLDP configuration of an LLDP capable ethernet port.
UMLPackagePath | string | CIM::Device::Ports
Version | string | 2.34.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
ConfigManVidTxEnable | boolean |
Description | string | This flag determines determines whether the IEEE 802.1 organizationally defined Management VID TLV transmission is allowed on this port.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2Xdot1ConfigManVidTxEnable
ConfigPortVlanTxEnable | boolean |
Description | string | This flag determines whether the IEEE 802.1 organizationally defined port VLAN TLV transmission is allowed on this port.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2Xdot1ConfigPortVlanTxEnable
LocChassisId | string |
Description | string | The string value used to identify the chassis component associated with the local system.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2LocChassisId
ModelCorrespondence | string | CIM_LLDPEthernetPort.LocChassisIdSubtype
LocChassisIdSubtype | uint8 |
Description | string | The type of encoding used to identify the chassis associated with the local system.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2LocChassisIdSubtype
ValueMap | string | 1, 2, 3, 4, 5, 6, 7, ..
Values | string | Chassis component, Interface alias, Port component, MAC address, Network address, Interface name, Locally assigned, DMTF Reserved
LocFbSystemValue | uint16 |
Description | string | Integer that indicates the value of fallback Tw_sys_tx that the local system requests from the remote system. This value is updated by the local system software.
LocPortDesc | string |
Description | string | The string value used to identify this port's description associated with the local system.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2LocPortDesc
ModelCorrespondence | string | CIM_LLDPEthernetPort.LocPortIdSubtype, CIM_LLDPEthernetPort.LocPortId
LocPortID | string |
Description | string | The string value used to identify the port component associated with a given port in the local system.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2LocPortId
ModelCorrespondence | string | CIM_LLDPEthernetPort.LocPortIdSubtype
LocPortIdSubtype | uint8 |
Description | string | The type of port identifier encoding used in identifying the port component associated with the local system.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2LocPortIdSubtype
ValueMap | string | 1, 2, 3, 4, 5, 6, 7, ..
Values | string | Interface alias, Port component, MAC address, Network address, Interface name, Agent circuit ID, Locally assigned, DMTF Reserved
LocResolvedRxSystemValue | uint16 |
Description | string | Integer that indicates the current Tw_sys_tx supported by the remote system.
LocResolvedTxSystemValue | uint16 |
Description | string | Integer that indicates the current Tw_sys_tx supported by the local system.
LocRxSystemValue | uint16 |
Description | string | Integer that indicates the value of Tw_sys_tx that the local system requests from the remote system. This value is updated by the EEE Receiver L2 state diagram.
LocRxSystemValueEcho | uint16 |
Description | string | Integer that indicates the remote systems Receive Tw_sys_tx that was used by the local system to compute the Tw_sys_tx that it can support.
LocSysDesc | string |
Description | string | The string value used to identify the system description of the local system.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2LocSysDesc
LocSysName | string |
Description | string | The string value used to identify the system name of the local system.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2LocSysName
LocTxSystemValue | uint16 |
Description | string | Integer that indicates the value of Tw_sys_tx that the local system can support on this port. This value is updated by the EEE DLL Transmitter state diagram. Tw_Sys_tx value is used in a timer that counts the time since the de-assertion of Low Poer Idle (LPI).
LocTxSystemValueEcho | uint16 |
Description | string | Integer that indicates the remote system's Transmit Tw_sys_tx that was used by the local system to compute the Tw_sys_tx that it wants to request from the remote system.
MaximumFrameSizeTLVEnabled | boolean |
Description | string | This flag indicates whether or not the transmission of Maximum frame size TLV is enabled on this port.
MessageFastTx | uint16 | 1
Description | string | The interval at which LLDP frames are transmitted on behalf of this LLDP agent during fast transmission period (e.g. when a new neighbor is detected) on this port.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2MessageFastTx
MaxValue | sint64 | 3600
MinValue | sint64 | 1
PUnit | string | second
MessageTxHoldMultiplier | uint8 | 4
Description | string | The value of this property is used, as a multiplier of MessageTxInterval, to determine the value of txTTL that is carried in LLDP frames transmitted by the LLDP agent on this port.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2MessageTxHoldMultiplier
MaxValue | sint64 | 100
MinValue | sint64 | 2
PUnit | string | second
MessageTxInterval | uint16 | 30
Description | string | The interval at which LLDP frames are transmitted on behalf of this LLDP agent on this port.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2MessageTxInterval
MaxValue | sint64 | 3600
MinValue | sint64 | 1
PUnit | string | second
NotificationInterval | uint16 | 30
Description | string | The value of this property indicates the interval between transmission of LLDP notifications during normal transmission periods on this port.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2NotificationInterval
MaxValue | sint64 | 3600
MinValue | sint64 | 5
PUnit | string | second
ReinitDelay | uint8 | 2
Description | string | The value of this property indicates the amount of delay from when adminStatus becomes disabled until reinitialization is attempted on this port.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2ReinitDelay
MaxValue | sint64 | 10
MinValue | sint64 | 1
PUnit | string | second
RemRxSystemValue | uint16 |
Description | string | Integer that indicates the value of Tw_sys_tx that the remote system requests from the local system.
RemRxSystemValueEcho | uint16 |
Description | string | Integer that indicates the value of Receive Tw_sys_tx echoed back by the remote system.
RemTxSystemValue | uint16 |
Description | string | Integer that indicates the value of Tw_sys_tx that the remote system can support.
RemTxSystemValueEcho | uint16 |
Description | string | Integer that indicates the value Transmit Tw_sys_tx echoed back by the remote system.
TxCreditMax | uint8 | 5
Description | string | The maximum number of consecutive LLDPDUs that can be transmitted at any time on this port.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2TxCreditMax
MaxValue | sint64 | 100
MinValue | sint64 | 1
TxFastInit | uint8 | 4
Description | string | The initial value used to initialize the variable which determines the number of transmissions that are made in fast transmission mode on this port.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2TxFastInit
MaxValue | sint64 | 8
MinValue | sint64 | 1
DestMacAddress | string[] |
ArrayType | string | Indexed
Description | string | This array identifies individual or group MAC addresses that are in use by LLDP as destination MAC addresses on this port. Each MAC address is formatted as twelve hexadecimal digits (for example, "010203040506"), with each pair representing one of the six octets of the MAC address in "canonical" bit order. (Therefore, the Group address bit is found in the low order bit of the first character of the string.)
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2DestMacAddress
LocManAddr | string[] |
ArrayType | string | Indexed
Description | string | The string values are used to identify the management addresses on the local system.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2LocManAddr
ModelCorrespondence | string | CIM_LLDPEthernetPort.LocManAddrSubtype
LocManAddrIfId | uint32[] |
ArrayType | string | Indexed
Description | string | The integer value used to identify the interface number regarding the management address on the local system.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2LocManAddrIfId
ModelCorrespondence | string | CIM_LLDPEthernetPort.LocManAddrSubtype, CIM_LLDPEthernetPort.LocManAddr, CIM_LLDPEthernetPort.LocManAddrIfSubtype
LocManAddrIfSubtype | uint16[] |
ArrayType | string | Indexed
Description | string | The enumeration value that identifies the interface numbering method used for defining the interface number (lldpV2LocManAddrIfId), associated with the local system.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2LocManAddrIfSubtype
ModelCorrespondence | string | CIM_LLDPEthernetPort.LocManAddrSubtype, CIM_LLDPEthernetPort.LocManAddr
ValueMap | string | 2, 3, ..
Values | string | ifIndex, systemPortNumber, DMTF Reserved
LocManAddrSubType | uint16[] |
ArrayType | string | Indexed
Description | string | The type of management address identifier encodings used for the management addresses represented by LocManAddr.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2LocManAddrSubtype
ValueMap | string | 3, 4, ..
Values | string | MAC address, Network address, DMTF Reserved
LocSysCapEnabled | boolean[] |
Description | string | These flags are used to identify which system capabilities are enabled on the local system.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2LocSysCapEnabled
ModelCorrespondence | string | CIM_LLDPEthernetPort.LocSysCapSupported
LocSysCapSupported | uint8[] |
Description | string | This property identifies which system capabilities are supported on the local system.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2LocSysCapSupported
ModelCorrespondence | string | CIM_LLDPEthernetPort.LocSysCapEnabled
ValueMap | string | 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, ..
Values | string | Repeater, MAC Bridge, WLAN Access Point, Router, Telephone, DOCSIS cable device, Station Only, C-VLAN Component of a VLAN Bridge, S-VLAN Component of a VLAN Bridge, Two-port MAC Relay (TPMR), DMTF Reserved
ManAddrConfigDestAddress | string[] |
ArrayType | string | Indexed
Description | string | The destination MAC address associated with ManAddrConfigTxEnable.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2ManAddrConfigDestAddressIndex
ManAddrConfigLocManAddr | string[] |
ArrayType | string | Indexed
Description | string | The string values used to identify the management addresses for which notifications from the agent are enabled on this port.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2ManAddrConfigLocManAddr
ModelCorrespondence | string | CIM_LLDPEthernetPort.ManAddrConfigDestAddress, CIM_LLDPEthernetPort.ManAddrConfigLocManAddrSubtype
ManAddrConfigLocManAddrSubtype | uint16[] |
ArrayType | string | Indexed
Description | string | This property represents the type of managment address identifiers encoding used to represent management addresses. "3 (MAC address)" value indicates that this string identifies a particular unicast MAC address (encoded in network byte order and IEEE 802.3 canonical bit order). "4 (Network address)" value identifies a network address. The first octet contains the IANA AddressFamilyNumbers enumeration value for the specific address type, and octets 2 through N contain the networkAddress address value in network byte order.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2ManAddrConfigLocManAddrSubtype
ModelCorrespondence | string | CIM_LLDPEthernetPort.ManAddrConfigDestAddress
ValueMap | string | 3, 4, ..
Values | string | MAC address, Network address, DMTF Reserved
ManAddrConfigTxEnable | boolean[] |
ArrayType | string | Indexed
Description | string | Flags for controlling the transmission of system management address instances for this port, destination, subtype and management address. If set to false, no transmission occurs. If set to true, the appropriate information is transmitted on this port.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2ManAddrConfigTxEnable
ModelCorrespondence | string | CIM_LLDPEthernetPort.ManAddrConfigDestAddress, CIM_LLDPEthernetPort.ManAddrConfigLocManAddrSubtype, CIM_LLDPEthernetPort.ManAddrConfigLocManAddr
PortConfigAdminStatus | uint8[] |
ArrayType | string | Indexed
Description | string | The administratively desired status of the local LLDP agent on this port. "txOnly" indicates that the LLDP agent transmits LLDPframes on this port and it does not store any information about the remote systems connected. "rxOnly" indicates that the LLDP agent receives, but it does not transmit LLDP frames on this port. "txAndRx" indicates the LLDP agent transmits and receives LLDP frames on this port. "disabled" indciates the LLDP agent does not transmit or receive LLDP frames on this port. If there is remote systems information which is received on this port and stored in other tables, before the port's PortConfigAdminStatus becomes disabled, then that information is deleted.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2PortConfigAdminStatus
ModelCorrespondence | string | CIM_LLDPEthernetPort.DestMacAddress
ValueMap | string | 1, 2, 3, 4, ..
Values | string | txOnly, rxOnly, txAndRx, disabled, DMTF Reserved
PortConfigNotificationEnable | boolean[] |
ArrayType | string | Indexed
Description | string | These flags control, on a per agent basis, whether or not notifications from the agent are enabled on this port.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2PortConfigNotificationEnable
ModelCorrespondence | string | CIM_LLDPEthernetPort.DestMacAddress, CIM_LLDPEthernetPort.PortConfigAdminStatus
PortConfigPortDescriptionTLVTxEnable | boolean[] |
ArrayType | string | Indexed
Description | string | These flags indicate that LLDP agents should transmit "Port Description TLV" on this port.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2PortConfigTLVsTxEnable
ModelCorrespondence | string | CIM_LLDPEthernetPort.DestMacAddress, CIM_LLDPEthernetPort.PortConfigAdminStatus, CIM_LLDPEthernetPort.PortConfigNotificationEnable
PortConfigSystemCapabilitiesTLVTxEnable | boolean[] |
ArrayType | string | Indexed
Description | string | These flags indicate that LLDP agents should transmit "System Capabilities TLV" on this port.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2PortConfigTLVsTxEnable
ModelCorrespondence | string | CIM_LLDPEthernetPort.DestMacAddress, CIM_LLDPEthernetPort.PortConfigAdminStatus, CIM_LLDPEthernetPort.PortConfigNotificationEnable, CIM_LLDPEthernetPort.PortConfigPortDescriptionTLVTxEnable, CIM_LLDPEthernetPort.PortConfigSystemNameTLVTxEnable, CIM_LLDPEthernetPort.PortConfigSystemDescriptionTLVTxEnable
PortConfigSystemDescriptionTLVTxEnable | boolean[] |
ArrayType | string | Indexed
Description | string | These flags indicate that LLDP agents should transmit "System Description TLV" on this port.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2PortConfigTLVsTxEnable
ModelCorrespondence | string | CIM_LLDPEthernetPort.DestMacAddress, CIM_LLDPEthernetPort.PortConfigAdminStatus, CIM_LLDPEthernetPort.PortConfigNotificationEnable, CIM_LLDPEthernetPort.PortConfigPortDescriptionTLVTxEnable, CIM_LLDPEthernetPort.PortConfigSystemNameTLVTxEnable
PortConfigSystemNameTLVTxEnable | boolean[] |
ArrayType | string | Indexed
Description | string | These flags indicate that LLDP agents should transmit "System Name TLV" on this port.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2PortConfigTLVsTxEnable
ModelCorrespondence | string | CIM_LLDPEthernetPort.DestMacAddress, CIM_LLDPEthernetPort.PortConfigAdminStatus, CIM_LLDPEthernetPort.PortConfigNotificationEnable, CIM_LLDPEthernetPort.PortConfigPortDescriptionTLVTxEnable
RemChassisId | string[] |
ArrayType | string | Indexed
Description | string | The string value used to identify the chassis component associated with the remote system.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2RemChassisId
ModelCorrespondence | string | CIM_LLDPEthernetPort.RemLocalDestMacAddress, CIM_LLDPEthernetPort.LocChassisIdSubtype
RemChassisIdSubtype | uint8[] |
ArrayType | string | Indexed
Description | string | The type of encoding used to identify the chassis associated with the remote system.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2RemChassisIdSubtype
ModelCorrespondence | string | CIM_LLDPEthernetPort.RemLocalDestMacAddress
ValueMap | string | 1, 2, 3, 4, 5, 6, 7, ..
Values | string | Chassis component, Interface alias, Port component, MAC address, Network address, Interface name, Locally assigned, DMTF Reserved
RemLocalDestMacAddress | string[] |
ArrayType | string | Indexed
Description | string | The destination MAC addresses used on the remote system.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2Xdot1RemLocalDestMacAddress
RemManAddr | string[] |
ArrayType | string | Indexed
Description | string | The string values are used to identify the management addresses on the remote system.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2RemManAddr
ModelCorrespondence | string | CIM_LLDPEthernetPort.RemLocalDestMacAddress, CIM_LLDPEthernetPort.RemManAddrSubtype
RemManAddrIfId | uint32[] |
ArrayType | string | Indexed
Description | string | The integer value used to identify the interface number regarding the management address on the remote system.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2RemManAddrIfId
ModelCorrespondence | string | CIM_LLDPEthernetPort.RemLocalDestMacAddress, CIM_LLDPEthernetPort.RemManAddrSubtype, CIM_LLDPEthernetPort.RemManAddr, CIM_LLDPEthernetPort.RemManAddrIfSubtype
RemManAddrIfSubtype | uint16[] |
ArrayType | string | Indexed
Description | string | The enumeration value that identifies the interface numbering method used for defining the interface number (lldpV2LocManAddrIfId), associated with the remote system.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2RemManAddrIfSubtype
ModelCorrespondence | string | CIM_LLDPEthernetPort.RemLocalDestMacAddress, CIM_LLDPEthernetPort.RemManAddrSubtype, CIM_LLDPEthernetPort.RemManAddr
ValueMap | string | 2, 3, ..
Values | string | ifIndex, systemPortNumber, DMTF Reserved
RemManAddrSubType | uint16[] |
ArrayType | string | Indexed
Description | string | The type of management address identifier encodings used for the management addresses represented by RemManAddr.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2RemManAddrSubtype
ModelCorrespondence | string | CIM_LLDPEthernetPort.RemLocalDestMacAddress
ValueMap | string | 3, 4, ..
Values | string | MAC address, Network address, DMTF Reserved
RemPortDesc | string[] |
ArrayType | string | Indexed
Description | string | The string value used to identify this port's description associated with the remote system.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2RemPortDesc
ModelCorrespondence | string | CIM_LLDPEthernetPort.RemLocalDestMacAddress, CIM_LLDPEthernetPort.RemPortIdSubtype, CIM_LLDPEthernetPort.RemPortId
RemPortID | string[] |
ArrayType | string | Indexed
Description | string | The string value used to identify the port component associated with a given port in the remote system.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2RemPortId
ModelCorrespondence | string | CIM_LLDPEthernetPort.RemLocalDestMacAddress, CIM_LLDPEthernetPort.RemPortIdSubtype
RemPortIdSubtype | uint8[] |
ArrayType | string | Indexed
Description | string | The type of port identifier encoding used in identifying the port component associated with the remote system.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2RemPortIdSubtype
ModelCorrespondence | string | CIM_LLDPEthernetPort.RemLocalDestMacAddress
ValueMap | string | 1, 2, 3, 4, 5, 6, 7, ..
Values | string | Interface alias, Port component, MAC address, Network address, Interface name, Agent circuit ID, Locally assigned, DMTF Reserved
RemSysCapEnabled | boolean[] |
ArrayType | string | Indexed
Description | string | These flags are used to identify which system capabilities are enabled on the remote system.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2RemSysCapEnabled
ModelCorrespondence | string | CIM_LLDPEthernetPort.RemLocalDestMacAddress, CIM_LLDPEthernetPort.RemSysCapSupported
RemSysCapSupported | uint8[] |
ArrayType | string | Indexed
Description | string | This property identifies which system capabilities are supported on the remote system.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2RemSysCapSupported
ModelCorrespondence | string | CIM_LLDPEthernetPort.RemLocalDestMacAddress, CIM_LLDPEthernetPort.RemSysCapEnabled
ValueMap | string | 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, ..
Values | string | Repeater, MAC Bridge, WLAN Access Point, Router, Telephone, DOCSIS cable device, Station Only, C-VLAN Component of a VLAN Bridge, S-VLAN Component of a VLAN Bridge, Two-port MAC Relay (TPMR), DMTF Reserved
RemSysDesc | string[] |
ArrayType | string | Indexed
Description | string | The string value used to identify the system description of the remote system.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2RemSysDesc
ModelCorrespondence | string | CIM_LLDPEthernetPort.RemLocalDestMacAddress
RemSysName | string[] |
ArrayType | string | Indexed
Description | string | The string value used to identify the system name of the remote system.
MappingStrings | string | MIB.IEEE|LLDP-EXT-DOT1-V2-MIB.lldpV2RemSysName
ModelCorrespondence | string | CIM_LLDPEthernetPort.RemLocalDestMacAddress

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
ActiveMaximumTransmissionUnit | uint64 | CIM_NetworkPort
AllocationState | string | CIM_LogicalDevice
AutoSense | boolean | CIM_NetworkPort
Availability | uint16 | CIM_LogicalDevice
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_LogicalDevice
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
DeviceID | string | CIM_LogicalDevice
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
ErrorCleared | boolean | CIM_LogicalDevice
ErrorDescription | string | CIM_LogicalDevice
FullDuplex | boolean | CIM_NetworkPort
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
LastErrorCode | uint32 | CIM_LogicalDevice
LinkTechnology | uint16 | CIM_NetworkPort
LocationIndicator | uint16 | CIM_LogicalDevice
MaxDataSize | uint32 | CIM_EthernetPort
MaxQuiesceTime | uint64 | CIM_LogicalDevice
MaxSpeed | uint64 | CIM_LogicalPort
Name | string | CIM_ManagedSystemElement
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
OtherLinkTechnology | string | CIM_NetworkPort
OtherNetworkPortType | string | CIM_NetworkPort
OtherPortType | string | CIM_LogicalPort
PermanentAddress | string | CIM_NetworkPort
PoEPowerEntityType | uint16 | CIM_EthernetPort
PortNumber | uint16 | CIM_NetworkPort
PortType | uint16 | CIM_EthernetPort
PowerManagementSupported | boolean | CIM_LogicalDevice
PowerOnHours | uint64 | CIM_LogicalDevice
PrimaryStatus | uint16 | CIM_ManagedSystemElement
PVID | uint16 | CIM_EthernetPort
RequestedSpeed | uint64 | CIM_LogicalPort
RequestedState | uint16 | CIM_EnabledLogicalElement
Speed | uint64 | CIM_NetworkPort
Status | string | CIM_ManagedSystemElement
StatusInfo | uint16 | CIM_LogicalDevice
SupportedMaximumTransmissionUnit | uint64 | CIM_NetworkPort
SystemCreationClassName | string | CIM_LogicalDevice
SystemName | string | CIM_LogicalDevice
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TotalPowerOnHours | uint64 | CIM_LogicalDevice
TransitioningToState | uint16 | CIM_EnabledLogicalElement
UsageRestriction | uint16 | CIM_LogicalPort
AdditionalAvailability | uint16[] | CIM_LogicalDevice
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
Capabilities | uint16[] | CIM_EthernetPort
CapabilityDescriptions | string[] | CIM_EthernetPort
EnabledCapabilities | uint16[] | CIM_EthernetPort
IdentifyingDescriptions | string[] | CIM_LogicalDevice
NetworkAddresses | string[] | CIM_EthernetPort
OperationalStatus | uint16[] | CIM_ManagedSystemElement
OtherEnabledCapabilities | string[] | CIM_EthernetPort
OtherIdentifyingInfo | string[] | CIM_LogicalDevice
PortDiscriminator | string[] | CIM_EthernetPort
PowerManagementCapabilities | uint16[] | CIM_LogicalDevice
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
EnableDevice | uint32 | CIM_LogicalDevice
OnlineDevice | uint32 | CIM_LogicalDevice
QuiesceDevice | uint32 | CIM_LogicalDevice
RequestStateChange | uint32 | CIM_EnabledLogicalElement
Reset | uint32 | CIM_LogicalDevice
RestoreProperties | uint32 | CIM_LogicalDevice
SaveProperties | uint32 | CIM_LogicalDevice
SetPowerState | uint32 | CIM_LogicalDevice