# Class CIM_OSPFAreaConfiguration
extends CIM_LogicalElement

Each OSPF router has an association to one or more OSPF areas. Into these areas, a router advertises summaries filtered by specific address ranges. This would natively be modeled as a ternary association (router/OSPFService to OSPFArea to RangeOfIPAddresses), which is problematic in some implementations. To get around this issue, the OSPFAreaConfiguration class is defined to act as a focal point to bring together the router (indicated as a ComputerSystem with an instance of OSPFService, associated to the AreaConfiguration using OSPFServiceConfiguration), the area (indicated as an OSPFArea, associated to the AreaConfiguration using AreaOfConfiguration) and the address ranges for advertising (indicated as instances of RangeOfIPAddresses, associated to the AreaConfiguration using RangesOfConfiguration). There would be an instance of OSPFAreaConfiguration for each connected area of a router/OSPFService. When network administrators want to control the advertisements of OSPF routers by filters, they first define the relevant ranges. In order for a router to handle a range, an instance of RangeOfIPAddresses MUST be associated to the relevant OSPFAreaConfiguration (using the relationship, RangesOf Configuration). The association between the range and area configuration contains a property defining the handling (EnableAdvertise) to allow or disallow advertisements in the range. Notes: - Because RangeOfIPAddresses is scoped by a System (via the HostedCollection association), an instance of RangeOfIPAddresses would be associated to an OSPFArea, satisfying this semantic. - This class is inherited from LogicalElement, because a suitable subclass 'lower' in the inheritance hiearchy does not exist.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_OSPFAreaConfiguration

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | Each OSPF router has an association to one or more OSPF areas. Into these areas, a router advertises summaries filtered by specific address ranges. This would natively be modeled as a ternary association (router/OSPFService to OSPFArea to RangeOfIPAddresses), which is problematic in some implementations. To get around this issue, the OSPFAreaConfiguration class is defined to act as a focal point to bring together the router (indicated as a ComputerSystem with an instance of OSPFService, associated to the AreaConfiguration using OSPFServiceConfiguration), the area (indicated as an OSPFArea, associated to the AreaConfiguration using AreaOfConfiguration) and the address ranges for advertising (indicated as instances of RangeOfIPAddresses, associated to the AreaConfiguration using RangesOfConfiguration). There would be an instance of OSPFAreaConfiguration for each connected area of a router/OSPFService. When network administrators want to control the advertisements of OSPF routers by filters, they first define the relevant ranges. In order for a router to handle a range, an instance of RangeOfIPAddresses MUST be associated to the relevant OSPFAreaConfiguration (using the relationship, RangesOf Configuration). The association between the range and area configuration contains a property defining the handling (EnableAdvertise) to allow or disallow advertisements in the range. Notes: - Because RangeOfIPAddresses is scoped by a System (via the HostedCollection association), an instance of RangeOfIPAddresses would be associated to an OSPFArea, satisfying this semantic. - This class is inherited from LogicalElement, because a suitable subclass 'lower' in the inheritance hiearchy does not exist.
UMLPackagePath | string | CIM::Network::OSPF
Version | string | 2.19.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
InstanceID | string |
Description | string | Within the scope of the instantiating Namespace, InstanceID opaquely and uniquely identifies an instance of this class. In order to ensure uniqueness within the NameSpace, the value of InstanceID SHOULD be constructed using the following 'preferred' algorithm: <OrgID>:<OSPFService ID><Area Configuration ID> where: <OrgID> and the remainder of the InstanceID are separated by a colon ':', and where <OrgID> MUST include a copyrighted, trademarked or otherwise unique name that is owned by the business entity creating/defining the InstanceID, or is a registered ID that is assigned to the business entity by a recognized global authority. (This is similar to the <Schema Name>_<Class Name> structure of Schema class names.) In addition, to ensure uniqueness <OrgID> MUST NOT contain a colon (':'). When using this algorithm, the first colon to appear in InstanceID MUST appear between <OrgID> and the <OSPFService ID>. For DMTF defined instances, the 'preferred' algorithm MUST be used, and the <OrgID> set to 'CIM'. <OSPFService ID> and <Area Configuration ID> MUST specify vendor-unique identifiers for the OSPFService and AreaConfiguration.
Key | boolean | true
Override | string | InstanceID
StubDefaultCost | uint32 |
Description | string | This attribute contains the value of the default route that this router advertises into a stub area, see C.2 RFC 2328.
MappingStrings | string | MIB.IETF|OSPF-MIB.ospfStubMetric
StubMetricType | uint16 |
Description | string | This attribute contains the type of metric advertised as a default route into a stub area, see 3. in RFC 1850.
MappingStrings | string | MIB.IETF|OSPF-MIB.ospfStubMetricType
ValueMap | string | 2, 3, 4
Values | string | OSPF Metric, Comparable Cost, NonComparable

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
ElementName | string | CIM_ManagedElement
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
Name | string | CIM_ManagedSystemElement
OperatingStatus | uint16 | CIM_ManagedSystemElement
PrimaryStatus | uint16 | CIM_ManagedSystemElement
Status | string | CIM_ManagedSystemElement
OperationalStatus | uint16[] | CIM_ManagedSystemElement
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods