# Class CIM_DataCenterEthernetPort
extends CIM_LLDPEthernetPort

This class defines the current configuration of a data center ethernet (DCE) port.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_LogicalPort
|
+--CIM_NetworkPort
|
+--CIM_EthernetPort
|
+--CIM_LLDPEthernetPort
|
+--CIM_DataCenterEthernetPort

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | This class defines the current configuration of a data center ethernet (DCE) port.
UMLPackagePath | string | CIM::Device::Ports
Version | string | 2.34.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
AdminETSConCreditBasedShaperSupport | boolean |
Description | string | Indicates support for the credit-based shaper Traffic Selection Algorithm.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxAdminETSConCreditBasedShaperSupport
AdminETSConTrafficClassesSupported | uint8 |
Description | string | Indicates the number of traffic classes supported on this port.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxAdminETSConTrafficClassesSupported
AdminETSConWilling | boolean |
Description | string | Indicates if the local system is willing to accept the ETS configuration recommended by the remote system.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxAdminETSConWilling
Write | boolean | true
AdminPFCCap | uint8 |
Description | string | Indicates the number of traffic classes on the local port that may simultaneously have PFC enabled.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxAdminPFCCap
ModelCorrespondence | string | CIM_DataCenterEthernetPort.AdminPFCWilling, CIM_DataCenterEthernetPort.AdminPFCMBC
AdminPFCMBC | boolean |
Description | string | Indicates if the local system is capable of bypassing MACsec processing when MACsec is disabled.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxAdminPFCMBC
ModelCorrespondence | string | CIM_DataCenterEthernetPort.AdminPFCWilling, CIM_DataCenterEthernetPort.AdminPFCCap
AdminPFCWilling | boolean |
Description | string | Indicates if the local system is willing to accept the PFC configuration of the remote system on this port.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxAdminPFCWilling
ModelCorrespondence | string | CIM_DataCenterEthernetPort.AdminPFCMBC, CIM_DataCenterEthernetPort.AdminPFCCap
Write | boolean | true
ApplicationPriorityTxEnable | boolean |
Description | string | This property determines whether the IEEE 802.1 organizationally defined Application Priority TLV transmission is allowed on a given LLDP transmission capable port.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxConfigApplicationPriorityTxEnable
ETSConfigurationTxEnable | boolean |
Description | string | This property determines whether the IEEE 802.1 organizationally defined ETS Configuration TLV transmission is allowed on a given LLDP transmission capable port.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxConfigETSConfigurationTxEnable
ETSRecommendationTxEnable | boolean |
Description | string | This property determines whether the IEEE 802.1 organizationally defined ETS Recommendation TLV transmission is allowed on a given LLDP transmission capable port.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxConfigETSRecommendationTxEnable
LocETSConCreditBasedShaperSupport | boolean |
Description | string | Indicates if the credit-based shaper Traffic Selection Algorithm is supported on this port.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxLocETSConCreditBasedShaperSupport
LocETSConTrafficClassesSupported | uint8 |
Description | string | Indicates the number of traffic classes supported on this port.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxLocETSConTrafficClassesSupported
LocETSConWilling | boolean |
Description | string | Indicates if the local system is willing to accept the ETS configuration recommended by the remote system.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxLocETSConWilling
LocPFCCap | uint8 |
Description | string | Indicates the number of traffic classes on the local port that may simultaneously have PFC enabled.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxLocPFCCap
ModelCorrespondence | string | CIM_DataCenterEthernetPort.LocPFCWilling, CIM_DataCenterEthernetPort.LocPFCMBC
LocPFCMBC | boolean |
Description | string | Indicates if the local system is capable of bypassing MACsec processing when MACsec is disabled.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxLocPFCMBC
ModelCorrespondence | string | CIM_DataCenterEthernetPort.LocPFCWilling, CIM_DataCenterEthernetPort.LocPFCCap
LocPFCWilling | boolean |
Description | string | Indicates if the local system is willing to accept the PFC configuration of the remote system on this port.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxLocPFCWilling
ModelCorrespondence | string | CIM_DataCenterEthernetPort.LocPFCMBC, CIM_DataCenterEthernetPort.LocPFCCap
PfcLinkDelayAllowance | uint32 |
Description | string | The allowance made for round-trip propagation delay of the link in bits. The value of this object must be retained across reinitializations of the management system.
MappingStrings | string | MIB.IEEE|IEEE8021-PFC-MIB.ieee8021PfcLinkDelayAllowance
PFCTxEnable | boolean |
Description | string | This property determines whether the IEEE 802.1 organizationally defined Priority-based Flow Control TLV transmission is allowed on a given LLDP transmission capable port.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxConfigPFCTxEnable
RemETSConCreditBasedShaperSupport | boolean |
Description | string | Indicates if the credit-based shaper Traffic Selection Algorithm is supported on the remote port.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxRemETSConCreditBasedShaperSupport
Write | boolean | false
RemETSConTrafficClassesSupported | uint8 |
Description | string | Indicates the number of traffic classes supported on the remote port.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxRemETSConTrafficClassesSupported
Write | boolean | false
RemETSConWilling | boolean |
Description | string | Indicates if the remote system is willing to accept the ETS configuration recommended by the local system.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxRemETSConWilling
Write | boolean | false
RemPFCCap | uint8 |
Description | string | Indicates the number of traffic classes on the remote port that may simultaneously have PFC enabled.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxRemPFCCap
ModelCorrespondence | string | CIM_DataCenterEthernetPort.RemPFCWilling, CIM_DataCenterEthernetPort.RemPFCMBC
Write | boolean | false
RemPFCMBC | boolean |
Description | string | Indicates if the remote system is capable of bypassing MACsec processing when MACsec is disabled.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxRemPFCMBC
ModelCorrespondence | string | CIM_DataCenterEthernetPort.RemPFCWilling, CIM_DataCenterEthernetPort.RemPFCCap
Write | boolean | false
RemPFCWilling | boolean |
Description | string | Indicates if the remote system is willing to accept the PFC configuration of the local system on this port.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxRemPFCWilling
ModelCorrespondence | string | CIM_DataCenterEthernetPort.RemPFCMBC, CIM_DataCenterEthernetPort.RemPFCCap
Write | boolean | false
AdminApplicationPriorityAEPriority | uint8[] |
ArrayType | string | Indexed
Description | string | The priority code point that should be used in frames transporting the protocol indicated by AdminApplicationPriorityAESelector and AdminApplicationPriorityAEProtocol properties.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxAdminApplicationPriorityAEPriority
ModelCorrespondence | string | CIM_DataCenterEthernetPort.AdminApplicationPriorityAESelector, CIM_DataCenterEthernetPort.AdminApplicationPriorityAEProtocol
Write | boolean | true
AdminApplicationPriorityAEProtocol | uint16[] |
ArrayType | string | Indexed
Description | string | The protocol indicator of the type indicated by AdminApplicationPriorityAESelector.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxAdminApplicationPriorityAEProtocol
ModelCorrespondence | string | CIM_DataCenterEthernetPort.AdminApplicationPriorityAESelector, CIM_DataCenterEthernetPort.AdminApplicationPriorityAEPriority
AdminApplicationPriorityAESelector | uint16[] |
ArrayType | string | Indexed
Description | string | Indicates the contents of the protocol object
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxAdminApplicationPriorityAESelector
ModelCorrespondence | string | CIM_DataCenterEthernetPort.AdminApplicationPriorityAEProtocol, CIM_DataCenterEthernetPort.AdminApplicationPriorityAEPriority
ValueMap | string | 1, 2, 3, 4, ..
Values | string | Ethertype, Well Known Port number over TCP/SCTP, Well Known Port number over UDP/DCCP, Well Known Port number over TCP/SCTP/UDP/DCCP, DMTF Reserved
AdminETSConPriority | uint8[] |
ArrayType | string | Indexed
Description | string | Indicates the priorities that are assigned to traffic classes.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxAdminETSConPriority
ModelCorrespondence | string | CIM_DataCenterEthernetPort.AdminETSConPriTrafficClass
AdminETSConPriTrafficClass | uint8[] |
ArrayType | string | Indexed
Description | string | Indicates the traffic classes to which priorities are assigned.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxAdminETSConPriTrafficClass
ModelCorrespondence | string | CIM_DataCenterEthernetPort.AdminETSConPriority
Write | boolean | true
AdminETSConTrafficClass | uint8[] |
ArrayType | string | Indexed
Description | string | Indicates the traffic classes to which bandwidth values indicated by the CIM_DataCenterEthernetPort.AdminETSConTrafficClassBandwidth apply.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxAdminETSConTrafficClass
ModelCorrespondence | string | CIM_DataCenterEthernetPort.AdminETSConTrafficClassBandwidth
AdminETSConTrafficClassBandwidth | uint8[] |
ArrayType | string | Indexed
Description | string | Indicates the % of link bandwidths assigned to traffic classes. The sum of % bandwidths in this array shall be 100.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxAdminETSConTrafficClassBandwidth
MaxValue | sint64 | 100
MinValue | sint64 | 0
ModelCorrespondence | string | CIM_DataCenterEthernetPort.AdminETSConTrafficClass
PUnit | string | percent
Write | boolean | true
AdminETSConTrafficSelectionAlgorithm | uint8[] |
ArrayType | string | Indexed
Description | string | Indicates the Traffic Selection Algorithms to which traffic classes are assigned."
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxAdminETSConTrafficSelectionAlgorithm
ModelCorrespondence | string | CIM_DataCenterEthernetPort.AdminETSConTSATrafficClass
ValueMap | string | 0, 1, 2, .., 255
Values | string | Strict Priority, Credit-based shaper, Enhanced transmission selection, DMTF Reserved, Vendor Reserved
Write | boolean | true
AdminETSConTSATrafficClass | uint8[] |
ArrayType | string | Indexed
Description | string | Indicates the traffic classes that are assigned traffic selection algorithms.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxAdminETSConTSATrafficClass
ModelCorrespondence | string | CIM_DataCenterEthernetPort.AdminETSConTrafficSelectionAlgorithm
AdminETSRecoTrafficClass | uint8[] |
ArrayType | string | Indexed
Description | string | Indicates the traffic classes to which bandwidths apply. Used for recommendation TLV.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxAdminETSRecoTrafficClass
ModelCorrespondence | string | CIM_DataCenterEthernetPort.AdminETSRecoTrafficClassBandwidth
AdminETSRecoTrafficClassBandwidth | uint64[] |
ArrayType | string | Indexed
Description | string | Indicates the bandwidths assigned to traffic classes for recommendation TLV.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxAdminETSRecoTrafficClassBandwidth
ModelCorrespondence | string | CIM_DataCenterEthernetPort.AdminETSRecoTrafficClass
PUnit | string | bit / second
Write | boolean | true
AdminETSRecoTrafficSelectionAlgorithm | uint8[] |
ArrayType | string | Indexed
Description | string | Indicates the Traffic Selection Algorithms to which traffic classes are to be assigned. Used for Recommendation TLV.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxAdminETSRecoTrafficSelectionAlgorithm
ModelCorrespondence | string | CIM_DataCenterEthernetPort.AdminETSRecoTSATrafficClass
ValueMap | string | 0, 1, 2, .., 255
Values | string | Strict Priority, Credit-based shaper, Enhanced transmission selection, DMTF Reserved, Vendor Reserved
Write | boolean | true
AdminETSRecoTSATrafficClass | uint8[] |
ArrayType | string | Indexed
Description | string | Indicates the traffic classes that are assigned to traffic selection algorithms. Used for Recommendation TLV.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxETSRecoTSATrafficClass
ModelCorrespondence | string | CIM_DataCenterEthernetPort.AdminETSRecoTrafficSelectionAlgorithm
AdminPFCEnableEnabled | boolean[] |
ArrayType | string | Indexed
Description | string | Indicates if PFC is enabled on the corresponding priority.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxAdminPFCEnableEnabled
ModelCorrespondence | string | CIM_DataCenterEthernetPort.AdminPFCEnablePriority
Write | boolean | true
AdminPFCEnablePriority | uint8[] |
ArrayType | string | Indexed
Description | string | Prioity for which PFC is enabled / disabled
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxAdminPFCEnablePriority
ModelCorrespondence | string | CIM_DataCenterEthernetPort.AdminPFCEnableEnabled
LocApplicationPriorityAEPriority | uint8[] |
ArrayType | string | Indexed
Description | string | The priority code point that should be used in frames transporting the protocol indicated by LocApplicationPriorityAESelector and LocApplicationPriorityAEProtocol properties.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxLocApplicationPriorityAEPriority
ModelCorrespondence | string | CIM_DataCenterEthernetPort.LocApplicationPriorityAESelector, CIM_DataCenterEthernetPort.LocApplicationPriorityAEProtocol
LocApplicationPriorityAEProtocol | uint16[] |
ArrayType | string | Indexed
Description | string | The protocol indicator of the type indicated by LocApplicationPriorityAESelector.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxLocApplicationPriorityAEProtocol
ModelCorrespondence | string | CIM_DataCenterEthernetPort.LocApplicationPriorityAESelector, CIM_DataCenterEthernetPort.LocApplicationPriorityAEPriority
LocApplicationPriorityAESelector | uint16[] |
ArrayType | string | Indexed
Description | string | Indicates the contents of the protocol object
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxLocApplicationPriorityAESelector
ModelCorrespondence | string | CIM_DataCenterEthernetPort.LocApplicationPriorityAEProtocol, CIM_DataCenterEthernetPort.LocApplicationPriorityAEPriority
ValueMap | string | 1, 2, 3, 4, ..
Values | string | Ethertype, Well Known Port number over TCP/SCTP, Well Known Port number over UDP/DCCP, Well Known Port number over TCP/SCTP/UDP/DCCP, DMTF Reserved
LocETSConPriority | uint8[] |
ArrayType | string | Indexed
Description | string | Indicates the priorities that are assigned to traffic classes.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxLocETSConPriority
ModelCorrespondence | string | CIM_DataCenterEthernetPort.LocETSConPriTrafficClass
LocETSConPriTrafficClass | uint8[] |
ArrayType | string | Indexed
Description | string | Indicates the traffic classes to which priorities are assigned.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxLocETSConPriTrafficClass
ModelCorrespondence | string | CIM_DataCenterEthernetPort.LocETSConPriority
LocETSConTrafficClass | uint8[] |
ArrayType | string | Indexed
Description | string | Indicates the traffic classes to which bandwidth values indicated by the CIM_DataCenterEthernetPort.LocETSConTrafficClassBandwidth apply.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxLocETSConTrafficClass
ModelCorrespondence | string | CIM_DataCenterEthernetPort.LocETSConTrafficClassBandwidth
LocETSConTrafficClassBandwidth | uint8[] |
ArrayType | string | Indexed
Description | string | Indicates the % of link bandwidths assigned to traffic classes. The sum of % bandwidths in this array shall be 100.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxLocETSConTrafficClassBandwidth
MaxValue | sint64 | 100
MinValue | sint64 | 0
ModelCorrespondence | string | CIM_DataCenterEthernetPort.LocETSConTrafficClass
PUnit | string | percent
LocETSConTrafficSelectionAlgorithm | uint8[] |
ArrayType | string | Indexed
Description | string | Indicates the Traffic Selection Algorithms to which traffic classes are assigned."
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxLocETSConTrafficSelectionAlgorithm
ModelCorrespondence | string | CIM_DataCenterEthernetPort.LocETSConTSATrafficClass
ValueMap | string | 0, 1, 2, .., 255
Values | string | Strict Priority, Credit-based shaper, Enhanced transmission selection, DMTF Reserved, Vendor Reserved
LocETSConTSATrafficClass | uint8[] |
ArrayType | string | Indexed
Description | string | Indicates the traffic classes that are assigned traffic selection algorithms.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxLocETSConTSATrafficClass
ModelCorrespondence | string | CIM_DataCenterEthernetPort.LocETSConTrafficSelectionAlgorithm
LocETSRecoTrafficClass | uint8[] |
ArrayType | string | Indexed
Description | string | Indicates the traffic classes to which bandwidths apply. Used for recommendation TLV.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxLocETSRecoTrafficClass
ModelCorrespondence | string | CIM_DataCenterEthernetPort.LocETSRecoTrafficClassBandwidth
LocETSRecoTrafficClassBandwidth | uint64[] |
ArrayType | string | Indexed
Description | string | Indicates the bandwidths assigned to traffic classes for recommendation TLV.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxLocETSRecoTrafficClassBandwidth
ModelCorrespondence | string | CIM_DataCenterEthernetPort.LocETSRecoTrafficClass
PUnit | string | bit / second
LocETSRecoTrafficSelectionAlgorithm | uint8[] |
ArrayType | string | Indexed
Description | string | Indicates the Traffic Selection Algorithms to which traffic classes are to be assigned. Used for Recommendation TLV.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxLocETSRecoTrafficSelectionAlgorithm
ModelCorrespondence | string | CIM_DataCenterEthernetPort.LocETSRecoTSATrafficClass
ValueMap | string | 0, 1, 2, .., 255
Values | string | Strict Priority, Credit-based shaper, Enhanced transmission selection, DMTF Reserved, Vendor Reserved
LocETSRecoTSATrafficClass | uint8[] |
ArrayType | string | Indexed
Description | string | Indicates the traffic classes that are assigned to traffic selection algorithms. Used for Recommendation TLV.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxETSRecoTSATrafficClass
ModelCorrespondence | string | CIM_DataCenterEthernetPort.LocETSRecoTrafficSelectionAlgorithm
LocPFCEnableEnabled | boolean[] |
ArrayType | string | Indexed
Description | string | Indicates if PFC is enabled on the corresponding priority.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxLocPFCEnableEnabled
ModelCorrespondence | string | CIM_DataCenterEthernetPort.LocPFCEnablePriority
LocPFCEnablePriority | uint8[] |
ArrayType | string | Indexed
Description | string | Prioity for which PFC is enabled / disabled
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxLocPFCEnablePriority
ModelCorrespondence | string | CIM_DataCenterEthernetPort.LocPFCEnableEnabled
RemApplicationPriorityAEPriority | uint8[] |
ArrayType | string | Indexed
Description | string | The priority code point that should be used in frames transporting the protocol indicated by RemApplicationPriorityAESelector and RemApplicationPriorityAEProtocol properties.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxRemApplicationPriorityAEPriority
ModelCorrespondence | string | CIM_DataCenterEthernetPort.RemApplicationPriorityAESelector, CIM_DataCenterEthernetPort.RemApplicationPriorityAEProtocol
Write | boolean | false
RemApplicationPriorityAEProtocol | uint16[] |
ArrayType | string | Indexed
Description | string | The protocol indicator of the type indicated by RemApplicationPriorityAESelector.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxRemApplicationPriorityAEProtocol
ModelCorrespondence | string | CIM_DataCenterEthernetPort.RemApplicationPriorityAESelector, CIM_DataCenterEthernetPort.RemApplicationPriorityAEPriority
Write | boolean | false
RemApplicationPriorityAESelector | uint16[] |
ArrayType | string | Indexed
Description | string | Indicates the contents of the protocol object
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxRemApplicationPriorityAESelector
ModelCorrespondence | string | CIM_DataCenterEthernetPort.RemApplicationPriorityAEProtocol, CIM_DataCenterEthernetPort.RemApplicationPriorityAEPriority
ValueMap | string | 1, 2, 3, 4, ..
Values | string | Ethertype, Well Known Port number over TCP/SCTP, Well Known Port number over UDP/DCCP, Well Known Port number over TCP/SCTP/UDP/DCCP, DMTF Reserved
Write | boolean | false
RemETSConPriority | uint8[] |
ArrayType | string | Indexed
Description | string | Indicates the priorities that are assigned to traffic classes on the remote port.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxRemETSConPriority
ModelCorrespondence | string | CIM_DataCenterEthernetPort.RemETSConPriTrafficClass
Write | boolean | false
RemETSConPriTrafficClass | uint8[] |
ArrayType | string | Indexed
Description | string | Indicates the traffic classes to which priorities are assigned on the remote port.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxRemETSConPriTrafficClass
ModelCorrespondence | string | CIM_DataCenterEthernetPort.RemETSConPriority
Write | boolean | false
RemETSConTrafficClass | uint8[] |
ArrayType | string | Indexed
Description | string | Indicates the traffic classes to which bandwidth values indicated by the CIM_DataCenterEthernetPort.RemETSConTrafficClassBandwidth apply.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxRemETSConTrafficClass
ModelCorrespondence | string | CIM_DataCenterEthernetPort.RemETSConTrafficClassBandwidth
Write | boolean | false
RemETSConTrafficClassBandwidth | uint8[] |
ArrayType | string | Indexed
Description | string | Indicates the % of link bandwidths assigned to traffic classes on the remote port. The sum of % bandwidths in this array shall be 100.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxRemETSConTrafficClassBandwidth
MaxValue | sint64 | 100
MinValue | sint64 | 0
ModelCorrespondence | string | CIM_DataCenterEthernetPort.RemETSConTrafficClass
PUnit | string | percent
Write | boolean | false
RemETSConTrafficSelectionAlgorithm | uint8[] |
ArrayType | string | Indexed
Description | string | Indicates the Traffic Selection Algorithms to which traffic classes are assigned on the remote port."
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxRemETSConTrafficSelectionAlgorithm
ModelCorrespondence | string | CIM_DataCenterEthernetPort.RemETSConTSATrafficClass
ValueMap | string | 0, 1, 2, .., 255
Values | string | Strict Priority, Credit-based shaper, Enhanced transmission selection, DMTF Reserved, Vendor Reserved
Write | boolean | false
RemETSConTSATrafficClass | uint8[] |
ArrayType | string | Indexed
Description | string | Indicates the traffic classes that are assigned traffic selection algorithms on the remote port.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxRemETSConTSATrafficClass
ModelCorrespondence | string | CIM_DataCenterEthernetPort.RemETSConTrafficSelectionAlgorithm
Write | boolean | false
RemETSRecoTrafficClass | uint8[] |
ArrayType | string | Indexed
Description | string | Indicates the traffic classes to which bandwidths apply on the remote port. Used for recommendation TLV.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxRemETSRecoTrafficClass
ModelCorrespondence | string | CIM_DataCenterEthernetPort.RemETSRecoTrafficClassBandwidth
RemETSRecoTrafficClassBandwidth | uint64[] |
ArrayType | string | Indexed
Description | string | Indicates the bandwidths assigned to traffic classes for recommendation TLV on the remote port.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxRemETSRecoTrafficClassBandwidth
ModelCorrespondence | string | CIM_DataCenterEthernetPort.RemETSRecoTrafficClass
PUnit | string | bit / second
Write | boolean | false
RemETSRecoTrafficSelectionAlgorithm | uint8[] |
ArrayType | string | Indexed
Description | string | Indicates the Traffic Selection Algorithms to which traffic classes are to be assigned on the remote port. Used for Recommendation TLV.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxRemETSRecoTrafficSelectionAlgorithm
ModelCorrespondence | string | CIM_DataCenterEthernetPort.RemETSRecoTSATrafficClass
ValueMap | string | 0, 1, 2, .., 255
Values | string | Strict Priority, Credit-based shaper, Enhanced transmission selection, DMTF Reserved, Vendor Reserved
Write | boolean | false
RemETSRecoTSATrafficClass | uint8[] |
ArrayType | string | Indexed
Description | string | Indicates the traffic classes that are assigned to traffic selection algorithms on the remote port. Used for Recommendation TLV.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxRemETSRecoTSATrafficClass
ModelCorrespondence | string | CIM_DataCenterEthernetPort.RemETSRecoTrafficSelectionAlgorithm
Write | boolean | false
RemPFCEnableEnabled | boolean[] |
ArrayType | string | Indexed
Description | string | Indicates if PFC is enabled on the corresponding priority on the remote port.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxRemPFCEnableEnabled
ModelCorrespondence | string | CIM_DataCenterEthernetPort.RemPFCEnablePriority
Write | boolean | false
RemPFCEnablePriority | uint8[] |
ArrayType | string | Indexed
Description | string | Priority for which PFC is enabled / disabled on the remote port.
MappingStrings | string | IEEE.MIB|LLDP-EXT-DOT1-V2-MIB.lldpXdot1dcbxRemPFCEnablePriority
ModelCorrespondence | string | CIM_DataCenterEthernetPort.RemPFCEnableEnabled
Write | boolean | false

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
ActiveMaximumTransmissionUnit | uint64 | CIM_NetworkPort
AllocationState | string | CIM_LogicalDevice
AutoSense | boolean | CIM_NetworkPort
Availability | uint16 | CIM_LogicalDevice
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
ConfigManVidTxEnable | boolean | CIM_LLDPEthernetPort
ConfigPortVlanTxEnable | boolean | CIM_LLDPEthernetPort
CreationClassName | string | CIM_LogicalDevice
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
DeviceID | string | CIM_LogicalDevice
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
ErrorCleared | boolean | CIM_LogicalDevice
ErrorDescription | string | CIM_LogicalDevice
FullDuplex | boolean | CIM_NetworkPort
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
LastErrorCode | uint32 | CIM_LogicalDevice
LinkTechnology | uint16 | CIM_NetworkPort
LocationIndicator | uint16 | CIM_LogicalDevice
LocChassisId | string | CIM_LLDPEthernetPort
LocChassisIdSubtype | uint8 | CIM_LLDPEthernetPort
LocFbSystemValue | uint16 | CIM_LLDPEthernetPort
LocPortDesc | string | CIM_LLDPEthernetPort
LocPortID | string | CIM_LLDPEthernetPort
LocPortIdSubtype | uint8 | CIM_LLDPEthernetPort
LocResolvedRxSystemValue | uint16 | CIM_LLDPEthernetPort
LocResolvedTxSystemValue | uint16 | CIM_LLDPEthernetPort
LocRxSystemValue | uint16 | CIM_LLDPEthernetPort
LocRxSystemValueEcho | uint16 | CIM_LLDPEthernetPort
LocSysDesc | string | CIM_LLDPEthernetPort
LocSysName | string | CIM_LLDPEthernetPort
LocTxSystemValue | uint16 | CIM_LLDPEthernetPort
LocTxSystemValueEcho | uint16 | CIM_LLDPEthernetPort
MaxDataSize | uint32 | CIM_EthernetPort
MaximumFrameSizeTLVEnabled | boolean | CIM_LLDPEthernetPort
MaxQuiesceTime | uint64 | CIM_LogicalDevice
MaxSpeed | uint64 | CIM_LogicalPort
MessageFastTx | uint16 | CIM_LLDPEthernetPort
MessageTxHoldMultiplier | uint8 | CIM_LLDPEthernetPort
MessageTxInterval | uint16 | CIM_LLDPEthernetPort
Name | string | CIM_ManagedSystemElement
NotificationInterval | uint16 | CIM_LLDPEthernetPort
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
OtherLinkTechnology | string | CIM_NetworkPort
OtherNetworkPortType | string | CIM_NetworkPort
OtherPortType | string | CIM_LogicalPort
PermanentAddress | string | CIM_NetworkPort
PoEPowerEntityType | uint16 | CIM_EthernetPort
PortNumber | uint16 | CIM_NetworkPort
PortType | uint16 | CIM_EthernetPort
PowerManagementSupported | boolean | CIM_LogicalDevice
PowerOnHours | uint64 | CIM_LogicalDevice
PrimaryStatus | uint16 | CIM_ManagedSystemElement
PVID | uint16 | CIM_EthernetPort
ReinitDelay | uint8 | CIM_LLDPEthernetPort
RemRxSystemValue | uint16 | CIM_LLDPEthernetPort
RemRxSystemValueEcho | uint16 | CIM_LLDPEthernetPort
RemTxSystemValue | uint16 | CIM_LLDPEthernetPort
RemTxSystemValueEcho | uint16 | CIM_LLDPEthernetPort
RequestedSpeed | uint64 | CIM_LogicalPort
RequestedState | uint16 | CIM_EnabledLogicalElement
Speed | uint64 | CIM_NetworkPort
Status | string | CIM_ManagedSystemElement
StatusInfo | uint16 | CIM_LogicalDevice
SupportedMaximumTransmissionUnit | uint64 | CIM_NetworkPort
SystemCreationClassName | string | CIM_LogicalDevice
SystemName | string | CIM_LogicalDevice
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TotalPowerOnHours | uint64 | CIM_LogicalDevice
TransitioningToState | uint16 | CIM_EnabledLogicalElement
TxCreditMax | uint8 | CIM_LLDPEthernetPort
TxFastInit | uint8 | CIM_LLDPEthernetPort
UsageRestriction | uint16 | CIM_LogicalPort
AdditionalAvailability | uint16[] | CIM_LogicalDevice
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
Capabilities | uint16[] | CIM_EthernetPort
CapabilityDescriptions | string[] | CIM_EthernetPort
DestMacAddress | string[] | CIM_LLDPEthernetPort
EnabledCapabilities | uint16[] | CIM_EthernetPort
IdentifyingDescriptions | string[] | CIM_LogicalDevice
LocManAddr | string[] | CIM_LLDPEthernetPort
LocManAddrIfId | uint32[] | CIM_LLDPEthernetPort
LocManAddrIfSubtype | uint16[] | CIM_LLDPEthernetPort
LocManAddrSubType | uint16[] | CIM_LLDPEthernetPort
LocSysCapEnabled | boolean[] | CIM_LLDPEthernetPort
LocSysCapSupported | uint8[] | CIM_LLDPEthernetPort
ManAddrConfigDestAddress | string[] | CIM_LLDPEthernetPort
ManAddrConfigLocManAddr | string[] | CIM_LLDPEthernetPort
ManAddrConfigLocManAddrSubtype | uint16[] | CIM_LLDPEthernetPort
ManAddrConfigTxEnable | boolean[] | CIM_LLDPEthernetPort
NetworkAddresses | string[] | CIM_EthernetPort
OperationalStatus | uint16[] | CIM_ManagedSystemElement
OtherEnabledCapabilities | string[] | CIM_EthernetPort
OtherIdentifyingInfo | string[] | CIM_LogicalDevice
PortConfigAdminStatus | uint8[] | CIM_LLDPEthernetPort
PortConfigNotificationEnable | boolean[] | CIM_LLDPEthernetPort
PortConfigPortDescriptionTLVTxEnable | boolean[] | CIM_LLDPEthernetPort
PortConfigSystemCapabilitiesTLVTxEnable | boolean[] | CIM_LLDPEthernetPort
PortConfigSystemDescriptionTLVTxEnable | boolean[] | CIM_LLDPEthernetPort
PortConfigSystemNameTLVTxEnable | boolean[] | CIM_LLDPEthernetPort
PortDiscriminator | string[] | CIM_EthernetPort
PowerManagementCapabilities | uint16[] | CIM_LogicalDevice
RemChassisId | string[] | CIM_LLDPEthernetPort
RemChassisIdSubtype | uint8[] | CIM_LLDPEthernetPort
RemLocalDestMacAddress | string[] | CIM_LLDPEthernetPort
RemManAddr | string[] | CIM_LLDPEthernetPort
RemManAddrIfId | uint32[] | CIM_LLDPEthernetPort
RemManAddrIfSubtype | uint16[] | CIM_LLDPEthernetPort
RemManAddrSubType | uint16[] | CIM_LLDPEthernetPort
RemPortDesc | string[] | CIM_LLDPEthernetPort
RemPortID | string[] | CIM_LLDPEthernetPort
RemPortIdSubtype | uint8[] | CIM_LLDPEthernetPort
RemSysCapEnabled | boolean[] | CIM_LLDPEthernetPort
RemSysCapSupported | uint8[] | CIM_LLDPEthernetPort
RemSysDesc | string[] | CIM_LLDPEthernetPort
RemSysName | string[] | CIM_LLDPEthernetPort
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
EnableDevice | uint32 | CIM_LogicalDevice
OnlineDevice | uint32 | CIM_LogicalDevice
QuiesceDevice | uint32 | CIM_LogicalDevice
RequestStateChange | uint32 | CIM_EnabledLogicalElement
Reset | uint32 | CIM_LogicalDevice
RestoreProperties | uint32 | CIM_LogicalDevice
SaveProperties | uint32 | CIM_LogicalDevice
SetPowerState | uint32 | CIM_LogicalDevice