# Class CIM_AGPVideoController
extends CIM_VideoController

Note: The use of the CIM_AGPVideoController class has been deprecated in lieu of CIM_AGPVideoDisplayController. Deprecated description: Capabilities and management of an AGPVideoController.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_Controller
|
+--CIM_VideoController
|
+--CIM_AGPVideoController

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Deprecated | string | CIM_AGPVideoDisplayController
Description | string | Note: The use of the CIM_AGPVideoController class has been deprecated in lieu of CIM_AGPVideoDisplayController. Deprecated description: Capabilities and management of an AGPVideoController.
UMLPackagePath | string | CIM::Device::Controller
Version | string | 2.10.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
AddressingMode | uint16 |
Deprecated | string | CIM_AGPVideoDisplayController.AddressingMode
Description | string | An integer enumeration that indicates the addressing mode of the graphics Controller.
ValueMap | string | 0, 1, 2, 3
Values | string | Unknown, Other, Sideband, Pipeline
AGPSpecificationVersionConformance | string |
Deprecated | string | CIM_AGPVideoDisplayController.AGPSpecificationVersionConformance
Description | string | A string that contains the AGP specification version to which this graphics Controller conforms.
DataTransferRate | uint16 |
Deprecated | string | CIM_AGPVideoDisplayController.DataTransferRate
Description | string | An integer enumeration that indicates the data transfer rate of the graphics Controller.
ValueMap | string | 0, 1, 2, 3, 4
Values | string | Unknown, Other, 1X, 2X, 4X
GraphicsApertureSize | uint32 |
Deprecated | string | CIM_AGPVideoDisplayController.GraphicsApertureSize
Description | string | Size of the graphics aperture in KB.
PUnit | string | byte * 2^10
Units | string | KiloBytes
LocalBusWidth | uint32 |
Deprecated | string | CIM_AGPVideoDisplayController.LocalBusWidth
Description | string | Width of the internal bus in the graphics Controller, in bits.
PUnit | string | bit
Units | string | Bits
MaximumAGPCommandQueuePath | uint32 |
Deprecated | string | CIM_AGPVideoDisplayController.MaximumAGPCommandQueuePath
Description | string | The maximum number of AGP Transaction requests that the master (AGP Graphics Controller) is allowed to enqueue into the target.
MaxNumberOfPipelinedAGPTransactions | uint32 |
Deprecated | string | CIM_AGPVideoDisplayController.MaxNumberOfPipelinedAGPTransactions
Description | string | The number of AGP Transaction that the core logic (chip set) can accept into its transaction request queue from the Controller.
NonlocalVideoMemorySize | uint32 |
Deprecated | string | CIM_AGPVideoDisplayController.NonlocalVideoMemorySize
Description | string | Size of the non-local video memory in KB.
PUnit | string | byte * 2^10
Units | string | KiloBytes
UsageModel | uint16 |
Deprecated | string | CIM_AGPVideoDisplayController.UsageModel
Description | string | An integer enumeration that indicates the usage model of the graphics Controller. The usage model indicates how the Controller does manipulations of graphics surfaces, textures, and so on in memory. DMA indicates that the graphics Controller brings structures from the system memory to its local memory to perform needed manipulations or renderings. Execute specifies that the Graphics Controller can directly access a specified region in main memory (called the graphics aperture) using GART (Graphics Aperture Remapping Table). It then performs manipulations in that range as if that whole graphics aperture were part of its local memory. A value of "Both" DMA and Execute models can also be specified.
ValueMap | string | 0, 1, 2, 3, 4
Values | string | Unknown, Other, Execute, DMA, Both
Capabilities | uint16[] |
ArrayType | string | Indexed
Deprecated | string | No value
Description | string | Note: The use of the CIM_AGPVideoController class has been deprecated in lieu of CIM_AGPVideoDisplayController. Deprecated description: Deprecated description: Capabilities of the AGP Graphics Controller. For example, the Device might support multiple monitors, PCI Mastering, and large memory addresses. In this case, the values 3, 4, and 6 would be written to the Capabilities array.
ModelCorrespondence | string | CIM_AGPVideoController.CapabilityDescriptions
ValueMap | string | 0, 1, 2, 3, 4, 5, 6
Values | string | Unknown, Other, PCI Fast Write, MultiMonitor Support, PCI Mastering, Second Monochrome Adapter Support, Large Memory Address Support

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
AllocationState | string | CIM_LogicalDevice
Availability | uint16 | CIM_LogicalDevice
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_LogicalDevice
CurrentBitsPerPixel | uint32 | CIM_VideoController
CurrentHorizontalResolution | uint32 | CIM_VideoController
CurrentNumberOfColors | uint64 | CIM_VideoController
CurrentNumberOfColumns | uint32 | CIM_VideoController
CurrentNumberOfRows | uint32 | CIM_VideoController
CurrentRefreshRate | uint32 | CIM_VideoController
CurrentScanMode | uint16 | CIM_VideoController
CurrentVerticalResolution | uint32 | CIM_VideoController
Description | string | CIM_VideoController
DetailedStatus | uint16 | CIM_ManagedSystemElement
DeviceID | string | CIM_LogicalDevice
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
ErrorCleared | boolean | CIM_LogicalDevice
ErrorDescription | string | CIM_LogicalDevice
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
LastErrorCode | uint32 | CIM_LogicalDevice
LocationIndicator | uint16 | CIM_LogicalDevice
MaxMemorySupported | uint32 | CIM_VideoController
MaxNumberControlled | uint32 | CIM_Controller
MaxQuiesceTime | uint64 | CIM_LogicalDevice
MaxRefreshRate | uint32 | CIM_VideoController
MinRefreshRate | uint32 | CIM_VideoController
Name | string | CIM_ManagedSystemElement
NumberOfVideoPages | uint32 | CIM_VideoController
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
PowerManagementSupported | boolean | CIM_LogicalDevice
PowerOnHours | uint64 | CIM_LogicalDevice
PrimaryStatus | uint16 | CIM_ManagedSystemElement
ProtocolDescription | string | CIM_Controller
ProtocolSupported | uint16 | CIM_Controller
RequestedState | uint16 | CIM_EnabledLogicalElement
Status | string | CIM_ManagedSystemElement
StatusInfo | uint16 | CIM_LogicalDevice
SystemCreationClassName | string | CIM_LogicalDevice
SystemName | string | CIM_LogicalDevice
TimeOfLastReset | datetime | CIM_Controller
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TotalPowerOnHours | uint64 | CIM_LogicalDevice
TransitioningToState | uint16 | CIM_EnabledLogicalElement
VideoMemoryType | uint16 | CIM_VideoController
VideoProcessor | string | CIM_VideoController
AcceleratorCapabilities | uint16[] | CIM_VideoController
AdditionalAvailability | uint16[] | CIM_LogicalDevice
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
CapabilityDescriptions | string[] | CIM_VideoController
IdentifyingDescriptions | string[] | CIM_LogicalDevice
OperationalStatus | uint16[] | CIM_ManagedSystemElement
OtherIdentifyingInfo | string[] | CIM_LogicalDevice
PowerManagementCapabilities | uint16[] | CIM_LogicalDevice
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
EnableDevice | uint32 | CIM_LogicalDevice
OnlineDevice | uint32 | CIM_LogicalDevice
QuiesceDevice | uint32 | CIM_LogicalDevice
RequestStateChange | uint32 | CIM_EnabledLogicalElement
Reset | uint32 | CIM_LogicalDevice
RestoreProperties | uint32 | CIM_LogicalDevice
SaveProperties | uint32 | CIM_LogicalDevice
SetPowerState | uint32 | CIM_LogicalDevice