# Class CIM_WirelessLANEndpoint
extends CIM_ProtocolEndpoint

A ProtocolEndpoint supporting 802.11 wireless networking.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_ServiceAccessPoint
|
+--CIM_ProtocolEndpoint
|
+--CIM_WirelessLANEndpoint

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | A ProtocolEndpoint supporting 802.11 wireless networking.
Experimental | boolean | true
UMLPackagePath | string | CIM::Network::ProtocolEndpoints
Version | string | 2.8.1000

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
Name | string |
Description | string | The MAC Address of the wireless endpoint.
Key | boolean | true
MaxLen | uint32 | 256
Override | string | Name
ProtocolIFType | uint16 | 71
Description | string | ProtocolIFType's enumeration is limited to wirelss-related and reserved values for this subclass of ProtocolEndpoint.
MappingStrings | string | MIB.IETF|IF-MIB.ifType
ModelCorrespondence | string | CIM_ProtocolEndpoint.OtherTypeDescription
Override | string | ProtocolIFType
ValueMap | string | 1, 71, 225..4095, 4112, 4113, 4114, 4115, 4301..32767, 32768..
Values | string | Other, IEEE 802.11, IANA Reserved, 802.11a, 802.11b, 802.11g, 802.11h, DMTF Reserved, Vendor Reserved
SSID | string |
Description | string | A 32-character identifier (the Service Set Identifier) that is inserted into the header of packets transmitted from the endpoint. This identifier helps to distinguish one Wireless LAN from another.
MaxLen | uint32 | 32
WEPEnabled | boolean | false
Description | string | Boolean indicating whether the Wired Equivalent Privacy algorithm is enabled for communications on this endpoint. By default, this property is set to FALSE.
WEPKeyMixEnabled | boolean | false
Description | string | Boolean indicating whether WEP key mixing is used. By default, this property is set to FALSE.

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
BroadcastResetSupported | boolean | CIM_ProtocolEndpoint
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_ServiceAccessPoint
Description | string | CIM_ProtocolEndpoint
DetailedStatus | uint16 | CIM_ManagedSystemElement
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_ProtocolEndpoint
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
NameFormat | string | CIM_ProtocolEndpoint
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
OtherTypeDescription | string | CIM_ProtocolEndpoint
PrimaryStatus | uint16 | CIM_ManagedSystemElement
ProtocolType | uint16 | CIM_ProtocolEndpoint
RequestedState | uint16 | CIM_EnabledLogicalElement
Status | string | CIM_ManagedSystemElement
SystemCreationClassName | string | CIM_ServiceAccessPoint
SystemName | string | CIM_ServiceAccessPoint
TimeOfLastStateChange | datetime | CIM_ProtocolEndpoint
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
OperationalStatus | uint16[] | CIM_ProtocolEndpoint
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
BroadcastReset | uint32 | CIM_ProtocolEndpoint
RequestStateChange | uint32 | CIM_EnabledLogicalElement