# Class CIM_TelnetProtocolEndpoint
extends CIM_ProtocolEndpoint

A representation of a communications endpoint where a Telnet server can be accessed using the Telnet protocol.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_ServiceAccessPoint
|
+--CIM_ProtocolEndpoint
|
+--CIM_TelnetProtocolEndpoint

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | A representation of a communications endpoint where a Telnet server can be accessed using the Telnet protocol.
UMLPackagePath | string | CIM::Network::ConsoleProtocols
Version | string | 2.22.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
CharacterDisplayMode | uint16 |
Description | string | The character display mode that is currently active.
ModelCorrespondence | string | CIM_TelnetProtocolEndpoint.OtherCharacterDisplayMode, CIM_TelnetProtocolEndpoint.EnabledCharacterDisplayModes
ValueMap | string | 0, 1, 2, 3, 4..32767, 32768..65535
Values | string | Unknown, Other, Console, Stream, DMTF Reserved, Vendor Reserved
Write | boolean | true
EscapeCharacter | string |
Description | string | String indicating the Escape Character is in effect.
Write | boolean | true
IdleTimeout | uint32 | 0
Description | string | IdleTimeout specifies how long the connection can be idle before it is closed. The default value, 0, indicates that there is no idle timeout period.
PUnit | string | second
Units | string | Seconds
Write | boolean | true
OtherCharacterDisplayMode | string |
Description | string | When the CharacterDisplayMode property is set to 1, "Other" then this is a free form string providing more information about the character display mode. If not set to 1, this string has no meaning.
ModelCorrespondence | string | CIM_TelnetProtocolEndpoint.CharacterDisplayMode, CIM_TelnetProtocolEndpoint.OtherEnabledCharacterDisplayMode
Write | boolean | true
OtherTerminalMode | string |
Description | string | Where the TerminalMode property contains a value of 1, "Other" then this is a free form string providing more information about the current terminal mode and this value shall be one of the values in OtherEnabledTerminalModes. If not set to 1, this string has no meaning.
ModelCorrespondence | string | CIM_TelnetProtocolEndpoint.TerminalMode, CIM_TelnetProtocolEndpoint.OtherEnabledTerminalMode
Write | boolean | true
TerminalMode | uint16 |
Description | string | The terminal mode in use for this Telnet endpoint.This value shall be one of the values in EnabledTerminalModes
ModelCorrespondence | string | CIM_TelnetProtocolEndpoint.OtherTerminalMode, CIM_TelnetProtocolEndpoint.EnabledTerminalModes
ValueMap | string | 0, 1, 2, 3, 4..32767, 32768..65535
Values | string | Unknown, Other, VT100, ANSI, DMTF Reserved, Vendor Reserved
Write | boolean | true
EnabledCharacterDisplayModes | uint16[] |
ArrayType | string | Indexed
Description | string | An array of integers indicating the character display modes enabled for the service. Additional character display modes may be supported but currently not enabled for use.
ModelCorrespondence | string | CIM_TelnetProtocolEndpoint.OtherEnabledCharacterDisplayMode
ValueMap | string | 0, 1, 2, 3, 4..32767, 32768..65535
Values | string | Unknown, Other, Console, Stream, DMTF Reserved, Vendor Reserved
Write | boolean | true
EnabledTerminalModes | uint16[] |
ArrayType | string | Indexed
Description | string | An array of integers indicating the terminal modes that are enabled for use in this server connection. Additional terminal modes may be supported by the service but not enabled for use.
ModelCorrespondence | string | CIM_TelnetProtocolEndpoint.OtherEnabledTerminalMode
ValueMap | string | 0, 1, 2, 3, 4..32767, 32768..65535
Values | string | Unknown, Other, VT100, ANSI, DMTF Reserved, Vendor Reserved
OtherEnabledCharacterDisplayMode | string[] |
ArrayType | string | Indexed
Description | string | If the EnabledCharacterDisplayModes property is set to 1, "Other" then free form string providing more information about the enabled mode. If not set to 1, this string has no meaning.
ModelCorrespondence | string | CIM_TelnetProtocolEndpoint.EnabledCharacterDisplayModes
OtherEnabledTerminalMode | string[] |
ArrayType | string | Indexed
Description | string | If the EnabledTerminalModes property is set to 1, "Other" then free form string providing more information about supported terminal mode. If not set to 1, this string has no meaning.
ModelCorrespondence | string | CIM_TelnetProtocolEndpoint.EnabledTerminalModes

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
BroadcastResetSupported | boolean | CIM_ProtocolEndpoint
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_ServiceAccessPoint
Description | string | CIM_ProtocolEndpoint
DetailedStatus | uint16 | CIM_ManagedSystemElement
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_ProtocolEndpoint
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
Name | string | CIM_ProtocolEndpoint
NameFormat | string | CIM_ProtocolEndpoint
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
OtherTypeDescription | string | CIM_ProtocolEndpoint
PrimaryStatus | uint16 | CIM_ManagedSystemElement
ProtocolIFType | uint16 | CIM_ProtocolEndpoint
ProtocolType | uint16 | CIM_ProtocolEndpoint
RequestedState | uint16 | CIM_EnabledLogicalElement
Status | string | CIM_ManagedSystemElement
SystemCreationClassName | string | CIM_ServiceAccessPoint
SystemName | string | CIM_ServiceAccessPoint
TimeOfLastStateChange | datetime | CIM_ProtocolEndpoint
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
OperationalStatus | uint16[] | CIM_ProtocolEndpoint
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
BroadcastReset | uint32 | CIM_ProtocolEndpoint
RequestStateChange | uint32 | CIM_EnabledLogicalElement