# Class CIM_MPLSCapabilities
extends CIM_Capabilities

This class specifies the capabilities of an MPLSService or MPLSProtocolEndpoint (interface) on a Label Switched Router (LSR). The association CIM_ElementCapabilities relates the instance with its MPLS Service and/or Endpoint.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_Capabilities
|
+--CIM_MPLSCapabilities

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | This class specifies the capabilities of an MPLSService or MPLSProtocolEndpoint (interface) on a Label Switched Router (LSR). The association CIM_ElementCapabilities relates the instance with its MPLS Service and/or Endpoint.
Experimental | boolean | true
UMLPackagePath | string | CIM::Network::MPLS
Version | string | 2.8.1000

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
LabelMaxIn | uint32 |
Description | string | This is the maximum value of an MPLS label that this Endpoint or MPLSService is willing to receive. The values of an MPLSProtocolEndpoint may overrule the values specified for the LSR as a whole, based on the Endpoint's boolean property OverruleLSR.
MappingStrings | string | MIB.IETF|MPLS-LSR-MIB.MPLSInterfaceLabelMaxIn
LabelMaxOut | uint32 |
Description | string | This is the maximum value of an MPLS label that this Endpoint or MPLSService is willing to send. The values of an MPLSProtocolEndpoint may overrule the values specified for the LSR as a whole, based on the Endpoint's boolean property OverruleLSR.
MappingStrings | string | MIB.IETF|MPLS-LSR-MIB.MPLSInterfaceLabelMaxOut
LabelMinIn | uint32 |
Description | string | This is the minimum value of an MPLS label that this Endpoint or MPLSService is willing to receive. The values of an MPLSProtocolEndpoint may overrule the values specified for the LSR as a whole, based on the Endpoint's boolean property OverruleLSR.
MappingStrings | string | MIB.IETF|MPLS-LSR-MIB.MPLSInterfaceLabelMinIn
LabelMinOut | uint32 |
Description | string | This is the minimum value of an MPLS label that this Endpoint or MPLSService is willing to send. The values of an MPLSProtocolEndpoint may overrule the values specified for the LSR as a whole, based on the Endpoint's boolean property OverruleLSR.
MappingStrings | string | MIB.IETF|MPLS-LSR-MIB.MPLSInterfaceLabelMinOut

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
Description | string | CIM_ManagedElement
ElementName | string | CIM_Capabilities
Generation | uint64 | CIM_ManagedElement
InstanceID | string | CIM_Capabilities

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
CreateGoalSettings | uint16 | CIM_Capabilities