# Class CIM_AsymmetricAccessibility
extends CIM_Dependency

This association indicates the accessibility of StorageVolumes in the StorageResourceLoadGroup through ports in the associated TargetPortGroup.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_Dependency
|
+--CIM_AsymmetricAccessibility

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Association | boolean | true
Description | string | This association indicates the accessibility of StorageVolumes in the StorageResourceLoadGroup through ports in the associated TargetPortGroup.
Experimental | boolean | true
UMLPackagePath | string | CIM::Device::StorageServices
Version | string | 2.18.1

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
CurrentAccessState | uint16 |
Description | string | This property indicates the current accessibility state of volumes in the StorageResourceLoadGroup through ports in the TargetPortGroup. With the exception of 'Unavailable', the states are those defined by the T10 SPC-4 Target Port Group Access States clause. 2(Unavailable): The volumes are not accessible in any way. 3(Standby): No data access to the volume is possible. Status and other non-data access commands are available. 4(Active Non-Optimized): Data access to the volume is available at less than full bandwidth. 5(Active Optimized): Data access to the volume is available at full bandwidth.
ValueMap | string | 2, 3, 4, 5
Values | string | Unavailable, Standby, Active Non-Optimized, Active Optimized
NormalAccessState | uint16 |
Description | string | This property indicates the normal accessibility state of volumes in the StorageResourceLoadGroup through ports in the TargetPortGroup when the primary storage processor hosting the groups is healthy. With the exception of 'Unavailable', the states are those defined by the T10 SPC-4 Target Port Group Access States clause. 2(Unavailable): The volumes are not accessible. 3(Standby): No data access to the volume is possible. Status and other non-data access commands are available. 4(Active Non-Optimized): Data access to the volume is available at less than full bandwidth. 5(Active Optimized): Data access to the volume is available at full bandwidth.
ValueMap | string | 2, 3, 4, 5
Values | string | Unavailable, Standby, Active Non-Optimized, Active Optimized

### Association References

Name | Class Origin | Reference Class
--- | --- | ---
Antecedent | CIM_AsymmetricAccessibility | CIM_TargetPortGroup
Dependent | CIM_AsymmetricAccessibility | CIM_StorageResourceLoadGroup

## Class Methods