# Class CIM_PhysicalElement
extends CIM_ManagedSystemElement

Subclasses of CIM_PhysicalElement define any component of a System that has a distinct physical identity. Instances of this class can be defined as an object that can be seen or touched. All Processes, Files, and LogicalDevices are considered not to be Physical Elements. For example, it is not possible to touch the functionality of a 'modem.' You can touch only the card or package that implements the modem. The same card could also implement a LAN adapter. PhysicalElements are tangible ManagedSystemElements that have a physical manifestation of some sort. Note that the properties of PhysicalElement describe a hardware entity. Possible replacement (FRU) information is defined by following the ElementFRU association to one or more instances of the ReplacementFRU class. This definition allows a client to determine what hardware can be replaced (FRUed) and what 'spare' parts might be required by a customer or engineer doing the replacement. If it can be instrumented or manually determined that an element actually replaced (FRUed) another, then this can be described in the model using the ElementHasBeenFRUed association.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_PhysicalElement

## Direct Known Subclasses

CIM_ComponentBay
CIM_PhysicalComponent
CIM_PhysicalConnector
CIM_PhysicalLink
CIM_PhysicalPackage

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Abstract | boolean | true
Description | string | Subclasses of CIM_PhysicalElement define any component of a System that has a distinct physical identity. Instances of this class can be defined as an object that can be seen or touched. All Processes, Files, and LogicalDevices are considered not to be Physical Elements. For example, it is not possible to touch the functionality of a 'modem.' You can touch only the card or package that implements the modem. The same card could also implement a LAN adapter. PhysicalElements are tangible ManagedSystemElements that have a physical manifestation of some sort. Note that the properties of PhysicalElement describe a hardware entity. Possible replacement (FRU) information is defined by following the ElementFRU association to one or more instances of the ReplacementFRU class. This definition allows a client to determine what hardware can be replaced (FRUed) and what 'spare' parts might be required by a customer or engineer doing the replacement. If it can be instrumented or manually determined that an element actually replaced (FRUed) another, then this can be described in the model using the ElementHasBeenFRUed association.
UMLPackagePath | string | CIM::Core::Physical
Version | string | 2.10.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
CanBeFRUed | boolean |
Description | string | Boolean that indicates whether this PhysicalElement can be FRUed (TRUE) or not (FALSE).
MappingStrings | string | MIB.IETF|Entity-MIB.entPhysicalIsFRU
CreationClassName | string |
Description | string | CreationClassName indicates the name of the class or the subclass used in the creation of an instance. When used with the other key properties of this class, this property allows all instances of this class and its subclasses to be uniquely identified.
Key | boolean | true
MaxLen | uint32 | 256
Description | string |
Description | string | A textual description of the PhysicalElement.
MappingStrings | string | MIF.DMTF|FRU|003.3
Override | string | Description
ElementName | string |
Description | string | A user-friendly name for the object. This property allows each instance to define a user-friendly name in addition to its key properties, identity data, and description information. Note that the Name property of ManagedSystemElement is also defined as a user-friendly name. But, it is often subclassed to be a Key. It is not reasonable that the same property can convey both identity and a user-friendly name, without inconsistencies. Where Name exists and is not a Key (such as for instances of LogicalDevice), the same information can be present in both the Name and ElementName properties. Note that if there is an associated instance of CIM_EnabledLogicalElementCapabilities, restrictions on this properties may exist as defined in ElementNameMask and MaxElementNameLen properties defined in that class.
MappingStrings | string | MIB.IETF|Entity-MIB.entPhysicalName
Override | string | ElementName
ManufactureDate | datetime |
Description | string | The date that this PhysicalElement was manufactured.
Manufacturer | string |
Description | string | The name of the organization responsible for producing the PhysicalElement. This organization might be the entity from whom the Element is purchased, but this is not necessarily true. The latter information is contained in the Vendor property of CIM_Product.
MappingStrings | string | MIB.IETF|Entity-MIB.entPhysicalMfgName, MIF.DMTF|FRU|003.4
MaxLen | uint32 | 256
Model | string |
Description | string | The name by which the PhysicalElement is generally known.
MappingStrings | string | MIB.IETF|Entity-MIB.entPhysicalDescr, MIF.DMTF|FRU|003.5
MaxLen | uint32 | 256
OtherIdentifyingInfo | string |
Description | string | OtherIdentifyingInfo captures data in addition to Tag information. This information could be used to identify a Physical Element. One example is bar code data associated with an Element that also has an asset tag. Note that if only bar code data is available and is unique or able to be used as an Element key, this property would be null and the bar code data would be used as the class key, in the Tag property.
MappingStrings | string | MIB.IETF|Entity-MIB.entPhysicalAlias
Write | boolean | true
PartNumber | string |
Description | string | The part number assigned by the organization that is responsible for producing or manufacturing the PhysicalElement.
MappingStrings | string | MIB.IETF|Entity-MIB.entPhysicalModelName
MaxLen | uint32 | 256
PoweredOn | boolean |
Description | string | Boolean that indicates whether the PhysicalElement is powered on (TRUE) or is currently off (FALSE).
SerialNumber | string |
Description | string | A manufacturer-allocated number used to identify the Physical Element.
MappingStrings | string | MIB.IETF|Entity-MIB.entPhysicalSerialNum, MIF.DMTF|FRU|003.7
MaxLen | uint32 | 256
SKU | string |
Description | string | The stock-keeping unit number for this PhysicalElement.
MaxLen | uint32 | 64
Tag | string |
Description | string | An arbitrary string that uniquely identifies the Physical Element and serves as the key of the Element. The Tag property can contain information such as asset tag or serial number data. The key for PhysicalElement is placed very high in the object hierarchy in order to independently identify the hardware or entity, regardless of physical placement in or on Cabinets, Adapters, and so on. For example, a hotswappable or removable component can be taken from its containing (scoping) Package and be temporarily unused. The object still continues to exist and can even be inserted into a different scoping container. Therefore, the key for Physical Element is an arbitrary string and is defined independently of any placement or location-oriented hierarchy.
Key | boolean | true
MaxLen | uint32 | 256
UserTracking | string |
Description | string | User-assigned and writeable asset-tracking identifier for the PhysicalElement.
MappingStrings | string | MIB.IETF|Entity-MIB.entPhysicalAssetID
Write | boolean | true
VendorEquipmentType | string |
Description | string | A vendor-specific hardware type for the PhysicalElement. It describes the specific equipment type for the element, as defined by the vendor or manufacturer.
MappingStrings | string | MIB.IETF|Entity-MIB.entPhysicalVendorType
Version | string |
Description | string | A string that indicates the version of the PhysicalElement.
MappingStrings | string | MIB.IETF|Entity-MIB.entPhysicalHardwareRev, MIF.DMTF|FRU|003.8
MaxLen | uint32 | 64

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
Name | string | CIM_ManagedSystemElement
OperatingStatus | uint16 | CIM_ManagedSystemElement
PrimaryStatus | uint16 | CIM_ManagedSystemElement
Status | string | CIM_ManagedSystemElement
OperationalStatus | uint16[] | CIM_ManagedSystemElement
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods