# Class CIM_NetworkAdapter
extends CIM_LogicalDevice

Note: The use of the CIM_NetworkAdpater class has been deprecated in lieu of CIM_NetworkPort. CIM_NetworkPort better reflects that the hardware of a single port is described and managed. Deprecated description: NetworkAdapter is an Abstract class that defines general networking hardware concepts (for example, PermanentAddress or Speed of operation).

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_NetworkAdapter

## Direct Known Subclasses

CIM_EthernetAdapter
CIM_FibreChannelAdapter
CIM_TokenRingAdapter

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Abstract | boolean | true
Deprecated | string | CIM_NetworkPort
Description | string | Note: The use of the CIM_NetworkAdpater class has been deprecated in lieu of CIM_NetworkPort. CIM_NetworkPort better reflects that the hardware of a single port is described and managed. Deprecated description: NetworkAdapter is an Abstract class that defines general networking hardware concepts (for example, PermanentAddress or Speed of operation).
UMLPackagePath | string | CIM::Device::NetworkAdapter
Version | string | 2.10.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
AutoSense | boolean |
Deprecated | string | CIM_NetworkPort.AutoSense
Description | string | Note: The use of this method has been deprecated. Deprecated description: A Boolean that indicates whether the NetworkAdapter is capable of automatically determining the speed or other communications characteristics of the attached network media.
FullDuplex | boolean |
Deprecated | string | CIM_NetworkPort.FullDuplex
Description | string | Note: The use of this method has been deprecated. Deprecated description: A Boolean that indicates that the Adapter is operating in full duplex mode.
MaxSpeed | uint64 |
Deprecated | string | CIM_NetworkPort.MaxSpeed
Description | string | Note: The use of this method has been deprecated. Deprecated description: The maximum speed, in Bits per Second, for the Network Adapter.
PUnit | string | bit / second
Units | string | Bits per Second
OctetsReceived | uint64 |
Counter | boolean | true
Deprecated | string | CIM_NetworkPortStatistics.BytesReceived
Description | string | Note: The use of OctetsReceived is deprecated. The replacement is CIM_NetworkPortStatistics.BytesReceived.
MappingStrings | string | MIB.IETF|RFC1213-MIB.ifInOctets, MIF.DMTF|Network Adapter 802 Port|001.9
OctetsTransmitted | uint64 |
Counter | boolean | true
Deprecated | string | CIM_NetworkPortStatistics.BytesTransmitted
Description | string | Note: The use of this method has been deprecated. The replacement is CIM_NetworkPortStatistics.BytesTransmitted.
MappingStrings | string | MIB.IETF|RFC1213-MIB.ifOutOctets, MIF.DMTF|Network Adapter 802 Port|001.7
PermanentAddress | string |
Deprecated | string | CIM_NetworkPort.PermanentAddress
Description | string | Note: The use of this method has been deprecated. Deprecated description: PermanentAddress defines the network address that is hardcoded into an adapter. This 'hardcoded' address might be changed through a firmware upgrade or software configuration. If so, this field should be updated when the change is made. PermanentAddress should be left blank if no 'hardcoded' address exists for the NetworkAdapter.
MappingStrings | string | MIF.DMTF|Network Adapter 802 Port|001.2
MaxLen | uint32 | 64
Speed | uint64 |
Deprecated | string | CIM_NetworkPort.Speed
Description | string | Note: The use of this method has been deprecated. Deprecated description: An estimate of the current bandwidth in Bits per Second. For Adapters that vary in bandwidth or for those where no accurate estimation can be made, this property should contain the nominal bandwidth.
MappingStrings | string | MIB.IETF|RFC1213-MIB.ifSpeed, MIF.DMTF|Network Adapter 802 Port|001.5
PUnit | string | bit / second
Units | string | Bits per Second
NetworkAddresses | string[] |
ArrayType | string | Indexed
Deprecated | string | CIM_NetworkPort.NetworkAddresses
Description | string | Note: The use of this method has been deprecated. Deprecated description: An array of strings that indicates the network addresses for an adapter.
MappingStrings | string | MIF.DMTF|Network Adapter 802 Port|001.3
MaxLen | uint32 | 64

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
AllocationState | string | CIM_LogicalDevice
Availability | uint16 | CIM_LogicalDevice
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CreationClassName | string | CIM_LogicalDevice
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
DeviceID | string | CIM_LogicalDevice
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
ErrorCleared | boolean | CIM_LogicalDevice
ErrorDescription | string | CIM_LogicalDevice
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
LastErrorCode | uint32 | CIM_LogicalDevice
LocationIndicator | uint16 | CIM_LogicalDevice
MaxQuiesceTime | uint64 | CIM_LogicalDevice
Name | string | CIM_ManagedSystemElement
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
PowerManagementSupported | boolean | CIM_LogicalDevice
PowerOnHours | uint64 | CIM_LogicalDevice
PrimaryStatus | uint16 | CIM_ManagedSystemElement
RequestedState | uint16 | CIM_EnabledLogicalElement
Status | string | CIM_ManagedSystemElement
StatusInfo | uint16 | CIM_LogicalDevice
SystemCreationClassName | string | CIM_LogicalDevice
SystemName | string | CIM_LogicalDevice
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TotalPowerOnHours | uint64 | CIM_LogicalDevice
TransitioningToState | uint16 | CIM_EnabledLogicalElement
AdditionalAvailability | uint16[] | CIM_LogicalDevice
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
IdentifyingDescriptions | string[] | CIM_LogicalDevice
OperationalStatus | uint16[] | CIM_ManagedSystemElement
OtherIdentifyingInfo | string[] | CIM_LogicalDevice
PowerManagementCapabilities | uint16[] | CIM_LogicalDevice
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
EnableDevice | uint32 | CIM_LogicalDevice
OnlineDevice | uint32 | CIM_LogicalDevice
QuiesceDevice | uint32 | CIM_LogicalDevice
RequestStateChange | uint32 | CIM_EnabledLogicalElement
Reset | uint32 | CIM_LogicalDevice
RestoreProperties | uint32 | CIM_LogicalDevice
SaveProperties | uint32 | CIM_LogicalDevice
SetPowerState | uint32 | CIM_LogicalDevice