# Class CIM_NonVolatileStorage
extends CIM_Memory

This class has been deprecated in favor of CIM_Memory with the volatile parameter set to false. Capabilities and management of NV Storage. Non-volatile memory natively includes flash and ROM storage. In addition, NV memory can be BasedOn VolatileStorage, if the volatile memory is backed by a Battery. This scenario would be completely described by an instance of the AssociatedBattery relationship, referencing the NonVolatileStorage as the Dependent and the Battery as the Antecedent, and an instance of the BasedOn relationship, referencing the NonVolatileStorage as the Dependent and the VolatileStorage as the Antecedent.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_ManagedSystemElement
|
+--CIM_LogicalElement
|
+--CIM_EnabledLogicalElement
|
+--CIM_AllocatedLogicalElement
|
+--CIM_LogicalDevice
|
+--CIM_StorageExtent
|
+--CIM_Memory
|
+--CIM_NonVolatileStorage

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Deprecated | string | CIM_Memory
Description | string | This class has been deprecated in favor of CIM_Memory with the volatile parameter set to false. Capabilities and management of NV Storage. Non-volatile memory natively includes flash and ROM storage. In addition, NV memory can be BasedOn VolatileStorage, if the volatile memory is backed by a Battery. This scenario would be completely described by an instance of the AssociatedBattery relationship, referencing the NonVolatileStorage as the Dependent and the Battery as the Antecedent, and an instance of the BasedOn relationship, referencing the NonVolatileStorage as the Dependent and the VolatileStorage as the Antecedent.
UMLPackagePath | string | CIM::Device::Memory
Version | string | 2.8.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
ApplicationWriteable | boolean |
Deprecated | string | No value
Description | string | Boolean indicating that at least some portion of the NonVolatileStorage is writeable by applications.
ApplicationWriteableSize | uint64 |
Deprecated | string | No value
Description | string | When at least some portion of the NonVolatileStorage is writeable (ApplicationWriteable property = TRUE), Application WritableSize indicates the number of bits available for application data. If the ApplicationWriteable property is FALSE, this property is undefined.
ModelCorrespondence | string | CIM_NonVolatileStorage.ApplicationWriteable
PUnit | string | bit
Units | string | Bits
IsWriteable | boolean |
Deprecated | string | CIM_Memory.Access
Description | string | Indicating that the NV storage is writeable.
StartAddressForApplicationWrite | uint64 |
Deprecated | string | No value
Description | string | When at least some portion of the NonVolatileStorage is writeable (ApplicationWriteable property = TRUE), StartAddress forApplcationWrite indicates the starting address for application data. If the ApplicationWriteable property is FALSE, this property is undefined.
ModelCorrespondence | string | CIM_NonVolatileStorage.ApplicationWriteable

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Access | uint16 | CIM_StorageExtent
AllocationState | string | CIM_LogicalDevice
Availability | uint16 | CIM_LogicalDevice
BlockSize | uint64 | CIM_StorageExtent
Caption | string | CIM_ManagedElement
CommunicationStatus | uint16 | CIM_ManagedSystemElement
CompressionRate | uint16 | CIM_StorageExtent
CompressionState | uint16 | CIM_StorageExtent
ConsumableBlocks | uint64 | CIM_StorageExtent
CorrectableError | boolean | CIM_Memory
CreationClassName | string | CIM_LogicalDevice
DataOrganization | uint16 | CIM_StorageExtent
DataRedundancy | uint16 | CIM_StorageExtent
DeltaReservation | uint8 | CIM_StorageExtent
Description | string | CIM_ManagedElement
DetailedStatus | uint16 | CIM_ManagedSystemElement
DeviceID | string | CIM_LogicalDevice
ElementName | string | CIM_ManagedElement
EnabledDefault | uint16 | CIM_EnabledLogicalElement
EnabledState | uint16 | CIM_EnabledLogicalElement
EndingAddress | uint64 | CIM_Memory
ErrorAccess | uint16 | CIM_Memory
ErrorAddress | uint64 | CIM_Memory
ErrorCleared | boolean | CIM_LogicalDevice
ErrorDataOrder | uint16 | CIM_Memory
ErrorDescription | string | CIM_LogicalDevice
ErrorInfo | uint16 | CIM_Memory
ErrorMethodology | string | CIM_Memory
ErrorResolution | uint64 | CIM_Memory
ErrorTime | datetime | CIM_Memory
ErrorTransferSize | uint32 | CIM_Memory
ExtentInterleaveDepth | uint64 | CIM_StorageExtent
ExtentStripeLength | uint64 | CIM_StorageExtent
Generation | uint64 | CIM_ManagedElement
HealthState | uint16 | CIM_ManagedSystemElement
InstallDate | datetime | CIM_ManagedSystemElement
InstanceID | string | CIM_ManagedElement
IsBasedOnUnderlyingRedundancy | boolean | CIM_StorageExtent
IsComposite | boolean | CIM_StorageExtent
IsCompressed | boolean | CIM_StorageExtent
IsConcatenated | boolean | CIM_StorageExtent
LastErrorCode | uint32 | CIM_LogicalDevice
LocationIndicator | uint16 | CIM_LogicalDevice
MaxQuiesceTime | uint64 | CIM_LogicalDevice
Name | string | CIM_StorageExtent
NameFormat | uint16 | CIM_StorageExtent
NameNamespace | uint16 | CIM_StorageExtent
NoSinglePointOfFailure | boolean | CIM_StorageExtent
NumberOfBlocks | uint64 | CIM_StorageExtent
OperatingStatus | uint16 | CIM_ManagedSystemElement
OtherEnabledState | string | CIM_EnabledLogicalElement
OtherErrorDescription | string | CIM_Memory
OtherNameFormat | string | CIM_StorageExtent
OtherNameNamespace | string | CIM_StorageExtent
OtherUsageDescription | string | CIM_StorageExtent
PackageRedundancy | uint16 | CIM_StorageExtent
PowerManagementSupported | boolean | CIM_LogicalDevice
PowerOnHours | uint64 | CIM_LogicalDevice
PrimaryStatus | uint16 | CIM_ManagedSystemElement
Primordial | boolean | CIM_StorageExtent
Purpose | string | CIM_StorageExtent
RequestedState | uint16 | CIM_EnabledLogicalElement
SequentialAccess | boolean | CIM_StorageExtent
StartingAddress | uint64 | CIM_Memory
Status | string | CIM_ManagedSystemElement
StatusInfo | uint16 | CIM_LogicalDevice
SystemCreationClassName | string | CIM_LogicalDevice
SystemLevelAddress | boolean | CIM_Memory
SystemName | string | CIM_LogicalDevice
TimeOfLastStateChange | datetime | CIM_EnabledLogicalElement
TotalPowerOnHours | uint64 | CIM_LogicalDevice
TransitioningToState | uint16 | CIM_EnabledLogicalElement
Usage | uint16 | CIM_StorageExtent
Volatile | boolean | CIM_Memory
AdditionalAvailability | uint16[] | CIM_LogicalDevice
AdditionalErrorData | uint8[] | CIM_Memory
AvailableRequestedStates | uint16[] | CIM_EnabledLogicalElement
ClientSettableUsage | uint16[] | CIM_StorageExtent
ErrorData | uint8[] | CIM_Memory
ExtentDiscriminator | string[] | CIM_StorageExtent
ExtentStatus | uint16[] | CIM_StorageExtent
IdentifyingDescriptions | string[] | CIM_LogicalDevice
OperationalStatus | uint16[] | CIM_ManagedSystemElement
OtherIdentifyingInfo | string[] | CIM_LogicalDevice
PowerManagementCapabilities | uint16[] | CIM_LogicalDevice
StatusDescriptions | string[] | CIM_ManagedSystemElement

## Class Methods

### Inherited Class Methods

Name | Return Type | Class Origin
--- | --- | ---
EnableDevice | uint32 | CIM_LogicalDevice
OnlineDevice | uint32 | CIM_LogicalDevice
QuiesceDevice | uint32 | CIM_LogicalDevice
RequestStateChange | uint32 | CIM_EnabledLogicalElement
Reset | uint32 | CIM_LogicalDevice
RestoreProperties | uint32 | CIM_LogicalDevice
SaveProperties | uint32 | CIM_LogicalDevice
SetPowerState | uint32 | CIM_LogicalDevice