# Class CIM_RedundancySetSettingData
extends CIM_SettingData

A class derived from SettingData that describes a possible configuration for an associated RedundancySet.

### Table of Contents
Hierarchy
Direct Known Subclasses
Class Qualifiers
Class Properties
Class Methods

## Class Hierarchy

CIM_ManagedElement
|
+--CIM_SettingData
|
+--CIM_RedundancySetSettingData

## Direct Known Subclasses

## Class Qualifiers

Name | Data Type | Value
--- | --- | ---
Description | string | A class derived from SettingData that describes a possible configuration for an associated RedundancySet.
Experimental | boolean | true
UMLPackagePath | string | CIM::Core::Redundancy
Version | string | 2.14.0

## Class Properties

### Local Class Properties

Name | Data Type | Default Value | Qualifiers
--- | --- | --- | ---
Name | Data Type | Value
LoadBalanceAlgorithm | uint16 |
Description | string | The desired load balance algorithm. Least Blocks, Least IO, and Address Region are used in storage device path redundancy drivers to optimize load balancing by routing requests to a path with the least queued blocks or IO requests, or based on locality of reference. 'Product Specific' indicates that the algorithm is optimized for a particular type of product. Information about that product SHOULD be provided in an associated CIM_Product instance.
ModelCorrespondence | string | CIM_RedundancySet.LoadBalanceAlgorithm
ValueMap | string | 2, 3, 4, 5, 6, 7, .., 0x8000..
Values | string | No Load Balancing, Round Robin, Least Blocks, Least IO, Address Region, Product Specific, DMTF Reserved, Vendor Reserved
Write | boolean | true
MaxNumberSupported | uint32 |
Description | string | MaxNumberSupported indicates the largest number of elements that will be able to participate in the RedundancySet. A value of 0 shall indicate no limit on the number of elements.
ModelCorrespondence | string | CIM_RedundancySet.MaxNumberSupported
MinNumberNeeded | uint32 |
Description | string | MinNumberNeeded indicates the smallest number of elements that will be required to be operational in order for components dependent on the redundancy set to function.
MinValue | sint64 | 0
ModelCorrespondence | string | CIM_RedundancySet.MinNumberNeeded
VendorIdentifyingInfo | string |
Description | string | VendorIdentifyingInfo captures the vendor identifying data for the RedundancySet. One example is the product name for a cluster.
ModelCorrespondence | string | CIM_RedundancySet.VendorIdentifyingInfo
Write | boolean | true
TypeOfSet | uint16[] |
ArrayType | string | Indexed
Description | string | TypeOfSet provides information on the type of redundancy. - N+1 (=2) indicates all members are active, are unaware and function independent of one another. However, there exist at least one extra member to achieve functionality. 'Sparing' is implied (i.e. each member can be a spare for the other(s). An example of N+1 is a system that has 2 power supplies, but needs only 1 power supply to functioning properly. - Load Balanced (=3) indicates all members are active. However, there functionality is not independent of each other. Their functioning is determined by some sort of load balancing algorithm (implemented in hardware and/or software). 'Sparing' is implied (i.e. each member can be a spare for the other(s). - Sparing (=4) indicates that all members are active and are aware of each others. However, their functionality is independent until failover. Each member can be a spare for the other(s). - Limited Sparing (=5) indicates that all members are active, and they may or may not be aware of each and they are not spares for each other. Instead, their redundancy is indicated by the IsSpare relationship.
ModelCorrespondence | string | CIM_RedundancySet.TypeOfSet
ValueMap | string | 2, 3, 4, 5, .., 0x8000..
Values | string | N+1, Load Balanced, Sparing, Limited Sparing, DMTF Reserved, Vendor Reserved
Write | boolean | true

### Inherited Properties

Name | Data Type | Class Origin
--- | --- | ---
Caption | string | CIM_ManagedElement
ChangeableType | uint16 | CIM_SettingData
ConfigurationName | string | CIM_SettingData
Description | string | CIM_ManagedElement
ElementName | string | CIM_SettingData
Generation | uint64 | CIM_ManagedElement
InstanceID | string | CIM_SettingData
SoID | string | CIM_SettingData
SoOrgID | string | CIM_SettingData
ComponentSetting | string[] | CIM_SettingData

## Class Methods