## unalignedvideoparse unalignedvideoparse |

## Properties

GValueArray * | channel-positions | Read / Write
GstRawAudioParseFormat | format | Read / Write
gboolean | interleaved | Read / Write
gint | num-channels | Read / Write
GstAudioFormat | pcm-format | Read / Write
gint | sample-rate | Read / Write

## Types and Values

struct | GstRawAudioParse

## Object Hierarchy

        GObject
        ╰── GInitiallyUnowned
            ╰── GstObject
                ╰── GstElement
                    ╰── GstBaseParse
                        ╰── GstRawBaseParse
                            ╰── GstRawAudioParse

## Description

## Synopsis

### Element Information

plugin | rawparse
author | Carlos Rafael Giani <dv@pseudoterminal.org>
class | Codec/Parser/Bin/Video

### Element Pads

name | sink
direction | sink
presence | always
details | video/x-unaligned-raw, format=(string){ I420, YV12, YUY2, UYVY, AYUV, VUYA, RGBx, BGRx, xRGB, xBGR, RGBA, BGRA, ARGB, ABGR, RGB, BGR, Y41B, Y42B, YVYU, Y444, v210, v216, Y210, Y410, NV12, NV21, GRAY8, GRAY16_BE, GRAY16_LE, v308, RGB16, BGR16, RGB15, BGR15, UYVP, A420, RGB8P, YUV9, YVU9, IYU1, ARGB64, AYUV64, r210, I420_10BE, I420_10LE, I422_10BE, I422_10LE, Y444_10BE, Y444_10LE, GBR, GBR_10BE, GBR_10LE, NV16, NV24, NV12_64Z32, A420_10BE, A420_10LE, A422_10BE, A422_10LE, A444_10BE, A444_10LE, NV61, P010_10BE, P010_10LE, IYU2, VYUY, GBRA, GBRA_10BE, GBRA_10LE, BGR10A2_LE, GBR_12BE, GBR_12LE, GBRA_12BE, GBRA_12LE, I420_12BE, I420_12LE, I422_12BE, I422_12LE, Y444_12BE, Y444_12LE, GRAY10_LE32, NV12_10LE32, NV16_10LE32, NV12_10LE40 }, width=(int)[ 1, 2147483647 ], height=(int)[ 1, 2147483647 ], framerate=(fraction)[ 0/1, 2147483647/1 ]

name | src
direction | source
presence | always
details | video/x-raw, format=(string){ I420, YV12, YUY2, UYVY, AYUV, VUYA, RGBx, BGRx, xRGB, xBGR, RGBA, BGRA, ARGB, ABGR, RGB, BGR, Y41B, Y42B, YVYU, Y444, v210, v216, Y210, Y410, NV12, NV21, GRAY8, GRAY16_BE, GRAY16_LE, v308, RGB16, BGR16, RGB15, BGR15, UYVP, A420, RGB8P, YUV9, YVU9, IYU1, ARGB64, AYUV64, r210, I420_10BE, I420_10LE, I422_10BE, I422_10LE, Y444_10BE, Y444_10LE, GBR, GBR_10BE, GBR_10LE, NV16, NV24, NV12_64Z32, A420_10BE, A420_10LE, A422_10BE, A422_10LE, A444_10BE, A444_10LE, NV61, P010_10BE, P010_10LE, IYU2, VYUY, GBRA, GBRA_10BE, GBRA_10LE, BGR10A2_LE, GBR_12BE, GBR_12LE, GBRA_12BE, GBRA_12LE, I420_12BE, I420_12LE, I422_12BE, I422_12LE, Y444_12BE, Y444_12LE, GRAY10_LE32, NV12_10LE32, NV16_10LE32, NV12_10LE40 }, width=(int)[ 1, 2147483647 ], height=(int)[ 1, 2147483647 ], framerate=(fraction)[ 0/1, 2147483647/1 ]

## Functions

## Types and Values

### struct GstRawAudioParse

    struct GstRawAudioParse;

## Property Details

### The `“channel-positions”` property

      “channel-positions”        GValueArray *

Channel positions used on the output.

Flags: Read / Write

### The `“format”` property

      “format”                   GstRawAudioParseFormat

Format of the raw audio stream.

Flags: Read / Write

Default value: PCM

### The `“interleaved”` property

      “interleaved”              gboolean

True if audio has interleaved layout.

Flags: Read / Write

Default value: TRUE

### The `“num-channels”` property

      “num-channels”             gint

Number of channels in raw stream.

Flags: Read / Write

Allowed values: >= 1

Default value: 2

### The `“pcm-format”` property

      “pcm-format”               GstAudioFormat

Format of audio samples in PCM stream (ignored if format property is not set to pcm).

Flags: Read / Write

Default value: GST_AUDIO_FORMAT_UNKNOWN

### The `“sample-rate”` property

      “sample-rate”              gint

Rate of audio samples in raw stream.

Flags: Read / Write

Allowed values: >= 1

Default value: 44100