## GstPad GstPad — Object contained by elements that allows links to other elements |

## Functions

const gchar * | gst_pad_link_get_name ()
#define | GST_PAD_LINK_FAILED()
#define | GST_PAD_LINK_SUCCESSFUL()
const gchar * | gst_flow_get_name ()
GQuark | gst_flow_to_quark ()
const gchar * | gst_pad_mode_get_name ()
GstFlowReturn | gst_pad_store_sticky_event ()
#define | gst_pad_get_name()
GstPadDirection | gst_pad_get_direction ()
#define | gst_pad_get_parent()
GstElement * | gst_pad_get_parent_element ()
GstPadTemplate * | gst_pad_get_pad_template ()
GstPadLinkReturn | gst_pad_link ()
GstPadLinkReturn | gst_pad_link_full ()
gboolean | gst_pad_link_maybe_ghosting ()
gboolean | gst_pad_link_maybe_ghosting_full ()
gboolean | gst_pad_unlink ()
gboolean | gst_pad_is_linked ()
gboolean | gst_pad_can_link ()
GstCaps * | gst_pad_get_allowed_caps ()
GstCaps * | gst_pad_get_current_caps ()
GstCaps * | gst_pad_get_pad_template_caps ()
GstPad * | gst_pad_get_peer ()
void | gst_pad_use_fixed_caps ()
gboolean | gst_pad_has_current_caps ()
GstEvent * | gst_pad_get_sticky_event ()
gboolean | (*GstPadStickyEventsForeachFunction) ()
void | gst_pad_sticky_events_foreach ()
gboolean | gst_pad_is_active ()
GstFlowReturn | gst_pad_get_last_flow_return ()
#define | GST_PAD_PROBE_INFO_TYPE()
#define | GST_PAD_PROBE_INFO_ID()
#define | GST_PAD_PROBE_INFO_DATA()
#define | GST_PAD_PROBE_INFO_BUFFER()
#define | GST_PAD_PROBE_INFO_BUFFER_LIST()
#define | GST_PAD_PROBE_INFO_EVENT()
#define | GST_PAD_PROBE_INFO_QUERY()
GstBuffer * | gst_pad_probe_info_get_buffer ()
GstBufferList * | gst_pad_probe_info_get_buffer_list ()
GstEvent * | gst_pad_probe_info_get_event ()
GstQuery * | gst_pad_probe_info_get_query ()
#define | GST_PAD_PROBE_INFO_OFFSET()
#define | GST_PAD_PROBE_INFO_SIZE()
#define | GST_PAD_PROBE_INFO_FLOW_RETURN()
GstPadProbeReturn | (*GstPadProbeCallback) ()
gulong | gst_pad_add_probe ()
void | gst_pad_remove_probe ()
gboolean | gst_pad_is_blocked ()
gboolean | gst_pad_is_blocking ()
gint64 | gst_pad_get_offset ()
void | gst_pad_set_offset ()
GstPad * | gst_pad_new ()
GstPad * | gst_pad_new_from_template ()
GstPad * | gst_pad_new_from_static_template ()
#define | gst_pad_set_chain_function()
void | gst_pad_set_chain_function_full ()
GstFlowReturn | (*GstPadChainFunction) ()
#define | gst_pad_set_chain_list_function()
void | gst_pad_set_chain_list_function_full ()
GstFlowReturn | (*GstPadChainListFunction) ()
GstFlowReturn | gst_pad_get_range ()
#define | gst_pad_set_getrange_function()
void | gst_pad_set_getrange_function_full ()
GstFlowReturn | (*GstPadGetRangeFunction) ()
#define | gst_pad_set_event_function()
void | gst_pad_set_event_function_full ()
gboolean | (*GstPadEventFunction) ()
#define | gst_pad_set_event_full_function()
void | gst_pad_set_event_full_function_full ()
GstFlowReturn | (*GstPadEventFullFunction) ()
#define | gst_pad_set_link_function()
void | gst_pad_set_link_function_full ()
GstPadLinkReturn | (*GstPadLinkFunction) ()
#define | gst_pad_set_unlink_function()
void | gst_pad_set_unlink_function_full ()
void | (*GstPadUnlinkFunction) ()
gboolean | gst_pad_proxy_query_caps ()
gboolean | gst_pad_proxy_query_accept_caps ()
#define | gst_pad_set_activate_function()
void | gst_pad_set_activate_function_full ()
gboolean | (*GstPadActivateFunction) ()
#define | gst_pad_set_activatemode_function()
void | gst_pad_set_activatemode_function_full ()
gboolean | (*GstPadActivateModeFunction) ()
gboolean | gst_pad_needs_reconfigure ()
gboolean | gst_pad_check_reconfigure ()
void | gst_pad_mark_reconfigure ()
GstFlowReturn | gst_pad_push ()
gboolean | gst_pad_push_event ()
GstFlowReturn | gst_pad_push_list ()
GstFlowReturn | gst_pad_pull_range ()
gboolean | gst_pad_activate_mode ()
gboolean | gst_pad_send_event ()
gboolean | gst_pad_event_default ()
gboolean | gst_pad_query ()
gboolean | gst_pad_peer_query ()
gboolean | gst_pad_query_default ()
gboolean | gst_pad_query_position ()
gboolean | gst_pad_query_duration ()
gboolean | gst_pad_query_convert ()
gboolean | gst_pad_query_accept_caps ()
GstCaps * | gst_pad_query_caps ()
gboolean | gst_pad_peer_query_position ()
gboolean | gst_pad_peer_query_duration ()
gboolean | gst_pad_peer_query_convert ()
gboolean | gst_pad_peer_query_accept_caps ()
GstCaps * | gst_pad_peer_query_caps ()
#define | gst_pad_set_query_function()
void | gst_pad_set_query_function_full ()
gboolean | (*GstPadQueryFunction) ()
#define | gst_pad_set_iterate_internal_links_function()
void | gst_pad_set_iterate_internal_links_function_full ()
GstIterator * | (*GstPadIterIntLinkFunction) ()
GstIterator * | gst_pad_iterate_internal_links ()
GstIterator * | gst_pad_iterate_internal_links_default ()
void | gst_pad_set_element_private ()
gpointer | gst_pad_get_element_private ()
gchar * | gst_pad_create_stream_id ()
gchar * | gst_pad_create_stream_id_printf ()
gchar * | gst_pad_create_stream_id_printf_valist ()
gchar * | gst_pad_get_stream_id ()
GstStream * | gst_pad_get_stream ()
gboolean | (*GstPadForwardFunction) ()
gboolean | gst_pad_forward ()
GstFlowReturn | gst_pad_chain ()
GstFlowReturn | gst_pad_chain_list ()
gboolean | gst_pad_start_task ()
gboolean | gst_pad_pause_task ()
gboolean | gst_pad_stop_task ()
GstTaskState | gst_pad_get_task_state ()
gboolean | gst_pad_set_active ()
#define | GST_PAD_GET_STREAM_LOCK()
#define | GST_PAD_STREAM_LOCK()
#define | GST_PAD_STREAM_TRYLOCK()
#define | GST_PAD_STREAM_UNLOCK()
#define | GST_PAD_NAME()
#define | GST_PAD_PARENT()
#define | GST_PAD_ELEMENT_PRIVATE()
#define | GST_PAD_PAD_TEMPLATE()
#define | GST_PAD_DIRECTION()
#define | GST_PAD_LAST_FLOW_RETURN()
#define | GST_PAD_TASK()
#define | GST_PAD_MODE()
#define | GST_PAD_ACTIVATEFUNC()
#define | GST_PAD_ACTIVATEMODEFUNC()
#define | GST_PAD_CHAINFUNC()
#define | GST_PAD_CHAINLISTFUNC()
#define | GST_PAD_EVENTFUNC()
#define | GST_PAD_EVENTFULLFUNC()
#define | GST_PAD_GETRANGEFUNC()
#define | GST_PAD_QUERYFUNC()
#define | GST_PAD_ITERINTLINKFUNC()
#define | GST_PAD_PEER()
#define | GST_PAD_LINKFUNC()
#define | GST_PAD_UNLINKFUNC()
#define | GST_PAD_IS_LINKED()
#define | GST_PAD_IS_SRC()
#define | GST_PAD_IS_SINK()
#define | GST_PAD_IS_ACTIVE()
#define | GST_PAD_IS_BLOCKED()
#define | GST_PAD_IS_BLOCKING()
#define | GST_PAD_IS_FLUSHING()
#define | GST_PAD_SET_FLUSHING()
#define | GST_PAD_UNSET_FLUSHING()
#define | GST_PAD_IS_EOS()
#define | GST_PAD_NEEDS_RECONFIGURE()
#define | GST_PAD_HAS_PENDING_EVENTS()
#define | GST_PAD_IS_FIXED_CAPS()
#define | GST_PAD_NEEDS_PARENT()
#define | GST_PAD_IS_PROXY_CAPS()
#define | GST_PAD_SET_PROXY_CAPS()
#define | GST_PAD_UNSET_PROXY_CAPS()
#define | GST_PAD_IS_PROXY_ALLOCATION()
#define | GST_PAD_SET_PROXY_ALLOCATION()
#define | GST_PAD_UNSET_PROXY_ALLOCATION()
#define | GST_PAD_SET_PROXY_SCHEDULING()
#define | GST_PAD_UNSET_PROXY_SCHEDULING()
#define | GST_PAD_IS_PROXY_SCHEDULING()
#define | GST_PAD_IS_ACCEPT_INTERSECT()
#define | GST_PAD_SET_ACCEPT_INTERSECT()
#define | GST_PAD_UNSET_ACCEPT_INTERSECT()
#define | GST_PAD_IS_ACCEPT_TEMPLATE()
#define | GST_PAD_SET_ACCEPT_TEMPLATE()
#define | GST_PAD_UNSET_ACCEPT_TEMPLATE()

## Properties

GstCaps * | caps | Read
GstPadDirection | direction | Read / Write / Construct Only
gint64 | offset | Read / Write
GstPadTemplate * | template | Read / Write

## Signals

void | linked | Run Last
void | unlinked | Run Last

## Types and Values

struct | GstPad
enum | GstPadDirection
enum | GstPadFlags
enum | GstPadLinkReturn
enum | GstPadLinkCheck
enum | GstFlowReturn
enum | GstPadMode
enum | GstPadProbeReturn
enum | GstPadProbeType
struct | GstPadProbeInfo

## Object Hierarchy

        GObject
        ╰── GInitiallyUnowned
            ╰── GstObject
                ╰── GstPad
                    ╰── GstProxyPad

## Includes

    #include <gst/gst.h>

## Description

A GstElement is linked to other elements via "pads", which are extremely light-weight generic link points.

Pads have a GstPadDirection, source pads produce data, sink pads consume data.

Pads are typically created from a GstPadTemplate with `gst_pad_new_from_template()` and are then added to a GstElement. This usually happens when the element is created but it can also happen dynamically based on the data that the element is processing or based on the pads that the application requests.

Pads without pad templates can be created with `gst_pad_new()`, which takes a direction and a name as an argument. If the name is `NULL`, then a guaranteed unique name will be assigned to it.

A GstElement creating a pad will typically use the various gst_pad_set_*_function() calls to register callbacks for events, queries or dataflow on the pads.

gst_pad_get_parent() will retrieve the GstElement that owns the pad.

After two pads are retrieved from an element by `gst_element_get_static_pad()`, the pads can be linked with `gst_pad_link()`. (For quick links, you can also use `gst_element_link()`, which will make the obvious link for you if it's straightforward.). Pads can be unlinked again with `gst_pad_unlink()`. `gst_pad_get_peer()` can be used to check what the pad is linked to.

Before dataflow is possible on the pads, they need to be activated with `gst_pad_set_active()`.

gst_pad_query() and `gst_pad_peer_query()` can be used to query various properties of the pad and the stream.

To send a GstEvent on a pad, use `gst_pad_send_event()` and `gst_pad_push_event()`. Some events will be sticky on the pad, meaning that after they pass on the pad they can be queried later with `gst_pad_get_sticky_event()` and `gst_pad_sticky_events_foreach()`. `gst_pad_get_current_caps()` and `gst_pad_has_current_caps()` are convenience functions to query the current sticky CAPS event on a pad.

GstElements will use `gst_pad_push()` and `gst_pad_pull_range()` to push out or pull in a buffer.

The dataflow, events and queries that happen on a pad can be monitored with probes that can be installed with `gst_pad_add_probe()`. `gst_pad_is_blocked()` can be used to check if a block probe is installed on the pad. `gst_pad_is_blocking()` checks if the blocking probe is currently blocking the pad. `gst_pad_remove_probe()` is used to remove a previously installed probe and unblock blocking probes if any.

Pad have an offset that can be retrieved with `gst_pad_get_offset()`. This offset will be applied to the running_time of all data passing over the pad. `gst_pad_set_offset()` can be used to change the offset.

Convenience functions exist to start, pause and stop the task on a pad with `gst_pad_start_task()`, `gst_pad_pause_task()` and `gst_pad_stop_task()` respectively.

## Functions

### gst_pad_link_get_name ()

    const gchar *
    gst_pad_link_get_name (GstPadLinkReturn ret);

Gets a string representing the given pad-link return.

#### Parameters

ret | a GstPadLinkReturn to get the name of. |

#### Returns

a static string with the name of the pad-link return.

Since: 1.4

### GST_PAD_LINK_FAILED()

    #define GST_PAD_LINK_FAILED(ret) ((ret) < GST_PAD_LINK_OK)

Macro to test if the given GstPadLinkReturn value indicates a failed link step.

#### Parameters

ret | the GstPadLinkReturn value |

### GST_PAD_LINK_SUCCESSFUL()

    #define GST_PAD_LINK_SUCCESSFUL(ret) ((ret) >= GST_PAD_LINK_OK)

Macro to test if the given GstPadLinkReturn value indicates a successful link step.

#### Parameters

ret | the GstPadLinkReturn value |

### gst_flow_get_name ()

    const gchar *
    gst_flow_get_name (GstFlowReturn ret);

Gets a string representing the given flow return.

#### Parameters

ret | a GstFlowReturn to get the name of. |

#### Returns

a static string with the name of the flow return.

### gst_flow_to_quark ()

    GQuark
    gst_flow_to_quark (GstFlowReturn ret);

Get the unique quark for the given GstFlowReturn.

#### Parameters

ret | a GstFlowReturn to get the quark of. |

#### Returns

the quark associated with the flow return or 0 if an invalid return was specified.

### gst_pad_mode_get_name ()

    const gchar *
    gst_pad_mode_get_name (GstPadMode mode);

Return the name of a pad mode, for use in debug messages mostly.

#### Parameters

mode | the pad mode |

#### Returns

short mnemonic for pad mode `mode`

### gst_pad_store_sticky_event ()

    GstFlowReturn
    gst_pad_store_sticky_event (GstPad *pad,
                                GstEvent *event);

Store the sticky `event` on `pad`

#### Parameters

pad | a GstPad |
event | a GstEvent. | [transfer none]

#### Returns

GST_FLOW_OK on success, GST_FLOW_FLUSHING when the pad was flushing or GST_FLOW_EOS when the pad was EOS.

Since: 1.2

### gst_pad_get_name()

    #define gst_pad_get_name(pad) gst_object_get_name (GST_OBJECT_CAST (pad))

Get a copy of the name of the pad. `g_free()` after usage.

MT safe.

#### Parameters

pad | the pad to get the name from |

### gst_pad_get_direction ()

    GstPadDirection
    gst_pad_get_direction (GstPad *pad);

Gets the direction of the pad. The direction of the pad is decided at construction time so this function does not take the LOCK.

#### Parameters

pad | a GstPad to get the direction of. |

#### Returns

the GstPadDirection of the pad.

MT safe.

### gst_pad_get_parent()

    #define gst_pad_get_parent(pad) gst_object_get_parent (GST_OBJECT_CAST (pad))

Get the parent of `pad` . This function increases the refcount of the parent object so you should `gst_object_unref()` it after usage. Can return `NULL` if the pad did not have a parent.

MT safe.

#### Parameters

pad | the pad to get the parent of |

#### Returns

the parent.

[nullable]

### gst_pad_get_parent_element ()

    GstElement *
    gst_pad_get_parent_element (GstPad *pad);

Gets the parent of `pad` , cast to a GstElement. If a `pad` has no parent or its parent is not an element, return `NULL`.

#### Parameters

pad | a pad |

#### Returns

the parent of the pad. The caller has a reference on the parent, so unref when you're finished with it.

MT safe.

[transfer full][nullable]

### gst_pad_get_pad_template ()

    GstPadTemplate *
    gst_pad_get_pad_template (GstPad *pad);

Gets the template for `pad` .

#### Parameters

pad | a GstPad. |

#### Returns

the GstPadTemplate from which this pad was instantiated, or `NULL` if this pad has no template. Unref after usage.

[transfer full][nullable]

### gst_pad_link ()

    GstPadLinkReturn
    gst_pad_link (GstPad *srcpad,
                  GstPad *sinkpad);

Links the source pad and the sink pad.

#### Parameters

srcpad | the source GstPad to link. |
sinkpad | the sink GstPad to link. |

#### Returns

A result code indicating if the connection worked or what went wrong.

MT Safe.

### gst_pad_link_full ()

    GstPadLinkReturn
    gst_pad_link_full (GstPad *srcpad,
                       GstPad *sinkpad,
                       GstPadLinkCheck flags);

Links the source pad and the sink pad.

This variant of gst_pad_link provides a more granular control on the checks being done when linking. While providing some considerable speedups the caller of this method must be aware that wrong usage of those flags can cause severe issues. Refer to the documentation of GstPadLinkCheck for more information.

MT Safe.

#### Parameters

srcpad | the source GstPad to link. |
sinkpad | the sink GstPad to link. |
flags | the checks to validate when linking |

#### Returns

A result code indicating if the connection worked or what went wrong.

### gst_pad_link_maybe_ghosting ()

    gboolean
    gst_pad_link_maybe_ghosting (GstPad *src,
                                 GstPad *sink);

Links `src` to `sink` , creating any GstGhostPad's in between as necessary.

This is a convenience function to save having to create and add intermediate GstGhostPad's as required for linking across GstBin boundaries.

If `src` or `sink` pads don't have parent elements or do not share a common ancestor, the link will fail.

#### Parameters

src | a GstPad |
sink | a GstPad |

#### Returns

whether the link succeeded.

Since: 1.10

### gst_pad_link_maybe_ghosting_full ()

    gboolean
    gst_pad_link_maybe_ghosting_full (GstPad *src,
                                      GstPad *sink,
                                      GstPadLinkCheck flags);

Links `src` to `sink` , creating any GstGhostPad's in between as necessary.

This is a convenience function to save having to create and add intermediate GstGhostPad's as required for linking across GstBin boundaries.

If `src` or `sink` pads don't have parent elements or do not share a common ancestor, the link will fail.

Calling `gst_pad_link_maybe_ghosting_full()` with `flags` == `GST_PAD_LINK_CHECK_DEFAULT` is the recommended way of linking pads with safety checks applied.

#### Parameters

src | a GstPad |
sink | a GstPad |
flags | some GstPadLinkCheck flags |

#### Returns

whether the link succeeded.

Since: 1.10

### gst_pad_unlink ()

    gboolean
    gst_pad_unlink (GstPad *srcpad,
                    GstPad *sinkpad);

Unlinks the source pad from the sink pad. Will emit the “unlinked” signal on both pads.

#### Parameters

srcpad | the source GstPad to unlink. |
sinkpad | the sink GstPad to unlink. |

#### Returns

`TRUE` if the pads were unlinked. This function returns `FALSE` if the pads were not linked together.

MT safe.

### gst_pad_is_linked ()

    gboolean
    gst_pad_is_linked (GstPad *pad);

Checks if a `pad` is linked to another pad or not.

#### Parameters

pad | pad to check |

#### Returns

`TRUE` if the pad is linked, `FALSE` otherwise.

MT safe.

### gst_pad_can_link ()

    gboolean
    gst_pad_can_link (GstPad *srcpad,
                      GstPad *sinkpad);

Checks if the source pad and the sink pad are compatible so they can be linked.

#### Parameters

srcpad | the source GstPad. |
sinkpad | the sink GstPad. |

#### Returns

`TRUE` if the pads can be linked.

### gst_pad_get_allowed_caps ()

    GstCaps *
    gst_pad_get_allowed_caps (GstPad *pad);

Gets the capabilities of the allowed media types that can flow through `pad` and its peer.

The allowed capabilities is calculated as the intersection of the results of calling `gst_pad_query_caps()` on `pad` and its peer. The caller owns a reference on the resulting caps.

#### Parameters

pad | a GstPad. |

#### Returns

the allowed GstCaps of the pad link. Unref the caps when you no longer need it. This function returns `NULL` when `pad` has no peer.

MT safe.

[transfer full][nullable]

### gst_pad_get_current_caps ()

    GstCaps *
    gst_pad_get_current_caps (GstPad *pad);

Gets the capabilities currently configured on `pad` with the last GST_EVENT_CAPS event.

#### Parameters

pad | a GstPad to get the current capabilities of. |

#### Returns

the current caps of the pad with incremented ref-count or `NULL` when pad has no caps. Unref after usage.

[transfer full][nullable]

### gst_pad_get_pad_template_caps ()

    GstCaps *
    gst_pad_get_pad_template_caps (GstPad *pad);

Gets the capabilities for `pad` 's template.

#### Parameters

pad | a GstPad to get the template capabilities from. |

#### Returns

the GstCaps of this pad template. Unref after usage.

[transfer full]

### gst_pad_get_peer ()

    GstPad *
    gst_pad_get_peer (GstPad *pad);

Gets the peer of `pad` . This function refs the peer pad so you need to unref it after use.

#### Parameters

pad | a GstPad to get the peer of. |

#### Returns

the peer GstPad. Unref after usage.

MT safe.

[transfer full][nullable]

### gst_pad_use_fixed_caps ()

    void
    gst_pad_use_fixed_caps (GstPad *pad);

A helper function you can use that sets the FIXED_CAPS flag This way the default CAPS query will always return the negotiated caps or in case the pad is not negotiated, the padtemplate caps.

The negotiated caps are the caps of the last CAPS event that passed on the pad. Use this function on a pad that, once it negotiated to a CAPS, cannot be renegotiated to something else.

#### Parameters

pad | the pad to use |

### gst_pad_has_current_caps ()

    gboolean
    gst_pad_has_current_caps (GstPad *pad);

Check if `pad` has caps set on it with a GST_EVENT_CAPS event.

#### Parameters

pad | a GstPad to check |

#### Returns

`TRUE` when `pad` has caps associated with it.

### gst_pad_get_sticky_event ()

    GstEvent *
    gst_pad_get_sticky_event (GstPad *pad,
                              GstEventType event_type,
                              guint idx);

Returns a new reference of the sticky event of type `event_type` from the event.

#### Parameters

pad | the GstPad to get the event from. |
event_type | the GstEventType that should be retrieved. |
idx | the index of the event |

#### Returns

a GstEvent of type `event_type` or `NULL` when no event of `event_type` was on `pad` . Unref after usage.

[transfer full][nullable]

### GstPadStickyEventsForeachFunction ()

    gboolean
    (*GstPadStickyEventsForeachFunction) (GstPad *pad,
                                          GstEvent **event,
                                          gpointer user_data);

Callback used by `gst_pad_sticky_events_foreach()`.

When this function returns `TRUE`, the next event will be returned. When `FALSE` is returned, `gst_pad_sticky_events_foreach()` will return.

When `event` is set to `NULL`, the item will be removed from the list of sticky events. `event` can be replaced by assigning a new reference to it. This function is responsible for unreffing the old event when removing or modifying.

#### Parameters

pad | the GstPad. |
event | a sticky GstEvent. | [allow-none]
user_data | the gpointer to optional user data. |

#### Returns

`TRUE` if the iteration should continue

### gst_pad_sticky_events_foreach ()

    void
    gst_pad_sticky_events_foreach (GstPad *pad,
                                   GstPadStickyEventsForeachFunction foreach_func,
                                   gpointer user_data);

Iterates all sticky events on `pad` and calls `foreach_func` for every event. If `foreach_func` returns `FALSE` the iteration is immediately stopped.

#### Parameters

pad | the GstPad that should be used for iteration. |
foreach_func | the GstPadStickyEventsForeachFunction that should be called for every event. | [scope call]
user_data | the optional user data. | [closure]

### gst_pad_is_active ()

    gboolean
    gst_pad_is_active (GstPad *pad);

Query if a pad is active

#### Parameters

pad | the GstPad to query |

#### Returns

`TRUE` if the pad is active.

MT safe.

### gst_pad_get_last_flow_return ()

    GstFlowReturn
    gst_pad_get_last_flow_return (GstPad *pad);

Gets the GstFlowReturn return from the last data passed by this pad.

#### Parameters

pad | the GstPad |

Since: 1.4

### GST_PAD_PROBE_INFO_TYPE()

    #define GST_PAD_PROBE_INFO_TYPE(d)         ((d)->type)

### GST_PAD_PROBE_INFO_ID()

    #define GST_PAD_PROBE_INFO_ID(d)           ((d)->id)

### GST_PAD_PROBE_INFO_DATA()

    #define GST_PAD_PROBE_INFO_DATA(d)         ((d)->data)

### GST_PAD_PROBE_INFO_BUFFER()

    #define GST_PAD_PROBE_INFO_BUFFER(d)       GST_BUFFER_CAST(GST_PAD_PROBE_INFO_DATA(d))

### GST_PAD_PROBE_INFO_BUFFER_LIST()

    #define GST_PAD_PROBE_INFO_BUFFER_LIST(d)  GST_BUFFER_LIST_CAST(GST_PAD_PROBE_INFO_DATA(d))

### GST_PAD_PROBE_INFO_EVENT()

    #define GST_PAD_PROBE_INFO_EVENT(d)        GST_EVENT_CAST(GST_PAD_PROBE_INFO_DATA(d))

### GST_PAD_PROBE_INFO_QUERY()

    #define GST_PAD_PROBE_INFO_QUERY(d)        GST_QUERY_CAST(GST_PAD_PROBE_INFO_DATA(d))

### gst_pad_probe_info_get_buffer ()

    GstBuffer *
    gst_pad_probe_info_get_buffer (GstPadProbeInfo *info);

#### Parameters

info | a GstPadProbeInfo |

#### Returns

The GstBuffer from the probe.

[transfer none][nullable]

### gst_pad_probe_info_get_buffer_list ()

    GstBufferList *
    gst_pad_probe_info_get_buffer_list (GstPadProbeInfo *info);

#### Parameters

info | a GstPadProbeInfo |

#### Returns

The GstBufferList from the probe.

[transfer none][nullable]

### gst_pad_probe_info_get_event ()

    GstEvent *
    gst_pad_probe_info_get_event (GstPadProbeInfo *info);

#### Parameters

info | a GstPadProbeInfo |

#### Returns

The GstEvent from the probe.

[transfer none][nullable]

### gst_pad_probe_info_get_query ()

    GstQuery *
    gst_pad_probe_info_get_query (GstPadProbeInfo *info);

#### Parameters

info | a GstPadProbeInfo |

#### Returns

The GstQuery from the probe.

[transfer none][nullable]

### GST_PAD_PROBE_INFO_OFFSET()

    #define GST_PAD_PROBE_INFO_OFFSET(d)       ((d)->offset)

### GST_PAD_PROBE_INFO_SIZE()

    #define GST_PAD_PROBE_INFO_SIZE(d)         ((d)->size)

### GST_PAD_PROBE_INFO_FLOW_RETURN()

    #define GST_PAD_PROBE_INFO_FLOW_RETURN(d)  ((d)->ABI.abi.flow_ret)

### GstPadProbeCallback ()

    GstPadProbeReturn
    (*GstPadProbeCallback) (GstPad *pad,
                            GstPadProbeInfo *info,
                            gpointer user_data);

Callback used by `gst_pad_add_probe()`. Gets called to notify about the current blocking type.

The callback is allowed to modify the data pointer in `info` .

#### Parameters

pad | the GstPad that is blocked |
info | GstPadProbeInfo |
user_data | the gpointer to optional user data. |

#### Returns

a GstPadProbeReturn

### gst_pad_add_probe ()

    gulong
    gst_pad_add_probe (GstPad *pad,
                       GstPadProbeType mask,
                       GstPadProbeCallback callback,
                       gpointer user_data,
                       GDestroyNotify destroy_data);

Be notified of different states of pads. The provided callback is called for every state that matches `mask` .

Probes are called in groups: First GST_PAD_PROBE_TYPE_BLOCK probes are called, then others, then finally GST_PAD_PROBE_TYPE_IDLE. The only exception here are GST_PAD_PROBE_TYPE_IDLE probes that are called immediately if the pad is already idle while calling `gst_pad_add_probe()`. In each of the groups, probes are called in the order in which they were added.

#### Parameters

pad | the GstPad to add the probe to |
mask | the probe mask |
callback | GstPadProbeCallback that will be called with notifications of the pad state |
user_data | user data passed to the callback. | [closure]
destroy_data | GDestroyNotify for user_data |

#### Returns

an id or 0 if no probe is pending. The id can be used to remove the probe with `gst_pad_remove_probe()`. When using GST_PAD_PROBE_TYPE_IDLE it can happen that the probe can be run immediately and if the probe returns GST_PAD_PROBE_REMOVE this functions returns 0.

MT safe.

### gst_pad_remove_probe ()

    void
    gst_pad_remove_probe (GstPad *pad,
                          gulong id);

Remove the probe with `id` from `pad` .

MT safe.

#### Parameters

pad | the GstPad with the probe |
id | the probe id to remove |

### gst_pad_is_blocked ()

    gboolean
    gst_pad_is_blocked (GstPad *pad);

Checks if the pad is blocked or not. This function returns the last requested state of the pad. It is not certain that the pad is actually blocking at this point (see `gst_pad_is_blocking()`).

#### Parameters

pad | the GstPad to query |

#### Returns

`TRUE` if the pad is blocked.

MT safe.

### gst_pad_is_blocking ()

    gboolean
    gst_pad_is_blocking (GstPad *pad);

Checks if the pad is blocking or not. This is a guaranteed state of whether the pad is actually blocking on a GstBuffer or a GstEvent.

#### Parameters

pad | the GstPad to query |

#### Returns

`TRUE` if the pad is blocking.

MT safe.

### gst_pad_get_offset ()

    gint64
    gst_pad_get_offset (GstPad *pad);

Get the offset applied to the running time of `pad` . `pad` has to be a source pad.

#### Parameters

pad | a GstPad |

#### Returns

the offset.

### gst_pad_set_offset ()

    void
    gst_pad_set_offset (GstPad *pad,
                        gint64 offset);

Set the offset that will be applied to the running time of `pad` .

#### Parameters

pad | a GstPad |
offset | the offset |

### gst_pad_new ()

    GstPad *
    gst_pad_new (const gchar *name,
                 GstPadDirection direction);

Creates a new pad with the given name in the given direction. If name is `NULL`, a guaranteed unique name (across all pads) will be assigned. This function makes a copy of the name so you can safely free the name.

#### Parameters

name | the name of the new pad. | [allow-none]
direction | the GstPadDirection of the pad. |

#### Returns

a new GstPad.

MT safe.

[transfer floating]

### gst_pad_new_from_template ()

    GstPad *
    gst_pad_new_from_template (GstPadTemplate *templ,
                               const gchar *name);

Creates a new pad with the given name from the given template. If name is `NULL`, a guaranteed unique name (across all pads) will be assigned. This function makes a copy of the name so you can safely free the name.

#### Parameters

templ | the pad template to use |
name | the name of the pad. | [allow-none]

#### Returns

a new GstPad.

[transfer floating]

### gst_pad_new_from_static_template ()

    GstPad *
    gst_pad_new_from_static_template (GstStaticPadTemplate *templ,
                                      const gchar *name);

Creates a new pad with the given name from the given static template. If name is `NULL`, a guaranteed unique name (across all pads) will be assigned. This function makes a copy of the name so you can safely free the name.

#### Parameters

templ | the GstStaticPadTemplate to use |
name | the name of the pad |

#### Returns

a new GstPad.

[transfer floating]

### gst_pad_set_chain_function()

    #define gst_pad_set_chain_function(p,f)         gst_pad_set_chain_function_full((p),(f),NULL,NULL)

Calls `gst_pad_set_chain_function_full()` with `NULL` for the user_data and notify.

#### Parameters

p | a sink GstPad. |
f | the GstPadChainFunction to set. |

### gst_pad_set_chain_function_full ()

    void
    gst_pad_set_chain_function_full (GstPad *pad,
                                     GstPadChainFunction chain,
                                     gpointer user_data,
                                     GDestroyNotify notify);

Sets the given chain function for the pad. The chain function is called to process a GstBuffer input buffer. see GstPadChainFunction for more details.

#### Parameters

pad | a sink GstPad. |
chain | the GstPadChainFunction to set. |
user_data | user_data passed to `notify` |
notify | notify called when `chain` will not be used anymore. |

### GstPadChainFunction ()

    GstFlowReturn
    (*GstPadChainFunction) (GstPad *pad,
                            GstObject *parent,
                            GstBuffer *buffer);

A function that will be called on sinkpads when chaining buffers. The function typically processes the data contained in the buffer and either consumes the data or passes it on to the internally linked pad(s).

The implementer of this function receives a refcount to `buffer` and should `gst_buffer_unref()` when the buffer is no longer needed.

When a chain function detects an error in the data stream, it must post an error on the bus and return an appropriate GstFlowReturn value.

#### Parameters

pad | the sink GstPad that performed the chain. |
parent | the parent of `pad` . If the GST_PAD_FLAG_NEED_PARENT flag is set, `parent` is guaranteed to be not-`NULL` and remain valid during the execution of this function. | [allow-none]
buffer | the GstBuffer that is chained, not `NULL`. | [transfer full]

#### Returns

GST_FLOW_OK for success

### gst_pad_set_chain_list_function()

    #define gst_pad_set_chain_list_function(p,f)    gst_pad_set_chain_list_function_full((p),(f),NULL,NULL)

Calls `gst_pad_set_chain_list_function_full()` with `NULL` for the user_data and notify.

#### Parameters

p | a sink GstPad. |
f | the GstPadChainListFunction to set. |

### gst_pad_set_chain_list_function_full ()

    void
    gst_pad_set_chain_list_function_full (GstPad *pad,
                                          GstPadChainListFunction chainlist,
                                          gpointer user_data,
                                          GDestroyNotify notify);

Sets the given chain list function for the pad. The chainlist function is called to process a GstBufferList input buffer list. See GstPadChainListFunction for more details.

#### Parameters

pad | a sink GstPad. |
chainlist | the GstPadChainListFunction to set. |
user_data | user_data passed to `notify` |
notify | notify called when `chainlist` will not be used anymore. |

### GstPadChainListFunction ()

    GstFlowReturn
    (*GstPadChainListFunction) (GstPad *pad,
                                GstObject *parent,
                                GstBufferList *list);

A function that will be called on sinkpads when chaining buffer lists. The function typically processes the data contained in the buffer list and either consumes the data or passes it on to the internally linked pad(s).

The implementer of this function receives a refcount to `list` and should `gst_buffer_list_unref()` when the list is no longer needed.

When a chainlist function detects an error in the data stream, it must post an error on the bus and return an appropriate GstFlowReturn value.

#### Parameters

pad | the sink GstPad that performed the chain. |
parent | the parent of `pad` . If the GST_PAD_FLAG_NEED_PARENT flag is set, `parent` is guaranteed to be not-`NULL` and remain valid during the execution of this function. | [allow-none]
list | the GstBufferList that is chained, not `NULL`. | [transfer full]

#### Returns

GST_FLOW_OK for success

### gst_pad_get_range ()

    GstFlowReturn
    gst_pad_get_range (GstPad *pad,
                       guint64 offset,
                       guint size,
                       GstBuffer **buffer);

When `pad` is flushing this function returns GST_FLOW_FLUSHING immediately and `buffer` is `NULL`.

Calls the getrange function of `pad` , see GstPadGetRangeFunction for a description of a getrange function. If `pad` has no getrange function installed (see `gst_pad_set_getrange_function()`) this function returns GST_FLOW_NOT_SUPPORTED.

If `buffer` points to a variable holding `NULL`, a valid new GstBuffer will be placed in `buffer` when this function returns GST_FLOW_OK. The new buffer must be freed with `gst_buffer_unref()` after usage.

When `buffer` points to a variable that points to a valid GstBuffer, the buffer will be filled with the result data when this function returns GST_FLOW_OK. If the provided buffer is larger than `size` , only `size` bytes will be filled in the result buffer and its size will be updated accordingly.

Note that less than `size` bytes can be returned in `buffer` when, for example, an EOS condition is near or when `buffer` is not large enough to hold `size` bytes. The caller should check the result buffer size to get the result size.

When this function returns any other result value than GST_FLOW_OK, `buffer` will be unchanged.

This is a lowlevel function. Usually `gst_pad_pull_range()` is used.

#### Parameters

pad | a src GstPad, returns GST_FLOW_ERROR if not. |
offset | The start offset of the buffer |
size | The length of the buffer |
buffer | a pointer to hold the GstBuffer, returns GST_FLOW_ERROR if `NULL`. | [out callee-allocates]

#### Returns

a GstFlowReturn from the pad.

MT safe.

### gst_pad_set_getrange_function()

    #define gst_pad_set_getrange_function(p,f)      gst_pad_set_getrange_function_full((p),(f),NULL,NULL)

Calls `gst_pad_set_getrange_function_full()` with `NULL` for the user_data and notify.

#### Parameters

p | a source GstPad. |
f | the GstPadGetRangeFunction to set. |

### gst_pad_set_getrange_function_full ()

    void
    gst_pad_set_getrange_function_full (GstPad *pad,
                                        GstPadGetRangeFunction get,
                                        gpointer user_data,
                                        GDestroyNotify notify);

Sets the given getrange function for the pad. The getrange function is called to produce a new GstBuffer to start the processing pipeline. see GstPadGetRangeFunction for a description of the getrange function.

#### Parameters

pad | a source GstPad. |
get | the GstPadGetRangeFunction to set. |
user_data | user_data passed to `notify` |
notify | notify called when `get` will not be used anymore. |

### GstPadGetRangeFunction ()

    GstFlowReturn
    (*GstPadGetRangeFunction) (GstPad *pad,
                               GstObject *parent,
                               guint64 offset,
                               guint length,
                               GstBuffer **buffer);

This function will be called on source pads when a peer element request a buffer at the specified `offset` and `length` . If this function returns GST_FLOW_OK, the result buffer will be stored in `buffer` . The contents of `buffer` is invalid for any other return value.

This function is installed on a source pad with `gst_pad_set_getrange_function()` and can only be called on source pads after they are successfully activated with `gst_pad_activate_mode()` with the GST_PAD_MODE_PULL.

`offset` and `length` are always given in byte units. `offset` must normally be a value between 0 and the length in bytes of the data available on `pad` . The length (duration in bytes) can be retrieved with a GST_QUERY_DURATION or with a GST_QUERY_SEEKING.

Any `offset` larger or equal than the length will make the function return GST_FLOW_EOS, which corresponds to EOS. In this case `buffer` does not contain a valid buffer.

The buffer size of `buffer` will only be smaller than `length` when `offset` is near the end of the stream. In all other cases, the size of `buffer` must be exactly the requested size.

It is allowed to call this function with a 0 `length` and valid `offset` , in which case `buffer` will contain a 0-sized buffer and the function returns GST_FLOW_OK.

When this function is called with a -1 `offset` , the sequentially next buffer of length `length` in the stream is returned.

When this function is called with a -1 `length` , a buffer with a default optimal length is returned in `buffer` . The length might depend on the value of `offset` .

#### Parameters

pad | the src GstPad to perform the getrange on. |
parent | the parent of `pad` . If the GST_PAD_FLAG_NEED_PARENT flag is set, `parent` is guaranteed to be not-`NULL` and remain valid during the execution of this function. | [allow-none]
offset | the offset of the range |
length | the length of the range |
buffer | a memory location to hold the result buffer, cannot be `NULL`. |

#### Returns

GST_FLOW_OK for success and a valid buffer in `buffer` . Any other return value leaves `buffer` undefined.

### gst_pad_set_event_function()

    #define gst_pad_set_event_function(p,f)         gst_pad_set_event_function_full((p),(f),NULL,NULL)

Calls `gst_pad_set_event_function_full()` with `NULL` for the user_data and notify.

#### Parameters

p | a GstPad of either direction. |
f | the GstPadEventFunction to set. |

### gst_pad_set_event_function_full ()

    void
    gst_pad_set_event_function_full (GstPad *pad,
                                     GstPadEventFunction event,
                                     gpointer user_data,
                                     GDestroyNotify notify);

Sets the given event handler for the pad.

#### Parameters

pad | a GstPad of either direction. |
event | the GstPadEventFunction to set. |
user_data | user_data passed to `notify` |
notify | notify called when `event` will not be used anymore. |

### GstPadEventFunction ()

    gboolean
    (*GstPadEventFunction) (GstPad *pad,
                            GstObject *parent,
                            GstEvent *event);

Function signature to handle an event for the pad.

#### Parameters

pad | the GstPad to handle the event. |
parent | the parent of `pad` . If the GST_PAD_FLAG_NEED_PARENT flag is set, `parent` is guaranteed to be not-`NULL` and remain valid during the execution of this function. | [allow-none]
event | the GstEvent to handle. | [transfer full]

#### Returns

`TRUE` if the pad could handle the event.

### gst_pad_set_event_full_function()

    #define gst_pad_set_event_full_function(p,f)    gst_pad_set_event_full_function_full((p),(f),NULL,NULL)

Calls `gst_pad_set_event_full_function_full()` with `NULL` for the user_data and notify.

#### Parameters

p | a GstPad of either direction. |
f | the GstPadEventFullFunction to set. |

### gst_pad_set_event_full_function_full ()

    void
    gst_pad_set_event_full_function_full (GstPad *pad,
                                          GstPadEventFullFunction event,
                                          gpointer user_data,
                                          GDestroyNotify notify);

Sets the given event handler for the pad.

#### Parameters

pad | a GstPad of either direction. |
event | the GstPadEventFullFunction to set. |
user_data | user_data passed to `notify` |
notify | notify called when `event` will not be used anymore. |

Since: 1.8

### GstPadEventFullFunction ()

    GstFlowReturn
    (*GstPadEventFullFunction) (GstPad *pad,
                                GstObject *parent,
                                GstEvent *event);

Function signature to handle an event for the pad.

This variant is for specific elements that will take into account the last downstream flow return (from a pad push), in which case they can return it.

#### Parameters

pad | the GstPad to handle the event. |
parent | the parent of `pad` . If the GST_PAD_FLAG_NEED_PARENT flag is set, `parent` is guaranteed to be not-`NULL` and remain valid during the execution of this function. | [allow-none]
event | the GstEvent to handle. | [transfer full]

#### Returns

`GST_FLOW_OK` if the event was handled properly, or any other GstFlowReturn dependent on downstream state.

Since: 1.8

### gst_pad_set_link_function()

    #define gst_pad_set_link_function(p,f)          gst_pad_set_link_function_full((p),(f),NULL,NULL)

Calls `gst_pad_set_link_function_full()` with `NULL` for the user_data and notify.

#### Parameters

p | a GstPad. |
f | the GstPadLinkFunction to set. |

### gst_pad_set_link_function_full ()

    void
    gst_pad_set_link_function_full (GstPad *pad,
                                    GstPadLinkFunction link,
                                    gpointer user_data,
                                    GDestroyNotify notify);

Sets the given link function for the pad. It will be called when the pad is linked with another pad.

The return value GST_PAD_LINK_OK should be used when the connection can be made.

The return value GST_PAD_LINK_REFUSED should be used when the connection cannot be made for some reason.

If `link` is installed on a source pad, it should call the GstPadLinkFunction of the peer sink pad, if present.

#### Parameters

pad | a GstPad. |
link | the GstPadLinkFunction to set. |
user_data | user_data passed to `notify` |
notify | notify called when `link` will not be used anymore. |

### GstPadLinkFunction ()

    GstPadLinkReturn
    (*GstPadLinkFunction) (GstPad *pad,
                           GstObject *parent,
                           GstPad *peer);

Function signature to handle a new link on the pad.

#### Parameters

pad | the GstPad that is linked. |
parent | the parent of `pad` . If the GST_PAD_FLAG_NEED_PARENT flag is set, `parent` is guaranteed to be not-`NULL` and remain valid during the execution of this function. | [allow-none]
peer | the peer GstPad of the link |

#### Returns

the result of the link with the specified peer.

### gst_pad_set_unlink_function()

    #define gst_pad_set_unlink_function(p,f)        gst_pad_set_unlink_function_full((p),(f),NULL,NULL)

Calls `gst_pad_set_unlink_function_full()` with `NULL` for the user_data and notify.

#### Parameters

p | a GstPad. |
f | the GstPadUnlinkFunction to set. |

### gst_pad_set_unlink_function_full ()

    void
    gst_pad_set_unlink_function_full (GstPad *pad,
                                      GstPadUnlinkFunction unlink,
                                      gpointer user_data,
                                      GDestroyNotify notify);

Sets the given unlink function for the pad. It will be called when the pad is unlinked.

Note that the pad's lock is already held when the unlink function is called, so most pad functions cannot be called from within the callback.

#### Parameters

pad | a GstPad. |
unlink | the GstPadUnlinkFunction to set. |
user_data | user_data passed to `notify` |
notify | notify called when `unlink` will not be used anymore. |

### GstPadUnlinkFunction ()

    void
    (*GstPadUnlinkFunction) (GstPad *pad,
                             GstObject *parent);

Function signature to handle a unlinking the pad prom its peer.

The pad's lock is already held when the unlink function is called, so most pad functions cannot be called from within the callback.

#### Parameters

pad | the GstPad that is linked. |
parent | the parent of `pad` . If the GST_PAD_FLAG_NEED_PARENT flag is set, `parent` is guaranteed to be not-`NULL` and remain valid during the execution of this function. | [allow-none]

### gst_pad_proxy_query_caps ()

    gboolean
    gst_pad_proxy_query_caps (GstPad *pad,
                              GstQuery *query);

Calls `gst_pad_query_caps()` for all internally linked pads of `pad` and returns the intersection of the results.

This function is useful as a default caps query function for an element that can handle any stream format, but requires all its pads to have the same caps. Two such elements are tee and adder.

#### Parameters

pad | a GstPad to proxy. |
query | a CAPS GstQuery. |

#### Returns

`TRUE` if `query` could be executed

### gst_pad_proxy_query_accept_caps ()

    gboolean
    gst_pad_proxy_query_accept_caps (GstPad *pad,
                                     GstQuery *query);

Checks if all internally linked pads of `pad` accepts the caps in `query` and returns the intersection of the results.

This function is useful as a default accept caps query function for an element that can handle any stream format, but requires caps that are acceptable for all opposite pads.

#### Parameters

pad | a GstPad to proxy. |
query | an ACCEPT_CAPS GstQuery. |

#### Returns

`TRUE` if `query` could be executed

### gst_pad_set_activate_function()

    #define gst_pad_set_activate_function(p,f)      gst_pad_set_activate_function_full((p),(f),NULL,NULL)

Calls `gst_pad_set_activate_function_full()` with `NULL` for the user_data and notify.

#### Parameters

p | a GstPad. |
f | the GstPadActivateFunction to set. |

### gst_pad_set_activate_function_full ()

    void
    gst_pad_set_activate_function_full (GstPad *pad,
                                        GstPadActivateFunction activate,
                                        gpointer user_data,
                                        GDestroyNotify notify);

Sets the given activate function for `pad` . The activate function will dispatch to `gst_pad_activate_mode()` to perform the actual activation. Only makes sense to set on sink pads.

Call this function if your sink pad can start a pull-based task.

#### Parameters

pad | a GstPad. |
activate | the GstPadActivateFunction to set. |
user_data | user_data passed to `notify` |
notify | notify called when `activate` will not be used anymore. |

### GstPadActivateFunction ()

    gboolean
    (*GstPadActivateFunction) (GstPad *pad,
                               GstObject *parent);

This function is called when the pad is activated during the element READY to PAUSED state change. By default this function will call the activate function that puts the pad in push mode but elements can override this function to activate the pad in pull mode if they wish.

#### Parameters

pad | a GstPad |
parent | the parent of `pad` |

#### Returns

`TRUE` if the pad could be activated.

### gst_pad_set_activatemode_function()

    #define gst_pad_set_activatemode_function(p,f)  gst_pad_set_activatemode_function_full((p),(f),NULL,NULL)

Calls `gst_pad_set_activatemode_function_full()` with `NULL` for the user_data and notify.

#### Parameters

p | a GstPad. |
f | the GstPadActivateModeFunction to set. |

### gst_pad_set_activatemode_function_full ()

    void
    gst_pad_set_activatemode_function_full
                                   (GstPad *pad,
                                    GstPadActivateModeFunction activatemode,
                                    gpointer user_data,
                                    GDestroyNotify notify);

Sets the given activate_mode function for the pad. An activate_mode function prepares the element for data passing.

#### Parameters

pad | a GstPad. |
activatemode | the GstPadActivateModeFunction to set. |
user_data | user_data passed to `notify` |
notify | notify called when `activatemode` will not be used anymore. |

### GstPadActivateModeFunction ()

    gboolean
    (*GstPadActivateModeFunction) (GstPad *pad,
                                   GstObject *parent,
                                   GstPadMode mode,
                                   gboolean active);

The prototype of the push and pull activate functions.

#### Parameters

pad | a GstPad |
parent | the parent of `pad` |
mode | the requested activation mode of `pad` |
active | activate or deactivate the pad. |

#### Returns

`TRUE` if the pad could be activated or deactivated.

### gst_pad_needs_reconfigure ()

    gboolean
    gst_pad_needs_reconfigure (GstPad *pad);

Check the GST_PAD_FLAG_NEED_RECONFIGURE flag on `pad` and return `TRUE` if the flag was set.

#### Parameters

pad | the GstPad to check |

#### Returns

`TRUE` is the GST_PAD_FLAG_NEED_RECONFIGURE flag is set on `pad` .

### gst_pad_check_reconfigure ()

    gboolean
    gst_pad_check_reconfigure (GstPad *pad);

Check and clear the GST_PAD_FLAG_NEED_RECONFIGURE flag on `pad` and return `TRUE` if the flag was set.

#### Parameters

pad | the GstPad to check |

#### Returns

`TRUE` is the GST_PAD_FLAG_NEED_RECONFIGURE flag was set on `pad` .

### gst_pad_mark_reconfigure ()

    void
    gst_pad_mark_reconfigure (GstPad *pad);

Mark a pad for needing reconfiguration. The next call to `gst_pad_check_reconfigure()` will return `TRUE` after this call.

#### Parameters

pad | the GstPad to mark |

### gst_pad_push ()

    GstFlowReturn
    gst_pad_push (GstPad *pad,
                  GstBuffer *buffer);

Pushes a buffer to the peer of `pad` .

This function will call installed block probes before triggering any installed data probes.

The function proceeds calling `gst_pad_chain()` on the peer pad and returns the value from that function. If `pad` has no peer, GST_FLOW_NOT_LINKED will be returned.

In all cases, success or failure, the caller loses its reference to `buffer` after calling this function.

#### Parameters

pad | a source GstPad, returns GST_FLOW_ERROR if not. |
buffer | the GstBuffer to push returns GST_FLOW_ERROR if not. | [transfer full]

#### Returns

a GstFlowReturn from the peer pad.

MT safe.

### gst_pad_push_event ()

    gboolean
    gst_pad_push_event (GstPad *pad,
                        GstEvent *event);

Sends the event to the peer of the given pad. This function is mainly used by elements to send events to their peer elements.

This function takes ownership of the provided event so you should `gst_event_ref()` it if you want to reuse the event after this call.

#### Parameters

pad | a GstPad to push the event to. |
event | the GstEvent to send to the pad. | [transfer full]

#### Returns

`TRUE` if the event was handled.

MT safe.

### gst_pad_push_list ()

    GstFlowReturn
    gst_pad_push_list (GstPad *pad,
                       GstBufferList *list);

Pushes a buffer list to the peer of `pad` .

This function will call installed block probes before triggering any installed data probes.

The function proceeds calling the chain function on the peer pad and returns the value from that function. If `pad` has no peer, GST_FLOW_NOT_LINKED will be returned. If the peer pad does not have any installed chainlist function every group buffer of the list will be merged into a normal GstBuffer and chained via `gst_pad_chain()`.

In all cases, success or failure, the caller loses its reference to `list` after calling this function.

#### Parameters

pad | a source GstPad, returns GST_FLOW_ERROR if not. |
list | the GstBufferList to push returns GST_FLOW_ERROR if not. | [transfer full]

#### Returns

a GstFlowReturn from the peer pad.

MT safe.

### gst_pad_pull_range ()

    GstFlowReturn
    gst_pad_pull_range (GstPad *pad,
                        guint64 offset,
                        guint size,
                        GstBuffer **buffer);

Pulls a `buffer` from the peer pad or fills up a provided buffer.

This function will first trigger the pad block signal if it was installed.

When `pad` is not linked GST_FLOW_NOT_LINKED is returned else this function returns the result of `gst_pad_get_range()` on the peer pad. See `gst_pad_get_range()` for a list of return values and for the semantics of the arguments of this function.

If `buffer` points to a variable holding `NULL`, a valid new GstBuffer will be placed in `buffer` when this function returns GST_FLOW_OK. The new buffer must be freed with `gst_buffer_unref()` after usage. When this function returns any other result value, `buffer` will still point to `NULL`.

When `buffer` points to a variable that points to a valid GstBuffer, the buffer will be filled with the result data when this function returns GST_FLOW_OK. When this function returns any other result value, `buffer` will be unchanged. If the provided buffer is larger than `size` , only `size` bytes will be filled in the result buffer and its size will be updated accordingly.

Note that less than `size` bytes can be returned in `buffer` when, for example, an EOS condition is near or when `buffer` is not large enough to hold `size` bytes. The caller should check the result buffer size to get the result size.

#### Parameters

pad | a sink GstPad, returns GST_FLOW_ERROR if not. |
offset | The start offset of the buffer |
size | The length of the buffer |
buffer | a pointer to hold the GstBuffer, returns GST_FLOW_ERROR if `NULL`. | [out callee-allocates]

#### Returns

a GstFlowReturn from the peer pad.

MT safe.

### gst_pad_activate_mode ()

    gboolean
    gst_pad_activate_mode (GstPad *pad,
                           GstPadMode mode,
                           gboolean active);

Activates or deactivates the given pad in `mode` via dispatching to the pad's activatemodefunc. For use from within pad activation functions only.

If you don't know what this is, you probably don't want to call it.

#### Parameters

pad | the GstPad to activate or deactivate. |
mode | the requested activation mode |
active | whether or not the pad should be active. |

#### Returns

`TRUE` if the operation was successful.

MT safe.

### gst_pad_send_event ()

    gboolean
    gst_pad_send_event (GstPad *pad,
                        GstEvent *event);

Sends the event to the pad. This function can be used by applications to send events in the pipeline.

If `pad` is a source pad, `event` should be an upstream event. If `pad` is a sink pad, `event` should be a downstream event. For example, you would not send a GST_EVENT_EOS on a src pad; EOS events only propagate downstream. Furthermore, some downstream events have to be serialized with data flow, like EOS, while some can travel out-of-band, like GST_EVENT_FLUSH_START. If the event needs to be serialized with data flow, this function will take the pad's stream lock while calling its event function.

To find out whether an event type is upstream, downstream, or downstream and serialized, see GstEventTypeFlags, `gst_event_type_get_flags()`, GST_EVENT_IS_UPSTREAM, GST_EVENT_IS_DOWNSTREAM, and GST_EVENT_IS_SERIALIZED. Note that in practice that an application or plugin doesn't need to bother itself with this information; the core handles all necessary locks and checks.

This function takes ownership of the provided event so you should `gst_event_ref()` it if you want to reuse the event after this call.

#### Parameters

pad | a GstPad to send the event to. |
event | the GstEvent to send to the pad. | [transfer full]

#### Returns

`TRUE` if the event was handled.

### gst_pad_event_default ()

    gboolean
    gst_pad_event_default (GstPad *pad,
                           GstObject *parent,
                           GstEvent *event);

Invokes the default event handler for the given pad.

The EOS event will pause the task associated with `pad` before it is forwarded to all internally linked pads,

The event is sent to all pads internally linked to `pad` . This function takes ownership of `event` .

#### Parameters

pad | a GstPad to call the default event handler on. |
parent | the parent of `pad` or `NULL`. | [allow-none]
event | the GstEvent to handle. | [transfer full]

#### Returns

`TRUE` if the event was sent successfully.

### gst_pad_query ()

    gboolean
    gst_pad_query (GstPad *pad,
                   GstQuery *query);

Dispatches a query to a pad. The query should have been allocated by the caller via one of the type-specific allocation functions. The element that the pad belongs to is responsible for filling the query with an appropriate response, which should then be parsed with a type-specific query parsing function.

Again, the caller is responsible for both the allocation and deallocation of the query structure.

Please also note that some queries might need a running pipeline to work.

#### Parameters

pad | a GstPad to invoke the default query on. |
query | the GstQuery to perform. | [transfer none]

#### Returns

`TRUE` if the query could be performed.

### gst_pad_peer_query ()

    gboolean
    gst_pad_peer_query (GstPad *pad,
                        GstQuery *query);

Performs `gst_pad_query()` on the peer of `pad` .

The caller is responsible for both the allocation and deallocation of the query structure.

#### Parameters

pad | a GstPad to invoke the peer query on. |
query | the GstQuery to perform. | [transfer none]

#### Returns

`TRUE` if the query could be performed. This function returns `FALSE` if `pad` has no peer.

### gst_pad_query_default ()

    gboolean
    gst_pad_query_default (GstPad *pad,
                           GstObject *parent,
                           GstQuery *query);

Invokes the default query handler for the given pad. The query is sent to all pads internally linked to `pad` . Note that if there are many possible sink pads that are internally linked to `pad` , only one will be sent the query. Multi-sinkpad elements should implement custom query handlers.

#### Parameters

pad | a GstPad to call the default query handler on. |
parent | the parent of `pad` or `NULL`. | [allow-none]
query | the GstQuery to handle. | [transfer none]

#### Returns

`TRUE` if the query was performed successfully.

### gst_pad_query_position ()

    gboolean
    gst_pad_query_position (GstPad *pad,
                            GstFormat format,
                            gint64 *cur);

Queries a pad for the stream position.

#### Parameters

pad | a GstPad to invoke the position query on. |
format | the GstFormat requested |
cur | A location in which to store the current position, or `NULL`. | [out][allow-none]

#### Returns

`TRUE` if the query could be performed.

### gst_pad_query_duration ()

    gboolean
    gst_pad_query_duration (GstPad *pad,
                            GstFormat format,
                            gint64 *duration);

Queries a pad for the total stream duration.

#### Parameters

pad | a GstPad to invoke the duration query on. |
format | the GstFormat requested |
duration | a location in which to store the total duration, or `NULL`. | [out][allow-none]

#### Returns

`TRUE` if the query could be performed.

### gst_pad_query_convert ()

    gboolean
    gst_pad_query_convert (GstPad *pad,
                           GstFormat src_format,
                           gint64 src_val,
                           GstFormat dest_format,
                           gint64 *dest_val);

Queries a pad to convert `src_val` in `src_format` to `dest_format` .

#### Parameters

pad | a GstPad to invoke the convert query on. |
src_format | a GstFormat to convert from. |
src_val | a value to convert. |
dest_format | the GstFormat to convert to. |
dest_val | a pointer to the result. | [out]

#### Returns

`TRUE` if the query could be performed.

### gst_pad_query_accept_caps ()

    gboolean
    gst_pad_query_accept_caps (GstPad *pad,
                               GstCaps *caps);

Check if the given pad accepts the caps.

#### Parameters

pad | a GstPad to check |
caps | a GstCaps to check on the pad |

#### Returns

`TRUE` if the pad can accept the caps.

### gst_pad_query_caps ()

    GstCaps *
    gst_pad_query_caps (GstPad *pad,
                        GstCaps *filter);

Gets the capabilities this pad can produce or consume. Note that this method doesn't necessarily return the caps set by sending a `gst_event_new_caps()` - use `gst_pad_get_current_caps()` for that instead. gst_pad_query_caps returns all possible caps a pad can operate with, using the pad's CAPS query function, If the query fails, this function will return `filter` , if not `NULL`, otherwise ANY.

When called on sinkpads `filter` contains the caps that upstream could produce in the order preferred by upstream. When called on srcpads `filter` contains the caps accepted by downstream in the preferred order. `filter` might be `NULL` but if it is not `NULL` the returned caps will be a subset of `filter` .

Note that this function does not return writable GstCaps, use `gst_caps_make_writable()` before modifying the caps.

#### Parameters

pad | a GstPad to get the capabilities of. |
filter | suggested GstCaps, or `NULL`. | [allow-none]

#### Returns

the caps of the pad with incremented ref-count.

[transfer full]

### gst_pad_peer_query_position ()

    gboolean
    gst_pad_peer_query_position (GstPad *pad,
                                 GstFormat format,
                                 gint64 *cur);

Queries the peer of a given sink pad for the stream position.

#### Parameters

pad | a GstPad on whose peer to invoke the position query on. Must be a sink pad. |
format | the GstFormat requested |
cur | a location in which to store the current position, or `NULL`. | [out][allow-none]

#### Returns

`TRUE` if the query could be performed.

### gst_pad_peer_query_duration ()

    gboolean
    gst_pad_peer_query_duration (GstPad *pad,
                                 GstFormat format,
                                 gint64 *duration);

Queries the peer pad of a given sink pad for the total stream duration.

#### Parameters

pad | a GstPad on whose peer pad to invoke the duration query on. Must be a sink pad. |
format | the GstFormat requested |
duration | a location in which to store the total duration, or `NULL`. | [out][allow-none]

#### Returns

`TRUE` if the query could be performed.

### gst_pad_peer_query_convert ()

    gboolean
    gst_pad_peer_query_convert (GstPad *pad,
                                GstFormat src_format,
                                gint64 src_val,
                                GstFormat dest_format,
                                gint64 *dest_val);

Queries the peer pad of a given sink pad to convert `src_val` in `src_format` to `dest_format` .

#### Parameters

pad | a GstPad, on whose peer pad to invoke the convert query on. Must be a sink pad. |
src_format | a GstFormat to convert from. |
src_val | a value to convert. |
dest_format | the GstFormat to convert to. |
dest_val | a pointer to the result. | [out]

#### Returns

`TRUE` if the query could be performed.

### gst_pad_peer_query_accept_caps ()

    gboolean
    gst_pad_peer_query_accept_caps (GstPad *pad,
                                    GstCaps *caps);

Check if the peer of `pad` accepts `caps` . If `pad` has no peer, this function returns `TRUE`.

#### Parameters

pad | a GstPad to check the peer of |
caps | a GstCaps to check on the pad |

#### Returns

`TRUE` if the peer of `pad` can accept the caps or `pad` has no peer.

### gst_pad_peer_query_caps ()

    GstCaps *
    gst_pad_peer_query_caps (GstPad *pad,
                             GstCaps *filter);

Gets the capabilities of the peer connected to this pad. Similar to `gst_pad_query_caps()`.

When called on srcpads `filter` contains the caps that upstream could produce in the order preferred by upstream. When called on sinkpads `filter` contains the caps accepted by downstream in the preferred order. `filter` might be `NULL` but if it is not `NULL` the returned caps will be a subset of `filter` .

#### Parameters

pad | a GstPad to get the capabilities of. |
filter | a GstCaps filter, or `NULL`. | [allow-none]

#### Returns

the caps of the peer pad with incremented ref-count. When there is no peer pad, this function returns `filter` or, when `filter` is `NULL`, ANY caps.

[transfer full]

### gst_pad_set_query_function()

    #define gst_pad_set_query_function(p,f)   gst_pad_set_query_function_full((p),(f),NULL,NULL)

Calls `gst_pad_set_query_function_full()` with `NULL` for the user_data and notify.

#### Parameters

p | a GstPad of either direction. |
f | the GstPadQueryFunction to set. |

### gst_pad_set_query_function_full ()

    void
    gst_pad_set_query_function_full (GstPad *pad,
                                     GstPadQueryFunction query,
                                     gpointer user_data,
                                     GDestroyNotify notify);

Set the given query function for the pad.

#### Parameters

pad | a GstPad of either direction. |
query | the GstPadQueryFunction to set. |
user_data | user_data passed to `notify` |
notify | notify called when `query` will not be used anymore. |

### GstPadQueryFunction ()

    gboolean
    (*GstPadQueryFunction) (GstPad *pad,
                            GstObject *parent,
                            GstQuery *query);

The signature of the query function.

#### Parameters

pad | the GstPad to query. |
parent | the parent of `pad` . If the GST_PAD_FLAG_NEED_PARENT flag is set, `parent` is guaranteed to be not-`NULL` and remain valid during the execution of this function. | [allow-none]
query | the GstQuery object to execute |

#### Returns

`TRUE` if the query could be performed.

### gst_pad_set_iterate_internal_links_function()

    #define gst_pad_set_iterate_internal_links_function(p,f) gst_pad_set_iterate_internal_links_function_full((p),(f),NULL,NULL)

Calls `gst_pad_set_iterate_internal_links_function_full()` with `NULL` for the user_data and notify.

#### Parameters

p | a GstPad of either direction. |
f | the GstPadIterIntLinkFunction to set. |

### gst_pad_set_iterate_internal_links_function_full ()

    void
    gst_pad_set_iterate_internal_links_function_full
                                   (GstPad *pad,
                                    GstPadIterIntLinkFunction iterintlink,
                                    gpointer user_data,
                                    GDestroyNotify notify);

Sets the given internal link iterator function for the pad.

#### Parameters

pad | a GstPad of either direction. |
iterintlink | the GstPadIterIntLinkFunction to set. |
user_data | user_data passed to `notify` |
notify | notify called when `iterintlink` will not be used anymore. |

### GstPadIterIntLinkFunction ()

    GstIterator *
    (*GstPadIterIntLinkFunction) (GstPad *pad,
                                  GstObject *parent);

The signature of the internal pad link iterator function.

#### Parameters

pad | The GstPad to query. |
parent | the parent of `pad` . If the GST_PAD_FLAG_NEED_PARENT flag is set, `parent` is guaranteed to be not-`NULL` and remain valid during the execution of this function. | [allow-none]

#### Returns

a new GstIterator that will iterate over all pads that are linked to the given pad on the inside of the parent element.

the caller must call `gst_iterator_free()` after usage.

### gst_pad_iterate_internal_links ()

    GstIterator *
    gst_pad_iterate_internal_links (GstPad *pad);

Gets an iterator for the pads to which the given pad is linked to inside of the parent element.

Each GstPad element yielded by the iterator will have its refcount increased, so unref after use.

Free-function: gst_iterator_free

#### Parameters

pad | the GstPad to get the internal links of. |

#### Returns

a new GstIterator of GstPad or `NULL` when the pad does not have an iterator function configured. Use `gst_iterator_free()` after usage.

[transfer full][nullable]

### gst_pad_iterate_internal_links_default ()

    GstIterator *
    gst_pad_iterate_internal_links_default
                                   (GstPad *pad,
                                    GstObject *parent);

Iterate the list of pads to which the given pad is linked to inside of the parent element. This is the default handler, and thus returns an iterator of all of the pads inside the parent element with opposite direction.

The caller must free this iterator after use with `gst_iterator_free()`.

#### Parameters

pad | the GstPad to get the internal links of. |
parent | the parent of `pad` or `NULL`. | [allow-none]

#### Returns

a GstIterator of GstPad, or `NULL` if `pad` has no parent. Unref each returned pad with `gst_object_unref()`.

[nullable]

### gst_pad_set_element_private ()

    void
    gst_pad_set_element_private (GstPad *pad,
                                 gpointer priv);

Set the given private data gpointer on the pad. This function can only be used by the element that owns the pad. No locking is performed in this function.

#### Parameters

pad | the GstPad to set the private data of. |
priv | The private data to attach to the pad. |

### gst_pad_get_element_private ()

    gpointer
    gst_pad_get_element_private (GstPad *pad);

Gets the private data of a pad. No locking is performed in this function.

#### Parameters

pad | the GstPad to get the private data of. |

#### Returns

a gpointer to the private data.

[transfer none][nullable]

### gst_pad_create_stream_id ()

    gchar *
    gst_pad_create_stream_id (GstPad *pad,
                              GstElement *parent,
                              const gchar *stream_id);

Creates a stream-id for the source GstPad `pad` by combining the upstream information with the optional `stream_id` of the stream of `pad` . `pad` must have a parent GstElement and which must have zero or one sinkpad. `stream_id` can only be `NULL` if the parent element of `pad` has only a single source pad.

This function generates an unique stream-id by getting the upstream stream-start event stream ID and appending `stream_id` to it. If the element has no sinkpad it will generate an upstream stream-id by doing an URI query on the element and in the worst case just uses a random number. Source elements that don't implement the URI handler interface should ideally generate a unique, deterministic stream-id manually instead.

Since stream IDs are sorted alphabetically, any numbers in the stream ID should be printed with a fixed number of characters, preceded by 0's, such as by using the format %03u instead of %u.

#### Parameters

pad | A source GstPad |
parent | Parent GstElement of `pad` |
stream_id | The stream-id. | [allow-none]

#### Returns

A stream-id for `pad` . `g_free()` after usage.

### gst_pad_create_stream_id_printf ()

    gchar *
    gst_pad_create_stream_id_printf (GstPad *pad,
                                     GstElement *parent,
                                     const gchar *stream_id,
                                     ...);

Creates a stream-id for the source GstPad `pad` by combining the upstream information with the optional `stream_id` of the stream of `pad` . `pad` must have a parent GstElement and which must have zero or one sinkpad. `stream_id` can only be `NULL` if the parent element of `pad` has only a single source pad.

This function generates an unique stream-id by getting the upstream stream-start event stream ID and appending `stream_id` to it. If the element has no sinkpad it will generate an upstream stream-id by doing an URI query on the element and in the worst case just uses a random number. Source elements that don't implement the URI handler interface should ideally generate a unique, deterministic stream-id manually instead.

#### Parameters

pad | A source GstPad |
parent | Parent GstElement of `pad` |
stream_id | The stream-id. | [allow-none]
... | parameters for the `stream_id` format string |

#### Returns

A stream-id for `pad` . `g_free()` after usage.

### gst_pad_create_stream_id_printf_valist ()

    gchar *
    gst_pad_create_stream_id_printf_valist
                                   (GstPad *pad,
                                    GstElement *parent,
                                    const gchar *stream_id,
                                    va_list var_args);

Creates a stream-id for the source GstPad `pad` by combining the upstream information with the optional `stream_id` of the stream of `pad` . `pad` must have a parent GstElement and which must have zero or one sinkpad. `stream_id` can only be `NULL` if the parent element of `pad` has only a single source pad.

This function generates an unique stream-id by getting the upstream stream-start event stream ID and appending `stream_id` to it. If the element has no sinkpad it will generate an upstream stream-id by doing an URI query on the element and in the worst case just uses a random number. Source elements that don't implement the URI handler interface should ideally generate a unique, deterministic stream-id manually instead.

#### Parameters

pad | A source GstPad |
parent | Parent GstElement of `pad` |
stream_id | The stream-id. | [allow-none]
var_args | parameters for the `stream_id` format string |

#### Returns

A stream-id for `pad` . `g_free()` after usage.

### gst_pad_get_stream_id ()

    gchar *
    gst_pad_get_stream_id (GstPad *pad);

Returns the current stream-id for the `pad` , or `NULL` if none has been set yet, i.e. the pad has not received a stream-start event yet.

This is a convenience wrapper around `gst_pad_get_sticky_event()` and `gst_event_parse_stream_start()`.

The returned stream-id string should be treated as an opaque string, its contents should not be interpreted.

#### Parameters

pad | A source GstPad |

#### Returns

a newly-allocated copy of the stream-id for `pad` , or `NULL`. `g_free()` the returned string when no longer needed.

[nullable]

Since: 1.2

### gst_pad_get_stream ()

    GstStream *
    gst_pad_get_stream (GstPad *pad);

Returns the current GstStream for the `pad` , or `NULL` if none has been set yet, i.e. the pad has not received a stream-start event yet.

This is a convenience wrapper around `gst_pad_get_sticky_event()` and `gst_event_parse_stream()`.

#### Parameters

pad | A source GstPad |

#### Returns

the current GstStream for `pad` , or `NULL`. unref the returned stream when no longer needed.

[nullable][transfer full]

Since: 1.10

### GstPadForwardFunction ()

    gboolean
    (*GstPadForwardFunction) (GstPad *pad,
                              gpointer user_data);

A forward function is called for all internally linked pads, see `gst_pad_forward()`.

#### Parameters

pad | the GstPad that is forwarded. |
user_data | the gpointer to optional user data. |

#### Returns

`TRUE` if the dispatching procedure has to be stopped.

### gst_pad_forward ()

    gboolean
    gst_pad_forward (GstPad *pad,
                     GstPadForwardFunction forward,
                     gpointer user_data);

Calls `forward` for all internally linked pads of `pad` . This function deals with dynamically changing internal pads and will make sure that the `forward` function is only called once for each pad.

When `forward` returns `TRUE`, no further pads will be processed.

#### Parameters

pad | a GstPad |
forward | a GstPadForwardFunction. | [scope call]
user_data | user data passed to `forward` |

#### Returns

`TRUE` if one of the dispatcher functions returned `TRUE`.

### gst_pad_chain ()

    GstFlowReturn
    gst_pad_chain (GstPad *pad,
                   GstBuffer *buffer);

Chain a buffer to `pad` .

The function returns GST_FLOW_FLUSHING if the pad was flushing.

If the buffer type is not acceptable for `pad` (as negotiated with a preceding GST_EVENT_CAPS event), this function returns GST_FLOW_NOT_NEGOTIATED.

The function proceeds calling the chain function installed on `pad` (see `gst_pad_set_chain_function()`) and the return value of that function is returned to the caller. GST_FLOW_NOT_SUPPORTED is returned if `pad` has no chain function.

In all cases, success or failure, the caller loses its reference to `buffer` after calling this function.

#### Parameters

pad | a sink GstPad, returns GST_FLOW_ERROR if not. |
buffer | the GstBuffer to send, return GST_FLOW_ERROR if not. | [transfer full]

#### Returns

a GstFlowReturn from the pad.

MT safe.

### gst_pad_chain_list ()

    GstFlowReturn
    gst_pad_chain_list (GstPad *pad,
                        GstBufferList *list);

Chain a bufferlist to `pad` .

The function returns GST_FLOW_FLUSHING if the pad was flushing.

If `pad` was not negotiated properly with a CAPS event, this function returns GST_FLOW_NOT_NEGOTIATED.

The function proceeds calling the chainlist function installed on `pad` (see `gst_pad_set_chain_list_function()`) and the return value of that function is returned to the caller. GST_FLOW_NOT_SUPPORTED is returned if `pad` has no chainlist function.

In all cases, success or failure, the caller loses its reference to `list` after calling this function.

MT safe.

#### Parameters

pad | a sink GstPad, returns GST_FLOW_ERROR if not. |
list | the GstBufferList to send, return GST_FLOW_ERROR if not. | [transfer full]

#### Returns

a GstFlowReturn from the pad.

### gst_pad_start_task ()

    gboolean
    gst_pad_start_task (GstPad *pad,
                        GstTaskFunction func,
                        gpointer user_data,
                        GDestroyNotify notify);

Starts a task that repeatedly calls `func` with `user_data` . This function is mostly used in pad activation functions to start the dataflow. The GST_PAD_STREAM_LOCK of `pad` will automatically be acquired before `func` is called.

#### Parameters

pad | the GstPad to start the task of |
func | the task function to call |
user_data | user data passed to the task function |
notify | called when `user_data` is no longer referenced |

#### Returns

a `TRUE` if the task could be started.

### gst_pad_pause_task ()

    gboolean
    gst_pad_pause_task (GstPad *pad);

Pause the task of `pad` . This function will also wait until the function executed by the task is finished if this function is not called from the task function.

#### Parameters

pad | the GstPad to pause the task of |

#### Returns

a `TRUE` if the task could be paused or `FALSE` when the pad has no task.

### gst_pad_stop_task ()

    gboolean
    gst_pad_stop_task (GstPad *pad);

Stop the task of `pad` . This function will also make sure that the function executed by the task will effectively stop if not called from the GstTaskFunction.

This function will deadlock if called from the GstTaskFunction of the task. Use `gst_task_pause()` instead.

Regardless of whether the pad has a task, the stream lock is acquired and released so as to ensure that streaming through this pad has finished.

#### Parameters

pad | the GstPad to stop the task of |

#### Returns

a `TRUE` if the task could be stopped or `FALSE` on error.

### gst_pad_get_task_state ()

    GstTaskState
    gst_pad_get_task_state (GstPad *pad);

Get `pad` task state. If no task is currently set, GST_TASK_STOPPED is returned.

#### Parameters

pad | the GstPad to get task state from |

#### Returns

The current state of `pad` 's task.

Since: 1.12

### gst_pad_set_active ()

    gboolean
    gst_pad_set_active (GstPad *pad,
                        gboolean active);

Activates or deactivates the given pad. Normally called from within core state change functions.

If `active` , makes sure the pad is active. If it is already active, either in push or pull mode, just return. Otherwise dispatches to the pad's activate function to perform the actual activation.

If not `active` , calls `gst_pad_activate_mode()` with the pad's current mode and a `FALSE` argument.

#### Parameters

pad | the GstPad to activate or deactivate. |
active | whether or not the pad should be active. |

#### Returns

`TRUE` if the operation was successful.

MT safe.

### GST_PAD_GET_STREAM_LOCK()

    #define GST_PAD_GET_STREAM_LOCK(pad)    (&(GST_PAD_CAST(pad)->stream_rec_lock))

Get the stream lock of `pad` . The stream lock is protecting the resources used in the data processing functions of `pad` . Accessor macro, use `GST_PAD_STREAM_LOCK()` and `GST_PAD_STREAM_UNLOCK()` instead to take/release the pad's stream lock.

#### Parameters

pad | a GstPad |

### GST_PAD_STREAM_LOCK()

    #define GST_PAD_STREAM_LOCK(pad)        g_rec_mutex_lock(GST_PAD_GET_STREAM_LOCK(pad))

Take the pad's stream lock. The stream lock is recursive and will be taken when buffers or serialized downstream events are pushed on a pad.

#### Parameters

pad | a GstPad |

### GST_PAD_STREAM_TRYLOCK()

    #define GST_PAD_STREAM_TRYLOCK(pad)     g_rec_mutex_trylock(GST_PAD_GET_STREAM_LOCK(pad))

Try to take the pad's stream lock, and return `TRUE` if the lock could be taken, and otherwise `FALSE`.

#### Parameters

pad | a GstPad |

### GST_PAD_STREAM_UNLOCK()

    #define GST_PAD_STREAM_UNLOCK(pad)      g_rec_mutex_unlock(GST_PAD_GET_STREAM_LOCK(pad))

Release the pad's stream lock.

#### Parameters

pad | a GstPad |

### GST_PAD_NAME()

    #define GST_PAD_NAME(pad)		(GST_OBJECT_NAME(pad))

Get name of the given pad. No locking is performed in this function, use `gst_pad_get_name()` instead.

#### Parameters

pad | a GstPad |

### GST_PAD_PARENT()

    #define GST_PAD_PARENT(pad)		(GST_ELEMENT_CAST(GST_OBJECT_PARENT(pad)))

Get the `pad` parent. No locking is performed in this function, use `gst_pad_get_parent()` instead.

#### Parameters

pad | a GstPad |

### GST_PAD_ELEMENT_PRIVATE()

    #define GST_PAD_ELEMENT_PRIVATE(pad)    (GST_PAD_CAST(pad)->element_private)

Get the private data of `pad` , which is usually some pad- or stream-specific structure created by the element and set on the pad when creating it. No locking is performed in this function.

#### Parameters

pad | a GstPad |

### GST_PAD_PAD_TEMPLATE()

    #define GST_PAD_PAD_TEMPLATE(pad) (GST_PAD_CAST(pad)->padtemplate)

Get the `pad` GstPadTemplate. It describes the possible media types a `pad` or an element factory can handle.

#### Parameters

pad | a GstPad |

### GST_PAD_DIRECTION()

    #define GST_PAD_DIRECTION(pad)		(GST_PAD_CAST(pad)->direction)

Get the GstPadDirection of the given `pad` . Accessor macro, use `gst_pad_get_direction()` instead.

#### Parameters

pad | a GstPad |

### GST_PAD_LAST_FLOW_RETURN()

    #define GST_PAD_LAST_FLOW_RETURN(pad)   (GST_PAD_CAST(pad)->ABI.abi.last_flowret)

Gets the last flow return on this pad

#### Parameters

pad | a GstPad |

Since: 1.4

### GST_PAD_TASK()

    #define GST_PAD_TASK(pad)		(GST_PAD_CAST(pad)->task)

Get the GstTask of `pad` . Accessor macro used by GStreamer. Use the `gst_pad_start_task()`, `gst_pad_stop_task()` and `gst_pad_pause_task()` functions instead.

#### Parameters

pad | a GstPad |

### GST_PAD_MODE()

    #define GST_PAD_MODE(pad)	        (GST_PAD_CAST(pad)->mode)

Get the GstPadMode of pad, which will be GST_PAD_MODE_NONE if the pad has not been activated yet, and otherwise either GST_PAD_MODE_PUSH or GST_PAD_MODE_PULL depending on which mode the pad was activated in.

#### Parameters

pad | a GstPad |

### GST_PAD_ACTIVATEFUNC()

    #define GST_PAD_ACTIVATEFUNC(pad) (GST_PAD_CAST(pad)->activatefunc)

Get the GstPadActivateFunction from `pad` .

#### Parameters

pad | a GstPad |

### GST_PAD_ACTIVATEMODEFUNC()

    #define GST_PAD_ACTIVATEMODEFUNC(pad) (GST_PAD_CAST(pad)->activatemodefunc)

Get the GstPadActivateModeFunction from the given `pad` .

#### Parameters

pad | a GstPad |

### GST_PAD_CHAINFUNC()

    #define GST_PAD_CHAINFUNC(pad)		(GST_PAD_CAST(pad)->chainfunc)

Get the GstPadChainFunction from the given `pad` .

#### Parameters

pad | a GstPad |

### GST_PAD_CHAINLISTFUNC()

    #define GST_PAD_CHAINLISTFUNC(pad)      (GST_PAD_CAST(pad)->chainlistfunc)

Get the GstPadChainListFunction from the given `pad` .

#### Parameters

pad | a GstPad |

### GST_PAD_EVENTFUNC()

    #define GST_PAD_EVENTFUNC(pad)		(GST_PAD_CAST(pad)->eventfunc)

Get the GstPadEventFunction from the given `pad` , which is the function that handles events on the pad. You can use this to set your own event handling function on a pad after you create it. If your element derives from a base class, use the base class's virtual functions instead.

#### Parameters

pad | a GstPad |

### GST_PAD_EVENTFULLFUNC()

    #define GST_PAD_EVENTFULLFUNC(pad) (GST_PAD_CAST(pad)->ABI.abi.eventfullfunc)

Get the GstPadEventFullFunction from the given `pad` , which is the function that handles events on the pad. You can use this to set your own event handling function on a pad after you create it. If your element derives from a base class, use the base class's virtual functions instead.

#### Parameters

pad | a GstPad |

Since: 1.8

### GST_PAD_GETRANGEFUNC()

    #define GST_PAD_GETRANGEFUNC(pad) (GST_PAD_CAST(pad)->getrangefunc)

Get the GstPadGetRangeFunction from the given `pad` .

#### Parameters

pad | a GstPad |

### GST_PAD_QUERYFUNC()

    #define GST_PAD_QUERYFUNC(pad)		(GST_PAD_CAST(pad)->queryfunc)

Get the GstPadQueryFunction from `pad` , which is the function that handles queries on the pad. You can use this to set your own query handling function on a pad after you create it. If your element derives from a base class, use the base class's virtual functions instead.

#### Parameters

pad | a GstPad |

### GST_PAD_ITERINTLINKFUNC()

    #define GST_PAD_ITERINTLINKFUNC(pad)    (GST_PAD_CAST(pad)->iterintlinkfunc)

Get the GstPadIterIntLinkFunction from the given `pad` .

#### Parameters

pad | a GstPad |

### GST_PAD_PEER()

    #define GST_PAD_PEER(pad)		(GST_PAD_CAST(pad)->peer)

Return the pad's peer member. This member is a pointer to the linked `pad` . No locking is performed in this function, use `gst_pad_get_peer()` instead.

#### Parameters

pad | a GstPad |

### GST_PAD_LINKFUNC()

    #define GST_PAD_LINKFUNC(pad)		(GST_PAD_CAST(pad)->linkfunc)

Get the GstPadLinkFunction for the given `pad` .

#### Parameters

pad | a GstPad |

### GST_PAD_UNLINKFUNC()

    #define GST_PAD_UNLINKFUNC(pad)		(GST_PAD_CAST(pad)->unlinkfunc)

Get the GstPadUnlinkFunction from the given `pad` .

#### Parameters

pad | a GstPad |

### GST_PAD_IS_LINKED()

    #define GST_PAD_IS_LINKED(pad)		(GST_PAD_PEER(pad) != NULL)

#### Parameters

pad | a GstPad |

#### Returns

`TRUE` if the pad is linked to another pad. Use `gst_pad_is_linked()` instead.

### GST_PAD_IS_SRC()

    #define GST_PAD_IS_SRC(pad)		(GST_PAD_DIRECTION(pad) == GST_PAD_SRC)

#### Parameters

pad | a GstPad |

#### Returns

`TRUE` if the pad is a source pad (i.e. produces data).

### GST_PAD_IS_SINK()

    #define GST_PAD_IS_SINK(pad)		(GST_PAD_DIRECTION(pad) == GST_PAD_SINK)

#### Parameters

pad | a GstPad |

#### Returns

`TRUE` if the pad is a sink pad (i.e. consumes data).

### GST_PAD_IS_ACTIVE()

    #define GST_PAD_IS_ACTIVE(pad)          (GST_PAD_MODE(pad) != GST_PAD_MODE_NONE)

#### Parameters

pad | a GstPad |

#### Returns

`TRUE` if the pad has been activated.

### GST_PAD_IS_BLOCKED()

    #define GST_PAD_IS_BLOCKED(pad)		(GST_OBJECT_FLAG_IS_SET (pad, GST_PAD_FLAG_BLOCKED))

Check if the dataflow on a `pad` is blocked. Use `gst_pad_is_blocked()` instead.

#### Parameters

pad | a GstPad |

### GST_PAD_IS_BLOCKING()

    #define GST_PAD_IS_BLOCKING(pad) (GST_OBJECT_FLAG_IS_SET (pad, GST_PAD_FLAG_BLOCKING))

Check if the `pad` is currently blocking on a buffer or event. Use `gst_pad_is_blocking()` instead.

#### Parameters

pad | a GstPad |

### GST_PAD_IS_FLUSHING()

    #define GST_PAD_IS_FLUSHING(pad) (GST_OBJECT_FLAG_IS_SET (pad, GST_PAD_FLAG_FLUSHING))

Check if the given `pad` is flushing.

#### Parameters

pad | a GstPad |

### GST_PAD_SET_FLUSHING()

    #define GST_PAD_SET_FLUSHING(pad) (GST_OBJECT_FLAG_SET (pad, GST_PAD_FLAG_FLUSHING))

Set the given `pad` to flushing state, which means it will not accept any more events, queries or buffers, and return GST_FLOW_FLUSHING if any buffers are pushed on it. This usually happens when the pad is shut down or when a flushing seek happens. This is used inside GStreamer when flush start/stop events pass through pads, or when an element state is changed and pads are activated or deactivated.

#### Parameters

pad | a GstPad |

### GST_PAD_UNSET_FLUSHING()

    #define GST_PAD_UNSET_FLUSHING(pad) (GST_OBJECT_FLAG_UNSET (pad, GST_PAD_FLAG_FLUSHING))

Unset the flushing flag.

#### Parameters

pad | a GstPad |

### GST_PAD_IS_EOS()

    #define GST_PAD_IS_EOS(pad)	        (GST_OBJECT_FLAG_IS_SET (pad, GST_PAD_FLAG_EOS))

Check if the `pad` is in EOS state.

#### Parameters

pad | a GstPad |

### GST_PAD_NEEDS_RECONFIGURE()

    #define GST_PAD_NEEDS_RECONFIGURE(pad)  (GST_OBJECT_FLAG_IS_SET (pad, GST_PAD_FLAG_NEED_RECONFIGURE))

Check if the `pad` should be reconfigured/renegotiated. The flag has to be unset manually after reconfiguration happened. Use `gst_pad_needs_reconfigure()` or `gst_pad_check_reconfigure()` instead.

#### Parameters

pad | a GstPad |

### GST_PAD_HAS_PENDING_EVENTS()

    #define GST_PAD_HAS_PENDING_EVENTS(pad) (GST_OBJECT_FLAG_IS_SET (pad, GST_PAD_FLAG_PENDING_EVENTS))

Check if the given `pad` has pending events. This is used internally by GStreamer.

#### Parameters

pad | a GstPad |

### GST_PAD_IS_FIXED_CAPS()

    #define GST_PAD_IS_FIXED_CAPS(pad) (GST_OBJECT_FLAG_IS_SET (pad, GST_PAD_FLAG_FIXED_CAPS))

Check if the given `pad` is using fixed caps, which means that once the caps are set on the `pad` , the caps query function will only return those caps. See `gst_pad_use_fixed_caps()`.

#### Parameters

pad | a GstPad |

### GST_PAD_NEEDS_PARENT()

    #define GST_PAD_NEEDS_PARENT(pad)       (GST_OBJECT_FLAG_IS_SET (pad, GST_PAD_FLAG_NEED_PARENT))

Check if there is a parent object before calling into the `pad` callbacks. This is used internally by GStreamer.

#### Parameters

pad | a GstPad |

### GST_PAD_IS_PROXY_CAPS()

    #define GST_PAD_IS_PROXY_CAPS(pad)      (GST_OBJECT_FLAG_IS_SET (pad, GST_PAD_FLAG_PROXY_CAPS))

Check if the given `pad` is set to proxy caps. This means that the default event and query handler will forward all events and queries to the internally linked `pads` instead of discarding them.

#### Parameters

pad | a GstPad |

### GST_PAD_SET_PROXY_CAPS()

    #define GST_PAD_SET_PROXY_CAPS(pad)     (GST_OBJECT_FLAG_SET (pad, GST_PAD_FLAG_PROXY_CAPS))

Set `pad` to proxy caps, so that all caps-related events and queries are proxied down- or upstream to the other side of the element automatically. Set this if the element always outputs data in the exact same format as it receives as input. This is just for convenience to avoid implementing some standard event and query handling code in an element.

#### Parameters

pad | a GstPad |

### GST_PAD_UNSET_PROXY_CAPS()

    #define GST_PAD_UNSET_PROXY_CAPS(pad)   (GST_OBJECT_FLAG_UNSET (pad, GST_PAD_FLAG_PROXY_CAPS))

Unset proxy caps flag.

#### Parameters

pad | a GstPad |

### GST_PAD_IS_PROXY_ALLOCATION()

    #define GST_PAD_IS_PROXY_ALLOCATION(pad)    (GST_OBJECT_FLAG_IS_SET (pad, GST_PAD_FLAG_PROXY_ALLOCATION))

Check if the given `pad` is set as proxy allocation which means that the default query handler will forward allocation queries to the internally linked `pads` instead of discarding them.

#### Parameters

pad | a GstPad |

### GST_PAD_SET_PROXY_ALLOCATION()

    #define GST_PAD_SET_PROXY_ALLOCATION(pad)   (GST_OBJECT_FLAG_SET (pad, GST_PAD_FLAG_PROXY_ALLOCATION))

Set `pad` to proxy allocation queries, which means that the default query handler will forward allocation queries to the internally linked `pads` instead of discarding them. Set this if the element always outputs data in the exact same format as it receives as input. This is just for convenience to avoid implementing some standard query handling code in an element.

#### Parameters

pad | a GstPad |

### GST_PAD_UNSET_PROXY_ALLOCATION()

    #define GST_PAD_UNSET_PROXY_ALLOCATION(pad) (GST_OBJECT_FLAG_UNSET (pad, GST_PAD_FLAG_PROXY_ALLOCATION))

Unset proxy allocation flag.

#### Parameters

pad | a GstPad |

### GST_PAD_SET_PROXY_SCHEDULING()

    #define GST_PAD_SET_PROXY_SCHEDULING(pad)   (GST_OBJECT_FLAG_SET (pad, GST_PAD_FLAG_PROXY_SCHEDULING))

Set `pad` to proxy scheduling queries, which means that the default query handler will forward scheduling queries to the internally linked `pads` instead of discarding them. You will usually want to handle scheduling queries explicitly if your element supports multiple scheduling modes.

#### Parameters

pad | a GstPad |

### GST_PAD_UNSET_PROXY_SCHEDULING()

    #define GST_PAD_UNSET_PROXY_SCHEDULING(pad) (GST_OBJECT_FLAG_UNSET (pad, GST_PAD_FLAG_PROXY_SCHEDULING))

Unset proxy scheduling flag.

#### Parameters

pad | a GstPad |

### GST_PAD_IS_PROXY_SCHEDULING()

    #define GST_PAD_IS_PROXY_SCHEDULING(pad)    (GST_OBJECT_FLAG_IS_SET (pad, GST_PAD_FLAG_PROXY_SCHEDULING))

Check if the given `pad` is set to proxy scheduling queries, which means that the default query handler will forward scheduling queries to the internally linked `pads` instead of discarding them.

#### Parameters

pad | a GstPad |

### GST_PAD_IS_ACCEPT_INTERSECT()

    #define GST_PAD_IS_ACCEPT_INTERSECT(pad)    (GST_OBJECT_FLAG_IS_SET (pad, GST_PAD_FLAG_ACCEPT_INTERSECT))

Check if the pad's accept intersect flag is set. The default accept-caps handler will check if the caps intersect the query-caps result instead of checking for a subset. This is interesting for parser elements that can accept incompletely specified caps.

#### Parameters

pad | a GstPad |

### GST_PAD_SET_ACCEPT_INTERSECT()

    #define GST_PAD_SET_ACCEPT_INTERSECT(pad)   (GST_OBJECT_FLAG_SET (pad, GST_PAD_FLAG_ACCEPT_INTERSECT))

Set `pad` to by default accept caps by intersecting the result instead of checking for a subset. This is interesting for parser elements that can accept incompletely specified caps.

#### Parameters

pad | a GstPad |

### GST_PAD_UNSET_ACCEPT_INTERSECT()

    #define GST_PAD_UNSET_ACCEPT_INTERSECT(pad) (GST_OBJECT_FLAG_UNSET (pad, GST_PAD_FLAG_ACCEPT_INTERSECT))

Unset accept intersect flag.

#### Parameters

pad | a GstPad |

### GST_PAD_IS_ACCEPT_TEMPLATE()

    #define GST_PAD_IS_ACCEPT_TEMPLATE(pad)    (GST_OBJECT_FLAG_IS_SET (pad, GST_PAD_FLAG_ACCEPT_TEMPLATE))

Check if the pad's accept caps operation will use the pad template caps. The default accept-caps will do a query caps to get the caps, which might be querying downstream causing unnecessary overhead. It is recommended to implement a proper accept-caps query handler or to use this flag to prevent recursive accept-caps handling.

#### Parameters

pad | a GstPad |

Since: 1.6

### GST_PAD_SET_ACCEPT_TEMPLATE()

    #define GST_PAD_SET_ACCEPT_TEMPLATE(pad)   (GST_OBJECT_FLAG_SET (pad, GST_PAD_FLAG_ACCEPT_TEMPLATE))

Set `pad` to by default use the pad template caps to compare with the accept caps instead of using a caps query result.

#### Parameters

pad | a GstPad |

Since: 1.6

### GST_PAD_UNSET_ACCEPT_TEMPLATE()

    #define GST_PAD_UNSET_ACCEPT_TEMPLATE(pad) (GST_OBJECT_FLAG_UNSET (pad, GST_PAD_FLAG_ACCEPT_TEMPLATE))

Unset accept template flag.

#### Parameters

pad | a GstPad |

Since: 1.6

## Types and Values

### struct GstPad

    struct GstPad {
      gpointer                       element_private;

      GstPadTemplate                *padtemplate;

      GstPadDirection                direction;
    };

The GstPad structure. Use the functions to update the variables.

#### Members

gpointer `element_private`; | private data owned by the parent element |
GstPadTemplate *`padtemplate`; | padtemplate for this pad |
GstPadDirection `direction`; | the direction of the pad, cannot change after creating the pad. |

### enum GstPadDirection

The direction of a pad.

#### Members

GST_PAD_UNKNOWN | direction is unknown. |
GST_PAD_SRC | the pad is a source pad. |
GST_PAD_SINK | the pad is a sink pad. |

### enum GstPadFlags

Pad state flags

#### Members

GST_PAD_FLAG_BLOCKED | is dataflow on a pad blocked |
GST_PAD_FLAG_FLUSHING | is pad flushing |
GST_PAD_FLAG_EOS | is pad in EOS state |
GST_PAD_FLAG_BLOCKING | is pad currently blocking on a buffer or event |
GST_PAD_FLAG_NEED_PARENT | ensure that there is a parent object before calling into the pad callbacks. |
GST_PAD_FLAG_NEED_RECONFIGURE | the pad should be reconfigured/renegotiated. The flag has to be unset manually after reconfiguration happened. |
GST_PAD_FLAG_PENDING_EVENTS | the pad has pending events |
GST_PAD_FLAG_FIXED_CAPS | the pad is using fixed caps. This means that once the caps are set on the pad, the default caps query function will only return those caps. |
GST_PAD_FLAG_PROXY_CAPS | the default event and query handler will forward all events and queries to the internally linked pads instead of discarding them. |
GST_PAD_FLAG_PROXY_ALLOCATION | the default query handler will forward allocation queries to the internally linked pads instead of discarding them. |
GST_PAD_FLAG_PROXY_SCHEDULING | the default query handler will forward scheduling queries to the internally linked pads instead of discarding them. |
GST_PAD_FLAG_ACCEPT_INTERSECT | the default accept-caps handler will check it the caps intersect the query-caps result instead of checking for a subset. This is interesting for parsers that can accept incompletely specified caps. |
GST_PAD_FLAG_ACCEPT_TEMPLATE | the default accept-caps handler will use the template pad caps instead of query caps to compare with the accept caps. Use this in combination with `GST_PAD_FLAG_ACCEPT_INTERSECT`. (Since: 1.6) |
GST_PAD_FLAG_LAST | offset to define more flags |

### enum GstPadLinkReturn

Result values from gst_pad_link and friends.

#### Members

GST_PAD_LINK_OK | link succeeded |
GST_PAD_LINK_WRONG_HIERARCHY | pads have no common grandparent |
GST_PAD_LINK_WAS_LINKED | pad was already linked |
GST_PAD_LINK_WRONG_DIRECTION | pads have wrong direction |
GST_PAD_LINK_NOFORMAT | pads do not have common format |
GST_PAD_LINK_NOSCHED | pads cannot cooperate in scheduling |
GST_PAD_LINK_REFUSED | refused for some reason |

### enum GstPadLinkCheck

The amount of checking to be done when linking pads. `GST_PAD_LINK_CHECK_CAPS` and `GST_PAD_LINK_CHECK_TEMPLATE_CAPS` are mutually exclusive. If both are specified, expensive but safe `GST_PAD_LINK_CHECK_CAPS` are performed.

> Only disable some of the checks if you are 100% certain you know the link will not fail because of hierarchy/caps compatibility failures. If uncertain, use the default checks (`GST_PAD_LINK_CHECK_DEFAULT`) or the regular methods for linking the pads.

#### Members

GST_PAD_LINK_CHECK_NOTHING | Don't check hierarchy or caps compatibility. |
GST_PAD_LINK_CHECK_HIERARCHY | Check the pads have same parents/grandparents. Could be omitted if it is already known that the two elements that own the pads are in the same bin. |
GST_PAD_LINK_CHECK_TEMPLATE_CAPS | Check if the pads are compatible by using their template caps. This is much faster than `GST_PAD_LINK_CHECK_CAPS` , but would be unsafe e.g. if one pad has `GST_CAPS_ANY`. |
GST_PAD_LINK_CHECK_CAPS | Check if the pads are compatible by comparing the caps returned by `gst_pad_query_caps()`. |
GST_PAD_LINK_CHECK_NO_RECONFIGURE | Disables pushing a reconfigure event when pads are linked. |
GST_PAD_LINK_CHECK_DEFAULT | The default checks done when linking pads (i.e. the ones used by `gst_pad_link()`). |

### enum GstFlowReturn

The result of passing data to a pad.

Note that the custom return values should not be exposed outside of the element scope.

#### Members

GST_FLOW_CUSTOM_SUCCESS_2 | Pre-defined custom success code. |
GST_FLOW_CUSTOM_SUCCESS_1 | Pre-defined custom success code (define your custom success code to this to avoid compiler warnings). |
GST_FLOW_CUSTOM_SUCCESS | Elements can use values starting from this (and higher) to define custom success codes. |
GST_FLOW_OK | Data passing was ok. |
GST_FLOW_NOT_LINKED | Pad is not linked. |
GST_FLOW_FLUSHING | Pad is flushing. |
GST_FLOW_EOS | Pad is EOS. |
GST_FLOW_NOT_NEGOTIATED | Pad is not negotiated. |
GST_FLOW_ERROR | Some (fatal) error occurred. Element generating this error should post an error message with more details. |
GST_FLOW_NOT_SUPPORTED | This operation is not supported. |
GST_FLOW_CUSTOM_ERROR | Elements can use values starting from this (and lower) to define custom error codes. |
GST_FLOW_CUSTOM_ERROR_1 | Pre-defined custom error code (define your custom error code to this to avoid compiler warnings). |
GST_FLOW_CUSTOM_ERROR_2 | Pre-defined custom error code. |

### enum GstPadMode

The status of a GstPad. After activating a pad, which usually happens when the parent element goes from READY to PAUSED, the GstPadMode defines if the pad operates in push or pull mode.

#### Members

GST_PAD_MODE_NONE | Pad will not handle dataflow |
GST_PAD_MODE_PUSH | Pad handles dataflow in downstream push mode |
GST_PAD_MODE_PULL | Pad handles dataflow in upstream pull mode |

### enum GstPadProbeReturn

Different return values for the GstPadProbeCallback.

#### Members

GST_PAD_PROBE_DROP | drop data in data probes. For push mode this means that the data item is not sent downstream. For pull mode, it means that the data item is not passed upstream. In both cases, no other probes are called for this item and `GST_FLOW_OK` or `TRUE` is returned to the caller. |
GST_PAD_PROBE_OK | normal probe return value. This leaves the probe in place, and defers decisions about dropping or passing data to other probes, if any. If there are no other probes, the default behaviour for the probe type applies ('block' for blocking probes, and 'pass' for non-blocking probes). |
GST_PAD_PROBE_REMOVE | remove this probe. |
GST_PAD_PROBE_PASS | pass the data item in the block probe and block on the next item. |
GST_PAD_PROBE_HANDLED | Data has been handled in the probe and will not be forwarded further. For events and buffers this is the same behaviour as `GST_PAD_PROBE_DROP` (except that in this case you need to unref the buffer or event yourself). For queries it will also return `TRUE` to the caller. The probe can also modify the GstFlowReturn value by using the `GST_PAD_PROBE_INFO_FLOW_RETURN()` accessor. Note that the resulting query must contain valid entries. Since: 1.6 |

### enum GstPadProbeType

The different probing types that can occur. When either one of `GST_PAD_PROBE_TYPE_IDLE` or `GST_PAD_PROBE_TYPE_BLOCK` is used, the probe will be a blocking probe.

#### Members

GST_PAD_PROBE_TYPE_INVALID | invalid probe type |
GST_PAD_PROBE_TYPE_IDLE | probe idle pads and block while the callback is called |
GST_PAD_PROBE_TYPE_BLOCK | probe and block pads |
GST_PAD_PROBE_TYPE_BUFFER | probe buffers |
GST_PAD_PROBE_TYPE_BUFFER_LIST | probe buffer lists |
GST_PAD_PROBE_TYPE_EVENT_DOWNSTREAM | probe downstream events |
GST_PAD_PROBE_TYPE_EVENT_UPSTREAM | probe upstream events |
GST_PAD_PROBE_TYPE_EVENT_FLUSH | probe flush events. This probe has to be explicitly enabled and is not included in the @`GST_PAD_PROBE_TYPE_EVENT_DOWNSTREAM` or @`GST_PAD_PROBE_TYPE_EVENT_UPSTREAM` probe types. |
GST_PAD_PROBE_TYPE_QUERY_DOWNSTREAM | probe downstream queries |
GST_PAD_PROBE_TYPE_QUERY_UPSTREAM | probe upstream queries |
GST_PAD_PROBE_TYPE_PUSH | probe push |
GST_PAD_PROBE_TYPE_PULL | probe pull |
GST_PAD_PROBE_TYPE_BLOCKING | probe and block at the next opportunity, at data flow or when idle |
GST_PAD_PROBE_TYPE_DATA_DOWNSTREAM | probe downstream data (buffers, buffer lists, and events) |
GST_PAD_PROBE_TYPE_DATA_UPSTREAM | probe upstream data (events) |
GST_PAD_PROBE_TYPE_DATA_BOTH | probe upstream and downstream data (buffers, buffer lists, and events) |
GST_PAD_PROBE_TYPE_BLOCK_DOWNSTREAM | probe and block downstream data (buffers, buffer lists, and events) |
GST_PAD_PROBE_TYPE_BLOCK_UPSTREAM | probe and block upstream data (events) |
GST_PAD_PROBE_TYPE_EVENT_BOTH | probe upstream and downstream events |
GST_PAD_PROBE_TYPE_QUERY_BOTH | probe upstream and downstream queries |
GST_PAD_PROBE_TYPE_ALL_BOTH | probe upstream events and queries and downstream buffers, buffer lists, events and queries |
GST_PAD_PROBE_TYPE_SCHEDULING | probe push and pull |

### struct GstPadProbeInfo

    struct GstPadProbeInfo {
      GstPadProbeType type;
      gulong id;
      gpointer data;
      guint64 offset;
      guint size;
    };

Info passed in the GstPadProbeCallback.

#### Members

GstPadProbeType `type`; | the current probe type |
gulong `id`; | the id of the probe |
gpointer `data`; | type specific data, check the `type` field to know the datatype. This field can be `NULL`. | [allow-none]
guint64 `offset`; | offset of pull probe, this field is valid when `type` contains GST_PAD_PROBE_TYPE_PULL |
guint `size`; | size of pull probe, this field is valid when `type` contains GST_PAD_PROBE_TYPE_PULL |

## Property Details

### The `“caps”` property

      “caps”                     GstCaps *

The capabilities of the pad.

Flags: Read

### The `“direction”` property

      “direction”                GstPadDirection

The direction of the pad.

Flags: Read / Write / Construct Only

Default value: GST_PAD_UNKNOWN

### The `“offset”` property

      “offset”                   gint64

The offset that will be applied to the running time of the pad.

Flags: Read / Write

Allowed values: >= 0

Default value: 0

Since: 1.6

### The `“template”` property

      “template”                 GstPadTemplate *

The GstPadTemplate of this pad.

Flags: Read / Write

## Signal Details

### The `“linked”` signal

    void
    user_function (GstPad  *pad,
                   GstPad  *peer,
                   gpointer user_data)

Signals that a pad has been linked to the peer pad.

#### Parameters

pad | the pad that emitted the signal |
peer | the peer pad that has been connected |
user_data | user data set when the signal handler was connected. |

Flags: Run Last

### The `“unlinked”` signal

    void
    user_function (GstPad  *pad,
                   GstPad  *peer,
                   gpointer user_data)

Signals that a pad has been unlinked from the peer pad.

#### Parameters

pad | the pad that emitted the signal |
peer | the peer pad that has been disconnected |
user_data | user data set when the signal handler was connected. |

Flags: Run Last

## See Also

GstPadTemplate, GstElement, GstEvent, GstQuery, GstBuffer