! Configuration File for keepalived
! This example demonstrates status_code, a component of LVS configuration.

global_defs {
   notification_email {
     acassen
   }
   notification_email_from Alexandre.Cassen@firewall.loc
   smtp_server 192.168.200.1
   smtp_connect_timeout 30
   router_id LVS_DEVEL
}

virtual_server 192.168.200.100 443 {
    delay_loop 6
    lb_algo rr
    lb_kind NAT
    persistence_timeout 50
    protocol TCP

    real_server 192.168.201.100 443 {
        weight 1
        SSL_GET {
            url {
              path /
              status_code 200-299 400-499 503 505 # Can specify a HTTP status_code or a section separated by '-' or both
            }
            url {
              path /mrtg/
              digest 9b3a0c85a887a256d6939da88aabd8cd
              status_code 200  # Can mix digest and status_code
            }
            connect_timeout 3
            retry 3
            delay_before_retry 3
        }
    }
}
