Prev |  | Next

## 7. CAC smartcard redirection

Spice has a dedicated channel for smartcard redirection, using libcacard, which currently supports limited CAC emulation.

You may consider redirecting your USB card reader instead. This is easier to setup but will prevent from sharing the smartcard with both the client and the remote simultaneously.

libcacard is actually emulating a simple CAC card, sharing the card and its certificates. It can successfully be used with the coolkey PKCS#11 module.

### 7.1. Configuration

Using virt-manager. In the hardware details, click on "Add Hardware", then select "Smartcard". Add a "passthrough" device type.

Using libvirt. Setup a "passthrough" smartcard of type "spicevmc" on a CCID controller:

    <controller type='ccid' index='0'/>
    <smartcard mode='passthrough' type='spicevmc'>
      <address type='ccid' controller='0' slot='0'/>
    </smartcard>

Using QEMU. With the qemu command line, you must add a USB CCID device, and a "ccid-card-passthru" associated with a "spicevmc" channel with the name "smartcard":

    -device usb-ccid -chardev spicevmc,name=smartcard,id=ccid -device ccid-card-passthru,chardev=ccid

### 7.2. Client

In order for the client certificates to be shared with the remote, you need a NSS database configured to access the smartcard. Please look for instructions on coolkey or NSS setup and make sure you certficates can be listed with certutil.

### Note

Most Spice clients disable smartcard support by default, and need `--spice-smartcard` or similar configuration.

Prev |  | Next
| Home |