| # Copy setup

Index XSane mode: Viewer mode Save mode Copy mode Multipage mode Fax mode E-mail mode Gimp plugin Scan options Medium selection Color management Color correction: Gamma correction Brightness Contrast Threshold RGB default Negative Autoenhancement Default Restore Store Histogram window Pipette functions Standard options window Advanced options window Preview: Pipette white Pipette gray Pipette black Unzoom Zoom out Zoom in Undo zoom Autoselect scanarea Autoraise scanarea Select visible area Delete preview cache Preset area Rotation Aspect ratio RGB values Select scanarea Move scanarea Batch scan: Empty batch list Open batch list Save batch list Add area to list Remove selection Rename selection Rotate image Mirror image Setup: Copy setup Display setup Enhancement setup Fax setup Filetype setup E-mail setup Saving setup Color management setup | You open the setup window via the menu preferences/setup in the main window of xsane. #### Name: Define the name for the following printer definition. #### Command: Enter the command with which you print files. The command has to read the file from the standard input. If you use the bsd printing system this is "lpr", if you use the old printing system this should be "lp". When you use KDE then you should try "kprinter --stdin". #### Copy number option: Enter the option of the printer command with wich the number of copies are specified. If you use the bsd printing system (lpr) or kprinter this is "-#", if you use the old printing system (lp) this should be "-n". This option is the last option passed to the printerrcommand so if you specify a ";#" then the option is ignored. #### Resolution: With resolution you specify the resolution that shall be used for printing. It is not always necessary to set this value to the resolution of the printer. Especially in grayscale and color mode it normally is good to set this value to the half or the quarter of the printer resolution because the printer needs a greater resolution to do the dithering. This value does not effect a change of the image size, the image size only depends on the given zoom factor. #### Print area (width, height, left offset, bottom offset): Each printer has it's own area size and position where it is able to print. #### Printer gamma values: Addidtional gamma value for printing. The Printer gamma value is used for grayscale and as common value for color mode. The red, green and blue values are for color correction. #### Printer ICM profile: Select the printer ICM profile. This profile is used for proofing and for printing! #### Embed scanner ICM profile as CSA: Embed the scanner ICM profile into the posctscript file (as Color Space Array). When you have a postscript printer then you should enable this option. In this case the scanner does the color transformation. When disabled the color transformation is done by xsane. #### Embed printer ICM profile as CRD: Embed the printer ICM profile into the posctscript file (as Color Rendering Device). When you have a postscript printer then you should try to disable this option - a good postscript printer should know its own CRD. When you use ghostscript or an other rendering software then it is possible that the rendering software does not know the ICM profile of the printer. In this case (or when your postscript printer does not know its CRD) you have to enable this option. When enabled then the printer ICM profile is embedded into the postscript file. When disabled the color transformation is done by xsane. When embed scanner ICM profile as CSA is disabled then embed printer ICM profile as CRD has no function because the color transformation is done by xsane. #### Apply black point compensation: When transformation is done then apply black point compensation. When CSA/CRD is embedded then prepare embedded data for black point compensation.

> Author: Oliver Rauch