## API break replacements API break replacements — List of deprecated methods, types and symbols. |

## Types and Values

#define | MM_MODEM_BAND_U2100
#define | MM_MODEM_BAND_U1900
#define | MM_MODEM_BAND_U1800
#define | MM_MODEM_BAND_U17IV
#define | MM_MODEM_BAND_U850
#define | MM_MODEM_BAND_U800
#define | MM_MODEM_BAND_U2600
#define | MM_MODEM_BAND_U900
#define | MM_MODEM_BAND_U17IX
#define | MM_MODEM_BAND_EUTRAN_I
#define | MM_MODEM_BAND_EUTRAN_II
#define | MM_MODEM_BAND_EUTRAN_III
#define | MM_MODEM_BAND_EUTRAN_IV
#define | MM_MODEM_BAND_EUTRAN_V
#define | MM_MODEM_BAND_EUTRAN_VI
#define | MM_MODEM_BAND_EUTRAN_VII
#define | MM_MODEM_BAND_EUTRAN_VIII
#define | MM_MODEM_BAND_EUTRAN_IX
#define | MM_MODEM_BAND_EUTRAN_X
#define | MM_MODEM_BAND_EUTRAN_XI
#define | MM_MODEM_BAND_EUTRAN_XII
#define | MM_MODEM_BAND_EUTRAN_XIII
#define | MM_MODEM_BAND_EUTRAN_XIV
#define | MM_MODEM_BAND_EUTRAN_XVII
#define | MM_MODEM_BAND_EUTRAN_XVIII
#define | MM_MODEM_BAND_EUTRAN_XIX
#define | MM_MODEM_BAND_EUTRAN_XX
#define | MM_MODEM_BAND_EUTRAN_XXI
#define | MM_MODEM_BAND_EUTRAN_XXII
#define | MM_MODEM_BAND_EUTRAN_XXIII
#define | MM_MODEM_BAND_EUTRAN_XXIV
#define | MM_MODEM_BAND_EUTRAN_XXV
#define | MM_MODEM_BAND_EUTRAN_XXVI
#define | MM_MODEM_BAND_EUTRAN_XXXIII
#define | MM_MODEM_BAND_EUTRAN_XXXIV
#define | MM_MODEM_BAND_EUTRAN_XXXV
#define | MM_MODEM_BAND_EUTRAN_XXXVI
#define | MM_MODEM_BAND_EUTRAN_XXXVII
#define | MM_MODEM_BAND_EUTRAN_XXXVIII
#define | MM_MODEM_BAND_EUTRAN_XXXIX
#define | MM_MODEM_BAND_EUTRAN_XL
#define | MM_MODEM_BAND_EUTRAN_XLI
#define | MM_MODEM_BAND_EUTRAN_XLII
#define | MM_MODEM_BAND_EUTRAN_XLIII
#define | MM_MODEM_BAND_EUTRAN_XLIV
#define | MM_MODEM_BAND_CDMA_BC0_CELLULAR_800
#define | MM_MODEM_BAND_CDMA_BC1_PCS_1900
#define | MM_MODEM_BAND_CDMA_BC2_TACS
#define | MM_MODEM_BAND_CDMA_BC3_JTACS
#define | MM_MODEM_BAND_CDMA_BC4_KOREAN_PCS
#define | MM_MODEM_BAND_CDMA_BC5_NMT450
#define | MM_MODEM_BAND_CDMA_BC6_IMT2000
#define | MM_MODEM_BAND_CDMA_BC7_CELLULAR_700
#define | MM_MODEM_BAND_CDMA_BC8_1800
#define | MM_MODEM_BAND_CDMA_BC9_900
#define | MM_MODEM_BAND_CDMA_BC10_SECONDARY_800
#define | MM_MODEM_BAND_CDMA_BC11_PAMR_400
#define | MM_MODEM_BAND_CDMA_BC12_PAMR_800
#define | MM_MODEM_BAND_CDMA_BC13_IMT2000_2500
#define | MM_MODEM_BAND_CDMA_BC14_PCS2_1900
#define | MM_MODEM_BAND_CDMA_BC15_AWS
#define | MM_MODEM_BAND_CDMA_BC16_US_2500
#define | MM_MODEM_BAND_CDMA_BC17_US_FLO_2500
#define | MM_MODEM_BAND_CDMA_BC18_US_PS_700
#define | MM_MODEM_BAND_CDMA_BC19_US_LOWER_700
#define | MM_MODEM_LOCATION_SOURCE_AGPS
#define | MM_MODEM_CAPABILITY_LTE_ADVANCED
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_ACTIVATION_REJECTED_BY_GGSN_OR_GW
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_ACTIVATION_REJECTED_UNSPECIFIED
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_AND_NON_GPRS_SERVICES_NOT_ALLOWED
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_CONDITIONAL_IE_ERROR
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_CONGESTION
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_FEATURE_NOT_SUPPORTED
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_IE_NOT_IMPLEMENTED
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_ILLEGAL_ME
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_ILLEGAL_MS
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_IMSI_UNKNOWN_IN_HLR
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_IMSI_UNKNOWN_IN_VLR
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_INSUFFICIENT_RESOURCES
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_INVALID_MOBILE_CLASS
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_LAST_PDN_DISCONNECTION_NOT_ALLOWED
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_LAST_PDN_DISCONNECTION_NOT_ALLOWED_LEGACY
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_LOCATION_NOT_ALLOWED
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_MANDATORY_IE_ERROR
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_MAXIMUM_NUMBER_OF_PDP_CONTEXTS_REACHED
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_MISSING_OR_UNKNOWN_APN
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_NETWORK_FAILURE
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_NOT_AUTHORIZED_FOR_CSG
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_NO_CELLS_IN_LOCATION_AREA
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_OPERATOR_DETERMINED_BARRING
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_PDP_AUTH_FAILURE
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_PDP_CONTEXT_WITHOUT_TFT_ALREADY_ACTIVATED
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_PLMN_NOT_ALLOWED
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_REQUESTED_APN_NOT_SUPPORTED
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_REQUEST_REJECTED_BCM_VIOLATION
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_ROAMING_NOT_ALLOWED
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_SEMANTICALLY_INCORRECT_MESSAGE
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_SEMANTIC_ERRORS_IN_PACKET_FILTER
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_SEMANTIC_ERROR_IN_TFT_OPERATION
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_SERVICE_NOT_ALLOWED
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_SERVICE_OPTION_NOT_SUBSCRIBED
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_SERVICE_OPTION_NOT_SUPPORTED
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_SERVICE_OPTION_OUT_OF_ORDER
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_SYNTACTICAL_ERROR_IN_PACKET_FILTER
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_SYNTACTICAL_ERROR_IN_TFT_OPERATION
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_UNKNOWN_PDP_ADDRESS_OR_TYPE
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_UNKNOWN_PDP_CONTEXT
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_UNSPECIFIED_PROTOCOL_ERROR
#define | MM_MOBILE_EQUIPMENT_ERROR_GPRS_USER_AUTHENTICATION_FAILED

## Description

These compatibility types and methods are flagged as deprecated and therefore shouldn't be used in newly written code. They are provided to avoid unnecessary API/ABI breaks.

## Functions

## Types and Values

### MM_MODEM_BAND_U2100

    #define MM_MODEM_BAND_U2100 ((MMModemBandDeprecated)MM_MODEM_BAND_UTRAN_1)

`MM_MODEM_BAND_U2100` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_UTRAN_1 instead.

WCDMA 2100 MHz (UTRAN band 1).

Since: 1.0

### MM_MODEM_BAND_U1900

    #define MM_MODEM_BAND_U1900 ((MMModemBandDeprecated)MM_MODEM_BAND_UTRAN_2)

`MM_MODEM_BAND_U1900` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_UTRAN_2 instead.

WCDMA 1900 MHz (UTRAN band 2).

Since: 1.0

### MM_MODEM_BAND_U1800

    #define MM_MODEM_BAND_U1800 ((MMModemBandDeprecated)MM_MODEM_BAND_UTRAN_3)

`MM_MODEM_BAND_U1800` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_UTRAN_3 instead.

WCDMA 1800 MHz (UTRAN band 3).

Since: 1.0

### MM_MODEM_BAND_U17IV

    #define MM_MODEM_BAND_U17IV ((MMModemBandDeprecated)MM_MODEM_BAND_UTRAN_4)

`MM_MODEM_BAND_U17IV` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_UTRAN_4 instead.

AWS 1700/2100 MHz (UTRAN band 4).

Since: 1.0

### MM_MODEM_BAND_U850

    #define MM_MODEM_BAND_U850 ((MMModemBandDeprecated)MM_MODEM_BAND_UTRAN_5)

`MM_MODEM_BAND_U850` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_UTRAN_5 instead.

UMTS 850 MHz (UTRAN band 5).

Since: 1.0

### MM_MODEM_BAND_U800

    #define MM_MODEM_BAND_U800 ((MMModemBandDeprecated)MM_MODEM_BAND_UTRAN_6)

`MM_MODEM_BAND_U800` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_UTRAN_6 instead.

UMTS 800 MHz (UTRAN band 6).

Since: 1.0

### MM_MODEM_BAND_U2600

    #define MM_MODEM_BAND_U2600 ((MMModemBandDeprecated)MM_MODEM_BAND_UTRAN_7)

`MM_MODEM_BAND_U2600` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_UTRAN_7 instead.

UMTS 2600 MHz (UTRAN band 7).

Since: 1.0

### MM_MODEM_BAND_U900

    #define MM_MODEM_BAND_U900 ((MMModemBandDeprecated)MM_MODEM_BAND_UTRAN_8)

`MM_MODEM_BAND_U900` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_UTRAN_8 instead.

UMTS 900 MHz (UTRAN band 8).

Since: 1.0

### MM_MODEM_BAND_U17IX

    #define MM_MODEM_BAND_U17IX ((MMModemBandDeprecated)MM_MODEM_BAND_UTRAN_9)

`MM_MODEM_BAND_U17IX` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_UTRAN_9 instead.

UMTS 1700 MHz (UTRAN band 9).

Since: 1.0

### MM_MODEM_BAND_EUTRAN_I

    #define MM_MODEM_BAND_EUTRAN_I ((MMModemBandDeprecated)MM_MODEM_BAND_EUTRAN_1)

`MM_MODEM_BAND_EUTRAN_I` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_EUTRAN_1 instead.

E-UTRAN band 1.

Since: 1.0

### MM_MODEM_BAND_EUTRAN_II

    #define MM_MODEM_BAND_EUTRAN_II ((MMModemBandDeprecated)MM_MODEM_BAND_EUTRAN_2)

`MM_MODEM_BAND_EUTRAN_II` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_EUTRAN_2 instead.

E-UTRAN band 2.

Since: 1.0

### MM_MODEM_BAND_EUTRAN_III

    #define MM_MODEM_BAND_EUTRAN_III ((MMModemBandDeprecated)MM_MODEM_BAND_EUTRAN_3)

`MM_MODEM_BAND_EUTRAN_III` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_EUTRAN_3 instead.

E-UTRAN band 3.

Since: 1.0

### MM_MODEM_BAND_EUTRAN_IV

    #define MM_MODEM_BAND_EUTRAN_IV ((MMModemBandDeprecated)MM_MODEM_BAND_EUTRAN_4)

`MM_MODEM_BAND_EUTRAN_IV` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_EUTRAN_4 instead.

E-UTRAN band 4.

Since: 1.0

### MM_MODEM_BAND_EUTRAN_V

    #define MM_MODEM_BAND_EUTRAN_V ((MMModemBandDeprecated)MM_MODEM_BAND_EUTRAN_5)

`MM_MODEM_BAND_EUTRAN_V` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_EUTRAN_5 instead.

E-UTRAN band 5.

Since: 1.0

### MM_MODEM_BAND_EUTRAN_VI

    #define MM_MODEM_BAND_EUTRAN_VI ((MMModemBandDeprecated)MM_MODEM_BAND_EUTRAN_6)

`MM_MODEM_BAND_EUTRAN_VI` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_EUTRAN_6 instead.

E-UTRAN band 6.

Since: 1.0

### MM_MODEM_BAND_EUTRAN_VII

    #define MM_MODEM_BAND_EUTRAN_VII ((MMModemBandDeprecated)MM_MODEM_BAND_EUTRAN_7)

`MM_MODEM_BAND_EUTRAN_VII` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_EUTRAN_7 instead.

E-UTRAN band 7.

Since: 1.0

### MM_MODEM_BAND_EUTRAN_VIII

    #define MM_MODEM_BAND_EUTRAN_VIII ((MMModemBandDeprecated)MM_MODEM_BAND_EUTRAN_8)

`MM_MODEM_BAND_EUTRAN_VIII` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_EUTRAN_8 instead.

E-UTRAN band 8.

Since: 1.0

### MM_MODEM_BAND_EUTRAN_IX

    #define MM_MODEM_BAND_EUTRAN_IX ((MMModemBandDeprecated)MM_MODEM_BAND_EUTRAN_9)

`MM_MODEM_BAND_EUTRAN_IX` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_EUTRAN_9 instead.

E-UTRAN band 9.

Since: 1.0

### MM_MODEM_BAND_EUTRAN_X

    #define MM_MODEM_BAND_EUTRAN_X ((MMModemBandDeprecated)MM_MODEM_BAND_EUTRAN_10)

`MM_MODEM_BAND_EUTRAN_X` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_EUTRAN_10 instead.

E-UTRAN band 10.

Since: 1.0

### MM_MODEM_BAND_EUTRAN_XI

    #define MM_MODEM_BAND_EUTRAN_XI ((MMModemBandDeprecated)MM_MODEM_BAND_EUTRAN_11)

`MM_MODEM_BAND_EUTRAN_XI` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_EUTRAN_11 instead.

E-UTRAN band 11.

Since: 1.0

### MM_MODEM_BAND_EUTRAN_XII

    #define MM_MODEM_BAND_EUTRAN_XII ((MMModemBandDeprecated)MM_MODEM_BAND_EUTRAN_12)

`MM_MODEM_BAND_EUTRAN_XII` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_EUTRAN_12 instead.

E-UTRAN band 12.

Since: 1.0

### MM_MODEM_BAND_EUTRAN_XIII

    #define MM_MODEM_BAND_EUTRAN_XIII ((MMModemBandDeprecated)MM_MODEM_BAND_EUTRAN_13)

`MM_MODEM_BAND_EUTRAN_XIII` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_EUTRAN_13 instead.

E-UTRAN band 13.

Since: 1.0

### MM_MODEM_BAND_EUTRAN_XIV

    #define MM_MODEM_BAND_EUTRAN_XIV ((MMModemBandDeprecated)MM_MODEM_BAND_EUTRAN_14)

`MM_MODEM_BAND_EUTRAN_XIV` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_EUTRAN_14 instead.

E-UTRAN band 14.

Since: 1.0

### MM_MODEM_BAND_EUTRAN_XVII

    #define MM_MODEM_BAND_EUTRAN_XVII ((MMModemBandDeprecated)MM_MODEM_BAND_EUTRAN_17)

`MM_MODEM_BAND_EUTRAN_XVII` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_EUTRAN_17 instead.

E-UTRAN band 17.

Since: 1.0

### MM_MODEM_BAND_EUTRAN_XVIII

    #define MM_MODEM_BAND_EUTRAN_XVIII ((MMModemBandDeprecated)MM_MODEM_BAND_EUTRAN_18)

`MM_MODEM_BAND_EUTRAN_XVIII` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_EUTRAN_18 instead.

E-UTRAN band 18.

Since: 1.0

### MM_MODEM_BAND_EUTRAN_XIX

    #define MM_MODEM_BAND_EUTRAN_XIX ((MMModemBandDeprecated)MM_MODEM_BAND_EUTRAN_19)

`MM_MODEM_BAND_EUTRAN_XIX` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_EUTRAN_19 instead.

E-UTRAN band 19.

Since: 1.0

### MM_MODEM_BAND_EUTRAN_XX

    #define MM_MODEM_BAND_EUTRAN_XX ((MMModemBandDeprecated)MM_MODEM_BAND_EUTRAN_20)

`MM_MODEM_BAND_EUTRAN_XX` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_EUTRAN_20 instead.

E-UTRAN band 20.

Since: 1.0

### MM_MODEM_BAND_EUTRAN_XXI

    #define MM_MODEM_BAND_EUTRAN_XXI ((MMModemBandDeprecated)MM_MODEM_BAND_EUTRAN_21)

`MM_MODEM_BAND_EUTRAN_XXI` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_EUTRAN_21 instead.

E-UTRAN band 21.

Since: 1.0

### MM_MODEM_BAND_EUTRAN_XXII

    #define MM_MODEM_BAND_EUTRAN_XXII ((MMModemBandDeprecated)MM_MODEM_BAND_EUTRAN_22)

`MM_MODEM_BAND_EUTRAN_XXII` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_EUTRAN_22 instead.

E-UTRAN band 22.

Since: 1.0

### MM_MODEM_BAND_EUTRAN_XXIII

    #define MM_MODEM_BAND_EUTRAN_XXIII ((MMModemBandDeprecated)MM_MODEM_BAND_EUTRAN_23)

`MM_MODEM_BAND_EUTRAN_XXIII` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_EUTRAN_23 instead.

E-UTRAN band 23.

Since: 1.0

### MM_MODEM_BAND_EUTRAN_XXIV

    #define MM_MODEM_BAND_EUTRAN_XXIV ((MMModemBandDeprecated)MM_MODEM_BAND_EUTRAN_24)

`MM_MODEM_BAND_EUTRAN_XXIV` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_EUTRAN_24 instead.

E-UTRAN band 24.

Since: 1.0

### MM_MODEM_BAND_EUTRAN_XXV

    #define MM_MODEM_BAND_EUTRAN_XXV ((MMModemBandDeprecated)MM_MODEM_BAND_EUTRAN_25)

`MM_MODEM_BAND_EUTRAN_XXV` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_EUTRAN_25 instead.

E-UTRAN band 25.

Since: 1.0

### MM_MODEM_BAND_EUTRAN_XXVI

    #define MM_MODEM_BAND_EUTRAN_XXVI ((MMModemBandDeprecated)MM_MODEM_BAND_EUTRAN_26)

`MM_MODEM_BAND_EUTRAN_XXVI` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_EUTRAN_26 instead.

E-UTRAN band 26.

Since: 1.0

### MM_MODEM_BAND_EUTRAN_XXXIII

    #define MM_MODEM_BAND_EUTRAN_XXXIII ((MMModemBandDeprecated)MM_MODEM_BAND_EUTRAN_33)

`MM_MODEM_BAND_EUTRAN_XXXIII` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_EUTRAN_33 instead.

E-UTRAN band 33.

Since: 1.0

### MM_MODEM_BAND_EUTRAN_XXXIV

    #define MM_MODEM_BAND_EUTRAN_XXXIV ((MMModemBandDeprecated)MM_MODEM_BAND_EUTRAN_34)

`MM_MODEM_BAND_EUTRAN_XXXIV` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_EUTRAN_34 instead.

E-UTRAN band 34.

Since: 1.0

### MM_MODEM_BAND_EUTRAN_XXXV

    #define MM_MODEM_BAND_EUTRAN_XXXV ((MMModemBandDeprecated)MM_MODEM_BAND_EUTRAN_35)

`MM_MODEM_BAND_EUTRAN_XXXV` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_EUTRAN_35 instead.

E-UTRAN band 35.

Since: 1.0

### MM_MODEM_BAND_EUTRAN_XXXVI

    #define MM_MODEM_BAND_EUTRAN_XXXVI ((MMModemBandDeprecated)MM_MODEM_BAND_EUTRAN_36)

`MM_MODEM_BAND_EUTRAN_XXXVI` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_EUTRAN_36 instead.

E-UTRAN band 36.

Since: 1.0

### MM_MODEM_BAND_EUTRAN_XXXVII

    #define MM_MODEM_BAND_EUTRAN_XXXVII ((MMModemBandDeprecated)MM_MODEM_BAND_EUTRAN_37)

`MM_MODEM_BAND_EUTRAN_XXXVII` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_EUTRAN_37 instead.

E-UTRAN band 37.

Since: 1.0

### MM_MODEM_BAND_EUTRAN_XXXVIII

    #define MM_MODEM_BAND_EUTRAN_XXXVIII ((MMModemBandDeprecated)MM_MODEM_BAND_EUTRAN_38)

`MM_MODEM_BAND_EUTRAN_XXXVIII` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_EUTRAN_38 instead.

E-UTRAN band 38.

Since: 1.0

### MM_MODEM_BAND_EUTRAN_XXXIX

    #define MM_MODEM_BAND_EUTRAN_XXXIX ((MMModemBandDeprecated)MM_MODEM_BAND_EUTRAN_39)

`MM_MODEM_BAND_EUTRAN_XXXIX` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_EUTRAN_39 instead.

E-UTRAN band 39.

Since: 1.0

### MM_MODEM_BAND_EUTRAN_XL

    #define MM_MODEM_BAND_EUTRAN_XL ((MMModemBandDeprecated)MM_MODEM_BAND_EUTRAN_40)

`MM_MODEM_BAND_EUTRAN_XL` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_EUTRAN_40 instead.

E-UTRAN band 40.

Since: 1.0

### MM_MODEM_BAND_EUTRAN_XLI

    #define MM_MODEM_BAND_EUTRAN_XLI ((MMModemBandDeprecated)MM_MODEM_BAND_EUTRAN_41)

`MM_MODEM_BAND_EUTRAN_XLI` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_EUTRAN_41 instead.

E-UTRAN band 41.

Since: 1.0

### MM_MODEM_BAND_EUTRAN_XLII

    #define MM_MODEM_BAND_EUTRAN_XLII ((MMModemBandDeprecated)MM_MODEM_BAND_EUTRAN_42)

`MM_MODEM_BAND_EUTRAN_XLII` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_EUTRAN_42 instead.

E-UTRAN band 42.

Since: 1.0

### MM_MODEM_BAND_EUTRAN_XLIII

    #define MM_MODEM_BAND_EUTRAN_XLIII ((MMModemBandDeprecated)MM_MODEM_BAND_EUTRAN_43)

`MM_MODEM_BAND_EUTRAN_XLIII` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_EUTRAN_43 instead.

E-UTRAN band 43.

Since: 1.0

### MM_MODEM_BAND_EUTRAN_XLIV

    #define MM_MODEM_BAND_EUTRAN_XLIV ((MMModemBandDeprecated)MM_MODEM_BAND_EUTRAN_44)

`MM_MODEM_BAND_EUTRAN_XLIV` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_EUTRAN_44 instead.

E-UTRAN band 44.

Since: 1.4

### MM_MODEM_BAND_CDMA_BC0_CELLULAR_800

    #define MM_MODEM_BAND_CDMA_BC0_CELLULAR_800 ((MMModemBandDeprecated)MM_MODEM_BAND_CDMA_BC0)

`MM_MODEM_BAND_CDMA_BC0_CELLULAR_800` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_CDMA_BC0 instead.

CDMA Band Class 0 (US Cellular 850MHz)

Since: 1.0

### MM_MODEM_BAND_CDMA_BC1_PCS_1900

    #define MM_MODEM_BAND_CDMA_BC1_PCS_1900 ((MMModemBandDeprecated)MM_MODEM_BAND_CDMA_BC1)

`MM_MODEM_BAND_CDMA_BC1_PCS_1900` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_CDMA_BC1 instead.

CDMA Band Class 1 (US PCS 1900MHz).

Since: 1.0

### MM_MODEM_BAND_CDMA_BC2_TACS

    #define MM_MODEM_BAND_CDMA_BC2_TACS ((MMModemBandDeprecated)MM_MODEM_BAND_CDMA_BC2)

`MM_MODEM_BAND_CDMA_BC2_TACS` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_CDMA_BC2 instead.

CDMA Band Class 2 (UK TACS 900MHz).

Since: 1.0

### MM_MODEM_BAND_CDMA_BC3_JTACS

    #define MM_MODEM_BAND_CDMA_BC3_JTACS ((MMModemBandDeprecated)MM_MODEM_BAND_CDMA_BC3)

`MM_MODEM_BAND_CDMA_BC3_JTACS` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_CDMA_BC3 instead.

CDMA Band Class 3 (Japanese TACS).

Since: 1.0

### MM_MODEM_BAND_CDMA_BC4_KOREAN_PCS

    #define MM_MODEM_BAND_CDMA_BC4_KOREAN_PCS ((MMModemBandDeprecated)MM_MODEM_BAND_CDMA_BC4)

`MM_MODEM_BAND_CDMA_BC4_KOREAN_PCS` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_CDMA_BC4 instead.

CDMA Band Class 4 (Korean PCS).

Since: 1.0

### MM_MODEM_BAND_CDMA_BC5_NMT450

    #define MM_MODEM_BAND_CDMA_BC5_NMT450 ((MMModemBandDeprecated)MM_MODEM_BAND_CDMA_BC5)

`MM_MODEM_BAND_CDMA_BC5_NMT450` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_CDMA_BC5 instead.

CDMA Band Class 5 (NMT 450MHz).

Since: 1.0

### MM_MODEM_BAND_CDMA_BC6_IMT2000

    #define MM_MODEM_BAND_CDMA_BC6_IMT2000 ((MMModemBandDeprecated)MM_MODEM_BAND_CDMA_BC6)

`MM_MODEM_BAND_CDMA_BC6_IMT2000` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_CDMA_BC6 instead.

CDMA Band Class 6 (IMT2000 2100MHz).

Since: 1.0

### MM_MODEM_BAND_CDMA_BC7_CELLULAR_700

    #define MM_MODEM_BAND_CDMA_BC7_CELLULAR_700 ((MMModemBandDeprecated)MM_MODEM_BAND_CDMA_BC7)

`MM_MODEM_BAND_CDMA_BC7_CELLULAR_700` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_CDMA_BC7 instead.

CDMA Band Class 7 (Cellular 700MHz).

Since: 1.0

### MM_MODEM_BAND_CDMA_BC8_1800

    #define MM_MODEM_BAND_CDMA_BC8_1800 ((MMModemBandDeprecated)MM_MODEM_BAND_CDMA_BC8)

`MM_MODEM_BAND_CDMA_BC8_1800` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_CDMA_BC8 instead.

CDMA Band Class 8 (1800MHz).

Since: 1.0

### MM_MODEM_BAND_CDMA_BC9_900

    #define MM_MODEM_BAND_CDMA_BC9_900 ((MMModemBandDeprecated)MM_MODEM_BAND_CDMA_BC9)

`MM_MODEM_BAND_CDMA_BC9_900` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_CDMA_BC9 instead.

CDMA Band Class 9 (900MHz).

Since: 1.0

### MM_MODEM_BAND_CDMA_BC10_SECONDARY_800

    #define MM_MODEM_BAND_CDMA_BC10_SECONDARY_800 ((MMModemBandDeprecated)MM_MODEM_BAND_CDMA_BC10)

`MM_MODEM_BAND_CDMA_BC10_SECONDARY_800` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_CDMA_BC10 instead.

CDMA Band Class 10 (US Secondary 800).

Since: 1.0

### MM_MODEM_BAND_CDMA_BC11_PAMR_400

    #define MM_MODEM_BAND_CDMA_BC11_PAMR_400 ((MMModemBandDeprecated)MM_MODEM_BAND_CDMA_BC11)

`MM_MODEM_BAND_CDMA_BC11_PAMR_400` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_CDMA_BC11 instead.

CDMA Band Class 11 (European PAMR 400MHz).

Since: 1.0

### MM_MODEM_BAND_CDMA_BC12_PAMR_800

    #define MM_MODEM_BAND_CDMA_BC12_PAMR_800 ((MMModemBandDeprecated)MM_MODEM_BAND_CDMA_BC12)

`MM_MODEM_BAND_CDMA_BC12_PAMR_800` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_CDMA_BC12 instead.

CDMA Band Class 12 (PAMR 800MHz).

Since: 1.0

### MM_MODEM_BAND_CDMA_BC13_IMT2000_2500

    #define MM_MODEM_BAND_CDMA_BC13_IMT2000_2500 ((MMModemBandDeprecated)MM_MODEM_BAND_CDMA_BC13)

`MM_MODEM_BAND_CDMA_BC13_IMT2000_2500` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_CDMA_BC13 instead.

CDMA Band Class 13 (IMT2000 2500MHz Expansion).

Since: 1.0

### MM_MODEM_BAND_CDMA_BC14_PCS2_1900

    #define MM_MODEM_BAND_CDMA_BC14_PCS2_1900 ((MMModemBandDeprecated)MM_MODEM_BAND_CDMA_BC14)

`MM_MODEM_BAND_CDMA_BC14_PCS2_1900` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_CDMA_BC14 instead.

CDMA Band Class 14 (More US PCS 1900MHz).

Since: 1.0

### MM_MODEM_BAND_CDMA_BC15_AWS

    #define MM_MODEM_BAND_CDMA_BC15_AWS ((MMModemBandDeprecated)MM_MODEM_BAND_CDMA_BC15)

`MM_MODEM_BAND_CDMA_BC15_AWS` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_CDMA_BC15 instead.

CDMA Band Class 15 (AWS 1700MHz).

Since: 1.0

### MM_MODEM_BAND_CDMA_BC16_US_2500

    #define MM_MODEM_BAND_CDMA_BC16_US_2500 ((MMModemBandDeprecated)MM_MODEM_BAND_CDMA_BC16)

`MM_MODEM_BAND_CDMA_BC16_US_2500` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_CDMA_BC16 instead.

CDMA Band Class 16 (US 2500MHz).

Since: 1.0

### MM_MODEM_BAND_CDMA_BC17_US_FLO_2500

    #define MM_MODEM_BAND_CDMA_BC17_US_FLO_2500 ((MMModemBandDeprecated)MM_MODEM_BAND_CDMA_BC17)

`MM_MODEM_BAND_CDMA_BC17_US_FLO_2500` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_CDMA_BC17 instead.

CDMA Band Class 17 (US 2500MHz Forward Link Only).

Since: 1.0

### MM_MODEM_BAND_CDMA_BC18_US_PS_700

    #define MM_MODEM_BAND_CDMA_BC18_US_PS_700 ((MMModemBandDeprecated)MM_MODEM_BAND_CDMA_BC18)

`MM_MODEM_BAND_CDMA_BC18_US_PS_700` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_CDMA_BC18 instead.

CDMA Band Class 18 (US 700MHz Public Safety).

Since: 1.0

### MM_MODEM_BAND_CDMA_BC19_US_LOWER_700

    #define MM_MODEM_BAND_CDMA_BC19_US_LOWER_700 ((MMModemBandDeprecated)MM_MODEM_BAND_CDMA_BC19)

`MM_MODEM_BAND_CDMA_BC19_US_LOWER_700` has been deprecated since version 1.8 and should not be used in newly-written code.

Use MM_MODEM_BAND_CDMA_BC19 instead.

CDMA Band Class 19 (US Lower 700MHz).

Since: 1.0

### MM_MODEM_LOCATION_SOURCE_AGPS

    #define MM_MODEM_LOCATION_SOURCE_AGPS ((MMModemLocationSourceDeprecated)MM_MODEM_LOCATION_SOURCE_AGPS_MSA)

`MM_MODEM_LOCATION_SOURCE_AGPS` has been deprecated since version 1.12.0 and should not be used in newly-written code.

Use MM_MODEM_LOCATION_SOURCE_AGPS_MSA instead.

A-GPS location requested.

Since: 1.6

### MM_MODEM_CAPABILITY_LTE_ADVANCED

    #define MM_MODEM_CAPABILITY_LTE_ADVANCED ((MMModemCapabilityDeprecated)(1 << 4))

`MM_MODEM_CAPABILITY_LTE_ADVANCED` has been deprecated since version 1.14.0. and should not be used in newly-written code.

Modem has LTE Advanced data capability.

This value is deprecated because it is not used anywhere. LTE Advanced capable devices are reported as LTE capable.

Since: 1.0

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_ACTIVATION_REJECTED_BY_GGSN_OR_GW

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_ACTIVATION_REJECTED_BY_GGSN_OR_GW (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_ACTIVATION_REJECTED_BY_GGSN_OR_GW

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_ACTIVATION_REJECTED_BY_GGSN_OR_GW` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_ACTIVATION_REJECTED_BY_GGSN_OR_GW instead.

Since: 1.8

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_ACTIVATION_REJECTED_UNSPECIFIED

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_ACTIVATION_REJECTED_UNSPECIFIED (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_ACTIVATION_REJECTED_UNSPECIFIED

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_ACTIVATION_REJECTED_UNSPECIFIED` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_ACTIVATION_REJECTED_UNSPECIFIED instead.

Since: 1.8

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_AND_NON_GPRS_SERVICES_NOT_ALLOWED

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_AND_NON_GPRS_SERVICES_NOT_ALLOWED (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_PS_AND_NON_PS_SERVICES_NOT_ALLOWED

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_AND_NON_GPRS_SERVICES_NOT_ALLOWED` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_PS_AND_NON_PS_SERVICES_NOT_ALLOWED instead.

Since: 1.8

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_CONDITIONAL_IE_ERROR

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_CONDITIONAL_IE_ERROR (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_CONDITIONAL_IE_ERROR

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_CONDITIONAL_IE_ERROR` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_CONDITIONAL_IE_ERROR instead.

Since: 1.8

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_CONGESTION

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_CONGESTION (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_CONGESTION

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_CONGESTION` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_CONGESTION instead.

Since: 1.0

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_FEATURE_NOT_SUPPORTED

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_FEATURE_NOT_SUPPORTED (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_FEATURE_NOT_SUPPORTED

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_FEATURE_NOT_SUPPORTED` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_FEATURE_NOT_SUPPORTED instead.

Since: 1.8

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_IE_NOT_IMPLEMENTED

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_IE_NOT_IMPLEMENTED (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_MESSAGE_TYPE_NOT_IMPLEMENTED

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_IE_NOT_IMPLEMENTED` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_MESSAGE_TYPE_NOT_IMPLEMENTED instead.

Since: 1.8

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_ILLEGAL_ME

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_ILLEGAL_ME (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_ILLEGAL_ME

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_ILLEGAL_ME` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_ILLEGAL_ME instead.

Since: 1.0

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_ILLEGAL_MS

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_ILLEGAL_MS (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_ILLEGAL_UE

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_ILLEGAL_MS` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_ILLEGAL_UE instead.

Since: 1.0

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_IMSI_UNKNOWN_IN_HLR

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_IMSI_UNKNOWN_IN_HLR (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_IMSI_UNKNOWN_IN_HSS

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_IMSI_UNKNOWN_IN_HLR` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_IMSI_UNKNOWN_IN_HSS instead.

Since: 1.0

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_IMSI_UNKNOWN_IN_VLR

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_IMSI_UNKNOWN_IN_VLR (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_IMSI_UNKNOWN_IN_VLR

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_IMSI_UNKNOWN_IN_VLR` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_IMSI_UNKNOWN_IN_VLR instead.

Since: 1.0

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_INSUFFICIENT_RESOURCES

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_INSUFFICIENT_RESOURCES (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_INSUFFICIENT_RESOURCES

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_INSUFFICIENT_RESOURCES` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_INSUFFICIENT_RESOURCES instead.

Since: 1.4

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_INVALID_MOBILE_CLASS

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_INVALID_MOBILE_CLASS (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_INVALID_MOBILE_CLASS

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_INVALID_MOBILE_CLASS` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_INVALID_MOBILE_CLASS instead.

Since: 1.0

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_LAST_PDN_DISCONNECTION_NOT_ALLOWED

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_LAST_PDN_DISCONNECTION_NOT_ALLOWED (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_LAST_PDN_DISCONNECTION_NOT_ALLOWED

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_LAST_PDN_DISCONNECTION_NOT_ALLOWED` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_LAST_PDN_DISCONNECTION_NOT_ALLOWED instead.

Since: 1.8

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_LAST_PDN_DISCONNECTION_NOT_ALLOWED_LEGACY

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_LAST_PDN_DISCONNECTION_NOT_ALLOWED_LEGACY (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_LAST_PDN_DISCONNECTION_NOT_ALLOWED_LEGACY

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_LAST_PDN_DISCONNECTION_NOT_ALLOWED_LEGACY` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_LAST_PDN_DISCONNECTION_NOT_ALLOWED_LEGACY instead.

Since: 1.14

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_LOCATION_NOT_ALLOWED

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_LOCATION_NOT_ALLOWED (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_AREA_NOT_ALLOWED

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_LOCATION_NOT_ALLOWED` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_AREA_NOT_ALLOWED instead.

Since: 1.0

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_MANDATORY_IE_ERROR

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_MANDATORY_IE_ERROR (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_INVALID_MANDATORY_INFORMATION

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_MANDATORY_IE_ERROR` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_INVALID_MANDATORY_INFORMATION instead.

Since: 1.8

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_MAXIMUM_NUMBER_OF_PDP_CONTEXTS_REACHED

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_MAXIMUM_NUMBER_OF_PDP_CONTEXTS_REACHED (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_MAXIMUM_NUMBER_OF_BEARERS_REACHED

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_MAXIMUM_NUMBER_OF_PDP_CONTEXTS_REACHED` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_MAXIMUM_NUMBER_OF_BEARERS_REACHED instead.

Since: 1.8

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_MISSING_OR_UNKNOWN_APN

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_MISSING_OR_UNKNOWN_APN (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_MISSING_OR_UNKNOWN_APN

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_MISSING_OR_UNKNOWN_APN` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_MISSING_OR_UNKNOWN_APN instead.

Since: 1.4

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_NETWORK_FAILURE

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_NETWORK_FAILURE (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_NETWORK_FAILURE_ATTACH

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_NETWORK_FAILURE` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_NETWORK_FAILURE_ATTACH instead.

Since: 1.0

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_NOT_AUTHORIZED_FOR_CSG

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_NOT_AUTHORIZED_FOR_CSG (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_NOT_AUTHORIZED_FOR_CSG

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_NOT_AUTHORIZED_FOR_CSG` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_NOT_AUTHORIZED_FOR_CSG instead.

Since: 1.8

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_NO_CELLS_IN_LOCATION_AREA

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_NO_CELLS_IN_LOCATION_AREA (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_NO_CELLS_IN_AREA

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_NO_CELLS_IN_LOCATION_AREA` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_NO_CELLS_IN_AREA instead.

Since: 1.0

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_OPERATOR_DETERMINED_BARRING

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_OPERATOR_DETERMINED_BARRING (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_OPERATOR_DETERMINED_BARRING

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_OPERATOR_DETERMINED_BARRING` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_OPERATOR_DETERMINED_BARRING instead.

Since: 1.8

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_PDP_AUTH_FAILURE

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_PDP_AUTH_FAILURE (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_PDP_AUTH_FAILURE

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_PDP_AUTH_FAILURE` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_PDP_AUTH_FAILURE instead.

Since: 1.0

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_PDP_CONTEXT_WITHOUT_TFT_ALREADY_ACTIVATED

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_PDP_CONTEXT_WITHOUT_TFT_ALREADY_ACTIVATED (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_PDP_CONTEXT_WITHOUT_TFT_ALREADY_ACTIVATED

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_PDP_CONTEXT_WITHOUT_TFT_ALREADY_ACTIVATED` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_PDP_CONTEXT_WITHOUT_TFT_ALREADY_ACTIVATED instead.

Since: 1.8

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_PLMN_NOT_ALLOWED

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_PLMN_NOT_ALLOWED (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_PLMN_NOT_ALLOWED

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_PLMN_NOT_ALLOWED` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_PLMN_NOT_ALLOWED instead.

Since: 1.0

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_REQUESTED_APN_NOT_SUPPORTED

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_REQUESTED_APN_NOT_SUPPORTED (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_REQUESTED_APN_NOT_SUPPORTED

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_REQUESTED_APN_NOT_SUPPORTED` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_REQUESTED_APN_NOT_SUPPORTED instead.

Since: 1.8

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_REQUEST_REJECTED_BCM_VIOLATION

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_REQUEST_REJECTED_BCM_VIOLATION (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_REQUEST_REJECTED_BCM_VIOLATION

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_REQUEST_REJECTED_BCM_VIOLATION` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_REQUEST_REJECTED_BCM_VIOLATION instead.

Since: 1.8

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_ROAMING_NOT_ALLOWED

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_ROAMING_NOT_ALLOWED (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_ROAMING_NOT_ALLOWED_IN_AREA

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_ROAMING_NOT_ALLOWED` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_ROAMING_NOT_ALLOWED_IN_AREA instead.

Since: 1.0

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_SEMANTICALLY_INCORRECT_MESSAGE

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_SEMANTICALLY_INCORRECT_MESSAGE (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_SEMANTICALLY_INCORRECT_MESSAGE

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_SEMANTICALLY_INCORRECT_MESSAGE` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_SEMANTICALLY_INCORRECT_MESSAGE instead.

Since: 1.8

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_SEMANTIC_ERRORS_IN_PACKET_FILTER

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_SEMANTIC_ERRORS_IN_PACKET_FILTER (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_SEMANTIC_ERRORS_IN_PACKET_FILTER

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_SEMANTIC_ERRORS_IN_PACKET_FILTER` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_SEMANTIC_ERRORS_IN_PACKET_FILTER instead.

Since: 1.8

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_SEMANTIC_ERROR_IN_TFT_OPERATION

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_SEMANTIC_ERROR_IN_TFT_OPERATION (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_SEMANTIC_ERROR_IN_TFT_OPERATION

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_SEMANTIC_ERROR_IN_TFT_OPERATION` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_SEMANTIC_ERROR_IN_TFT_OPERATION instead.

Since: 1.8

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_SERVICE_NOT_ALLOWED

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_SERVICE_NOT_ALLOWED (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_PS_SERVICES_NOT_ALLOWED

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_SERVICE_NOT_ALLOWED` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_PS_SERVICES_NOT_ALLOWED instead.

Since: 1.0

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_SERVICE_OPTION_NOT_SUBSCRIBED

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_SERVICE_OPTION_NOT_SUBSCRIBED (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_SERVICE_OPTION_NOT_SUBSCRIBED

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_SERVICE_OPTION_NOT_SUBSCRIBED` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_SERVICE_OPTION_NOT_SUBSCRIBED instead.

Since: 1.0

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_SERVICE_OPTION_NOT_SUPPORTED

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_SERVICE_OPTION_NOT_SUPPORTED (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_SERVICE_OPTION_NOT_SUPPORTED

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_SERVICE_OPTION_NOT_SUPPORTED` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_SERVICE_OPTION_NOT_SUPPORTED instead.

Since: 1.0

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_SERVICE_OPTION_OUT_OF_ORDER

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_SERVICE_OPTION_OUT_OF_ORDER (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_SERVICE_OPTION_OUT_OF_ORDER

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_SERVICE_OPTION_OUT_OF_ORDER` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_SERVICE_OPTION_OUT_OF_ORDER instead.

Since: 1.0

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_SYNTACTICAL_ERROR_IN_PACKET_FILTER

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_SYNTACTICAL_ERROR_IN_PACKET_FILTER (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_SYNTACTICAL_ERROR_IN_PACKET_FILTER

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_SYNTACTICAL_ERROR_IN_PACKET_FILTER` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_SYNTACTICAL_ERROR_IN_PACKET_FILTER instead.

Since: 1.8

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_SYNTACTICAL_ERROR_IN_TFT_OPERATION

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_SYNTACTICAL_ERROR_IN_TFT_OPERATION (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_SYNTACTICAL_ERROR_IN_TFT_OPERATION

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_SYNTACTICAL_ERROR_IN_TFT_OPERATION` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_SYNTACTICAL_ERROR_IN_TFT_OPERATION instead.

Since: 1.8

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_UNKNOWN_PDP_ADDRESS_OR_TYPE

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_UNKNOWN_PDP_ADDRESS_OR_TYPE (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_UNKNOWN_PDP_ADDRESS_OR_TYPE

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_UNKNOWN_PDP_ADDRESS_OR_TYPE` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_UNKNOWN_PDP_ADDRESS_OR_TYPE instead.

Since: 1.8

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_UNKNOWN_PDP_CONTEXT

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_UNKNOWN_PDP_CONTEXT (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_UNKNOWN_PDP_CONTEXT

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_UNKNOWN_PDP_CONTEXT` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_UNKNOWN_PDP_CONTEXT instead.

Since: 1.8

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_UNSPECIFIED_PROTOCOL_ERROR

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_UNSPECIFIED_PROTOCOL_ERROR (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_UNSPECIFIED_PROTOCOL_ERROR

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_UNSPECIFIED_PROTOCOL_ERROR` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_UNSPECIFIED_PROTOCOL_ERROR instead.

Since: 1.8

### MM_MOBILE_EQUIPMENT_ERROR_GPRS_USER_AUTHENTICATION_FAILED

    #define MM_MOBILE_EQUIPMENT_ERROR_GPRS_USER_AUTHENTICATION_FAILED (MMMobileEquipmentErrorDeprecated)MM_MOBILE_EQUIPMENT_ERROR_USER_AUTHENTICATION_FAILED

`MM_MOBILE_EQUIPMENT_ERROR_GPRS_USER_AUTHENTICATION_FAILED` has been deprecated since version 1.18.0 and should not be used in newly-written code.

Use MM_MOBILE_EQUIPMENT_ERROR_USER_AUTHENTICATION_FAILED instead.

Since: 1.4