## MMModemLocation MMModemLocation — The Location interface |

## Functions

const gchar * | mm_modem_location_get_path ()
gchar * | mm_modem_location_dup_path ()
MMModemLocationSource | mm_modem_location_get_capabilities ()
MMModemLocationSource | mm_modem_location_get_enabled ()
guint | mm_modem_location_get_gps_refresh_rate ()
gboolean | mm_modem_location_signals_location ()
gchar * | mm_modem_location_dup_supl_server ()
const gchar * | mm_modem_location_get_supl_server ()
MMModemLocationAssistanceDataType | mm_modem_location_get_supported_assistance_data ()
gchar ** | mm_modem_location_dup_assistance_data_servers ()
const gchar ** | mm_modem_location_get_assistance_data_servers ()
void | mm_modem_location_setup ()
gboolean | mm_modem_location_setup_finish ()
gboolean | mm_modem_location_setup_sync ()
void | mm_modem_location_set_supl_server ()
gboolean | mm_modem_location_set_supl_server_finish ()
gboolean | mm_modem_location_set_supl_server_sync ()
void | mm_modem_location_inject_assistance_data ()
gboolean | mm_modem_location_inject_assistance_data_finish ()
gboolean | mm_modem_location_inject_assistance_data_sync ()
void | mm_modem_location_set_gps_refresh_rate ()
gboolean | mm_modem_location_set_gps_refresh_rate_finish ()
gboolean | mm_modem_location_set_gps_refresh_rate_sync ()
void | mm_modem_location_get_3gpp ()
MMLocation3gpp * | mm_modem_location_get_3gpp_finish ()
MMLocation3gpp * | mm_modem_location_get_3gpp_sync ()
MMLocation3gpp * | mm_modem_location_peek_signaled_3gpp ()
MMLocation3gpp * | mm_modem_location_get_signaled_3gpp ()
void | mm_modem_location_get_gps_nmea ()
MMLocationGpsNmea * | mm_modem_location_get_gps_nmea_finish ()
MMLocationGpsNmea * | mm_modem_location_get_gps_nmea_sync ()
MMLocationGpsNmea * | mm_modem_location_peek_signaled_gps_nmea ()
MMLocationGpsNmea * | mm_modem_location_get_signaled_gps_nmea ()
void | mm_modem_location_get_gps_raw ()
MMLocationGpsRaw * | mm_modem_location_get_gps_raw_finish ()
MMLocationGpsRaw * | mm_modem_location_get_gps_raw_sync ()
MMLocationGpsRaw * | mm_modem_location_peek_signaled_gps_raw ()
MMLocationGpsRaw * | mm_modem_location_get_signaled_gps_raw ()
void | mm_modem_location_get_cdma_bs ()
MMLocationCdmaBs * | mm_modem_location_get_cdma_bs_finish ()
MMLocationCdmaBs * | mm_modem_location_get_cdma_bs_sync ()
MMLocationCdmaBs * | mm_modem_location_peek_signaled_cdma_bs ()
MMLocationCdmaBs * | mm_modem_location_get_signaled_cdma_bs ()
void | mm_modem_location_get_full ()
gboolean | mm_modem_location_get_full_finish ()
gboolean | mm_modem_location_get_full_sync ()

## Types and Values

struct | MMModemLocation
#define | MM_LOCATION_LONGITUDE_UNKNOWN
#define | MM_LOCATION_LATITUDE_UNKNOWN
#define | MM_LOCATION_ALTITUDE_UNKNOWN

## Object Hierarchy

        GObject
        ╰── GDBusProxy
            ╰── MmGdbusModemLocationProxy
                ╰── MMModemLocation

## Implemented Interfaces

MMModemLocation implements GDBusInterface, GInitable, GAsyncInitable and MmGdbusModemLocation.

## Description

The MMModemLocation is an object providing access to the methods, signals and properties of the Location interface.

The Location interface is exposed whenever a modem has location capabilities.

## Functions

### mm_modem_location_get_path ()

    const gchar *
    mm_modem_location_get_path (MMModemLocation *self);

Gets the DBus path of the MMObject which implements this interface.

#### Parameters

self | A MMModemLocation. |

#### Returns

The DBus path of the MMObject object.

[transfer none]

Since: 1.0

### mm_modem_location_dup_path ()

    gchar *
    mm_modem_location_dup_path (MMModemLocation *self);

Gets a copy of the DBus path of the MMObject object which implements this interface.

#### Parameters

self | A MMModemLocation. |

#### Returns

The DBus path of the MMObject. The returned value should be freed with `g_free()`.

[transfer full]

Since: 1.0

### mm_modem_location_get_capabilities ()

    MMModemLocationSource
    mm_modem_location_get_capabilities (MMModemLocation *self);

Gets a bitmask of the location capabilities supported by this MMModemLocation.

#### Parameters

self | A MMModemLocation. |

#### Returns

A MMModemLocationSource.

Since: 1.0

### mm_modem_location_get_enabled ()

    MMModemLocationSource
    mm_modem_location_get_enabled (MMModemLocation *self);

Gets a bitmask of the location capabilities which are enabled in this MMModemLocation.

#### Parameters

self | A MMModemLocation. |

#### Returns

A MMModemLocationSource.

Since: 1.0

### mm_modem_location_get_gps_refresh_rate ()

    guint
    mm_modem_location_get_gps_refresh_rate
                                   (MMModemLocation *self);

Gets the GPS refresh rate, in seconds.

#### Parameters

self | A MMModemLocation. |

#### Returns

The GPS refresh rate, or 0 if no fixed rate is used.

Since: 1.0

### mm_modem_location_signals_location ()

    gboolean
    mm_modem_location_signals_location (MMModemLocation *self);

Gets the status of the location signaling in the MMModemLocation.

#### Parameters

self | A MMModemLocation. |

#### Returns

`TRUE` if location changes are signaled, `FALSE` otherwise.

Since: 1.0

### mm_modem_location_dup_supl_server ()

    gchar *
    mm_modem_location_dup_supl_server (MMModemLocation *self);

Gets the address of the SUPL server.

#### Parameters

self | A MMModemLocation. |

#### Returns

The SUPL server address, or `NULL` if none available. The returned value should be freed with `g_free()`.

[transfer full]

Since: 1.6

### mm_modem_location_get_supl_server ()

    const gchar *
    mm_modem_location_get_supl_server (MMModemLocation *self);

Gets the address of the SUPL server.

The returned value is only valid until the property changes so it is only safe to use this function on the thread where `self` was constructed. Use `mm_modem_location_dup_supl_server()` if on another thread.

#### Parameters

self | A MMModemLocation. |

#### Returns

The SUPL server address, or `NULL` if none available. Do not free the returned value, it belongs to `self` .

[transfer none]

Since: 1.6

### mm_modem_location_get_supported_assistance_data ()

    MMModemLocationAssistanceDataType
    mm_modem_location_get_supported_assistance_data
                                   (MMModemLocation *self);

Gets a bitmask of the supported assistance data types.

#### Parameters

self | A MMModemLocation. |

#### Returns

A MMModemLocationAssistanceDataType.

Since: 1.10

### mm_modem_location_dup_assistance_data_servers ()

    gchar **
    mm_modem_location_dup_assistance_data_servers
                                   (MMModemLocation *self);

Gets the list of assistance data servers.

#### Parameters

self | A MMModemLocation. |

#### Returns

a `NULL`-terminated array of server addresses, or `NULL` if none available. The returned value should be freed with `g_strfreev()`.

[transfer full]

Since: 1.10

### mm_modem_location_get_assistance_data_servers ()

    const gchar **
    mm_modem_location_get_assistance_data_servers
                                   (MMModemLocation *self);

Gets the list of assistance data servers.

The returned value is only valid until the property changes so it is only safe to use this function on the thread where `self` was constructed. Use `mm_modem_location_dup_assistance_data_servers()` if on another thread.

#### Parameters

self | A MMModemLocation. |

#### Returns

a `NULL`-terminated array of server addresses, or `NULL` if none available. Do not free the returned value, it belongs to `self` .

[transfer none]

Since: 1.10

### mm_modem_location_setup ()

    void
    mm_modem_location_setup (MMModemLocation *self,
                             MMModemLocationSource sources,
                             gboolean signal_location,
                             GCancellable *cancellable,
                             GAsyncReadyCallback callback,
                             gpointer user_data);

Asynchronously configures the location sources to use when gathering location information. Also enable or disable location information gathering.

When the operation is finished, `callback` will be invoked in the

thread-default main loop

of the thread you are calling this method from. You can then call `mm_modem_location_setup_finish()` to get the result of the operation.

See `mm_modem_location_setup_sync()` for the synchronous, blocking version of this method.

#### Parameters

self | A MMModemLocation. |
sources | Bitmask of MMModemLocationSource values specifying which locations should get enabled. |
signal_location | Flag to enable or disable location signaling. |
cancellable | A GCancellable or `NULL`. | [allow-none]
callback | A GAsyncReadyCallback to call when the request is satisfied or `NULL`. |
user_data | User data to pass to `callback` . |

Since: 1.0

### mm_modem_location_setup_finish ()

    gboolean
    mm_modem_location_setup_finish (MMModemLocation *self,
                                    GAsyncResult *res,
                                    GError **error);

Finishes an operation started with `mm_modem_location_setup()`.

#### Parameters

self | A MMModemLocation. |
res | The GAsyncResult obtained from the GAsyncReadyCallback passed to `mm_modem_location_setup()`. |
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if the setup was successful, `FALSE` if `error` is set.

Since: 1.0

### mm_modem_location_setup_sync ()

    gboolean
    mm_modem_location_setup_sync (MMModemLocation *self,
                                  MMModemLocationSource sources,
                                  gboolean signal_location,
                                  GCancellable *cancellable,
                                  GError **error);

Synchronously configures the location sources to use when gathering location information. Also enable or disable location information gathering.

The calling thread is blocked until a reply is received. See `mm_modem_location_setup()` for the asynchronous version of this method.

#### Parameters

self | A MMModemLocation. |
sources | Bitmask of MMModemLocationSource values specifying which locations should get enabled. |
signal_location | Flag to enable or disable location signaling. |
cancellable | A GCancellable or `NULL`. | [allow-none]
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if the setup was successful, `FALSE` if `error` is set.

Since: 1.0

### mm_modem_location_set_supl_server ()

    void
    mm_modem_location_set_supl_server (MMModemLocation *self,
                                       const gchar *supl,
                                       GCancellable *cancellable,
                                       GAsyncReadyCallback callback,
                                       gpointer user_data);

Asynchronously configures the address of the SUPL server for A-GPS operation.

When the operation is finished, `callback` will be invoked in the

thread-default main loop

of the thread you are calling this method from. You can then call `mm_modem_location_set_supl_server_finish()` to get the result of the operation.

See `mm_modem_location_set_supl_server_sync()` for the synchronous, blocking version of this method.

#### Parameters

self | A MMModemLocation. |
supl | The SUPL server address, given as IP:PORT or with a full URL. |
cancellable | A GCancellable or `NULL`. | [allow-none]
callback | A GAsyncReadyCallback to call when the request is satisfied or `NULL`. |
user_data | User data to pass to `callback` . |

Since: 1.6

### mm_modem_location_set_supl_server_finish ()

    gboolean
    mm_modem_location_set_supl_server_finish
                                   (MMModemLocation *self,
                                    GAsyncResult *res,
                                    GError **error);

Finishes an operation started with `mm_modem_location_set_supl_server()`.

#### Parameters

self | A MMModemLocation. |
res | The GAsyncResult obtained from the GAsyncReadyCallback passed to `mm_modem_location_set_supl_server()`. |
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if setting the SUPL server was successful, `FALSE` if `error` is set.

Since: 1.6

### mm_modem_location_set_supl_server_sync ()

    gboolean
    mm_modem_location_set_supl_server_sync
                                   (MMModemLocation *self,
                                    const gchar *supl,
                                    GCancellable *cancellable,
                                    GError **error);

Synchronously configures the address of the SUPL server for A-GPS operation.

The calling thread is blocked until a reply is received. See `mm_modem_location_set_supl_server()` for the asynchronous version of this method.

#### Parameters

self | A MMModemLocation. |
supl | The SUPL server address, given as IP:PORT or with a full URL. |
cancellable | A GCancellable or `NULL`. | [allow-none]
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if setting the SUPL server was successful, `FALSE` if `error` is set.

Since: 1.6

### mm_modem_location_inject_assistance_data ()

    void
    mm_modem_location_inject_assistance_data
                                   (MMModemLocation *self,
                                    const guint8 *data,
                                    gsize data_size,
                                    GCancellable *cancellable,
                                    GAsyncReadyCallback callback,
                                    gpointer user_data);

Aynchronously injects assistance data to the GNSS module.

When the operation is finished, `callback` will be invoked in the

thread-default main loop

of the thread you are calling this method from. You can then call `mm_modem_location_inject_assistance_data_finish()` to get the result of the operation.

See `mm_modem_location_inject_assistance_data_sync()` for the synchronous, blocking version of this method.

#### Parameters

self | A MMModemLocation. |
data | Data to inject. | [array length=data_size]
data_size | size of `data` . |
cancellable | A GCancellable or `NULL`. | [allow-none]
callback | A GAsyncReadyCallback to call when the request is satisfied or `NULL`. |
user_data | User data to pass to `callback` . |

Since: 1.10

### mm_modem_location_inject_assistance_data_finish ()

    gboolean
    mm_modem_location_inject_assistance_data_finish
                                   (MMModemLocation *self,
                                    GAsyncResult *res,
                                    GError **error);

Finishes an operation started with `mm_modem_location_inject_assistance_data()`.

#### Parameters

self | A MMModemLocation. |
res | The GAsyncResult obtained from the GAsyncReadyCallback passed to `mm_modem_location_inject_assistance_data()`. |
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if the injection was successful, `FALSE` if `error` is set.

Since: 1.10

### mm_modem_location_inject_assistance_data_sync ()

    gboolean
    mm_modem_location_inject_assistance_data_sync
                                   (MMModemLocation *self,
                                    const guint8 *data,
                                    gsize data_size,
                                    GCancellable *cancellable,
                                    GError **error);

Synchronously injects assistance data to the GNSS module.

The calling thread is blocked until a reply is received. See `mm_modem_location_inject_assistance_data()` for the asynchronous version of this method.

#### Parameters

self | A MMModemLocation. |
data | Data to inject. | [array length=data_size]
data_size | size of `data` . |
cancellable | A GCancellable or `NULL`. | [allow-none]
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if the injection was successful, `FALSE` if `error` is set.

Since: 1.10

### mm_modem_location_set_gps_refresh_rate ()

    void
    mm_modem_location_set_gps_refresh_rate
                                   (MMModemLocation *self,
                                    guint rate,
                                    GCancellable *cancellable,
                                    GAsyncReadyCallback callback,
                                    gpointer user_data);

Asynchronously configures the GPS refresh rate.

If a 0 rate is used, the GPS location updates will be immediately propagated to the interface.

When the operation is finished, `callback` will be invoked in the

thread-default main loop

of the thread you are calling this method from. You can then call `mm_modem_location_set_gps_refresh_rate_finish()` to get the result of the operation.

See `mm_modem_location_set_gps_refresh_rate_sync()` for the synchronous, blocking version of this method.

#### Parameters

self | A MMModemLocation. |
rate | The GPS refresh rate, in seconds. |
cancellable | A GCancellable or `NULL`. | [allow-none]
callback | A GAsyncReadyCallback to call when the request is satisfied or `NULL`. |
user_data | User data to pass to `callback` . |

Since: 1.0

### mm_modem_location_set_gps_refresh_rate_finish ()

    gboolean
    mm_modem_location_set_gps_refresh_rate_finish
                                   (MMModemLocation *self,
                                    GAsyncResult *res,
                                    GError **error);

Finishes an operation started with `mm_modem_location_set_gps_refresh_rate()`.

#### Parameters

self | A MMModemLocation. |
res | The GAsyncResult obtained from the GAsyncReadyCallback passed to `mm_modem_location_set_gps_refresh_rate()`. |
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if setting the GPS refresh rate was successful, `FALSE` if `error` is set.

Since: 1.0

### mm_modem_location_set_gps_refresh_rate_sync ()

    gboolean
    mm_modem_location_set_gps_refresh_rate_sync
                                   (MMModemLocation *self,
                                    guint rate,
                                    GCancellable *cancellable,
                                    GError **error);

Synchronously configures the GPS refresh rate.

If a 0 rate is used, the GPS location updates will be immediately propagated to the interface.

The calling thread is blocked until a reply is received. See `mm_modem_location_set_gps_refresh_rate()` for the asynchronous version of this method.

#### Parameters

self | A MMModemLocation. |
rate | The GPS refresh rate, in seconds. |
cancellable | A GCancellable or `NULL`. | [allow-none]
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if setting the refresh rate was successful, `FALSE` if `error` is set.

Since: 1.0

### mm_modem_location_get_3gpp ()

    void
    mm_modem_location_get_3gpp (MMModemLocation *self,
                                GCancellable *cancellable,
                                GAsyncReadyCallback callback,
                                gpointer user_data);

Asynchronously gets the current 3GPP location information.

When the operation is finished, `callback` will be invoked in the

thread-default main loop

of the thread you are calling this method from. You can then call `mm_modem_location_get_3gpp_finish()` to get the result of the operation.

See `mm_modem_location_get_3gpp_sync()` for the synchronous, blocking version of this method.

#### Parameters

self | A MMModemLocation. |
cancellable | A GCancellable or `NULL`. | [allow-none]
callback | A GAsyncReadyCallback to call when the request is satisfied or `NULL`. |
user_data | User data to pass to `callback` . |

Since: 1.0

### mm_modem_location_get_3gpp_finish ()

    MMLocation3gpp *
    mm_modem_location_get_3gpp_finish (MMModemLocation *self,
                                       GAsyncResult *res,
                                       GError **error);

Finishes an operation started with `mm_modem_location_get_3gpp()`.

#### Parameters

self | A MMModemLocation. |
res | The GAsyncResult obtained from the GAsyncReadyCallback passed to `mm_modem_location_get_3gpp()`. |
error | Return location for error or `NULL`. |

#### Returns

A MMLocation3gpp, or NULL if not available. The returned value should be freed with `g_object_unref()`.

[transfer full]

Since: 1.0

### mm_modem_location_get_3gpp_sync ()

    MMLocation3gpp *
    mm_modem_location_get_3gpp_sync (MMModemLocation *self,
                                     GCancellable *cancellable,
                                     GError **error);

Synchronously gets the current 3GPP location information.

The calling thread is blocked until a reply is received. See `mm_modem_location_get_3gpp()` for the asynchronous version of this method.

#### Parameters

self | A MMModemLocation. |
cancellable | A GCancellable or `NULL`. | [allow-none]
error | Return location for error or `NULL`. |

#### Returns

A MMLocation3gpp, or NULL if not available. The returned value should be freed with `g_object_unref()`.

[transfer full]

Since: 1.0

### mm_modem_location_peek_signaled_3gpp ()

    MMLocation3gpp *
    mm_modem_location_peek_signaled_3gpp (MMModemLocation *self);

Gets a MMLocation3gpp object with the current 3GPP location information.

Unlike `mm_modem_location_get_3gpp()` or `mm_modem_location_get_3gpp_sync()`, this method does not perform an explicit query. Instead, this method will return the location information that may have been signaled by the modem. Therefore, this method will only succeed if location signaling is enabled (e.g. with `mm_modem_location_setup()` in the MMModemLocation).

The returned value is only valid until the property changes so it is only safe to use this function on the thread where `self` was constructed. Use `mm_modem_location_get_signaled_3gpp()` if on another thread.

#### Parameters

self | A MMModemLocation. |

#### Returns

A MMLocation3gpp, or `NULL` if none available. Do not free the returned value, it belongs to `self` .

[transfer none]

Since: 1.18

### mm_modem_location_get_signaled_3gpp ()

    MMLocation3gpp *
    mm_modem_location_get_signaled_3gpp (MMModemLocation *self);

Gets a MMLocation3gpp object with the current 3GPP location information.

Unlike `mm_modem_location_get_3gpp()` or `mm_modem_location_get_3gpp_sync()`, this method does not perform an explicit query. Instead, this method will return the location information that may have been signaled by the modem. Therefore, this method will only succeed if location signaling is enabled (e.g. with `mm_modem_location_setup()` in the MMModemLocation).

The values reported by `self` are not updated when the values in the interface change. Instead, the client is expected to call `mm_modem_location_get_signaled_3gpp()` again to get a new MMLocation3gpp with the new values.

#### Parameters

self | A MMModemLocation. |

#### Returns

A MMLocation3gpp that must be freed with `g_object_unref()` or `NULL` if none available.

[transfer full]

Since: 1.18

### mm_modem_location_get_gps_nmea ()

    void
    mm_modem_location_get_gps_nmea (MMModemLocation *self,
                                    GCancellable *cancellable,
                                    GAsyncReadyCallback callback,
                                    gpointer user_data);

Asynchronously gets the current GPS NMEA location information.

When the operation is finished, `callback` will be invoked in the

thread-default main loop

of the thread you are calling this method from. You can then call `mm_modem_location_get_gps_nmea_finish()` to get the result of the operation.

See `mm_modem_location_get_gps_nmea_sync()` for the synchronous, blocking version of this method.

#### Parameters

self | A MMModemLocation. |
cancellable | A GCancellable or `NULL`. | [allow-none]
callback | A GAsyncReadyCallback to call when the request is satisfied or `NULL`. |
user_data | User data to pass to `callback` . |

Since: 1.0

### mm_modem_location_get_gps_nmea_finish ()

    MMLocationGpsNmea *
    mm_modem_location_get_gps_nmea_finish (MMModemLocation *self,
                                           GAsyncResult *res,
                                           GError **error);

Finishes an operation started with `mm_modem_location_get_gps_nmea()`.

#### Parameters

self | A MMModemLocation. |
res | The GAsyncResult obtained from the GAsyncReadyCallback passed to `mm_modem_location_get_gps_nmea()`. |
error | Return location for error or `NULL`. |

#### Returns

A MMLocationGpsNmea, or NULL if not available. The returned value should be freed with `g_object_unref()`.

[transfer full]

Since: 1.0

### mm_modem_location_get_gps_nmea_sync ()

    MMLocationGpsNmea *
    mm_modem_location_get_gps_nmea_sync (MMModemLocation *self,
                                         GCancellable *cancellable,
                                         GError **error);

Synchronously gets the current GPS NMEA location information.

The calling thread is blocked until a reply is received. See `mm_modem_location_get_gps_nmea()` for the asynchronous version of this method.

#### Parameters

self | A MMModemLocation. |
cancellable | A GCancellable or `NULL`. | [allow-none]
error | Return location for error or `NULL`. |

#### Returns

A MMLocationGpsNmea, or NULL if not available. The returned value should be freed with `g_object_unref()`.

[transfer full]

Since: 1.0

### mm_modem_location_peek_signaled_gps_nmea ()

    MMLocationGpsNmea *
    mm_modem_location_peek_signaled_gps_nmea
                                   (MMModemLocation *self);

Gets a MMLocationGpsNmea object with the current GPS NMEA location information.

Unlike `mm_modem_location_get_gps_nmea()` or `mm_modem_location_get_gps_nmea_sync()`, this method does not perform an explicit query. Instead, this method will return the location information that may have been signaled by the modem. Therefore, this method will only succeed if location signaling is enabled (e.g. with `mm_modem_location_setup()` in the MMModemLocation).

The returned value is only valid until the property changes so it is only safe to use this function on the thread where `self` was constructed. Use `mm_modem_location_get_signaled_gps_nmea()` if on another thread.

#### Parameters

self | A MMModemLocation. |

#### Returns

A MMLocationGpsNmea, or `NULL` if none available. Do not free the returned value, it belongs to `self` .

[transfer none]

Since: 1.18

### mm_modem_location_get_signaled_gps_nmea ()

    MMLocationGpsNmea *
    mm_modem_location_get_signaled_gps_nmea
                                   (MMModemLocation *self);

Gets a MMLocationGpsNmea object with the current GPS NMEA location information.

Unlike `mm_modem_location_get_gps_nmea()` or `mm_modem_location_get_gps_nmea_sync()`, this method does not perform an explicit query. Instead, this method will return the location information that may have been signaled by the modem. Therefore, this method will only succeed if location signaling is enabled (e.g. with `mm_modem_location_setup()` in the MMModemLocation).

The values reported by `self` are not updated when the values in the interface change. Instead, the client is expected to call `mm_modem_location_get_signaled_gps_nmea()` again to get a new MMLocationGpsNmea with the new values.

#### Parameters

self | A MMModemLocation. |

#### Returns

A MMLocationGpsNmea that must be freed with `g_object_unref()` or `NULL` if none available.

[transfer full]

Since: 1.18

### mm_modem_location_get_gps_raw ()

    void
    mm_modem_location_get_gps_raw (MMModemLocation *self,
                                   GCancellable *cancellable,
                                   GAsyncReadyCallback callback,
                                   gpointer user_data);

Asynchronously gets the current GPS raw location information.

When the operation is finished, `callback` will be invoked in the

thread-default main loop

of the thread you are calling this method from. You can then call `mm_modem_location_get_gps_raw_finish()` to get the result of the operation.

See `mm_modem_location_get_gps_raw_sync()` for the synchronous, blocking version of this method.

#### Parameters

self | A MMModemLocation. |
cancellable | A GCancellable or `NULL`. | [allow-none]
callback | A GAsyncReadyCallback to call when the request is satisfied or `NULL`. |
user_data | User data to pass to `callback` . |

Since: 1.0

### mm_modem_location_get_gps_raw_finish ()

    MMLocationGpsRaw *
    mm_modem_location_get_gps_raw_finish (MMModemLocation *self,
                                          GAsyncResult *res,
                                          GError **error);

Finishes an operation started with `mm_modem_location_get_gps_raw()`.

#### Parameters

self | A MMModemLocation. |
res | The GAsyncResult obtained from the GAsyncReadyCallback passed to `mm_modem_location_get_gps_raw()`. |
error | Return location for error or `NULL`. |

#### Returns

A MMLocationGpsRaw, or NULL if not available. The returned value should be freed with `g_object_unref()`.

[transfer full]

Since: 1.0

### mm_modem_location_get_gps_raw_sync ()

    MMLocationGpsRaw *
    mm_modem_location_get_gps_raw_sync (MMModemLocation *self,
                                        GCancellable *cancellable,
                                        GError **error);

Synchronously gets the current GPS raw location information.

The calling thread is blocked until a reply is received. See `mm_modem_location_get_gps_raw()` for the asynchronous version of this method.

#### Parameters

self | A MMModemLocation. |
cancellable | A GCancellable or `NULL`. | [allow-none]
error | Return location for error or `NULL`. |

#### Returns

A MMLocationGpsRaw, or NULL if not available. The returned value should be freed with `g_object_unref()`.

[transfer full]

Since: 1.0

### mm_modem_location_peek_signaled_gps_raw ()

    MMLocationGpsRaw *
    mm_modem_location_peek_signaled_gps_raw
                                   (MMModemLocation *self);

Gets a MMLocationGpsRaw object with the current GPS raw location information.

Unlike `mm_modem_location_get_gps_raw()` or `mm_modem_location_get_gps_raw_sync()`, this method does not perform an explicit query. Instead, this method will return the location information that may have been signaled by the modem. Therefore, this method will only succeed if location signaling is enabled (e.g. with `mm_modem_location_setup()` in the MMModemLocation).

The returned value is only valid until the property changes so it is only safe to use this function on the thread where `self` was constructed. Use `mm_modem_location_get_signaled_gps_raw()` if on another thread.

#### Parameters

self | A MMModemLocation. |

#### Returns

A MMLocationGpsRaw, or `NULL` if none available. Do not free the returned value, it belongs to `self` .

[transfer none]

Since: 1.18

### mm_modem_location_get_signaled_gps_raw ()

    MMLocationGpsRaw *
    mm_modem_location_get_signaled_gps_raw
                                   (MMModemLocation *self);

Gets a MMLocationGpsRaw object with the current GPS raw location information.

Unlike `mm_modem_location_get_gps_raw()` or `mm_modem_location_get_gps_raw_sync()`, this method does not perform an explicit query. Instead, this method will return the location information that may have been signaled by the modem. Therefore, this method will only succeed if location signaling is enabled (e.g. with `mm_modem_location_setup()` in the MMModemLocation).

The values reported by `self` are not updated when the values in the interface change. Instead, the client is expected to call `mm_modem_location_get_signaled_gps_raw()` again to get a new MMLocationGpsRaw with the new values.

#### Parameters

self | A MMModemLocation. |

#### Returns

A MMLocationGpsRaw that must be freed with `g_object_unref()` or `NULL` if none available.

[transfer full]

Since: 1.18

### mm_modem_location_get_cdma_bs ()

    void
    mm_modem_location_get_cdma_bs (MMModemLocation *self,
                                   GCancellable *cancellable,
                                   GAsyncReadyCallback callback,
                                   gpointer user_data);

Asynchronously gets the current CDMA base station location information.

When the operation is finished, `callback` will be invoked in the

thread-default main loop

of the thread you are calling this method from. You can then call `mm_modem_location_get_cdma_bs_finish()` to get the result of the operation.

See `mm_modem_location_get_cdma_bs_sync()` for the synchronous, blocking version of this method.

#### Parameters

self | A MMModemLocation. |
cancellable | A GCancellable or `NULL`. | [allow-none]
callback | A GAsyncReadyCallback to call when the request is satisfied or `NULL`. |
user_data | User data to pass to `callback` . |

Since: 1.0

### mm_modem_location_get_cdma_bs_finish ()

    MMLocationCdmaBs *
    mm_modem_location_get_cdma_bs_finish (MMModemLocation *self,
                                          GAsyncResult *res,
                                          GError **error);

Finishes an operation started with `mm_modem_location_get_cdma_bs()`.

#### Parameters

self | A MMModemLocation. |
res | The GAsyncResult obtained from the GAsyncReadyCallback passed to `mm_modem_location_get_cdma_bs()`. |
error | Return location for error or `NULL`. |

#### Returns

A MMLocationCdmaBs, or NULL if not available. The returned value should be freed with `g_object_unref()`.

[transfer full]

Since: 1.0

### mm_modem_location_get_cdma_bs_sync ()

    MMLocationCdmaBs *
    mm_modem_location_get_cdma_bs_sync (MMModemLocation *self,
                                        GCancellable *cancellable,
                                        GError **error);

Synchronously gets the current CDMA base station location information.

The calling thread is blocked until a reply is received. See `mm_modem_location_get_cdma_bs()` for the asynchronous version of this method.

#### Parameters

self | A MMModemLocation. |
cancellable | A GCancellable or `NULL`. | [allow-none]
error | Return location for error or `NULL`. |

#### Returns

A MMLocationCdmaBs, or NULL if not available. The returned value should be freed with `g_object_unref()`.

[transfer full]

Since: 1.0

### mm_modem_location_peek_signaled_cdma_bs ()

    MMLocationCdmaBs *
    mm_modem_location_peek_signaled_cdma_bs
                                   (MMModemLocation *self);

Gets a MMLocationCdmaBs object with the current CDMA base station location information.

Unlike `mm_modem_location_get_cdma_bs()` or `mm_modem_location_get_cdma_bs_sync()`, this method does not perform an explicit query. Instead, this method will return the location information that may have been signaled by the modem. Therefore, this method will only succeed if location signaling is enabled (e.g. with `mm_modem_location_setup()` in the MMModemLocation).

The returned value is only valid until the property changes so it is only safe to use this function on the thread where `self` was constructed. Use `mm_modem_location_get_signaled_cdma_bs()` if on another thread.

#### Parameters

self | A MMModemLocation. |

#### Returns

A MMLocationCdmaBs, or `NULL` if none available. Do not free the returned value, it belongs to `self` .

[transfer none]

Since: 1.18

### mm_modem_location_get_signaled_cdma_bs ()

    MMLocationCdmaBs *
    mm_modem_location_get_signaled_cdma_bs
                                   (MMModemLocation *self);

Gets a MMLocationCdmaBs object with the current CDMA base station location information.

Unlike `mm_modem_location_get_cdma_bs()` or `mm_modem_location_get_cdma_bs_sync()`, this method does not perform an explicit query. Instead, this method will return the location information that may have been signaled by the modem. Therefore, this method will only succeed if location signaling is enabled (e.g. with `mm_modem_location_setup()` in the MMModemLocation).

The values reported by `self` are not updated when the values in the interface change. Instead, the client is expected to call `mm_modem_location_get_signaled_cdma_bs()` again to get a new MMLocationCdmaBs with the new values.

#### Parameters

self | A MMModemLocation. |

#### Returns

A MMLocationCdmaBs that must be freed with `g_object_unref()` or `NULL` if none available.

[transfer full]

Since: 1.18

### mm_modem_location_get_full ()

    void
    mm_modem_location_get_full (MMModemLocation *self,
                                GCancellable *cancellable,
                                GAsyncReadyCallback callback,
                                gpointer user_data);

Asynchronously gets the current location information.

When the operation is finished, `callback` will be invoked in the

thread-default main loop

of the thread you are calling this method from. You can then call `mm_modem_location_get_full_finish()` to get the result of the operation.

See `mm_modem_location_get_full_sync()` for the synchronous, blocking version of this method.

#### Parameters

self | A MMModemLocation. |
cancellable | A GCancellable or `NULL`. | [allow-none]
callback | A GAsyncReadyCallback to call when the request is satisfied or `NULL`. |
user_data | User data to pass to `callback` . |

Since: 1.0

### mm_modem_location_get_full_finish ()

    gboolean
    mm_modem_location_get_full_finish (MMModemLocation *self,
                                       GAsyncResult *res,
                                       MMLocation3gpp **location_3gpp,
                                       MMLocationGpsNmea **location_gps_nmea,
                                       MMLocationGpsRaw **location_gps_raw,
                                       MMLocationCdmaBs **location_cdma_bs,
                                       GError **error);

Finishes an operation started with `mm_modem_location_get_full()`.

#### Parameters

self | A MMModemLocation. |
location_3gpp | Return location for a MMLocation3gpp if 3GPP location is requested, or NULL if not required. The returned value should be freed with `g_object_unref()`. | [out][allow-none][transfer full]
location_gps_nmea | Return location for a MMLocationGpsNmea if GPS NMEA location is requested, or NULL if not required. The returned value should be freed with `g_object_unref()`. | [out][allow-none][transfer full]
location_gps_raw | Return location for a MMLocationGpsRaw if GPS raw location is requested, or NULL if not required. The returned value should be freed with `g_object_unref()`. | [out][allow-none][transfer full]
location_cdma_bs | Return location for a MMLocationCdmaBs if CDMA Base Station location is requested, or NULL if not required. The returned value should be freed with `g_object_unref()`. | [out][allow-none][transfer full]
res | The GAsyncResult obtained from the GAsyncReadyCallback passed to `mm_modem_location_get_full()`. |
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if the retrieval was successful, `FALSE` if `error` is set.

Since: 1.0

### mm_modem_location_get_full_sync ()

    gboolean
    mm_modem_location_get_full_sync (MMModemLocation *self,
                                     MMLocation3gpp **location_3gpp,
                                     MMLocationGpsNmea **location_gps_nmea,
                                     MMLocationGpsRaw **location_gps_raw,
                                     MMLocationCdmaBs **location_cdma_bs,
                                     GCancellable *cancellable,
                                     GError **error);

Synchronously gets the current location information.

The calling thread is blocked until a reply is received. See `mm_modem_location_get_full()` for the asynchronous version of this method.

#### Parameters

self | A MMModemLocation. |
location_3gpp | Return location for a MMLocation3gpp if 3GPP location is requested, or NULL if not required. The returned value should be freed with `g_object_unref()`. | [out][allow-none][transfer full]
location_gps_nmea | Return location for a MMLocationGpsNmea if GPS NMEA location is requested, or NULL if not required. The returned value should be freed with `g_object_unref()`. | [out][allow-none][transfer full]
location_gps_raw | Return location for a MMLocationGpsRaw if GPS raw location is requested, or NULL if not required. The returned value should be freed with `g_object_unref()`. | [out][allow-none][transfer full]
location_cdma_bs | Return location for a MMLocationCdmaBs if CDMA Base Station location is requested, or NULL if not required. The returned value should be freed with `g_object_unref()`. | [out][allow-none][transfer full]
cancellable | A GCancellable or `NULL`. | [allow-none]
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if the setup was successful, `FALSE` if `error` is set.

Since: 1.0

## Types and Values

### struct MMModemLocation

    struct MMModemLocation;

The MMModemLocation structure contains private data and should only be accessed using the provided API.

### MM_LOCATION_LONGITUDE_UNKNOWN

    #define MM_LOCATION_LONGITUDE_UNKNOWN -G_MAXDOUBLE

Identifier for an unknown longitude value.

Proper longitude values fall in the [-180,180] range.

Since: 1.0

### MM_LOCATION_LATITUDE_UNKNOWN

    #define MM_LOCATION_LATITUDE_UNKNOWN  -G_MAXDOUBLE

Identifier for an unknown latitude value.

Proper latitude values fall in the [-90,90] range.

Since: 1.0

### MM_LOCATION_ALTITUDE_UNKNOWN

    #define MM_LOCATION_ALTITUDE_UNKNOWN  -G_MAXDOUBLE

Identifier for an unknown altitude value.

Since: 1.0