## Flags and Enumerations Flags and Enumerations — Common enumerations and types in the API. |

## Types and Values

enum | MMBearerType
enum | MMBearerIpFamily
enum | MMBearerIpMethod
enum | MMBearerAllowedAuth
enum | MMBearerMultiplexSupport
enum | MMBearerApnType
enum | MMCallDirection
enum | MMCallState
enum | MMCallStateReason
enum | MMFirmwareImageType
enum | MMModem3gppFacility
enum | MMModem3gppNetworkAvailability
enum | MMModem3gppSubscriptionState
enum | MMModem3gppRegistrationState
enum | MMModem3gppUssdSessionState
enum | MMModem3gppEpsUeModeOperation
enum | MMModemAccessTechnology
enum | MMModemBand
enum | MMModemCapability
enum | MMModemCdmaActivationState
enum | MMModemCdmaRegistrationState
enum | MMModemCdmaRmProtocol
enum | MMModemContactsStorage
enum | MMModemLocationSource
enum | MMModemLocationAssistanceDataType
enum | MMModemLock
enum | MMModemMode
enum | MMModemState
enum | MMModemStateFailedReason
enum | MMModemStateChangeReason
enum | MMModemPowerState
enum | MMModemPortType
enum | MMModemFirmwareUpdateMethod
enum | MMOmaFeature
enum | MMOmaSessionState
enum | MMOmaSessionStateFailedReason
enum | MMOmaSessionType
enum | MMSmsPduType
enum | MMSmsState
enum | MMSmsDeliveryState
enum | MMSmsStorage
enum | MMSmsValidityType
enum | MMSmsCdmaTeleserviceId
enum | MMSmsCdmaServiceCategory

## Description

This section defines enumerations and types that are used in the ModemManager interface.

## Functions

## Types and Values

### enum MMBearerType

Type of context (2G/3G) or bearer (4G).

#### Members

MM_BEARER_TYPE_UNKNOWN | Unknown bearer. |
MM_BEARER_TYPE_DEFAULT | Primary context (2G/3G) or default bearer (4G), defined by the user of the API. |
MM_BEARER_TYPE_DEFAULT_ATTACH | The initial default bearer established during LTE attach procedure, automatically connected as long as the device is regitered in the LTE network. |
MM_BEARER_TYPE_DEDICATED | Secondary context (2G/3G) or dedicated bearer (4G), defined by the user of the API. These bearers use the same IP address used by a primary context or default bearer and provide a dedicated flow for specific traffic with different QoS settings. |

Since: 1.10

### enum MMBearerIpFamily

Type of IP family to be used in a given Bearer.

#### Members

MM_BEARER_IP_FAMILY_NONE | None or unknown. |
MM_BEARER_IP_FAMILY_IPV4 | IPv4. |
MM_BEARER_IP_FAMILY_IPV6 | IPv6. |
MM_BEARER_IP_FAMILY_IPV4V6 | IPv4 and IPv6. |
MM_BEARER_IP_FAMILY_ANY | Mask specifying all IP families. |

Since: 1.0

### enum MMBearerIpMethod

Type of IP method configuration to be used in a given Bearer.

#### Members

MM_BEARER_IP_METHOD_UNKNOWN | Unknown method. |
MM_BEARER_IP_METHOD_PPP | Use PPP to get IP addresses and DNS information. For IPv6, use PPP to retrieve the 64-bit Interface Identifier, use the IID to construct an IPv6 link-local address by following RFC 5072, and then run DHCP over the PPP link to retrieve DNS settings. |
MM_BEARER_IP_METHOD_STATIC | Use the provided static IP configuration given by the modem to configure the IP data interface. Note that DNS servers may not be provided by the network or modem firmware. |
MM_BEARER_IP_METHOD_DHCP | Begin DHCP or IPv6 SLAAC on the data interface to obtain any necessary IP configuration details that are not already provided by the IP configuration. For IPv4 bearers DHCP should be used. For IPv6 bearers SLAAC should be used, and the IP configuration may already contain a link-local address that should be assigned to the interface before SLAAC is started to obtain the rest of the configuration. |

Since: 1.0

### enum MMBearerAllowedAuth

Allowed authentication methods when authenticating with the network.

#### Members

MM_BEARER_ALLOWED_AUTH_UNKNOWN | Unknown. |
MM_BEARER_ALLOWED_AUTH_NONE | None. |
MM_BEARER_ALLOWED_AUTH_PAP | PAP. |
MM_BEARER_ALLOWED_AUTH_CHAP | CHAP. |
MM_BEARER_ALLOWED_AUTH_MSCHAP | MS-CHAP. |
MM_BEARER_ALLOWED_AUTH_MSCHAPV2 | MS-CHAP v2. |
MM_BEARER_ALLOWED_AUTH_EAP | EAP. |

Since: 1.0

### enum MMBearerMultiplexSupport

Multiplex support requested by the user.

#### Members

MM_BEARER_MULTIPLEX_SUPPORT_UNKNOWN | Unknown. |
MM_BEARER_MULTIPLEX_SUPPORT_NONE | No multiplex support should be used. |
MM_BEARER_MULTIPLEX_SUPPORT_REQUESTED | If available, multiplex support should be used. |
MM_BEARER_MULTIPLEX_SUPPORT_REQUIRED | Multiplex support must be used or otherwise the connection attempt will fail. |

Since: 1.18

### enum MMBearerApnType

Purpose of the APN used in a given Bearer.

This information may be stored in the device configuration (e.g. if carrier specific configurations have been enabled for the SIM in use), or provided explicitly by the user.

If the mask of types includes `MM_BEARER_APN_TYPE_DEFAULT`, it is expected that the connection manager will include a default route through the specific bearer connection to the public Internet.

For any other mask type, it is expected that the connection manager will not setup a default route and will therefore require additional custom routing rules to provide access to the different services. E.g. a bearer connected with `MM_BEARER_APN_TYPE_MMS` will probably require an explicit additional route in the host to access the MMSC server at the address specified by the operator. If this address relies on a domain name instead of a fixed IP address, the name resolution should be performed using the DNS servers specified in the corresponding bearer connection settings.

If not explicitly specified during a connection attempt, the connection manager should be free to treat it with its own logic. E.g. a good default could be to treat the first connection as `MM_BEARER_APN_TYPE_DEFAULT` (with a default route) and any other additional connection as `MM_BEARER_APN_TYPE_PRIVATE` (without a default route).

#### Members

MM_BEARER_APN_TYPE_NONE | Unknown or unsupported. |
MM_BEARER_APN_TYPE_INITIAL | APN used for the initial attach procedure. |
MM_BEARER_APN_TYPE_DEFAULT | Default connection APN providing access to the Internet. |
MM_BEARER_APN_TYPE_IMS | APN providing access to IMS services. |
MM_BEARER_APN_TYPE_MMS | APN providing access to MMS services. |
MM_BEARER_APN_TYPE_MANAGEMENT | APN providing access to over-the-air device management procedures. |
MM_BEARER_APN_TYPE_VOICE | APN providing access to voice-over-IP services. |
MM_BEARER_APN_TYPE_EMERGENCY | APN providing access to emergency services. |
MM_BEARER_APN_TYPE_PRIVATE | APN providing access to private networks. |

Since: 1.18

### enum MMCallDirection

Direction of the call.

#### Members

MM_CALL_DIRECTION_UNKNOWN | unknown. |
MM_CALL_DIRECTION_INCOMING | call from network. |
MM_CALL_DIRECTION_OUTGOING | call to network. |

Since: 1.6

### enum MMCallState

State of Call.

#### Members

MM_CALL_STATE_UNKNOWN | default state for a new outgoing call. |
MM_CALL_STATE_DIALING | outgoing call started. Wait for free channel. |
MM_CALL_STATE_RINGING_OUT | outgoing call attached to GSM network, waiting for an answer. |
MM_CALL_STATE_RINGING_IN | incoming call is waiting for an answer. |
MM_CALL_STATE_ACTIVE | call is active between two peers. |
MM_CALL_STATE_HELD | held call (by +CHLD AT command). |
MM_CALL_STATE_WAITING | waiting call (by +CCWA AT command). |
MM_CALL_STATE_TERMINATED | call is terminated. |

Since: 1.6

### enum MMCallStateReason

Reason for the state change in the call.

#### Members

MM_CALL_STATE_REASON_UNKNOWN | Default value for a new outgoing call. |
MM_CALL_STATE_REASON_OUTGOING_STARTED | Outgoing call is started. |
MM_CALL_STATE_REASON_INCOMING_NEW | Received a new incoming call. |
MM_CALL_STATE_REASON_ACCEPTED | Dialing or Ringing call is accepted. |
MM_CALL_STATE_REASON_TERMINATED | Call is correctly terminated. |
MM_CALL_STATE_REASON_REFUSED_OR_BUSY | Remote peer is busy or refused call. |
MM_CALL_STATE_REASON_ERROR | Wrong number or generic network error. |
MM_CALL_STATE_REASON_AUDIO_SETUP_FAILED | Error setting up audio channel. Since 1.10. |
MM_CALL_STATE_REASON_TRANSFERRED | Call has been transferred. Since 1.12. |
MM_CALL_STATE_REASON_DEFLECTED | Call has been deflected to a new number. Since 1.12. |

Since: 1.6

### enum MMFirmwareImageType

Type of firmware image.

#### Members

MM_FIRMWARE_IMAGE_TYPE_UNKNOWN | Unknown firmware type. |
MM_FIRMWARE_IMAGE_TYPE_GENERIC | Generic firmware image. |
MM_FIRMWARE_IMAGE_TYPE_GOBI | Firmware image of Gobi devices. |

Since: 1.0

### enum MMModem3gppFacility

A bitfield describing which facilities have a lock enabled, i.e., requires a pin or unlock code. The facilities include the personalizations (device locks) described in 3GPP spec TS 22.022, and the PIN and PIN2 locks, which are SIM locks.

#### Members

MM_MODEM_3GPP_FACILITY_NONE | No facility. |
MM_MODEM_3GPP_FACILITY_SIM | SIM lock. |
MM_MODEM_3GPP_FACILITY_FIXED_DIALING | Fixed dialing (PIN2) SIM lock. |
MM_MODEM_3GPP_FACILITY_PH_SIM | Device is locked to a specific SIM. |
MM_MODEM_3GPP_FACILITY_PH_FSIM | Device is locked to first SIM inserted. |
MM_MODEM_3GPP_FACILITY_NET_PERS | Network personalization. |
MM_MODEM_3GPP_FACILITY_NET_SUB_PERS | Network subset personalization. |
MM_MODEM_3GPP_FACILITY_PROVIDER_PERS | Service provider personalization. |
MM_MODEM_3GPP_FACILITY_CORP_PERS | Corporate personalization. |

Since: 1.0

### enum MMModem3gppNetworkAvailability

Network availability status as defined in 3GPP TS 27.007 section 7.3.

#### Members

MM_MODEM_3GPP_NETWORK_AVAILABILITY_UNKNOWN | Unknown availability. |
MM_MODEM_3GPP_NETWORK_AVAILABILITY_AVAILABLE | Network is available. |
MM_MODEM_3GPP_NETWORK_AVAILABILITY_CURRENT | Network is the current one. |
MM_MODEM_3GPP_NETWORK_AVAILABILITY_FORBIDDEN | Network is forbidden. |

Since: 1.0

### enum MMModem3gppSubscriptionState

Describes the current subscription status of the SIM. This value is only available after the modem attempts to register with the network.

#### Members

MM_MODEM_3GPP_SUBSCRIPTION_STATE_UNKNOWN | The subscription state is unknown. |
MM_MODEM_3GPP_SUBSCRIPTION_STATE_UNPROVISIONED | The account is unprovisioned. |
MM_MODEM_3GPP_SUBSCRIPTION_STATE_PROVISIONED | The account is provisioned and has data available. |
MM_MODEM_3GPP_SUBSCRIPTION_STATE_OUT_OF_DATA | The account is provisioned but there is no data left. |

Since: 1.2

### enum MMModem3gppRegistrationState

GSM registration code as defined in 3GPP TS 27.007.

#### Members

MM_MODEM_3GPP_REGISTRATION_STATE_IDLE | Not registered, not searching for new operator to register. |
MM_MODEM_3GPP_REGISTRATION_STATE_HOME | Registered on home network. |
MM_MODEM_3GPP_REGISTRATION_STATE_SEARCHING | Not registered, searching for new operator to register with. |
MM_MODEM_3GPP_REGISTRATION_STATE_DENIED | Registration denied. |
MM_MODEM_3GPP_REGISTRATION_STATE_UNKNOWN | Unknown registration status. |
MM_MODEM_3GPP_REGISTRATION_STATE_ROAMING | Registered on a roaming network. |
MM_MODEM_3GPP_REGISTRATION_STATE_HOME_SMS_ONLY | Registered for "SMS only", home network (applicable only when on LTE). Since 1.8. |
MM_MODEM_3GPP_REGISTRATION_STATE_ROAMING_SMS_ONLY | Registered for "SMS only", roaming network (applicable only when on LTE). Since 1.8. |
MM_MODEM_3GPP_REGISTRATION_STATE_EMERGENCY_ONLY | Emergency services only. Since 1.8. |
MM_MODEM_3GPP_REGISTRATION_STATE_HOME_CSFB_NOT_PREFERRED | Registered for "CSFB not preferred", home network (applicable only when on LTE). Since 1.8. |
MM_MODEM_3GPP_REGISTRATION_STATE_ROAMING_CSFB_NOT_PREFERRED | Registered for "CSFB not preferred", roaming network (applicable only when on LTE). Since 1.8. |
MM_MODEM_3GPP_REGISTRATION_STATE_ATTACHED_RLOS | Attached for access to Restricted Local Operator Services (applicable only when on LTE). Since 1.14. |

Since: 1.0

### enum MMModem3gppUssdSessionState

State of a USSD session.

#### Members

MM_MODEM_3GPP_USSD_SESSION_STATE_UNKNOWN | Unknown state. |
MM_MODEM_3GPP_USSD_SESSION_STATE_IDLE | No active session. |
MM_MODEM_3GPP_USSD_SESSION_STATE_ACTIVE | A session is active and the mobile is waiting for a response. |
MM_MODEM_3GPP_USSD_SESSION_STATE_USER_RESPONSE | The network is waiting for the client's response. |

Since: 1.0

### enum MMModem3gppEpsUeModeOperation

UE mode of operation for EPS, as per 3GPP TS 24.301.

#### Members

MM_MODEM_3GPP_EPS_UE_MODE_OPERATION_UNKNOWN | Unknown or not applicable. |
MM_MODEM_3GPP_EPS_UE_MODE_OPERATION_PS_1 | PS mode 1 of operation: EPS only, voice-centric. |
MM_MODEM_3GPP_EPS_UE_MODE_OPERATION_PS_2 | PS mode 2 of operation: EPS only, data-centric. |
MM_MODEM_3GPP_EPS_UE_MODE_OPERATION_CSPS_1 | CS/PS mode 1 of operation: EPS and non-EPS, voice-centric. |
MM_MODEM_3GPP_EPS_UE_MODE_OPERATION_CSPS_2 | CS/PS mode 2 of operation: EPS and non-EPS, data-centric. |

Since: 1.8

### enum MMModemAccessTechnology

Describes various access technologies that a device uses when registered with or connected to a network.

#### Members

MM_MODEM_ACCESS_TECHNOLOGY_UNKNOWN | The access technology used is unknown. |
MM_MODEM_ACCESS_TECHNOLOGY_POTS | Analog wireline telephone. |
MM_MODEM_ACCESS_TECHNOLOGY_GSM | GSM. |
MM_MODEM_ACCESS_TECHNOLOGY_GSM_COMPACT | Compact GSM. |
MM_MODEM_ACCESS_TECHNOLOGY_GPRS | GPRS. |
MM_MODEM_ACCESS_TECHNOLOGY_EDGE | EDGE (ETSI 27.007: "GSM w/EGPRS"). |
MM_MODEM_ACCESS_TECHNOLOGY_UMTS | UMTS (ETSI 27.007: "UTRAN"). |
MM_MODEM_ACCESS_TECHNOLOGY_HSDPA | HSDPA (ETSI 27.007: "UTRAN w/HSDPA"). |
MM_MODEM_ACCESS_TECHNOLOGY_HSUPA | HSUPA (ETSI 27.007: "UTRAN w/HSUPA"). |
MM_MODEM_ACCESS_TECHNOLOGY_HSPA | HSPA (ETSI 27.007: "UTRAN w/HSDPA and HSUPA"). |
MM_MODEM_ACCESS_TECHNOLOGY_HSPA_PLUS | HSPA+ (ETSI 27.007: "UTRAN w/HSPA+"). |
MM_MODEM_ACCESS_TECHNOLOGY_1XRTT | CDMA2000 1xRTT. |
MM_MODEM_ACCESS_TECHNOLOGY_EVDO0 | CDMA2000 EVDO revision 0. |
MM_MODEM_ACCESS_TECHNOLOGY_EVDOA | CDMA2000 EVDO revision A. |
MM_MODEM_ACCESS_TECHNOLOGY_EVDOB | CDMA2000 EVDO revision B. |
MM_MODEM_ACCESS_TECHNOLOGY_LTE | LTE (ETSI 27.007: "E-UTRAN") |
MM_MODEM_ACCESS_TECHNOLOGY_5GNR | 5GNR (ETSI 27.007: "NG-RAN"). Since 1.14. |
MM_MODEM_ACCESS_TECHNOLOGY_ANY | Mask specifying all access technologies. |

Since: 1.0

### enum MMModemBand

Radio bands supported by the device when connecting to a mobile network.

#### Members

MM_MODEM_BAND_UNKNOWN | Unknown or invalid band. |
MM_MODEM_BAND_EGSM | GSM/GPRS/EDGE 900 MHz. |
MM_MODEM_BAND_DCS | GSM/GPRS/EDGE 1800 MHz. |
MM_MODEM_BAND_PCS | GSM/GPRS/EDGE 1900 MHz. |
MM_MODEM_BAND_G850 | GSM/GPRS/EDGE 850 MHz. |
MM_MODEM_BAND_UTRAN_1 | UMTS 2100 MHz (IMT, UTRAN band 1). Since 1.8. |
MM_MODEM_BAND_UTRAN_3 | UMTS 1800 MHz (DCS, UTRAN band 3). Since 1.8. |
MM_MODEM_BAND_UTRAN_4 | UMTS 1700 MHz (AWS A-F, UTRAN band 4). Since 1.8. |
MM_MODEM_BAND_UTRAN_6 | UMTS 800 MHz (UTRAN band 6). Since 1.8. |
MM_MODEM_BAND_UTRAN_5 | UMTS 850 MHz (CLR, UTRAN band 5). Since 1.8. |
MM_MODEM_BAND_UTRAN_8 | UMTS 900 MHz (E-GSM, UTRAN band 8). Since 1.8. |
MM_MODEM_BAND_UTRAN_9 | UMTS 1700 MHz (UTRAN band 9). Since 1.8. |
MM_MODEM_BAND_UTRAN_2 | UMTS 1900 MHz (PCS A-F, UTRAN band 2). Since 1.8. |
MM_MODEM_BAND_UTRAN_7 | UMTS 2600 MHz (IMT-E, UTRAN band 7). Since 1.8. |
MM_MODEM_BAND_G450 | GSM/GPRS/EDGE 450 MHz. |
MM_MODEM_BAND_G480 | GSM/GPRS/EDGE 480 MHz. |
MM_MODEM_BAND_G750 | GSM/GPRS/EDGE 750 MHz. |
MM_MODEM_BAND_G380 | GSM/GPRS/EDGE 380 MHz. |
MM_MODEM_BAND_G410 | GSM/GPRS/EDGE 410 MHz. |
MM_MODEM_BAND_G710 | GSM/GPRS/EDGE 710 MHz. |
MM_MODEM_BAND_G810 | GSM/GPRS/EDGE 810 MHz. |
MM_MODEM_BAND_EUTRAN_1 | E-UTRAN band 1. Since 1.8. |
MM_MODEM_BAND_EUTRAN_2 | E-UTRAN band 2. Since 1.8. |
MM_MODEM_BAND_EUTRAN_3 | E-UTRAN band 3. Since 1.8. |
MM_MODEM_BAND_EUTRAN_4 | E-UTRAN band 4. Since 1.8. |
MM_MODEM_BAND_EUTRAN_5 | E-UTRAN band 5. Since 1.8. |
MM_MODEM_BAND_EUTRAN_6 | E-UTRAN band 6. Since 1.8. |
MM_MODEM_BAND_EUTRAN_7 | E-UTRAN band 7. Since 1.8. |
MM_MODEM_BAND_EUTRAN_8 | E-UTRAN band 8. Since 1.8. |
MM_MODEM_BAND_EUTRAN_9 | E-UTRAN band 9. Since 1.8. |
MM_MODEM_BAND_EUTRAN_10 | E-UTRAN band 10. Since 1.8. |
MM_MODEM_BAND_EUTRAN_11 | E-UTRAN band 11. Since 1.8. |
MM_MODEM_BAND_EUTRAN_12 | E-UTRAN band 12. Since 1.8. |
MM_MODEM_BAND_EUTRAN_13 | E-UTRAN band 13. Since 1.8. |
MM_MODEM_BAND_EUTRAN_14 | E-UTRAN band 14. Since 1.8. |
MM_MODEM_BAND_EUTRAN_17 | E-UTRAN band 17. Since 1.8. |
MM_MODEM_BAND_EUTRAN_18 | E-UTRAN band 18. Since 1.8. |
MM_MODEM_BAND_EUTRAN_19 | E-UTRAN band 19. Since 1.8. |
MM_MODEM_BAND_EUTRAN_20 | E-UTRAN band 20. Since 1.8. |
MM_MODEM_BAND_EUTRAN_21 | E-UTRAN band 21. Since 1.8. |
MM_MODEM_BAND_EUTRAN_22 | E-UTRAN band 22. Since 1.8. |
MM_MODEM_BAND_EUTRAN_23 | E-UTRAN band 23. Since 1.8. |
MM_MODEM_BAND_EUTRAN_24 | E-UTRAN band 24. Since 1.8. |
MM_MODEM_BAND_EUTRAN_25 | E-UTRAN band 25. Since 1.8. |
MM_MODEM_BAND_EUTRAN_26 | E-UTRAN band 26. Since 1.8. |
MM_MODEM_BAND_EUTRAN_27 | E-UTRAN band 27. Since 1.8. |
MM_MODEM_BAND_EUTRAN_28 | E-UTRAN band 28. Since 1.8. |
MM_MODEM_BAND_EUTRAN_29 | E-UTRAN band 29. Since 1.8. |
MM_MODEM_BAND_EUTRAN_30 | E-UTRAN band 30. Since 1.8. |
MM_MODEM_BAND_EUTRAN_31 | E-UTRAN band 31. Since 1.8. |
MM_MODEM_BAND_EUTRAN_32 | E-UTRAN band 32. Since 1.8. |
MM_MODEM_BAND_EUTRAN_33 | E-UTRAN band 33. Since 1.8. |
MM_MODEM_BAND_EUTRAN_34 | E-UTRAN band 34. Since 1.8. |
MM_MODEM_BAND_EUTRAN_35 | E-UTRAN band 35. Since 1.8. |
MM_MODEM_BAND_EUTRAN_36 | E-UTRAN band 36. Since 1.8. |
MM_MODEM_BAND_EUTRAN_37 | E-UTRAN band 37. Since 1.8. |
MM_MODEM_BAND_EUTRAN_38 | E-UTRAN band 38. Since 1.8. |
MM_MODEM_BAND_EUTRAN_39 | E-UTRAN band 39. Since 1.8. |
MM_MODEM_BAND_EUTRAN_40 | E-UTRAN band 40. Since 1.8. |
MM_MODEM_BAND_EUTRAN_41 | E-UTRAN band 41. Since 1.8. |
MM_MODEM_BAND_EUTRAN_42 | E-UTRAN band 42. Since 1.8. |
MM_MODEM_BAND_EUTRAN_43 | E-UTRAN band 43. Since 1.8. |
MM_MODEM_BAND_EUTRAN_44 | E-UTRAN band 44. Since 1.8. |
MM_MODEM_BAND_EUTRAN_45 | E-UTRAN band 45. Since 1.8. |
MM_MODEM_BAND_EUTRAN_46 | E-UTRAN band 46. Since 1.8. |
MM_MODEM_BAND_EUTRAN_47 | E-UTRAN band 47. Since 1.8. |
MM_MODEM_BAND_EUTRAN_48 | E-UTRAN band 48. Since 1.8. |
MM_MODEM_BAND_EUTRAN_49 | E-UTRAN band 49. Since 1.10. |
MM_MODEM_BAND_EUTRAN_50 | E-UTRAN band 50. Since 1.10. |
MM_MODEM_BAND_EUTRAN_51 | E-UTRAN band 51. Since 1.10. |
MM_MODEM_BAND_EUTRAN_52 | E-UTRAN band 52. Since 1.10. |
MM_MODEM_BAND_EUTRAN_53 | E-UTRAN band 53. Since 1.10. |
MM_MODEM_BAND_EUTRAN_54 | E-UTRAN band 54. Since 1.10. |
MM_MODEM_BAND_EUTRAN_55 | E-UTRAN band 55. Since 1.10. |
MM_MODEM_BAND_EUTRAN_56 | E-UTRAN band 56. Since 1.10. |
MM_MODEM_BAND_EUTRAN_57 | E-UTRAN band 57. Since 1.10. |
MM_MODEM_BAND_EUTRAN_58 | E-UTRAN band 58. Since 1.10. |
MM_MODEM_BAND_EUTRAN_59 | E-UTRAN band 59. Since 1.10. |
MM_MODEM_BAND_EUTRAN_60 | E-UTRAN band 60. Since 1.10. |
MM_MODEM_BAND_EUTRAN_61 | E-UTRAN band 61. Since 1.10. |
MM_MODEM_BAND_EUTRAN_62 | E-UTRAN band 62. Since 1.10. |
MM_MODEM_BAND_EUTRAN_63 | E-UTRAN band 63. Since 1.10. |
MM_MODEM_BAND_EUTRAN_64 | E-UTRAN band 64. Since 1.10. |
MM_MODEM_BAND_EUTRAN_65 | E-UTRAN band 65. Since 1.8. |
MM_MODEM_BAND_EUTRAN_66 | E-UTRAN band 66. Since 1.8. |
MM_MODEM_BAND_EUTRAN_67 | E-UTRAN band 67. Since 1.8. |
MM_MODEM_BAND_EUTRAN_68 | E-UTRAN band 68. Since 1.8. |
MM_MODEM_BAND_EUTRAN_69 | E-UTRAN band 69. Since 1.8. |
MM_MODEM_BAND_EUTRAN_70 | E-UTRAN band 70. Since 1.8. |
MM_MODEM_BAND_EUTRAN_71 | E-UTRAN band 71. Since 1.8. |
MM_MODEM_BAND_CDMA_BC0 | CDMA Band Class 0 (US Cellular 850MHz). Since 1.8. |
MM_MODEM_BAND_CDMA_BC1 | CDMA Band Class 1 (US PCS 1900MHz). Since 1.8. |
MM_MODEM_BAND_CDMA_BC2 | CDMA Band Class 2 (UK TACS 900MHz). Since 1.8. |
MM_MODEM_BAND_CDMA_BC3 | CDMA Band Class 3 (Japanese TACS). Since 1.8. |
MM_MODEM_BAND_CDMA_BC4 | CDMA Band Class 4 (Korean PCS). Since 1.8. |
MM_MODEM_BAND_CDMA_BC5 | CDMA Band Class 5 (NMT 450MHz). Since 1.8. |
MM_MODEM_BAND_CDMA_BC6 | CDMA Band Class 6 (IMT2000 2100MHz). Since 1.8. |
MM_MODEM_BAND_CDMA_BC7 | CDMA Band Class 7 (Cellular 700MHz). Since 1.8. |
MM_MODEM_BAND_CDMA_BC8 | CDMA Band Class 8 (1800MHz). Since 1.8. |
MM_MODEM_BAND_CDMA_BC9 | CDMA Band Class 9 (900MHz). Since 1.8. |
MM_MODEM_BAND_CDMA_BC10 | CDMA Band Class 10 (US Secondary 800). Since 1.8. |
MM_MODEM_BAND_CDMA_BC11 | CDMA Band Class 11 (European PAMR 400MHz). Since 1.8. |
MM_MODEM_BAND_CDMA_BC12 | CDMA Band Class 12 (PAMR 800MHz). Since 1.8. |
MM_MODEM_BAND_CDMA_BC13 | CDMA Band Class 13 (IMT2000 2500MHz Expansion). Since 1.8. |
MM_MODEM_BAND_CDMA_BC14 | CDMA Band Class 14 (More US PCS 1900MHz). Since 1.8. |
MM_MODEM_BAND_CDMA_BC15 | CDMA Band Class 15 (AWS 1700MHz). Since 1.8. |
MM_MODEM_BAND_CDMA_BC16 | CDMA Band Class 16 (US 2500MHz). Since 1.8. |
MM_MODEM_BAND_CDMA_BC17 | CDMA Band Class 17 (US 2500MHz Forward Link Only). Since 1.8. |
MM_MODEM_BAND_CDMA_BC18 | CDMA Band Class 18 (US 700MHz Public Safety). Since 1.8. |
MM_MODEM_BAND_CDMA_BC19 | CDMA Band Class 19 (US Lower 700MHz). Since 1.8. |
MM_MODEM_BAND_UTRAN_10 | UMTS 1700 MHz (EAWS A-G, UTRAN band 10). Since 1.8. |
MM_MODEM_BAND_UTRAN_11 | UMTS 1500 MHz (LPDC, UTRAN band 11). Since 1.8. |
MM_MODEM_BAND_UTRAN_12 | UMTS 700 MHz (LSMH A/B/C, UTRAN band 12). Since 1.8. |
MM_MODEM_BAND_UTRAN_13 | UMTS 700 MHz (USMH C, UTRAN band 13). Since 1.8. |
MM_MODEM_BAND_UTRAN_14 | UMTS 700 MHz (USMH D, UTRAN band 14). Since 1.8. |
MM_MODEM_BAND_UTRAN_19 | UMTS 800 MHz (UTRAN band 19). Since 1.8. |
MM_MODEM_BAND_UTRAN_20 | UMTS 800 MHz (EUDD, UTRAN band 20). Since 1.8. |
MM_MODEM_BAND_UTRAN_21 | UMTS 1500 MHz (UPDC, UTRAN band 21). Since 1.8. |
MM_MODEM_BAND_UTRAN_22 | UMTS 3500 MHz (UTRAN band 22). Since 1.8. |
MM_MODEM_BAND_UTRAN_25 | UMTS 1900 MHz (EPCS A-G, UTRAN band 25). Since 1.8. |
MM_MODEM_BAND_UTRAN_26 | UMTS 850 MHz (ECLR, UTRAN band 26). Since 1.8. |
MM_MODEM_BAND_UTRAN_32 | UMTS 1500 MHz (L-band, UTRAN band 32). Since 1.8. |
MM_MODEM_BAND_ANY | For certain operations, allow the modem to select a band automatically. |

Since: 1.0

### enum MMModemCapability

Flags describing one or more of the general access technology families that a modem supports.

#### Members

MM_MODEM_CAPABILITY_NONE | Modem has no capabilities. |
MM_MODEM_CAPABILITY_POTS | Modem supports the analog wired telephone network (ie 56k dialup) and does not have wireless/cellular capabilities. |
MM_MODEM_CAPABILITY_CDMA_EVDO | Modem supports at least one of CDMA 1xRTT, EVDO revision 0, EVDO revision A, or EVDO revision B. |
MM_MODEM_CAPABILITY_GSM_UMTS | Modem supports at least one of GSM, GPRS, EDGE, UMTS, HSDPA, HSUPA, or HSPA+ packet switched data capability. |
MM_MODEM_CAPABILITY_LTE | Modem has LTE data capability. |
MM_MODEM_CAPABILITY_IRIDIUM | Modem has Iridium capabilities. |
MM_MODEM_CAPABILITY_5GNR | Modem has 5GNR capabilities. Since 1.14. |
MM_MODEM_CAPABILITY_ANY | Mask specifying all capabilities. |

Since: 1.0

### enum MMModemCdmaActivationState

Activation state of a CDMA modem.

#### Members

MM_MODEM_CDMA_ACTIVATION_STATE_UNKNOWN | Unknown activation state. |
MM_MODEM_CDMA_ACTIVATION_STATE_NOT_ACTIVATED | Device is not activated |
MM_MODEM_CDMA_ACTIVATION_STATE_ACTIVATING | Device is activating |
MM_MODEM_CDMA_ACTIVATION_STATE_PARTIALLY_ACTIVATED | Device is partially activated; carrier-specific steps required to continue. |
MM_MODEM_CDMA_ACTIVATION_STATE_ACTIVATED | Device is ready for use. |

Since: 1.0

### enum MMModemCdmaRegistrationState

Registration state of a CDMA modem.

#### Members

MM_MODEM_CDMA_REGISTRATION_STATE_UNKNOWN | Registration status is unknown or the device is not registered. |
MM_MODEM_CDMA_REGISTRATION_STATE_REGISTERED | Registered, but roaming status is unknown or cannot be provided by the device. The device may or may not be roaming. |
MM_MODEM_CDMA_REGISTRATION_STATE_HOME | Currently registered on the home network. |
MM_MODEM_CDMA_REGISTRATION_STATE_ROAMING | Currently registered on a roaming network. |

Since: 1.0

### enum MMModemCdmaRmProtocol

Protocol of the Rm interface in modems with CDMA capabilities.

#### Members

MM_MODEM_CDMA_RM_PROTOCOL_UNKNOWN | Unknown protocol. |
MM_MODEM_CDMA_RM_PROTOCOL_ASYNC | Asynchronous data or fax. |
MM_MODEM_CDMA_RM_PROTOCOL_PACKET_RELAY | Packet data service, Relay Layer Rm interface. |
MM_MODEM_CDMA_RM_PROTOCOL_PACKET_NETWORK_PPP | Packet data service, Network Layer Rm interface, PPP. |
MM_MODEM_CDMA_RM_PROTOCOL_PACKET_NETWORK_SLIP | Packet data service, Network Layer Rm interface, SLIP. |
MM_MODEM_CDMA_RM_PROTOCOL_STU_III | STU-III service. |

Since: 1.0

### enum MMModemContactsStorage

Specifies different storage locations for contact information.

#### Members

MM_MODEM_CONTACTS_STORAGE_UNKNOWN | Unknown location. |
MM_MODEM_CONTACTS_STORAGE_ME | Device's local memory. |
MM_MODEM_CONTACTS_STORAGE_SM | Card inserted in the device (like a SIM/RUIM). |
MM_MODEM_CONTACTS_STORAGE_MT | Combined device/ME and SIM/SM phonebook. |

Since: 1.0

### enum MMModemLocationSource

Sources of location information supported by the modem.

#### Members

MM_MODEM_LOCATION_SOURCE_NONE | None. |
MM_MODEM_LOCATION_SOURCE_3GPP_LAC_CI | Location Area Code and Cell ID. |
MM_MODEM_LOCATION_SOURCE_GPS_RAW | GPS location given by predefined keys. |
MM_MODEM_LOCATION_SOURCE_GPS_NMEA | GPS location given as NMEA traces. |
MM_MODEM_LOCATION_SOURCE_CDMA_BS | CDMA base station position. |
MM_MODEM_LOCATION_SOURCE_GPS_UNMANAGED | No location given, just GPS module setup. Since 1.4. |
MM_MODEM_LOCATION_SOURCE_AGPS_MSA | Mobile Station Assisted A-GPS location requested. Since 1.12. |
MM_MODEM_LOCATION_SOURCE_AGPS_MSB | Mobile Station Based A-GPS location requested. Since 1.12. |

Since: 1.0

### enum MMModemLocationAssistanceDataType

Type of assistance data that may be injected to the GNSS module.

#### Members

MM_MODEM_LOCATION_ASSISTANCE_DATA_TYPE_NONE | None. |
MM_MODEM_LOCATION_ASSISTANCE_DATA_TYPE_XTRA | Qualcomm gpsOneXTRA. |

Since: 1.10

### enum MMModemLock

Enumeration of possible lock reasons.

#### Members

MM_MODEM_LOCK_UNKNOWN | Lock reason unknown. |
MM_MODEM_LOCK_NONE | Modem is unlocked. |
MM_MODEM_LOCK_SIM_PIN | SIM requires the PIN code. |
MM_MODEM_LOCK_SIM_PIN2 | SIM requires the PIN2 code. |
MM_MODEM_LOCK_SIM_PUK | SIM requires the PUK code. |
MM_MODEM_LOCK_SIM_PUK2 | SIM requires the PUK2 code. |
MM_MODEM_LOCK_PH_SP_PIN | Modem requires the service provider PIN code. |
MM_MODEM_LOCK_PH_SP_PUK | Modem requires the service provider PUK code. |
MM_MODEM_LOCK_PH_NET_PIN | Modem requires the network PIN code. |
MM_MODEM_LOCK_PH_NET_PUK | Modem requires the network PUK code. |
MM_MODEM_LOCK_PH_SIM_PIN | Modem requires the PIN code. |
MM_MODEM_LOCK_PH_CORP_PIN | Modem requires the corporate PIN code. |
MM_MODEM_LOCK_PH_CORP_PUK | Modem requires the corporate PUK code. |
MM_MODEM_LOCK_PH_FSIM_PIN | Modem requires the PH-FSIM PIN code. |
MM_MODEM_LOCK_PH_FSIM_PUK | Modem requires the PH-FSIM PUK code. |
MM_MODEM_LOCK_PH_NETSUB_PIN | Modem requires the network subset PIN code. |
MM_MODEM_LOCK_PH_NETSUB_PUK | Modem requires the network subset PUK code. |

Since: 1.0

### enum MMModemMode

Bitfield to indicate which access modes are supported, allowed or preferred in a given device.

#### Members

MM_MODEM_MODE_NONE | None. |
MM_MODEM_MODE_CS | CSD, GSM, and other circuit-switched technologies. |
MM_MODEM_MODE_2G | GPRS, EDGE. |
MM_MODEM_MODE_3G | UMTS, HSxPA. |
MM_MODEM_MODE_4G | LTE. |
MM_MODEM_MODE_5G | 5GNR. Since 1.14. |
MM_MODEM_MODE_ANY | Any mode can be used (only this value allowed for POTS modems). |

Since: 1.0

### enum MMModemState

Enumeration of possible modem states.

#### Members

MM_MODEM_STATE_FAILED | The modem is unusable. |
MM_MODEM_STATE_UNKNOWN | State unknown or not reportable. |
MM_MODEM_STATE_INITIALIZING | The modem is currently being initialized. |
MM_MODEM_STATE_LOCKED | The modem needs to be unlocked. |
MM_MODEM_STATE_DISABLED | The modem is not enabled and is powered down. |
MM_MODEM_STATE_DISABLING | The modem is currently transitioning to the `MM_MODEM_STATE_DISABLED` state. |
MM_MODEM_STATE_ENABLING | The modem is currently transitioning to the `MM_MODEM_STATE_ENABLED` state. |
MM_MODEM_STATE_ENABLED | The modem is enabled and powered on but not registered with a network provider and not available for data connections. |
MM_MODEM_STATE_SEARCHING | The modem is searching for a network provider to register with. |
MM_MODEM_STATE_REGISTERED | The modem is registered with a network provider, and data connections and messaging may be available for use. |
MM_MODEM_STATE_DISCONNECTING | The modem is disconnecting and deactivating the last active packet data bearer. This state will not be entered if more than one packet data bearer is active and one of the active bearers is deactivated. |
MM_MODEM_STATE_CONNECTING | The modem is activating and connecting the first packet data bearer. Subsequent bearer activations when another bearer is already active do not cause this state to be entered. |
MM_MODEM_STATE_CONNECTED | One or more packet data bearers is active and connected. |

Since: 1.0

### enum MMModemStateFailedReason

Enumeration of possible errors when the modem is in `MM_MODEM_STATE_FAILED` .

#### Members

MM_MODEM_STATE_FAILED_REASON_NONE | No error. |
MM_MODEM_STATE_FAILED_REASON_UNKNOWN | Unknown error. |
MM_MODEM_STATE_FAILED_REASON_SIM_MISSING | SIM is required but missing. |
MM_MODEM_STATE_FAILED_REASON_SIM_ERROR | SIM is available, but unusable (e.g. permanently locked). |

Since: 1.0

### enum MMModemStateChangeReason

Enumeration of possible reasons to have changed the modem state.

#### Members

MM_MODEM_STATE_CHANGE_REASON_UNKNOWN | Reason unknown or not reportable. |
MM_MODEM_STATE_CHANGE_REASON_USER_REQUESTED | State change was requested by an interface user. |
MM_MODEM_STATE_CHANGE_REASON_SUSPEND | State change was caused by a system suspend. |
MM_MODEM_STATE_CHANGE_REASON_FAILURE | State change was caused by an unrecoverable error. |

Since: 1.0

### enum MMModemPowerState

Power state of the modem.

#### Members

MM_MODEM_POWER_STATE_UNKNOWN | Unknown power state. |
MM_MODEM_POWER_STATE_OFF | Off. |
MM_MODEM_POWER_STATE_LOW | Low-power mode. |
MM_MODEM_POWER_STATE_ON | Full power mode. |

Since: 1.0

### enum MMModemPortType

Type of modem port.

#### Members

MM_MODEM_PORT_TYPE_UNKNOWN | Unknown. |
MM_MODEM_PORT_TYPE_NET | Net port. |
MM_MODEM_PORT_TYPE_AT | AT port. |
MM_MODEM_PORT_TYPE_QCDM | QCDM port. |
MM_MODEM_PORT_TYPE_GPS | GPS port. |
MM_MODEM_PORT_TYPE_QMI | QMI port. |
MM_MODEM_PORT_TYPE_MBIM | MBIM port. |
MM_MODEM_PORT_TYPE_AUDIO | Audio port. Since 1.12. |
MM_MODEM_PORT_TYPE_IGNORED | Ignored port. Since 1.16. |

Since: 1.0

### enum MMModemFirmwareUpdateMethod

Type of firmware update method supported by the module.

#### Members

MM_MODEM_FIRMWARE_UPDATE_METHOD_NONE | No method specified. |
MM_MODEM_FIRMWARE_UPDATE_METHOD_FASTBOOT | Device supports fastboot-based update. |
MM_MODEM_FIRMWARE_UPDATE_METHOD_QMI_PDC | Device supports QMI PDC based update. |
MM_MODEM_FIRMWARE_UPDATE_METHOD_MBIM_QDU | Device supports MBIM QDU based update. Since 1.18. |
MM_MODEM_FIRMWARE_UPDATE_METHOD_FIREHOSE | Device supports Firehose based update. Since 1.18. |

Since: 1.10

### enum MMOmaFeature

Features that can be enabled or disabled in the OMA device management support.

#### Members

MM_OMA_FEATURE_NONE | None. |
MM_OMA_FEATURE_DEVICE_PROVISIONING | Device provisioning service. |
MM_OMA_FEATURE_PRL_UPDATE | PRL update service. |
MM_OMA_FEATURE_HANDS_FREE_ACTIVATION | Hands free activation service. |

Since: 1.2

### enum MMOmaSessionState

State of the OMA device management session.

#### Members

MM_OMA_SESSION_STATE_FAILED | Failed. |
MM_OMA_SESSION_STATE_UNKNOWN | Unknown. |
MM_OMA_SESSION_STATE_STARTED | Started. |
MM_OMA_SESSION_STATE_RETRYING | Retrying. |
MM_OMA_SESSION_STATE_CONNECTING | Connecting. |
MM_OMA_SESSION_STATE_CONNECTED | Connected. |
MM_OMA_SESSION_STATE_AUTHENTICATED | Authenticated. |
MM_OMA_SESSION_STATE_MDN_DOWNLOADED | MDN downloaded. |
MM_OMA_SESSION_STATE_MSID_DOWNLOADED | MSID downloaded. |
MM_OMA_SESSION_STATE_PRL_DOWNLOADED | PRL downloaded. |
MM_OMA_SESSION_STATE_MIP_PROFILE_DOWNLOADED | MIP profile downloaded. |
MM_OMA_SESSION_STATE_COMPLETED | Session completed. |

Since: 1.2

### enum MMOmaSessionStateFailedReason

Reason of failure in the OMA device management session.

#### Members

MM_OMA_SESSION_STATE_FAILED_REASON_UNKNOWN | No reason or unknown. |
MM_OMA_SESSION_STATE_FAILED_REASON_NETWORK_UNAVAILABLE | Network unavailable. |
MM_OMA_SESSION_STATE_FAILED_REASON_SERVER_UNAVAILABLE | Server unavailable. |
MM_OMA_SESSION_STATE_FAILED_REASON_AUTHENTICATION_FAILED | Authentication failed. |
MM_OMA_SESSION_STATE_FAILED_REASON_MAX_RETRY_EXCEEDED | Maximum retries exceeded. |
MM_OMA_SESSION_STATE_FAILED_REASON_SESSION_CANCELLED | Session cancelled. |

Since: 1.2

### enum MMOmaSessionType

Type of OMA device management session.

#### Members

MM_OMA_SESSION_TYPE_UNKNOWN | Unknown session type. |
MM_OMA_SESSION_TYPE_CLIENT_INITIATED_DEVICE_CONFIGURE | Client-initiated device configure. |
MM_OMA_SESSION_TYPE_CLIENT_INITIATED_PRL_UPDATE | Client-initiated PRL update. |
MM_OMA_SESSION_TYPE_CLIENT_INITIATED_HANDS_FREE_ACTIVATION | Client-initiated hands free activation. |
MM_OMA_SESSION_TYPE_NETWORK_INITIATED_DEVICE_CONFIGURE | Network-initiated device configure. |
MM_OMA_SESSION_TYPE_NETWORK_INITIATED_PRL_UPDATE | Network-initiated PRL update. |
MM_OMA_SESSION_TYPE_DEVICE_INITIATED_PRL_UPDATE | Device-initiated PRL update. |
MM_OMA_SESSION_TYPE_DEVICE_INITIATED_HANDS_FREE_ACTIVATION | Device-initiated hands free activation. |

Since: 1.2

### enum MMSmsPduType

Type of PDUs used in the SMS.

#### Members

MM_SMS_PDU_TYPE_UNKNOWN | Unknown type. |
MM_SMS_PDU_TYPE_DELIVER | 3GPP Mobile-Terminated (MT) message. |
MM_SMS_PDU_TYPE_SUBMIT | 3GPP Mobile-Originated (MO) message. |
MM_SMS_PDU_TYPE_STATUS_REPORT | 3GPP status report (MT). |
MM_SMS_PDU_TYPE_CDMA_DELIVER | 3GPP2 Mobile-Terminated (MT) message. Since 1.2. |
MM_SMS_PDU_TYPE_CDMA_SUBMIT | 3GPP2 Mobile-Originated (MO) message. Since 1.2. |
MM_SMS_PDU_TYPE_CDMA_CANCELLATION | 3GPP2 Cancellation (MO) message. Since 1.2. |
MM_SMS_PDU_TYPE_CDMA_DELIVERY_ACKNOWLEDGEMENT | 3GPP2 Delivery Acknowledgement (MT) message. Since 1.2. |
MM_SMS_PDU_TYPE_CDMA_USER_ACKNOWLEDGEMENT | 3GPP2 User Acknowledgement (MT or MO) message. Since 1.2. |
MM_SMS_PDU_TYPE_CDMA_READ_ACKNOWLEDGEMENT | 3GPP2 Read Acknowledgement (MT or MO) message. Since 1.2. |

Since: 1.0

### enum MMSmsState

State of a given SMS.

#### Members

MM_SMS_STATE_UNKNOWN | State unknown or not reportable. |
MM_SMS_STATE_STORED | The message has been neither received nor yet sent. |
MM_SMS_STATE_RECEIVING | The message is being received but is not yet complete. |
MM_SMS_STATE_RECEIVED | The message has been completely received. |
MM_SMS_STATE_SENDING | The message is queued for delivery. |
MM_SMS_STATE_SENT | The message was successfully sent. |

Since: 1.0

### enum MMSmsDeliveryState

Enumeration of known SMS delivery states as defined in 3GPP TS 03.40 and 3GPP2 N.S0005-O, section 6.5.2.125.

States out of the known ranges may also be valid (either reserved or SC-specific).

#### Members

MM_SMS_DELIVERY_STATE_COMPLETED_RECEIVED | Delivery completed, message received by the SME. |
MM_SMS_DELIVERY_STATE_COMPLETED_FORWARDED_UNCONFIRMED | Forwarded by the SC to the SME but the SC is unable to confirm delivery. |
MM_SMS_DELIVERY_STATE_COMPLETED_REPLACED_BY_SC | Message replaced by the SC. |
MM_SMS_DELIVERY_STATE_TEMPORARY_ERROR_CONGESTION | Temporary error, congestion. |
MM_SMS_DELIVERY_STATE_TEMPORARY_ERROR_SME_BUSY | Temporary error, SME busy. |
MM_SMS_DELIVERY_STATE_TEMPORARY_ERROR_NO_RESPONSE_FROM_SME | Temporary error, no response from the SME. |
MM_SMS_DELIVERY_STATE_TEMPORARY_ERROR_SERVICE_REJECTED | Temporary error, service rejected. |
MM_SMS_DELIVERY_STATE_TEMPORARY_ERROR_QOS_NOT_AVAILABLE | Temporary error, QoS not available. |
MM_SMS_DELIVERY_STATE_TEMPORARY_ERROR_IN_SME | Temporary error in the SME. |
MM_SMS_DELIVERY_STATE_ERROR_REMOTE_PROCEDURE | Permanent remote procedure error. |
MM_SMS_DELIVERY_STATE_ERROR_INCOMPATIBLE_DESTINATION | Permanent error, incompatible destination. |
MM_SMS_DELIVERY_STATE_ERROR_CONNECTION_REJECTED | Permanent error, connection rejected by the SME. |
MM_SMS_DELIVERY_STATE_ERROR_NOT_OBTAINABLE | Permanent error, not obtainable. |
MM_SMS_DELIVERY_STATE_ERROR_QOS_NOT_AVAILABLE | Permanent error, QoS not available. |
MM_SMS_DELIVERY_STATE_ERROR_NO_INTERWORKING_AVAILABLE | Permanent error, no interworking available. |
MM_SMS_DELIVERY_STATE_ERROR_VALIDITY_PERIOD_EXPIRED | Permanent error, message validity period expired. |
MM_SMS_DELIVERY_STATE_ERROR_DELETED_BY_ORIGINATING_SME | Permanent error, deleted by originating SME. |
MM_SMS_DELIVERY_STATE_ERROR_DELETED_BY_SC_ADMINISTRATION | Permanent error, deleted by SC administration. |
MM_SMS_DELIVERY_STATE_ERROR_MESSAGE_DOES_NOT_EXIST | Permanent error, message does no longer exist. |
MM_SMS_DELIVERY_STATE_TEMPORARY_FATAL_ERROR_CONGESTION | Permanent error, congestion. |
MM_SMS_DELIVERY_STATE_TEMPORARY_FATAL_ERROR_SME_BUSY | Permanent error, SME busy. |
MM_SMS_DELIVERY_STATE_TEMPORARY_FATAL_ERROR_NO_RESPONSE_FROM_SME | Permanent error, no response from the SME. |
MM_SMS_DELIVERY_STATE_TEMPORARY_FATAL_ERROR_SERVICE_REJECTED | Permanent error, service rejected. |
MM_SMS_DELIVERY_STATE_TEMPORARY_FATAL_ERROR_QOS_NOT_AVAILABLE | Permanent error, QoS not available. |
MM_SMS_DELIVERY_STATE_TEMPORARY_FATAL_ERROR_IN_SME | Permanent error in SME. |
MM_SMS_DELIVERY_STATE_UNKNOWN | Unknown state. |
MM_SMS_DELIVERY_STATE_NETWORK_PROBLEM_ADDRESS_VACANT | Permanent error in network, address vacant. Since 1.2. |
MM_SMS_DELIVERY_STATE_NETWORK_PROBLEM_ADDRESS_TRANSLATION_FAILURE | Permanent error in network, address translation failure. Since 1.2. |
MM_SMS_DELIVERY_STATE_NETWORK_PROBLEM_NETWORK_RESOURCE_OUTAGE | Permanent error in network, network resource outage. Since 1.2. |
MM_SMS_DELIVERY_STATE_NETWORK_PROBLEM_NETWORK_FAILURE | Permanent error in network, network failure. Since 1.2. |
MM_SMS_DELIVERY_STATE_NETWORK_PROBLEM_INVALID_TELESERVICE_ID | Permanent error in network, invalid teleservice id. Since 1.2. |
MM_SMS_DELIVERY_STATE_NETWORK_PROBLEM_OTHER | Permanent error, other network problem. Since 1.2. |
MM_SMS_DELIVERY_STATE_TERMINAL_PROBLEM_NO_PAGE_RESPONSE | Permanent error in terminal, no page response. Since 1.2. |
MM_SMS_DELIVERY_STATE_TERMINAL_PROBLEM_DESTINATION_BUSY | Permanent error in terminal, destination busy. Since 1.2. |
MM_SMS_DELIVERY_STATE_TERMINAL_PROBLEM_NO_ACKNOWLEDGMENT | Permanent error in terminal, no acknowledgement. Since 1.2. |
MM_SMS_DELIVERY_STATE_TERMINAL_PROBLEM_DESTINATION_RESOURCE_SHORTAGE | Permanent error in terminal, destination resource shortage. Since 1.2. |
MM_SMS_DELIVERY_STATE_TERMINAL_PROBLEM_SMS_DELIVERY_POSTPONED | Permanent error in terminal, SMS delivery postponed. Since 1.2. |
MM_SMS_DELIVERY_STATE_TERMINAL_PROBLEM_DESTINATION_OUT_OF_SERVICE | Permanent error in terminal, destination out of service. Since 1.2. |
MM_SMS_DELIVERY_STATE_TERMINAL_PROBLEM_DESTINATION_NO_LONGER_AT_THIS_ADDRESS | Permanent error in terminal, destination no longer at this address. Since 1.2. |
MM_SMS_DELIVERY_STATE_TERMINAL_PROBLEM_OTHER | Permanent error, other terminal problem. Since 1.2. |
MM_SMS_DELIVERY_STATE_RADIO_INTERFACE_PROBLEM_RESOURCE_SHORTAGE | Permanent error in radio interface, resource shortage. Since 1.2. |
MM_SMS_DELIVERY_STATE_RADIO_INTERFACE_PROBLEM_INCOMPATIBILITY | Permanent error in radio interface, problem incompatibility. Since 1.2. |
MM_SMS_DELIVERY_STATE_RADIO_INTERFACE_PROBLEM_OTHER | Permanent error, other radio interface problem. Since 1.2. |
MM_SMS_DELIVERY_STATE_GENERAL_PROBLEM_ENCODING | Permanent error, encoding. Since 1.2. |
MM_SMS_DELIVERY_STATE_GENERAL_PROBLEM_SMS_ORIGINATION_DENIED | Permanent error, SMS origination denied. Since 1.2. |
MM_SMS_DELIVERY_STATE_GENERAL_PROBLEM_SMS_TERMINATION_DENIED | Permanent error, SMS termination denied. Since 1.2. |
MM_SMS_DELIVERY_STATE_GENERAL_PROBLEM_SUPPLEMENTARY_SERVICE_NOT_SUPPORTED | Permanent error, supplementary service not supported. Since 1.2. |
MM_SMS_DELIVERY_STATE_GENERAL_PROBLEM_SMS_NOT_SUPPORTED | Permanent error, SMS not supported. Since 1.22. |
MM_SMS_DELIVERY_STATE_GENERAL_PROBLEM_MISSING_EXPECTED_PARAMETER | Permanent error, missing expected parameter. Since 1.2. |
MM_SMS_DELIVERY_STATE_GENERAL_PROBLEM_MISSING_MANDATORY_PARAMETER | Permanent error, missing mandatory parameter. Since 1.2. |
MM_SMS_DELIVERY_STATE_GENERAL_PROBLEM_UNRECOGNIZED_PARAMETER_VALUE | Permanent error, unrecognized parameter value. Since 1.2. |
MM_SMS_DELIVERY_STATE_GENERAL_PROBLEM_UNEXPECTED_PARAMETER_VALUE | Permanent error, unexpected parameter value. Since 1.2. |
MM_SMS_DELIVERY_STATE_GENERAL_PROBLEM_USER_DATA_SIZE_ERROR | Permanent error, user data size error. Since 1.2. |
MM_SMS_DELIVERY_STATE_GENERAL_PROBLEM_OTHER | Permanent error, other general problem. Since 1.2. |
MM_SMS_DELIVERY_STATE_TEMPORARY_NETWORK_PROBLEM_ADDRESS_VACANT | Temporary error in network, address vacant. Since 1.2. |
MM_SMS_DELIVERY_STATE_TEMPORARY_NETWORK_PROBLEM_ADDRESS_TRANSLATION_FAILURE | Temporary error in network, address translation failure. Since 1.2. |
MM_SMS_DELIVERY_STATE_TEMPORARY_NETWORK_PROBLEM_NETWORK_RESOURCE_OUTAGE | Temporary error in network, network resource outage. Since 1.2. |
MM_SMS_DELIVERY_STATE_TEMPORARY_NETWORK_PROBLEM_NETWORK_FAILURE | Temporary error in network, network failure. Since 1.2. |
MM_SMS_DELIVERY_STATE_TEMPORARY_NETWORK_PROBLEM_INVALID_TELESERVICE_ID | Temporary error in network, invalid teleservice id. Since 1.2. |
MM_SMS_DELIVERY_STATE_TEMPORARY_NETWORK_PROBLEM_OTHER | Temporary error, other network problem. Since 1.2. |
MM_SMS_DELIVERY_STATE_TEMPORARY_TERMINAL_PROBLEM_NO_PAGE_RESPONSE | Temporary error in terminal, no page response. Since 1.2. |
MM_SMS_DELIVERY_STATE_TEMPORARY_TERMINAL_PROBLEM_DESTINATION_BUSY | Temporary error in terminal, destination busy. Since 1.2. |
MM_SMS_DELIVERY_STATE_TEMPORARY_TERMINAL_PROBLEM_NO_ACKNOWLEDGMENT | Temporary error in terminal, no acknowledgement. Since 1.2. |
MM_SMS_DELIVERY_STATE_TEMPORARY_TERMINAL_PROBLEM_DESTINATION_RESOURCE_SHORTAGE | Temporary error in terminal, destination resource shortage. Since 1.2. |
MM_SMS_DELIVERY_STATE_TEMPORARY_TERMINAL_PROBLEM_SMS_DELIVERY_POSTPONED | Temporary error in terminal, SMS delivery postponed. Since 1.2. |
MM_SMS_DELIVERY_STATE_TEMPORARY_TERMINAL_PROBLEM_DESTINATION_OUT_OF_SERVICE | Temporary error in terminal, destination out of service. Since 1.2. |
MM_SMS_DELIVERY_STATE_TEMPORARY_TERMINAL_PROBLEM_DESTINATION_NO_LONGER_AT_THIS_ADDRESS | Temporary error in terminal, destination no longer at this address. Since 1.2. |
MM_SMS_DELIVERY_STATE_TEMPORARY_TERMINAL_PROBLEM_OTHER | Temporary error, other terminal problem. Since 1.2. |
MM_SMS_DELIVERY_STATE_TEMPORARY_RADIO_INTERFACE_PROBLEM_RESOURCE_SHORTAGE | Temporary error in radio interface, resource shortage. Since 1.2. |
MM_SMS_DELIVERY_STATE_TEMPORARY_RADIO_INTERFACE_PROBLEM_INCOMPATIBILITY | Temporary error in radio interface, problem incompatibility. Since 1.2. |
MM_SMS_DELIVERY_STATE_TEMPORARY_RADIO_INTERFACE_PROBLEM_OTHER | Temporary error, other radio interface problem. Since 1.2. |
MM_SMS_DELIVERY_STATE_TEMPORARY_GENERAL_PROBLEM_ENCODING | Temporary error, encoding. Since 1.2. |
MM_SMS_DELIVERY_STATE_TEMPORARY_GENERAL_PROBLEM_SMS_ORIGINATION_DENIED | Temporary error, SMS origination denied. Since 1.2. |
MM_SMS_DELIVERY_STATE_TEMPORARY_GENERAL_PROBLEM_SMS_TERMINATION_DENIED | Temporary error, SMS termination denied. Since 1.2. |
MM_SMS_DELIVERY_STATE_TEMPORARY_GENERAL_PROBLEM_SUPPLEMENTARY_SERVICE_NOT_SUPPORTED | Temporary error, supplementary service not supported. Since 1.2. |
MM_SMS_DELIVERY_STATE_TEMPORARY_GENERAL_PROBLEM_SMS_NOT_SUPPORTED | Temporary error, SMS not supported. Since 1.2. |
MM_SMS_DELIVERY_STATE_TEMPORARY_GENERAL_PROBLEM_MISSING_EXPECTED_PARAMETER | Temporary error, missing expected parameter. Since 1.2. |
MM_SMS_DELIVERY_STATE_TEMPORARY_GENERAL_PROBLEM_MISSING_MANDATORY_PARAMETER | Temporary error, missing mandatory parameter. Since 1.2. |
MM_SMS_DELIVERY_STATE_TEMPORARY_GENERAL_PROBLEM_UNRECOGNIZED_PARAMETER_VALUE | Temporary error, unrecognized parameter value. Since 1.2. |
MM_SMS_DELIVERY_STATE_TEMPORARY_GENERAL_PROBLEM_UNEXPECTED_PARAMETER_VALUE | Temporary error, unexpected parameter value. Since 1.2. |
MM_SMS_DELIVERY_STATE_TEMPORARY_GENERAL_PROBLEM_USER_DATA_SIZE_ERROR | Temporary error, user data size error. Since 1.2. |
MM_SMS_DELIVERY_STATE_TEMPORARY_GENERAL_PROBLEM_OTHER | Temporary error, other general problem. Since 1.2. |

Since: 1.0

### enum MMSmsStorage

Storage for SMS messages.

#### Members

MM_SMS_STORAGE_UNKNOWN | Storage unknown. |
MM_SMS_STORAGE_SM | SIM card storage area. |
MM_SMS_STORAGE_ME | Mobile equipment storage area. |
MM_SMS_STORAGE_MT | Sum of SIM and Mobile equipment storages |
MM_SMS_STORAGE_SR | Status report message storage area. |
MM_SMS_STORAGE_BM | Broadcast message storage area. |
MM_SMS_STORAGE_TA | Terminal adaptor message storage area. |

Since: 1.0

### enum MMSmsValidityType

Type of SMS validity value.

#### Members

MM_SMS_VALIDITY_TYPE_UNKNOWN | Validity type unknown. |
MM_SMS_VALIDITY_TYPE_RELATIVE | Relative validity. |
MM_SMS_VALIDITY_TYPE_ABSOLUTE | Absolute validity. |
MM_SMS_VALIDITY_TYPE_ENHANCED | Enhanced validity. |

Since: 1.0

### enum MMSmsCdmaTeleserviceId

Teleservice IDs supported for CDMA SMS, as defined in 3GPP2 X.S0004-550-E (section 2.256) and 3GPP2 C.S0015-B (section 3.4.3.1).

#### Members

MM_SMS_CDMA_TELESERVICE_ID_UNKNOWN | Unknown. |
MM_SMS_CDMA_TELESERVICE_ID_CMT91 | IS-91 Extended Protocol Enhanced Services. |
MM_SMS_CDMA_TELESERVICE_ID_WPT | Wireless Paging Teleservice. |
MM_SMS_CDMA_TELESERVICE_ID_WMT | Wireless Messaging Teleservice. |
MM_SMS_CDMA_TELESERVICE_ID_VMN | Voice Mail Notification. |
MM_SMS_CDMA_TELESERVICE_ID_WAP | Wireless Application Protocol. |
MM_SMS_CDMA_TELESERVICE_ID_WEMT | Wireless Enhanced Messaging Teleservice. |
MM_SMS_CDMA_TELESERVICE_ID_SCPT | Service Category Programming Teleservice. |
MM_SMS_CDMA_TELESERVICE_ID_CATPT | Card Application Toolkit Protocol Teleservice. |

Since: 1.2

### enum MMSmsCdmaServiceCategory

Service category for CDMA SMS, as defined in 3GPP2 C.R1001-D (section 9.3).

#### Members

MM_SMS_CDMA_SERVICE_CATEGORY_UNKNOWN | Unknown. |
MM_SMS_CDMA_SERVICE_CATEGORY_EMERGENCY_BROADCAST | Emergency broadcast. |
MM_SMS_CDMA_SERVICE_CATEGORY_ADMINISTRATIVE | Administrative. |
MM_SMS_CDMA_SERVICE_CATEGORY_MAINTENANCE | Maintenance. |
MM_SMS_CDMA_SERVICE_CATEGORY_GENERAL_NEWS_LOCAL | General news (local). |
MM_SMS_CDMA_SERVICE_CATEGORY_GENERAL_NEWS_REGIONAL | General news (regional). |
MM_SMS_CDMA_SERVICE_CATEGORY_GENERAL_NEWS_NATIONAL | General news (national). |
MM_SMS_CDMA_SERVICE_CATEGORY_GENERAL_NEWS_INTERNATIONAL | General news (international). |
MM_SMS_CDMA_SERVICE_CATEGORY_BUSINESS_NEWS_LOCAL | Business/Financial news (local). |
MM_SMS_CDMA_SERVICE_CATEGORY_BUSINESS_NEWS_REGIONAL | Business/Financial news (regional). |
MM_SMS_CDMA_SERVICE_CATEGORY_BUSINESS_NEWS_NATIONAL | Business/Financial news (national). |
MM_SMS_CDMA_SERVICE_CATEGORY_BUSINESS_NEWS_INTERNATIONAL | Business/Financial news (international). |
MM_SMS_CDMA_SERVICE_CATEGORY_SPORTS_NEWS_LOCAL | Sports news (local). |
MM_SMS_CDMA_SERVICE_CATEGORY_SPORTS_NEWS_REGIONAL | Sports news (regional). |
MM_SMS_CDMA_SERVICE_CATEGORY_SPORTS_NEWS_NATIONAL | Sports news (national). |
MM_SMS_CDMA_SERVICE_CATEGORY_SPORTS_NEWS_INTERNATIONAL | Sports news (international). |
MM_SMS_CDMA_SERVICE_CATEGORY_ENTERTAINMENT_NEWS_LOCAL | Entertainment news (local). |
MM_SMS_CDMA_SERVICE_CATEGORY_ENTERTAINMENT_NEWS_REGIONAL | Entertainment news (regional). |
MM_SMS_CDMA_SERVICE_CATEGORY_ENTERTAINMENT_NEWS_NATIONAL | Entertainment news (national). |
MM_SMS_CDMA_SERVICE_CATEGORY_ENTERTAINMENT_NEWS_INTERNATIONAL | Entertainment news (international). |
MM_SMS_CDMA_SERVICE_CATEGORY_LOCAL_WEATHER | Local weather. |
MM_SMS_CDMA_SERVICE_CATEGORY_TRAFFIC_REPORT | Area traffic report. |
MM_SMS_CDMA_SERVICE_CATEGORY_FLIGHT_SCHEDULES | Local airport flight schedules. |
MM_SMS_CDMA_SERVICE_CATEGORY_RESTAURANTS | Restaurants. |
MM_SMS_CDMA_SERVICE_CATEGORY_LODGINGS | Lodgings. |
MM_SMS_CDMA_SERVICE_CATEGORY_RETAIL_DIRECTORY | Retail directory. |
MM_SMS_CDMA_SERVICE_CATEGORY_ADVERTISEMENTS | Advertisements. |
MM_SMS_CDMA_SERVICE_CATEGORY_STOCK_QUOTES | Stock quotes. |
MM_SMS_CDMA_SERVICE_CATEGORY_EMPLOYMENT | Employment. |
MM_SMS_CDMA_SERVICE_CATEGORY_HOSPITALS | Medical / Health / Hospitals. |
MM_SMS_CDMA_SERVICE_CATEGORY_TECHNOLOGY_NEWS | Technology news. |
MM_SMS_CDMA_SERVICE_CATEGORY_MULTICATEGORY | Multi-category. |
MM_SMS_CDMA_SERVICE_CATEGORY_CMAS_PRESIDENTIAL_ALERT | Presidential alert. |
MM_SMS_CDMA_SERVICE_CATEGORY_CMAS_EXTREME_THREAT | Extreme threat. |
MM_SMS_CDMA_SERVICE_CATEGORY_CMAS_SEVERE_THREAT | Severe threat. |
MM_SMS_CDMA_SERVICE_CATEGORY_CMAS_CHILD_ABDUCTION_EMERGENCY | Child abduction emergency. |
MM_SMS_CDMA_SERVICE_CATEGORY_CMAS_TEST | CMAS test. |

Since: 1.2