## MMSimpleStatus MMSimpleStatus — Helper object to handle overall modem status. |

## Functions

MMModemState | mm_simple_status_get_state ()
guint32 | mm_simple_status_get_signal_quality ()
MMModemAccessTechnology | mm_simple_status_get_access_technologies ()
void | mm_simple_status_get_current_bands ()
MMModem3gppRegistrationState | mm_simple_status_get_3gpp_registration_state ()
const gchar * | mm_simple_status_get_3gpp_operator_code ()
const gchar * | mm_simple_status_get_3gpp_operator_name ()
MMModemCdmaRegistrationState | mm_simple_status_get_cdma_cdma1x_registration_state ()
MMModemCdmaRegistrationState | mm_simple_status_get_cdma_evdo_registration_state ()
guint | mm_simple_status_get_cdma_nid ()
guint | mm_simple_status_get_cdma_sid ()

## Properties

MMModemAccessTechnology | access-technologies | Read / Write
MMModemCdmaRegistrationState | cdma-cdma1x-registration-state | Read / Write
MMModemCdmaRegistrationState | cdma-evdo-registration-state | Read / Write
guint | cdma-nid | Read / Write
guint | cdma-sid | Read / Write
GVariant * | current-bands | Read / Write
char * | m3gpp-operator-code | Read / Write
char * | m3gpp-operator-name | Read / Write
MMModem3gppRegistrationState | m3gpp-registration-state | Read / Write
MMModem3gppSubscriptionState | m3gpp-subscription-state | Read / Write
GVariant * | signal-quality | Read / Write
MMModemState | state | Read / Write

## Types and Values

struct | MMSimpleStatus

## Object Hierarchy

        GObject
        ╰── MMSimpleStatus

## Description

The MMSimpleStatus is an object handling the general modem status properties, available in the Simple interface.

This object is retrieved with either `mm_modem_simple_get_status()` or `mm_modem_simple_get_status_sync()`.

## Functions

### mm_simple_status_get_state ()

    MMModemState
    mm_simple_status_get_state (MMSimpleStatus *self);

Gets the state of the modem.

#### Parameters

self | a MMSimpleStatus. |

#### Returns

a MMModemState.

Since: 1.0

### mm_simple_status_get_signal_quality ()

    guint32
    mm_simple_status_get_signal_quality (MMSimpleStatus *self,
                                         gboolean *recent);

Gets the signal quality.

#### Parameters

self | a MMSimpleStatus. |
recent | indication of whether the given signal quality is considered recent. | [out][allow-none]

#### Returns

the signal quality.

Since: 1.0

### mm_simple_status_get_access_technologies ()

    MMModemAccessTechnology
    mm_simple_status_get_access_technologies
                                   (MMSimpleStatus *self);

Gets the currently used access technologies.

#### Parameters

self | a MMSimpleStatus. |

#### Returns

a bitmask of MMModemAccessTechnology values.

Since: 1.0

### mm_simple_status_get_current_bands ()

    void
    mm_simple_status_get_current_bands (MMSimpleStatus *self,
                                        const MMModemBand **bands,
                                        guint *n_bands);

Gets the currently used frequency bands.

#### Parameters

self | a MMSimpleStatus. |
bands | location for an array of MMModemBand values. Do not free the returned value, it is owned by `self` . | [out]
n_bands | number of elements in `bands` . | [out]

Since: 1.0

### mm_simple_status_get_3gpp_registration_state ()

    MMModem3gppRegistrationState
    mm_simple_status_get_3gpp_registration_state
                                   (MMSimpleStatus *self);

Gets the current state of the registration in the 3GPP network.

#### Parameters

self | a MMSimpleStatus. |

#### Returns

a MMModem3gppRegistrationState.

Since: 1.0

### mm_simple_status_get_3gpp_operator_code ()

    const gchar *
    mm_simple_status_get_3gpp_operator_code
                                   (MMSimpleStatus *self);

Gets the MCC/MNC of the operator of the 3GPP network where the modem is registered.

#### Parameters

self | a MMSimpleStatus. |

#### Returns

the operator code, or `NULL` if unknown. Do not free the returned value, it is owned by `self` .

Since: 1.0

### mm_simple_status_get_3gpp_operator_name ()

    const gchar *
    mm_simple_status_get_3gpp_operator_name
                                   (MMSimpleStatus *self);

Gets the name of the operator of the 3GPP network where the modem is registered.

#### Parameters

self | a MMSimpleStatus. |

#### Returns

the operator name, or `NULL` if unknown. Do not free the returned value, it is owned by `self` .

Since: 1.0

### mm_simple_status_get_cdma_cdma1x_registration_state ()

    MMModemCdmaRegistrationState
    mm_simple_status_get_cdma_cdma1x_registration_state
                                   (MMSimpleStatus *self);

Gets the current state of the registration in the CDMA-1x network.

#### Parameters

self | a MMSimpleStatus. |

#### Returns

a MMModemCdmaRegistrationState.

Since: 1.0

### mm_simple_status_get_cdma_evdo_registration_state ()

    MMModemCdmaRegistrationState
    mm_simple_status_get_cdma_evdo_registration_state
                                   (MMSimpleStatus *self);

Gets the current state of the registration in the EV-DO network.

#### Parameters

self | a MMSimpleStatus. |

#### Returns

a MMModemCdmaRegistrationState.

Since: 1.0

### mm_simple_status_get_cdma_nid ()

    guint
    mm_simple_status_get_cdma_nid (MMSimpleStatus *self);

Gets the Network Identification number of the CDMA network.

#### Parameters

self | a MMSimpleStatus. |

#### Returns

the NID, or `MM_MODEM_CDMA_NID_UNKNOWN` if unknown.

Since: 1.0

### mm_simple_status_get_cdma_sid ()

    guint
    mm_simple_status_get_cdma_sid (MMSimpleStatus *self);

Gets the System Identification number of the CDMA network.

#### Parameters

self | a MMSimpleStatus. |

#### Returns

the SID, or `MM_MODEM_CDMA_SID_UNKNOWN` if unknown.

Since: 1.0

## Types and Values

### struct MMSimpleStatus

    struct MMSimpleStatus;

The MMSimpleStatus structure contains private data and should only be accessed using the provided API.

## Property Details

### The `“access-technologies”` property

      “access-technologies”      MMModemAccessTechnology

Access technologies used by the modem.

Owner: MMSimpleStatus

Flags: Read / Write

### The `“cdma-cdma1x-registration-state”` property

      “cdma-cdma1x-registration-state” MMModemCdmaRegistrationState

Registration state in the CDMA1x network.

Owner: MMSimpleStatus

Flags: Read / Write

Default value: MM_MODEM_CDMA_REGISTRATION_STATE_UNKNOWN

### The `“cdma-evdo-registration-state”` property

      “cdma-evdo-registration-state” MMModemCdmaRegistrationState

Registration state in the EV-DO network.

Owner: MMSimpleStatus

Flags: Read / Write

Default value: MM_MODEM_CDMA_REGISTRATION_STATE_UNKNOWN

### The `“cdma-nid”` property

      “cdma-nid”                 guint

Network Identifier of the serving CDMA1x network.

Owner: MMSimpleStatus

Flags: Read / Write

Allowed values: <= 99999

Default value: 99999

### The `“cdma-sid”` property

      “cdma-sid”                 guint

System Identifier of the serving CDMA1x network.

Owner: MMSimpleStatus

Flags: Read / Write

Allowed values: <= 99999

Default value: 99999

### The `“current-bands”` property

      “current-bands”            GVariant *

Frequency bands used by the modem.

Owner: MMSimpleStatus

Flags: Read / Write

Allowed values: GVariant<au>

Default value: NULL

### The `“m3gpp-operator-code”` property

      “m3gpp-operator-code”      char *

Code of the current operator in the 3GPP network.

Owner: MMSimpleStatus

Flags: Read / Write

Default value: NULL

### The `“m3gpp-operator-name”` property

      “m3gpp-operator-name”      char *

Name of the current operator in the 3GPP network.

Owner: MMSimpleStatus

Flags: Read / Write

Default value: NULL

### The `“m3gpp-registration-state”` property

      “m3gpp-registration-state” MMModem3gppRegistrationState

Registration state in the 3GPP network.

Owner: MMSimpleStatus

Flags: Read / Write

Default value: MM_MODEM_3GPP_REGISTRATION_STATE_UNKNOWN

### The `“m3gpp-subscription-state”` property

      “m3gpp-subscription-state” MMModem3gppSubscriptionState

Subscription state of the account (deprecated).

Owner: MMSimpleStatus

Flags: Read / Write

Default value: MM_MODEM_3GPP_SUBSCRIPTION_STATE_UNKNOWN

### The `“signal-quality”` property

      “signal-quality”           GVariant *

Signal quality reported by the modem.

Owner: MMSimpleStatus

Flags: Read / Write

Allowed values: GVariant<(ub)>

Default value: NULL

### The `“state”` property

      “state”                    MMModemState

State of the modem.

Owner: MMSimpleStatus

Flags: Read / Write

Default value: MM_MODEM_STATE_UNKNOWN