## MMModemFirmware MMModemFirmware — The Firmware interface |

## Functions

const gchar * | mm_modem_firmware_get_path ()
gchar * | mm_modem_firmware_dup_path ()
void | mm_modem_firmware_list ()
gboolean | mm_modem_firmware_list_finish ()
gboolean | mm_modem_firmware_list_sync ()
void | mm_modem_firmware_select ()
gboolean | mm_modem_firmware_select_finish ()
gboolean | mm_modem_firmware_select_sync ()
MMFirmwareUpdateSettings * | mm_modem_firmware_get_update_settings ()
MMFirmwareUpdateSettings * | mm_modem_firmware_peek_update_settings ()

## Types and Values

struct | MMModemFirmware

## Object Hierarchy

        GObject
        ╰── GDBusProxy
            ╰── MmGdbusModemFirmwareProxy
                ╰── MMModemFirmware

## Implemented Interfaces

MMModemFirmware implements GDBusInterface, GInitable, GAsyncInitable and MmGdbusModemFirmware.

## Description

The MMModemFirmware is an object providing access to the methods, signals and properties of the Firmware interface.

The Firmware interface is exposed whenever a modem has firmware capabilities.

## Functions

### mm_modem_firmware_get_path ()

    const gchar *
    mm_modem_firmware_get_path (MMModemFirmware *self);

Gets the DBus path of the MMObject which implements this interface.

#### Parameters

self | A MMModemFirmware. |

#### Returns

The DBus path of the MMObject object.

[transfer none]

Since: 1.0

### mm_modem_firmware_dup_path ()

    gchar *
    mm_modem_firmware_dup_path (MMModemFirmware *self);

Gets a copy of the DBus path of the MMObject object which implements this interface.

#### Parameters

self | A MMModemFirmware. |

#### Returns

The DBus path of the MMObject. The returned value should be freed with `g_free()`.

[transfer full]

Since: 1.0

### mm_modem_firmware_list ()

    void
    mm_modem_firmware_list (MMModemFirmware *self,
                            GCancellable *cancellable,
                            GAsyncReadyCallback callback,
                            gpointer user_data);

Asynchronously gets the list of available firmware images.

When the operation is finished, `callback` will be invoked in the

thread-default main loop

of the thread you are calling this method from. You can then call `mm_modem_firmware_list_finish()` to get the result of the operation.

See `mm_modem_firmware_list_sync()` for the synchronous, blocking version of this method.

#### Parameters

self | A MMModemFirmware. |
cancellable | A GCancellable or `NULL`. | [allow-none]
callback | A GAsyncReadyCallback to call when the request is satisfied or `NULL`. |
user_data | User data to pass to `callback` . |

Since: 1.0

### mm_modem_firmware_list_finish ()

    gboolean
    mm_modem_firmware_list_finish (MMModemFirmware *self,
                                   GAsyncResult *res,
                                   MMFirmwareProperties **selected,
                                   GList **installed,
                                   GError **error);

Finishes an operation started with `mm_modem_firmware_list()`.

#### Parameters

self | A MMModemFirmware. |
selected | The selected firmware slot, or `NULL` if no slot is selected (such as if all slots are empty, or no slots exist). The returned value should be freed with `g_object_unref()`. | [out][allow-none][transfer full]
installed | A list of MMFirmwareProperties objects specifying the installed images. The returned value should be freed with `g_list_free_full()` using `g_object_unref()` as GDestroyNotify. | [out][allow-none][transfer full][element-type ModemManager.FirmwareProperties]
res | The GAsyncResult obtained from the GAsyncReadyCallback passed to `mm_modem_firmware_list()`. |
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if the list was correctly retrieved, `FALSE` if `error` is set.

Since: 1.0

### mm_modem_firmware_list_sync ()

    gboolean
    mm_modem_firmware_list_sync (MMModemFirmware *self,
                                 MMFirmwareProperties **selected,
                                 GList **installed,
                                 GCancellable *cancellable,
                                 GError **error);

Synchronously gets the list of available firmware images.

The calling thread is blocked until a reply is received. See `mm_modem_firmware_list()` for the asynchronous version of this method.

#### Parameters

self | A MMModemFirmware. |
selected | The selected firmware slot, or NULL if no slot is selected (such as if all slots are empty, or no slots exist). The returned value should be freed with `g_object_unref()`. | [out][allow-none][transfer full]
installed | A list of MMFirmwareProperties objects specifying the installed images. The returned value should be freed with `g_list_free_full()` using `g_object_unref()` as GDestroyNotify. | [out][allow-none][transfer full][element-type ModemManager.FirmwareProperties]
cancellable | A GCancellable or `NULL`. | [allow-none]
error | Return firmware for error or `NULL`. |

#### Returns

`TRUE` if the list was correctly retrieved, `FALSE` if `error` is set.

Since: 1.0

### mm_modem_firmware_select ()

    void
    mm_modem_firmware_select (MMModemFirmware *self,
                              const gchar *unique_id,
                              GCancellable *cancellable,
                              GAsyncReadyCallback callback,
                              gpointer user_data);

Asynchronously selects a firmware image to boot.

The modem will possibly disappear once this action is run, as it needs to reboot in order to select the new image.

When the operation is finished, `callback` will be invoked in the

thread-default main loop

of the thread you are calling this method from. You can then call `mm_modem_firmware_select_finish()` to get the result of the operation.

See `mm_modem_firmware_select_sync()` for the synchronous, blocking version of this method.

#### Parameters

self | A MMModemFirmware. |
unique_id | Unique ID of the firmware image to select. |
cancellable | A GCancellable or `NULL`. | [allow-none]
callback | A GAsyncReadyCallback to call when the request is satisfied or `NULL`. |
user_data | User data to pass to `callback` . |

Since: 1.0

### mm_modem_firmware_select_finish ()

    gboolean
    mm_modem_firmware_select_finish (MMModemFirmware *self,
                                     GAsyncResult *res,
                                     GError **error);

Finishes an operation started with `mm_modem_firmware_select()`.

#### Parameters

self | A MMModemFirmware. |
res | The GAsyncResult obtained from the GAsyncReadyCallback passed to `mm_modem_firmware_select()`. |
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if the selection was successful, `FALSE` if `error` is set.

Since: 1.0

### mm_modem_firmware_select_sync ()

    gboolean
    mm_modem_firmware_select_sync (MMModemFirmware *self,
                                   const gchar *unique_id,
                                   GCancellable *cancellable,
                                   GError **error);

Synchronously selects a firmware image to boot.

The modem will possibly disappear once this action is run, as it needs to reboot in order to select the new image.

The calling thread is blocked until a reply is received. See `mm_modem_firmware_select()` for the asynchronous version of this method.

#### Parameters

self | A MMModemFirmware. |
unique_id | Unique ID of the firmware image to select. |
cancellable | A GCancellable or `NULL`. | [allow-none]
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if the selection was successful, `FALSE` if `error` is set.

Since: 1.0

### mm_modem_firmware_get_update_settings ()

    MMFirmwareUpdateSettings *
    mm_modem_firmware_get_update_settings (MMModemFirmware *self);

Gets a MMFirmwareUpdateSettings object specifying the expected update settings.

The values reported by `self` are not updated when the values in the interface change. Instead, the client is expected to call `mm_modem_firmware_get_update_settings()` again to get a new MMFirmwareUpdateSettings with the new values.

#### Parameters

self | A MMModemFirmware. |

#### Returns

A MMFirmwareUpdateSettings that must be freed with `g_object_unref()` or `NULL` if unknown.

[transfer full]

Since: 1.10

### mm_modem_firmware_peek_update_settings ()

    MMFirmwareUpdateSettings *
    mm_modem_firmware_peek_update_settings
                                   (MMModemFirmware *self);

Gets a MMFirmwareUpdateSettings object specifying the expected update settings.

The returned value is only valid until the property changes so it is only safe to use this function on the thread where `self` was constructed. Use `mm_modem_firmware_get_update_settings()` if on another thread.

#### Parameters

self | A MMModemFirmware. |

#### Returns

A MMFirmwareUpdateSettings. Do not free the returned value, it belongs to `self` .

[transfer none]

Since: 1.10

## Types and Values

### struct MMModemFirmware

    struct MMModemFirmware;

The MMModemFirmware structure contains private data and should only be accessed using the provided API.