## MMModem MMModem — The Modem interface |

## Functions

const gchar * | mm_modem_get_path ()
gchar * | mm_modem_dup_path ()
MMModemState | mm_modem_get_state ()
MMModemStateFailedReason | mm_modem_get_state_failed_reason ()
MMModemPowerState | mm_modem_get_power_state ()
gboolean | mm_modem_peek_supported_capabilities ()
gboolean | mm_modem_get_supported_capabilities ()
MMModemCapability | mm_modem_get_current_capabilities ()
const gchar * | mm_modem_get_manufacturer ()
gchar * | mm_modem_dup_manufacturer ()
const gchar * | mm_modem_get_model ()
gchar * | mm_modem_dup_model ()
const gchar * | mm_modem_get_revision ()
gchar * | mm_modem_dup_revision ()
const gchar * | mm_modem_get_carrier_configuration ()
gchar * | mm_modem_dup_carrier_configuration ()
const gchar * | mm_modem_get_carrier_configuration_revision ()
gchar * | mm_modem_dup_carrier_configuration_revision ()
const gchar * | mm_modem_get_hardware_revision ()
gchar * | mm_modem_dup_hardware_revision ()
const gchar * const * | mm_modem_get_drivers ()
gchar ** | mm_modem_dup_drivers ()
const gchar * | mm_modem_get_plugin ()
gchar * | mm_modem_dup_plugin ()
const gchar * | mm_modem_get_primary_port ()
gchar * | mm_modem_dup_primary_port ()
gboolean | mm_modem_peek_ports ()
gboolean | mm_modem_get_ports ()
const gchar * | mm_modem_get_device ()
gchar * | mm_modem_dup_device ()
const gchar * | mm_modem_get_equipment_identifier ()
gchar * | mm_modem_dup_equipment_identifier ()
const gchar * | mm_modem_get_device_identifier ()
gchar * | mm_modem_dup_device_identifier ()
MMModemLock | mm_modem_get_unlock_required ()
MMUnlockRetries * | mm_modem_peek_unlock_retries ()
MMUnlockRetries * | mm_modem_get_unlock_retries ()
guint | mm_modem_get_max_bearers ()
guint | mm_modem_get_max_active_bearers ()
guint | mm_modem_get_max_active_multiplexed_bearers ()
const gchar * const * | mm_modem_get_bearer_paths ()
gchar ** | mm_modem_dup_bearer_paths ()
const gchar *const * | mm_modem_get_own_numbers ()
gchar ** | mm_modem_dup_own_numbers ()
gboolean | mm_modem_peek_supported_modes ()
gboolean | mm_modem_get_supported_modes ()
gboolean | mm_modem_get_current_modes ()
gboolean | mm_modem_peek_supported_bands ()
gboolean | mm_modem_get_supported_bands ()
gboolean | mm_modem_peek_current_bands ()
gboolean | mm_modem_get_current_bands ()
MMBearerIpFamily | mm_modem_get_supported_ip_families ()
guint | mm_modem_get_signal_quality ()
MMModemAccessTechnology | mm_modem_get_access_technologies ()
const gchar * | mm_modem_get_sim_path ()
gchar * | mm_modem_dup_sim_path ()
void | mm_modem_get_sim ()
MMSim * | mm_modem_get_sim_finish ()
MMSim * | mm_modem_get_sim_sync ()
const gchar * const * | mm_modem_get_sim_slot_paths ()
gchar ** | mm_modem_dup_sim_slot_paths ()
guint | mm_modem_get_primary_sim_slot ()
void | mm_modem_list_sim_slots ()
GPtrArray * | mm_modem_list_sim_slots_finish ()
GPtrArray * | mm_modem_list_sim_slots_sync ()
void | mm_modem_set_primary_sim_slot ()
gboolean | mm_modem_set_primary_sim_slot_finish ()
gboolean | mm_modem_set_primary_sim_slot_sync ()
void | mm_modem_enable ()
gboolean | mm_modem_enable_finish ()
gboolean | mm_modem_enable_sync ()
void | mm_modem_disable ()
gboolean | mm_modem_disable_finish ()
gboolean | mm_modem_disable_sync ()
void | mm_modem_set_power_state ()
gboolean | mm_modem_set_power_state_finish ()
gboolean | mm_modem_set_power_state_sync ()
void | mm_modem_set_current_modes ()
gboolean | mm_modem_set_current_modes_finish ()
gboolean | mm_modem_set_current_modes_sync ()
void | mm_modem_set_current_bands ()
gboolean | mm_modem_set_current_bands_finish ()
gboolean | mm_modem_set_current_bands_sync ()
void | mm_modem_set_current_capabilities ()
gboolean | mm_modem_set_current_capabilities_finish ()
gboolean | mm_modem_set_current_capabilities_sync ()
void | mm_modem_reset ()
gboolean | mm_modem_reset_finish ()
gboolean | mm_modem_reset_sync ()
void | mm_modem_factory_reset ()
gboolean | mm_modem_factory_reset_finish ()
gboolean | mm_modem_factory_reset_sync ()
void | mm_modem_list_bearers ()
GList * | mm_modem_list_bearers_finish ()
GList * | mm_modem_list_bearers_sync ()
void | mm_modem_create_bearer ()
MMBearer * | mm_modem_create_bearer_finish ()
MMBearer * | mm_modem_create_bearer_sync ()
void | mm_modem_delete_bearer ()
gboolean | mm_modem_delete_bearer_finish ()
gboolean | mm_modem_delete_bearer_sync ()
void | mm_modem_command ()
gchar * | mm_modem_command_finish ()
gchar * | mm_modem_command_sync ()
void | mm_modem_port_info_array_free ()

## Types and Values

struct | MMModem
struct | MMModemModeCombination
struct | MMModemPortInfo

## Object Hierarchy

        GObject
        ╰── GDBusProxy
            ╰── MmGdbusModemProxy
                ╰── MMModem

## Implemented Interfaces

MMModem implements GDBusInterface, GInitable, GAsyncInitable and MmGdbusModem.

## Description

The MMModem is an object providing access to the methods, signals and properties of the Modem interface.

When the modem is exposed and available in the bus, it is ensured that at least this interface is also available.

## Functions

### mm_modem_get_path ()

    const gchar *
    mm_modem_get_path (MMModem *self);

Gets the DBus path of the MMObject which implements this interface.

[skip]

#### Parameters

self | A MMModem. |

#### Returns

The DBus path of the MMObject object. Do not free the returned value, it belongs to `self` .

[transfer none]

Since: 1.0

### mm_modem_dup_path ()

    gchar *
    mm_modem_dup_path (MMModem *self);

Gets a copy of the DBus path of the MMObject object which implements this interface.

#### Parameters

self | A MMModem. |

#### Returns

The DBus path of the MMObject. The returned value should be freed with `g_free()`.

[transfer full]

Since: 1.0

### mm_modem_get_state ()

    MMModemState
    mm_modem_get_state (MMModem *self);

Gets the overall state of the MMModem.

#### Parameters

self | A MMModem. |

#### Returns

A MMModemState value.

Since: 1.0

### mm_modem_get_state_failed_reason ()

    MMModemStateFailedReason
    mm_modem_get_state_failed_reason (MMModem *self);

Gets the reason specifying why the modem is in MM_MODEM_STATE_FAILED state.

#### Parameters

self | A MMModem. |

#### Returns

A MMModemStateFailedReason value.

Since: 1.0

### mm_modem_get_power_state ()

    MMModemPowerState
    mm_modem_get_power_state (MMModem *self);

Gets the power state of the MMModem.

#### Parameters

self | A MMModem. |

#### Returns

A MMModemPowerState value.

Since: 1.0

### mm_modem_peek_supported_capabilities ()

    gboolean
    mm_modem_peek_supported_capabilities (MMModem *self,
                                          const MMModemCapability **capabilities,
                                          guint *n_capabilities);

Gets the list of combinations of generic families of access technologies supported by this MMModem.

#### Parameters

self | A MMModem. |
capabilities | Return location for the array of MMModemCapability values. Do not free the returned array, it is owned by `self` . | [out][array length=n_capabilities]
n_capabilities | Return location for the number of values in `capabilities` . | [out]

#### Returns

`TRUE` if `capabilities` and `n_capabilities` are set, `FALSE` otherwise.

Since: 1.0

### mm_modem_get_supported_capabilities ()

    gboolean
    mm_modem_get_supported_capabilities (MMModem *self,
                                         MMModemCapability **capabilities,
                                         guint *n_capabilities);

Gets the list of combinations of generic families of access technologies supported by this MMModem.

#### Parameters

self | A MMModem. |
capabilities | Return location for the array of MMModemCapability values. The returned array should be freed with `g_free()` when no longer needed. | [out][array length=n_capabilities]
n_capabilities | Return location for the number of values in `capabilities` . | [out]

#### Returns

`TRUE` if `capabilities` and `n_capabilities` are set, `FALSE` otherwise.

Since: 1.0

### mm_modem_get_current_capabilities ()

    MMModemCapability
    mm_modem_get_current_capabilities (MMModem *self);

Gets the list of generic families of access technologies supported by this MMModem without a firmware reload or reinitialization.

#### Parameters

self | A MMModem. |

#### Returns

A bitmask of MMModemCapability flags.

Since: 1.0

### mm_modem_get_manufacturer ()

    const gchar *
    mm_modem_get_manufacturer (MMModem *self);

Gets the equipment manufacturer, as reported by this MMModem.

The returned value is only valid until the property changes so it is only safe to use this function on the thread where `self` was constructed. Use `mm_modem_dup_manufacturer()` if on another thread.

#### Parameters

self | A MMModem. |

#### Returns

The equipment manufacturer, or `NULL` if none available. Do not free the returned value, it belongs to `self` .

[transfer none]

Since: 1.0

### mm_modem_dup_manufacturer ()

    gchar *
    mm_modem_dup_manufacturer (MMModem *self);

Gets a copy of the equipment manufacturer, as reported by this MMModem.

#### Parameters

self | A MMModem. |

#### Returns

The equipment manufacturer, or `NULL` if none available. The returned value should be freed with `g_free()`.

[transfer full]

Since: 1.0

### mm_modem_get_model ()

    const gchar *
    mm_modem_get_model (MMModem *self);

Gets the equipment model, as reported by this MMModem.

The returned value is only valid until the property changes so it is only safe to use this function on the thread where `self` was constructed. Use `mm_modem_dup_model()` if on another thread.

#### Parameters

self | A MMModem. |

#### Returns

The equipment model, or `NULL` if none available. Do not free the returned value, it belongs to `self` .

[transfer none]

Since: 1.0

### mm_modem_dup_model ()

    gchar *
    mm_modem_dup_model (MMModem *self);

Gets a copy of the equipment model, as reported by this MMModem.

#### Parameters

self | A MMModem. |

#### Returns

The equipment model, or `NULL` if none available. The returned value should be freed with `g_free()`.

[transfer full]

Since: 1.0

### mm_modem_get_revision ()

    const gchar *
    mm_modem_get_revision (MMModem *self);

Gets the equipment revision, as reported by this MMModem.

The returned value is only valid until the property changes so it is only safe to use this function on the thread where `self` was constructed. Use `mm_modem_dup_revision()` if on another thread.

#### Parameters

self | A MMModem. |

#### Returns

The equipment revision, or `NULL` if none available. Do not free the returned value, it belongs to `self` .

[transfer none]

Since: 1.0

### mm_modem_dup_revision ()

    gchar *
    mm_modem_dup_revision (MMModem *self);

Gets a copy of the equipment revision, as reported by this MMModem.

#### Parameters

self | A MMModem. |

#### Returns

The equipment revision, or `NULL` if none available. The returned value should be freed with `g_free()`.

[transfer full]

Since: 1.0

### mm_modem_get_carrier_configuration ()

    const gchar *
    mm_modem_get_carrier_configuration (MMModem *self);

Gets the carrier-specific configuration (MCFG) in use, as reported by this MMModem.

The returned value is only valid until the property changes so it is only safe to use this function on the thread where `self` was constructed. Use `mm_modem_dup_carrier_configuration()` if on another thread.

#### Parameters

self | A MMModem. |

#### Returns

The carrier configuration, or `NULL` if none available. Do not free the returned value, it belongs to `self` .

[transfer none]

Since: 1.12

### mm_modem_dup_carrier_configuration ()

    gchar *
    mm_modem_dup_carrier_configuration (MMModem *self);

Gets a copy of the carrier-specific configuration (MCFG) in use, as reported by this MMModem.

#### Parameters

self | A MMModem. |

#### Returns

The carrier configuration, or `NULL` if none available. The returned value should be freed with `g_free()`.

[transfer full]

Since: 1.12

### mm_modem_get_carrier_configuration_revision ()

    const gchar *
    mm_modem_get_carrier_configuration_revision
                                   (MMModem *self);

Gets the carrier-specific configuration revision in use, as reported by this MMModem.

The returned value is only valid until the property changes so it is only safe to use this function on the thread where `self` was constructed. Use `mm_modem_dup_carrier_configuration()` if on another thread.

#### Parameters

self | A MMModem. |

#### Returns

The carrier configuration revision, or `NULL` if none available. Do not free the returned value, it belongs to `self` .

[transfer none]

Since: 1.12

### mm_modem_dup_carrier_configuration_revision ()

    gchar *
    mm_modem_dup_carrier_configuration_revision
                                   (MMModem *self);

Gets a copy of the carrier-specific configuration revision in use, as reported by this MMModem.

#### Parameters

self | A MMModem. |

#### Returns

The carrier configuration revision, or `NULL` if none available. The returned value should be freed with `g_free()`.

[transfer full]

Since: 1.12

### mm_modem_get_hardware_revision ()

    const gchar *
    mm_modem_get_hardware_revision (MMModem *self);

Gets the equipment hardware revision, as reported by this MMModem.

The returned value is only valid until the property changes so it is only safe to use this function on the thread where `self` was constructed. Use `mm_modem_dup_hardware_revision()` if on another thread.

#### Parameters

self | A MMModem. |

#### Returns

The equipment hardware revision, or `NULL` if none available. Do not free the returned value, it belongs to `self` .

[transfer none]

Since: 1.8

### mm_modem_dup_hardware_revision ()

    gchar *
    mm_modem_dup_hardware_revision (MMModem *self);

Gets a copy of the equipment hardware revision, as reported by this MMModem.

#### Parameters

self | A MMModem. |

#### Returns

The equipment hardware revision, or `NULL` if none available. The returned value should be freed with `g_free()`.

[transfer full]

Since: 1.8

### mm_modem_get_drivers ()

    const gchar * const  *
    mm_modem_get_drivers (MMModem *self);

Gets the Operating System device drivers handling communication with the modem hardware.

The returned value is only valid until the property changes so it is only safe to use this function on the thread where `self` was constructed. Use `mm_modem_dup_drivers()` if on another thread.

#### Parameters

self | A MMModem. |

#### Returns

The drivers, or `NULL` if none available. Do not free the returned value, it belongs to `self` .

[transfer none]

Since: 1.0

### mm_modem_dup_drivers ()

    gchar **
    mm_modem_dup_drivers (MMModem *self);

Gets a copy of the Operating System device driver handling communication with the modem hardware.

#### Parameters

self | A MMModem. |

#### Returns

The drivers, or `NULL` if none available. The returned value should be freed with `g_strfreev()`.

[transfer full]

Since: 1.0

### mm_modem_get_plugin ()

    const gchar *
    mm_modem_get_plugin (MMModem *self);

Gets the name of the plugin handling this MMModem.

The returned value is only valid until the property changes so it is only safe to use this function on the thread where `self` was constructed. Use `mm_modem_dup_plugin()` if on another thread.

#### Parameters

self | A MMModem. |

#### Returns

The name of the plugin, or `NULL` if none available. Do not free the returned value, it belongs to `self` .

[transfer none]

Since: 1.0

### mm_modem_dup_plugin ()

    gchar *
    mm_modem_dup_plugin (MMModem *self);

Gets a copy of the name of the plugin handling this MMModem.

#### Parameters

self | A MMModem. |

#### Returns

The name of the plugin, or `NULL` if none available. The returned value should be freed with `g_free()`.

[transfer full]

Since: 1.0

### mm_modem_get_primary_port ()

    const gchar *
    mm_modem_get_primary_port (MMModem *self);

Gets the name of the primary port controlling this MMModem.

The returned value is only valid until the property changes so it is only safe to use this function on the thread where `self` was constructed. Use `mm_modem_dup_primary_port()` if on another thread.

#### Parameters

self | A MMModem. |

#### Returns

The name of the primary port. Do not free the returned value, it belongs to `self` .

[transfer none]

Since: 1.0

### mm_modem_dup_primary_port ()

    gchar *
    mm_modem_dup_primary_port (MMModem *self);

Gets a copy of the name of the primary port controlling this MMModem.

#### Parameters

self | A MMModem. |

#### Returns

The name of the primary port. The returned value should be freed with `g_free()`.

[transfer full]

Since: 1.0

### mm_modem_peek_ports ()

    gboolean
    mm_modem_peek_ports (MMModem *self,
                         const MMModemPortInfo **ports,
                         guint *n_ports);

Gets the list of ports in the modem.

#### Parameters

self | A MMModem. |
ports | Return location for the array of MMModemPortInfo values. Do not free the returned value, it is owned by `self` . | [out][array length=n_ports][transfer none]
n_ports | Return location for the number of values in `ports` . | [out]

#### Returns

`TRUE` if `ports` and `n_ports` are set, `FALSE` otherwise.

Since: 1.0

### mm_modem_get_ports ()

    gboolean
    mm_modem_get_ports (MMModem *self,
                        MMModemPortInfo **ports,
                        guint *n_ports);

Gets the list of ports in the modem.

#### Parameters

self | A MMModem. |
ports | Return location for the array of MMModemPortInfo values. The returned array should be freed with `mm_modem_port_info_array_free()` when no longer needed. | [out][array length=n_ports]
n_ports | Return location for the number of values in `ports` . | [out]

#### Returns

`TRUE` if `ports` and `n_ports` are set, `FALSE` otherwise.

Since: 1.0

### mm_modem_get_device ()

    const gchar *
    mm_modem_get_device (MMModem *self);

Gets the physical modem device reference (ie, USB, PCI, PCMCIA device), which may be dependent upon the operating system.

The returned value is only valid until the property changes so it is only safe to use this function on the thread where `self` was constructed. Use `mm_modem_dup_device()` if on another thread.

#### Parameters

self | A MMModem. |

#### Returns

The device, or `NULL` if none available. Do not free the returned value, it belongs to `self` .

[transfer none]

Since: 1.0

### mm_modem_dup_device ()

    gchar *
    mm_modem_dup_device (MMModem *self);

Gets a copy of the physical modem device reference (ie, USB, PCI, PCMCIA device), which may be dependent upon the operating system.

#### Parameters

self | A MMModem. |

#### Returns

The device, or `NULL` if none available. The returned value should be freed with `g_free()`.

[transfer full]

Since: 1.0

### mm_modem_get_equipment_identifier ()

    const gchar *
    mm_modem_get_equipment_identifier (MMModem *self);

Gets the identity of the MMModem.

This will be the IMEI number for GSM devices and the hex-format ESN/MEID for CDMA devices.

The returned value is only valid until the property changes so it is only safe to use this function on the thread where `self` was constructed. Use `mm_modem_dup_equipment_identifier()` if on another thread.

#### Parameters

self | A MMModem. |

#### Returns

The equipment identifier, or `NULL` if none available. Do not free the returned value, it belongs to `self` .

[transfer none]

Since: 1.0

### mm_modem_dup_equipment_identifier ()

    gchar *
    mm_modem_dup_equipment_identifier (MMModem *self);

Gets a copy of the identity of the MMModem.

This will be the IMEI number for GSM devices and the hex-format ESN/MEID for CDMA devices.

#### Parameters

self | A MMModem. |

#### Returns

The equipment identifier, or `NULL` if none available. The returned value should be freed with `g_free()`.

[transfer full]

Since: 1.0

### mm_modem_get_device_identifier ()

    const gchar *
    mm_modem_get_device_identifier (MMModem *self);

Gets a best-effort device identifier based on various device information like model name, firmware revision, USB/PCI/PCMCIA IDs, and other properties.

This ID is not guaranteed to be unique and may be shared between identical devices with the same firmware, but is intended to be "unique enough" for use as a casual device identifier for various user experience operations.

This is not the device's IMEI or ESN since those may not be available before unlocking the device via a PIN.

The returned value is only valid until the property changes so it is only safe to use this function on the thread where `self` was constructed. Use `mm_modem_dup_device_identifier()` if on another thread.

#### Parameters

self | A MMModem. |

#### Returns

The device identifier, or `NULL` if none available. Do not free the returned value, it belongs to `self` .

[transfer none]

Since: 1.0

### mm_modem_dup_device_identifier ()

    gchar *
    mm_modem_dup_device_identifier (MMModem *self);

Gets a copy of a best-effort device identifier based on various device information like model name, firmware revision, USB/PCI/PCMCIA IDs, and other properties.

This ID is not guaranteed to be unique and may be shared between identical devices with the same firmware, but is intended to be "unique enough" for use as a casual device identifier for various user experience operations.

This is not the device's IMEI or ESN since those may not be available before unlocking the device via a PIN.

#### Parameters

self | A MMModem. |

#### Returns

The device identifier, or `NULL` if none available. The returned value should be freed with `g_free()`.

[transfer full]

Since: 1.0

### mm_modem_get_unlock_required ()

    MMModemLock
    mm_modem_get_unlock_required (MMModem *self);

Gets current lock state of the MMModem.

#### Parameters

self | A MMModem. |

#### Returns

A MMModemLock value, specifying the current lock state.

Since: 1.0

### mm_modem_peek_unlock_retries ()

    MMUnlockRetries *
    mm_modem_peek_unlock_retries (MMModem *self);

Gets a MMUnlockRetries object, which provides, for each

MMModemLock handled by the modem, the

number of PIN tries remaining before the code becomes blocked (requiring a PUK) or permanently blocked.

The returned value is only valid until the property changes so it is only safe to use this function on the thread where `self` was constructed. Use `mm_modem_get_unlock_retries()` if on another thread.

#### Parameters

self | A MMModem. |

#### Returns

A MMUnlockRetries. Do not free the returned value, it belongs to `self` .

[transfer none]

Since: 1.0

### mm_modem_get_unlock_retries ()

    MMUnlockRetries *
    mm_modem_get_unlock_retries (MMModem *self);

Gets a MMUnlockRetries object, which provides, for each

MMModemLock handled by the modem, the

number of PIN tries remaining before the code becomes blocked (requiring a PUK) or permanently blocked.

The values reported by `self` are not updated when the values in the interface change. Instead, the client is expected to call `mm_modem_get_unlock_retries()` again to get a new MMUnlockRetries with the new values.

#### Parameters

self | A MMModem. |

#### Returns

A MMUnlockRetries that must be freed with `g_object_unref()` or `NULL` if unknown.

[transfer full]

Since: 1.0

### mm_modem_get_max_bearers ()

    guint
    mm_modem_get_max_bearers (MMModem *self);

`mm_modem_get_max_bearers` has been deprecated since version 1.18. and should not be used in newly-written code.

There is no way to query the modem how many bearers it supports, so the value exposed in this property in all the different implementations is always equal to the one retrieved with `mm_modem_get_max_active_bearers()`, so there is no point in using this method.

Gets the maximum number of defined packet data bearers this MMModem supports.

This is not the number of active/connected bearers the modem supports, but simply the number of bearers that may be defined at any given time. For example, POTS and CDMA2000-only devices support only one bearer, while GSM/UMTS devices typically support three or more, and any LTE-capable device (whether LTE-only, GSM/UMTS-capable, and/or CDMA2000-capable) also typically support three or more.

#### Parameters

self | a MMModem. |

#### Returns

the maximum number of defined packet data bearers.

Since: 1.0

### mm_modem_get_max_active_bearers ()

    guint
    mm_modem_get_max_active_bearers (MMModem *self);

Gets the maximum number of active packet data bearers this MMModem supports without enabling multiplexing support.

POTS and CDMA2000-only devices support one active bearer, while GSM/UMTS and LTE/5GNR capable devices (including 3GPP+3GPP3 multimode devices) may support one or more active bearers, depending on the amount of physical ports exposed by the device.

#### Parameters

self | a MMModem. |

#### Returns

the maximum number of active packet data bearers.

Since: 1.0

### mm_modem_get_max_active_multiplexed_bearers ()

    guint
    mm_modem_get_max_active_multiplexed_bearers
                                   (MMModem *self);

Gets the maximum number of active packet data bearers this MMModem supports after enabling multiplexing support on one single network interface.

#### Parameters

self | a MMModem. |

#### Returns

the maximum number of active packet data bearers, or 0 if multiplexing is not supported.

Since: 1.18

### mm_modem_get_bearer_paths ()

    const gchar * const *
    mm_modem_get_bearer_paths (MMModem *self);

Gets the DBus paths of the MMBearer handled in this MMModem.

The returned value is only valid until the property changes so it is only safe to use this function on the thread where `self` was constructed. Use `mm_modem_dup_bearer_paths()` if on another thread.

#### Parameters

self | A MMModem. |

#### Returns

The DBus paths of the MMBearer handled in this MMModem, or `NULL` if none available. Do not free the returned value, it belongs to `self` .

[transfer none]

Since: 1.0

### mm_modem_dup_bearer_paths ()

    gchar **
    mm_modem_dup_bearer_paths (MMModem *self);

Gets a copy of the DBus paths of the MMBearer handled in this MMModem.

#### Parameters

self | A MMModem. |

#### Returns

The DBus paths of the MMBearer handled in this MMModem, or `NULL` if none available. The returned value should be freed with `g_strfreev()`.

[transfer full]

Since: 1.0

### mm_modem_get_own_numbers ()

    const gchar *const  *
    mm_modem_get_own_numbers (MMModem *self);

Gets the list of numbers (e.g. MSISDN in 3GPP) being currently handled by this modem.

The returned value is only valid until the property changes so it is only safe to use this function on the thread where `self` was constructed. Use `mm_modem_dup_own_numbers()` if on another thread.

[skip]

#### Parameters

self | A MMModem. |

#### Returns

The list of own numbers or `NULL` if none available. Do not free the returned value, it belongs to `self` .

[transfer none]

Since: 1.0

### mm_modem_dup_own_numbers ()

    gchar **
    mm_modem_dup_own_numbers (MMModem *self);

Gets a copy of the list of numbers (e.g. MSISDN in 3GPP) being currently handled by this modem.

#### Parameters

self | A MMModem. |

#### Returns

The list of own numbers or `NULL` if none is available. The returned value should be freed with `g_strfreev()`.

[transfer full]

Since: 1.0

### mm_modem_peek_supported_modes ()

    gboolean
    mm_modem_peek_supported_modes (MMModem *self,
                                   const MMModemModeCombination **modes,
                                   guint *n_modes);

Gets the list of supported mode combinations.

#### Parameters

self | A MMModem. |
modes | Return location for the array of MMModemModeCombination values. Do not free the returned array, it is owned by `self` . | [out][array length=n_modes]
n_modes | Return location for the number of values in `modes` . | [out]

#### Returns

`TRUE` if `modes` and `n_modes` are set, `FALSE` otherwise.

Since: 1.0

### mm_modem_get_supported_modes ()

    gboolean
    mm_modem_get_supported_modes (MMModem *self,
                                  MMModemModeCombination **modes,
                                  guint *n_modes);

Gets the list of supported mode combinations.

#### Parameters

self | A MMModem. |
modes | Return location for the array of MMModemModeCombination structs. The returned array should be freed with `g_free()` when no longer needed. | [out][array length=n_modes]
n_modes | Return location for the number of values in `modes` . | [out]

#### Returns

`TRUE` if `modes` and `n_modes` are set, `FALSE` otherwise.

Since: 1.0

### mm_modem_get_current_modes ()

    gboolean
    mm_modem_get_current_modes (MMModem *self,
                                MMModemMode *allowed,
                                MMModemMode *preferred);

Gets the list of modes specifying the access technologies (eg 2G/3G/4G) the MMModem is currently allowed to use when connecting to a network, as well as the preferred one, if any.

#### Parameters

self | A MMModem. |
allowed | Return location for a bitmask of MMModemMode values. | [out]
preferred | Return location for a MMModemMode value. | [out]

#### Returns

`TRUE` if `allowed` and `preferred` are set, `FALSE` otherwise.

Since: 1.0

### mm_modem_peek_supported_bands ()

    gboolean
    mm_modem_peek_supported_bands (MMModem *self,
                                   const MMModemBand **bands,
                                   guint *n_bands);

Gets the list of radio frequency and technology bands supported by the MMModem.

For POTS devices, only MM_MODEM_BAND_ANY will be returned in `bands` .

#### Parameters

self | A MMModem. |
bands | Return location for the array of MMModemBand values. Do not free the returned array, it is owned by `self` . | [out][array length=n_bands]
n_bands | Return location for the number of values in `bands` . | [out]

#### Returns

`TRUE` if `bands` and `n_bands` are set, `FALSE` otherwise.

Since: 1.0

### mm_modem_get_supported_bands ()

    gboolean
    mm_modem_get_supported_bands (MMModem *self,
                                  MMModemBand **bands,
                                  guint *n_bands);

Gets the list of radio frequency and technology bands supported by the MMModem.

For POTS devices, only MM_MODEM_BAND_ANY will be returned in `bands` .

#### Parameters

self | A MMModem. |
bands | Return location for the array of MMModemBand values. The returned array should be freed with `g_free()` when no longer needed. | [out][array length=n_bands]
n_bands | Return location for the number of values in `bands` . | [out]

#### Returns

`TRUE` if `bands` and `n_bands` are set, `FALSE` otherwise.

Since: 1.0

### mm_modem_peek_current_bands ()

    gboolean
    mm_modem_peek_current_bands (MMModem *self,
                                 const MMModemBand **bands,
                                 guint *n_bands);

Gets the list of radio frequency and technology bands the MMModem is currently using when connecting to a network.

For POTS devices, only the MM_MODEM_BAND_ANY band is supported.

#### Parameters

self | A MMModem. |
bands | Return location for the array of MMModemBand values. Do not free the returned value, it is owned by `self` . | [out][array length=n_bands]
n_bands | Return location for the number of values in `bands` . | [out]

#### Returns

`TRUE` if `bands` and `n_bands` are set, `FALSE` otherwise.

Since: 1.0

### mm_modem_get_current_bands ()

    gboolean
    mm_modem_get_current_bands (MMModem *self,
                                MMModemBand **bands,
                                guint *n_bands);

Gets the list of radio frequency and technology bands the MMModem is currently using when connecting to a network.

For POTS devices, only the MM_MODEM_BAND_ANY band is supported.

#### Parameters

self | A MMModem. |
bands | Return location for the array of MMModemBand values. The returned array should be freed with `g_free()` when no longer needed. | [out][array length=n_bands]
n_bands | Return location for the number of values in `bands` . | [out]

#### Returns

`TRUE` if `bands` and `n_bands` are set, `FALSE` otherwise.

Since: 1.0

### mm_modem_get_supported_ip_families ()

    MMBearerIpFamily
    mm_modem_get_supported_ip_families (MMModem *self);

Gets the list of supported IP families.

#### Parameters

self | A MMModem. |

#### Returns

A bitmask of MMBearerIpFamily values.

Since: 1.0

### mm_modem_get_signal_quality ()

    guint
    mm_modem_get_signal_quality (MMModem *self,
                                 gboolean *recent);

Gets the signal quality value in percent (0 - 100) of the dominant access technology the MMModem is using to communicate with the network.

Always 0 for POTS devices.

#### Parameters

self | A MMModem. |
recent | Return location for the flag specifying if the signal quality value was recent or not. | [out]

#### Returns

The signal quality.

Since: 1.0

### mm_modem_get_access_technologies ()

    MMModemAccessTechnology
    mm_modem_get_access_technologies (MMModem *self);

Gets the current network access technology used by the MMModem to communicate with the network.

#### Parameters

self | A MMModem. |

#### Returns

A #MMModemAccessTechnology value.

Since: 1.0

### mm_modem_get_sim_path ()

    const gchar *
    mm_modem_get_sim_path (MMModem *self);

Gets the DBus path of the MMSim handled in this MMModem.

The returned value is only valid until the property changes so it is only safe to use this function on the thread where `self` was constructed. Use `mm_modem_dup_sim_path()` if on another thread.

[skip]

#### Parameters

self | A MMModem. |

#### Returns

The DBus path of the MMSim handled in this MMModem, or `NULL` if none available. Do not free the returned value, it belongs to `self` .

[transfer none]

Since: 1.0

### mm_modem_dup_sim_path ()

    gchar *
    mm_modem_dup_sim_path (MMModem *self);

Gets a copy of the DBus path of the MMSim handled in this MMModem.

#### Parameters

self | A MMModem. |

#### Returns

The DBus path of the MMSim handled in this MMModem, or `NULL` if none available. The returned value should be freed with `g_free()`.

[transfer full]

Since: 1.0

### mm_modem_get_sim ()

    void
    mm_modem_get_sim (MMModem *self,
                      GCancellable *cancellable,
                      GAsyncReadyCallback callback,
                      gpointer user_data);

Asynchronously gets the MMSim object managed by this MMModem.

When the operation is finished, `callback` will be invoked in the

thread-default main loop

of the thread you are calling this method from. You can then call `mm_modem_get_sim_finish()` to get the result of the operation.

See `mm_modem_get_sim_sync()` for the synchronous, blocking version of this method.

#### Parameters

self | A MMModem. |
cancellable | A GCancellable or `NULL`. | [allow-none]
callback | A GAsyncReadyCallback to call when the request is satisfied or `NULL`. |
user_data | User data to pass to `callback` . |

Since: 1.0

### mm_modem_get_sim_finish ()

    MMSim *
    mm_modem_get_sim_finish (MMModem *self,
                             GAsyncResult *res,
                             GError **error);

Finishes an operation started with `mm_modem_get_sim()`.

#### Parameters

self | A MMModem. |
res | The GAsyncResult obtained from the GAsyncReadyCallback passed to `mm_modem_get_sim()`. |
error | Return location for error or `NULL`. |

#### Returns

a MMSim or NULL if `error` is set. The returned value should be freed with `g_object_unref()`.

[transfer full]

Since: 1.0

### mm_modem_get_sim_sync ()

    MMSim *
    mm_modem_get_sim_sync (MMModem *self,
                           GCancellable *cancellable,
                           GError **error);

Synchronously gets the MMSim object managed by this MMModem.

The calling thread is blocked until a reply is received. See `mm_modem_get_sim()` for the asynchronous version of this method.

#### Parameters

self | A MMModem. |
cancellable | A GCancellable or `NULL`. | [allow-none]
error | Return location for error or `NULL`. |

#### Returns

a MMSim or NULL if `error` is set. The returned value should be freed with `g_object_unref()`.

[transfer full]

Since: 1.0

### mm_modem_get_sim_slot_paths ()

    const gchar * const *
    mm_modem_get_sim_slot_paths (MMModem *self);

Gets the DBus paths of the MMSim objects available in the different SIM slots handled in this MMModem. If a given SIM slot at a given index doesn't have a SIM card available, an empty object path will be given. This list includes the currently active SIM object path.

The returned value is only valid until the property changes so it is only safe to use this function on the thread where `self` was constructed. Use `mm_modem_dup_sim_slot_paths()` if on another thread.

#### Parameters

self | A MMModem. |

#### Returns

The DBus paths of the MMSim objects handled in this MMModem, or `NULL` if none available. Do not free the returned value, it belongs to `self` .

[transfer none]

Since: 1.16

### mm_modem_dup_sim_slot_paths ()

    gchar **
    mm_modem_dup_sim_slot_paths (MMModem *self);

Gets a copy of the DBus paths of the MMSim objects available in the different SIM slots handled in this MMModem. If a given SIM slot at a given index doesn't have a SIM card available, an empty object path will be given. This list includes the currently active SIM object path.

#### Parameters

self | A MMModem. |

#### Returns

The DBus paths of the MMSim objects handled in this MMModem, or `NULL` if none available. The returned value should be freed with `g_strfreev()`.

[transfer full]

Since: 1.16

### mm_modem_get_primary_sim_slot ()

    guint
    mm_modem_get_primary_sim_slot (MMModem *self);

Gets the SIM slot number of the primary active SIM.

#### Parameters

self | A MMModem. |

#### Returns

slot number, in the [1,N] range.

Since: 1.16

### mm_modem_list_sim_slots ()

    void
    mm_modem_list_sim_slots (MMModem *self,
                             GCancellable *cancellable,
                             GAsyncReadyCallback callback,
                             gpointer user_data);

Asynchronously lists the SIM slots available in the MMModem.

The returned array contains one element per slot available in the system; a MMSim in each of the slots that contains a valid SIM card or `NULL` if no SIM card is found.

When the operation is finished, `callback` will be invoked in the

thread-default main loop

of the thread you are calling this method from. You can then call `mm_modem_list_sim_slots_finish()` to get the result of the operation.

See `mm_modem_list_sim_slots_sync()` for the synchronous, blocking version of this method.

#### Parameters

self | A MMModem. |
cancellable | A GCancellable or `NULL`. | [allow-none]
callback | A GAsyncReadyCallback to call when the request is satisfied or `NULL`. |
user_data | User data to pass to `callback` . |

Since: 1.16

### mm_modem_list_sim_slots_finish ()

    GPtrArray *
    mm_modem_list_sim_slots_finish (MMModem *self,
                                    GAsyncResult *res,
                                    GError **error);

Finishes an operation started with `mm_modem_list_sim_slots()`.

#### Parameters

self | A MMModem. |
res | The GAsyncResult obtained from the GAsyncReadyCallback passed to `mm_modem_list_sim_slots()`. |
error | Return location for error or `NULL`. |

#### Returns

The array of MMSim objects, or `NULL` if `error` is set.

[transfer full][element-type ModemManager.Sim]

Since: 1.16

### mm_modem_list_sim_slots_sync ()

    GPtrArray *
    mm_modem_list_sim_slots_sync (MMModem *self,
                                  GCancellable *cancellable,
                                  GError **error);

Synchronously lists the SIM slots available in the MMModem.

The returned array contains one element per slot available in the system; a MMSim in each of the slots that contains a valid SIM card or `NULL` if no SIM card is found.

The calling thread is blocked until a reply is received. See `mm_modem_list_sim_slots()` for the asynchronous version of this method.

#### Parameters

self | A MMModem. |
cancellable | A GCancellable or `NULL`. | [allow-none]
error | Return location for error or `NULL`. |

#### Returns

The array of MMSim objects, or `NULL` if `error` is set.

[transfer full][element-type ModemManager.Sim]

Since: 1.16

### mm_modem_set_primary_sim_slot ()

    void
    mm_modem_set_primary_sim_slot (MMModem *self,
                                   guint sim_slot,
                                   GCancellable *cancellable,
                                   GAsyncReadyCallback callback,
                                   gpointer user_data);

Asynchronously requests to select which SIM slot to be considered as primary.

When the operation is finished, `callback` will be invoked in the

thread-default main loop

of the thread you are calling this method from. You can then call `mm_modem_set_primary_sim_slot_finish()` to get the result of the operation.

See `mm_modem_set_primary_sim_slot_sync()` for the synchronous, blocking version of this method.

#### Parameters

self | A MMModem. |
sim_slot | SIM slot number. |
cancellable | A GCancellable or `NULL`. | [allow-none]
callback | A GAsyncReadyCallback to call when the request is satisfied or `NULL`. |
user_data | User data to pass to `callback` . |

Since: 1.16

### mm_modem_set_primary_sim_slot_finish ()

    gboolean
    mm_modem_set_primary_sim_slot_finish (MMModem *self,
                                          GAsyncResult *res,
                                          GError **error);

Finishes an operation started with `mm_modem_set_primary_sim_slot()`.

#### Parameters

self | A MMModem. |
res | The GAsyncResult obtained from the GAsyncReadyCallback passed to `mm_modem_set_primary_sim_slot()`. |
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if the SIM slot switch has been successfully requested, `FALSE` if `error` is set.

Since: 1.16

### mm_modem_set_primary_sim_slot_sync ()

    gboolean
    mm_modem_set_primary_sim_slot_sync (MMModem *self,
                                        guint sim_slot,
                                        GCancellable *cancellable,
                                        GError **error);

Synchronously requests to select which SIM slot to be considered as primary.

The calling thread is blocked until a reply is received. See `mm_modem_set_primary_sim_slot()` for the asynchronous version of this method.

#### Parameters

self | A MMModem. |
sim_slot | SIM slot number. |
cancellable | A GCancellable or `NULL`. | [allow-none]
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if the SIM slot switch has been successfully requested, `FALSE` if `error` is set.

Since: 1.16

### mm_modem_enable ()

    void
    mm_modem_enable (MMModem *self,
                     GCancellable *cancellable,
                     GAsyncReadyCallback callback,
                     gpointer user_data);

Asynchronously tries to enable the MMModem. When enabled, the modem's radio is powered on and data sessions, voice calls, location services, and Short Message Service may be available.

When the operation is finished, `callback` will be invoked in the

thread-default main loop

of the thread you are calling this method from. You can then call `mm_modem_enable_finish()` to get the result of the operation.

See `mm_modem_enable_sync()` for the synchronous, blocking version of this method.

#### Parameters

self | A MMModem. |
cancellable | A GCancellable or `NULL`. | [allow-none]
callback | A GAsyncReadyCallback to call when the request is satisfied or `NULL`. |
user_data | User data to pass to `callback` . |

Since: 1.0

### mm_modem_enable_finish ()

    gboolean
    mm_modem_enable_finish (MMModem *self,
                            GAsyncResult *res,
                            GError **error);

Finishes an operation started with `mm_modem_enable()`.

#### Parameters

self | A MMModem. |
res | The GAsyncResult obtained from the GAsyncReadyCallback passed to `mm_modem_enable()`. |
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if the modem was properly enabled, `FALSE` if `error` is set.

Since: 1.0

### mm_modem_enable_sync ()

    gboolean
    mm_modem_enable_sync (MMModem *self,
                          GCancellable *cancellable,
                          GError **error);

Synchronously tries to enable the MMModem. When enabled, the modem's radio is powered on and data sessions, voice calls, location services, and Short Message Service may be available.

The calling thread is blocked until a reply is received. See `mm_modem_enable()` for the asynchronous version of this method.

#### Parameters

self | A MMModem. |
cancellable | A GCancellable or `NULL`. | [allow-none]
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if the modem was properly enabled, `FALSE` if `error` is set.

Since: 1.0

### mm_modem_disable ()

    void
    mm_modem_disable (MMModem *self,
                      GCancellable *cancellable,
                      GAsyncReadyCallback callback,
                      gpointer user_data);

Asynchronously tries to disable the MMModem. When disabled, the modem enters low-power state and no network-related operations are available.

When the operation is finished, `callback` will be invoked in the

thread-default main loop

of the thread you are calling this method from. You can then call `mm_modem_disable_finish()` to get the result of the operation.

See `mm_modem_disable_sync()` for the synchronous, blocking version of this method.

#### Parameters

self | A MMModem. |
cancellable | A GCancellable or `NULL`. | [allow-none]
callback | A GAsyncReadyCallback to call when the request is satisfied or `NULL`. |
user_data | User data to pass to `callback` . |

Since: 1.0

### mm_modem_disable_finish ()

    gboolean
    mm_modem_disable_finish (MMModem *self,
                             GAsyncResult *res,
                             GError **error);

Finishes an operation started with `mm_modem_disable()`.

#### Parameters

self | A MMModem. |
res | The GAsyncResult obtained from the GAsyncReadyCallback passed to `mm_modem_disable()`. |
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if the modem was properly disabled, `FALSE` if `error` is set.

Since: 1.0

### mm_modem_disable_sync ()

    gboolean
    mm_modem_disable_sync (MMModem *self,
                           GCancellable *cancellable,
                           GError **error);

Synchronously tries to disable the MMModem. When disabled, the modem enters low-power state and no network-related operations are available.

The calling thread is blocked until a reply is received. See `mm_modem_disable()` for the asynchronous version of this method.

#### Parameters

self | A MMModem. |
cancellable | A GCancellable or `NULL`. | [allow-none]
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if the modem was properly disabled, `FALSE` if `error` is set.

Since: 1.0

### mm_modem_set_power_state ()

    void
    mm_modem_set_power_state (MMModem *self,
                              MMModemPowerState state,
                              GCancellable *cancellable,
                              GAsyncReadyCallback callback,
                              gpointer user_data);

Asynchronously sets the power state of the device. This method can only be used while the modem is in `MM_MODEM_STATE_DISABLED` state.

When the operation is finished, `callback` will be invoked in the

thread-default main loop

of the thread you are calling this method from. You can then call `mm_modem_set_power_state_finish()` to get the result of the operation.

See `mm_modem_set_power_state_sync()` for the synchronous, blocking version of this method.

#### Parameters

self | A MMModem. |
state | Either `MM_MODEM_POWER_STATE_LOW` or `MM_MODEM_POWER_STATE_ON`. Every other MMModemPowerState value is not allowed. |
cancellable | A GCancellable or `NULL`. | [allow-none]
callback | A GAsyncReadyCallback to call when the request is satisfied or `NULL`. |
user_data | User data to pass to `callback` . |

Since: 1.0

### mm_modem_set_power_state_finish ()

    gboolean
    mm_modem_set_power_state_finish (MMModem *self,
                                     GAsyncResult *res,
                                     GError **error);

Finishes an operation started with `mm_modem_set_power_state()`.

#### Parameters

self | A MMModem. |
res | The GAsyncResult obtained from the GAsyncReadyCallback passed to `mm_modem_set_power_state()`. |
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if the power state was successfully set, `FALSE` if `error` is set.

Since: 1.0

### mm_modem_set_power_state_sync ()

    gboolean
    mm_modem_set_power_state_sync (MMModem *self,
                                   MMModemPowerState state,
                                   GCancellable *cancellable,
                                   GError **error);

Synchronously sets the power state of the device. This method can only be used while the modem is in `MM_MODEM_STATE_DISABLED` state.

The calling thread is blocked until a reply is received. See `mm_modem_set_power_state()` for the asynchronous version of this method.

#### Parameters

self | A MMModem. |
state | Either `MM_MODEM_POWER_STATE_LOW` or `MM_MODEM_POWER_STATE_ON`. Every other MMModemPowerState value is not allowed. |
cancellable | A GCancellable or `NULL`. | [allow-none]
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if the power state was successfully set, `FALSE` if `error` is set.

Since: 1.0

### mm_modem_set_current_modes ()

    void
    mm_modem_set_current_modes (MMModem *self,
                                MMModemMode modes,
                                MMModemMode preferred,
                                GCancellable *cancellable,
                                GAsyncReadyCallback callback,
                                gpointer user_data);

Asynchronously sets the access technologies (e.g. 2G/3G/4G preference) the device is currently allowed to use when connecting to a network.

When the operation is finished, `callback` will be invoked in the

thread-default main loop

of the thread you are calling this method from. You can then call `mm_modem_set_current_modes_finish()` to get the result of the operation.

See `mm_modem_set_current_modes_sync()` for the synchronous, blocking version of this method.

#### Parameters

self | A MMModem. |
modes | Mask of MMModemMode values specifying which modes are allowed. |
preferred | A MMModemMode value specifying which of the modes given in `modes` is the preferred one, or MM_MODEM_MODE_NONE if none. |
cancellable | A GCancellable or `NULL`. | [allow-none]
callback | A GAsyncReadyCallback to call when the request is satisfied or `NULL`. |
user_data | User data to pass to `callback` . |

Since: 1.0

### mm_modem_set_current_modes_finish ()

    gboolean
    mm_modem_set_current_modes_finish (MMModem *self,
                                       GAsyncResult *res,
                                       GError **error);

Finishes an operation started with `mm_modem_set_current_modes()`.

#### Parameters

self | A MMModem. |
res | The GAsyncResult obtained from the GAsyncReadyCallback passed to `mm_modem_set_current_modes()`. |
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if the allowed modes were successfully set, `FALSE` if `error` is set.

Since: 1.0

### mm_modem_set_current_modes_sync ()

    gboolean
    mm_modem_set_current_modes_sync (MMModem *self,
                                     MMModemMode modes,
                                     MMModemMode preferred,
                                     GCancellable *cancellable,
                                     GError **error);

Synchronously sets the access technologies (e.g. 2G/3G/4G preference) the device is currently allowed to use when connecting to a network.

The calling thread is blocked until a reply is received. See `mm_modem_set_current_modes()` for the asynchronous version of this method.

#### Parameters

self | A MMModem. |
modes | Mask of MMModemMode values specifying which modes are allowed. |
preferred | A MMModemMode value specifying which of the modes given in `modes` is the preferred one, or MM_MODEM_MODE_NONE if none. |
cancellable | A GCancellable or `NULL`. | [allow-none]
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if the allowed modes were successfully set, `FALSE` if `error` is set.

Since: 1.0

### mm_modem_set_current_bands ()

    void
    mm_modem_set_current_bands (MMModem *self,
                                const MMModemBand *bands,
                                guint n_bands,
                                GCancellable *cancellable,
                                GAsyncReadyCallback callback,
                                gpointer user_data);

Asynchronously sets the radio frequency and technology bands the device is currently allowed to use when connecting to a network.

When the operation is finished, `callback` will be invoked in the

thread-default main loop

of the thread you are calling this method from. You can then call `mm_modem_set_current_bands_finish()` to get the result of the operation.

See `mm_modem_set_current_bands_sync()` for the synchronous, blocking version of this method.

#### Parameters

self | A MMModem. |
bands | An array of MMModemBand values specifying which bands are allowed. |
n_bands | Number of elements in `bands` . |
cancellable | A GCancellable or `NULL`. | [allow-none]
callback | A GAsyncReadyCallback to call when the request is satisfied or `NULL`. |
user_data | User data to pass to `callback` . |

Since: 1.0

### mm_modem_set_current_bands_finish ()

    gboolean
    mm_modem_set_current_bands_finish (MMModem *self,
                                       GAsyncResult *res,
                                       GError **error);

Finishes an operation started with `mm_modem_set_current_bands()`.

#### Parameters

self | A MMModem. |
res | The GAsyncResult obtained from the GAsyncReadyCallback passed to `mm_modem_set_current_bands()`. |
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if the bands were successfully set, `FALSE` if `error` is set.

Since: 1.0

### mm_modem_set_current_bands_sync ()

    gboolean
    mm_modem_set_current_bands_sync (MMModem *self,
                                     const MMModemBand *bands,
                                     guint n_bands,
                                     GCancellable *cancellable,
                                     GError **error);

Synchronously sets the radio frequency and technology bands the device is currently allowed to use when connecting to a network.

The calling thread is blocked until a reply is received. See `mm_modem_set_current_bands()` for the asynchronous version of this method.

#### Parameters

self | A MMModem. |
bands | An array of MMModemBand values specifying which bands are allowed. |
n_bands | Number of elements in `bands` . |
cancellable | A GCancellable or `NULL`. | [allow-none]
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if the bands were successfully set, `FALSE` if `error` is set.

Since: 1.0

### mm_modem_set_current_capabilities ()

    void
    mm_modem_set_current_capabilities (MMModem *self,
                                       MMModemCapability capabilities,
                                       GCancellable *cancellable,
                                       GAsyncReadyCallback callback,
                                       gpointer user_data);

Asynchronously sets the capabilities of the device. A restart of the modem may be required.

When the operation is finished, `callback` will be invoked in the

thread-default main loop

of the thread you are calling this method from. You can then call `mm_modem_set_current_capabilities_finish()` to get the result of the operation.

See `mm_modem_set_current_capabilities_sync()` for the synchronous, blocking version of this method.

#### Parameters

self | A MMModem. |
capabilities | A MMModemCapability mask. |
cancellable | A GCancellable or `NULL`. | [allow-none]
callback | A GAsyncReadyCallback to call when the request is satisfied or `NULL`. |
user_data | User data to pass to `callback` . |

Since: 1.0

### mm_modem_set_current_capabilities_finish ()

    gboolean
    mm_modem_set_current_capabilities_finish
                                   (MMModem *self,
                                    GAsyncResult *res,
                                    GError **error);

Finishes an operation started with `mm_modem_set_current_capabilities()`.

#### Parameters

self | A MMModem. |
res | The GAsyncResult obtained from the GAsyncReadyCallback passed to `mm_modem_set_current_capabilities()`. |
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if the capabilities were successfully set, `FALSE` if `error` is set.

Since: 1.0

### mm_modem_set_current_capabilities_sync ()

    gboolean
    mm_modem_set_current_capabilities_sync
                                   (MMModem *self,
                                    MMModemCapability capabilities,
                                    GCancellable *cancellable,
                                    GError **error);

Synchronously sets the capabilities of the device. A restart of the modem may be required.

The calling thread is blocked until a reply is received. See `mm_modem_set_current_capabilities()` for the asynchronous version of this method.

#### Parameters

self | A MMModem. |
capabilities | A MMModemCapability mask. |
cancellable | A GCancellable or `NULL`. | [allow-none]
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if the capabilities were successfully set, `FALSE` if `error` is set.

Since: 1.0

### mm_modem_reset ()

    void
    mm_modem_reset (MMModem *self,
                    GCancellable *cancellable,
                    GAsyncReadyCallback callback,
                    gpointer user_data);

Asynchronously clears non-persistent configuration and state, and returns the device to a newly-powered-on state.

When the operation is finished, `callback` will be invoked in the

thread-default main loop

of the thread you are calling this method from. You can then call `mm_modem_reset_finish()` to get the result of the operation.

See `mm_modem_reset_sync()` for the synchronous, blocking version of this method.

#### Parameters

self | A MMModem. |
cancellable | A GCancellable or `NULL`. | [allow-none]
callback | A GAsyncReadyCallback to call when the request is satisfied or `NULL`. |
user_data | User data to pass to `callback` . |

Since: 1.0

### mm_modem_reset_finish ()

    gboolean
    mm_modem_reset_finish (MMModem *self,
                           GAsyncResult *res,
                           GError **error);

Finishes an operation started with `mm_modem_reset()`.

#### Parameters

self | A MMModem. |
res | The GAsyncResult obtained from the GAsyncReadyCallback passed to `mm_modem_reset()`. |
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if the reset was successful, `FALSE` if `error` is set.

Since: 1.0

### mm_modem_reset_sync ()

    gboolean
    mm_modem_reset_sync (MMModem *self,
                         GCancellable *cancellable,
                         GError **error);

Synchronously clears non-persistent configuration and state, and returns the device to a newly-powered-on state.

The calling thread is blocked until a reply is received. See `mm_modem_reset()` for the asynchronous version of this method.

#### Parameters

self | A MMModem. |
cancellable | A GCancellable or `NULL`. | [allow-none]
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if the reset was successful, `FALSE` if `error` is set.

Since: 1.0

### mm_modem_factory_reset ()

    void
    mm_modem_factory_reset (MMModem *self,
                            const gchar *code,
                            GCancellable *cancellable,
                            GAsyncReadyCallback callback,
                            gpointer user_data);

Asynchronously clears the modem's configuration (including persistent configuration and state), and returns the device to a factory-default state.

When the operation is finished, `callback` will be invoked in the

thread-default main loop

of the thread you are calling this method from. You can then call `mm_modem_factory_reset_finish()` to get the result of the operation.

See `mm_modem_factory_reset_sync()` for the synchronous, blocking version of this method.

#### Parameters

self | A MMModem. |
code | Carrier-supplied code required to reset the modem. |
cancellable | A GCancellable or `NULL`. | [allow-none]
callback | A GAsyncReadyCallback to call when the request is satisfied or `NULL`. |
user_data | User data to pass to `callback` . |

Since: 1.0

### mm_modem_factory_reset_finish ()

    gboolean
    mm_modem_factory_reset_finish (MMModem *self,
                                   GAsyncResult *res,
                                   GError **error);

Finishes an operation started with `mm_modem_factory_reset()`.

#### Parameters

self | A MMModem. |
res | The GAsyncResult obtained from the GAsyncReadyCallback passed to `mm_modem_factory_reset()`. |
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if the factory_reset was successful, `FALSE` if `error` is set.

Since: 1.0

### mm_modem_factory_reset_sync ()

    gboolean
    mm_modem_factory_reset_sync (MMModem *self,
                                 const gchar *code,
                                 GCancellable *cancellable,
                                 GError **error);

Synchronously clears the modem's configuration (including persistent configuration and state), and returns the device to a factory-default state.

The calling thread is blocked until a reply is received. See `mm_modem_factory_reset()` for the asynchronous version of this method.

#### Parameters

self | A MMModem. |
code | Carrier-supplied code required to reset the modem. |
cancellable | A GCancellable or `NULL`. | [allow-none]
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if the factory reset was successful, `FALSE` if `error` is set.

Since: 1.0

### mm_modem_list_bearers ()

    void
    mm_modem_list_bearers (MMModem *self,
                           GCancellable *cancellable,
                           GAsyncReadyCallback callback,
                           gpointer user_data);

Asynchronously lists the packet data bearers in the MMModem.

When the operation is finished, `callback` will be invoked in the

thread-default main loop

of the thread you are calling this method from. You can then call `mm_modem_list_bearers_finish()` to get the result of the operation.

See `mm_modem_list_bearers_sync()` for the synchronous, blocking version of this method.

#### Parameters

self | A MMModem. |
cancellable | A GCancellable or `NULL`. | [allow-none]
callback | A GAsyncReadyCallback to call when the request is satisfied or `NULL`. |
user_data | User data to pass to `callback` . |

Since: 1.0

### mm_modem_list_bearers_finish ()

    GList *
    mm_modem_list_bearers_finish (MMModem *self,
                                  GAsyncResult *res,
                                  GError **error);

Finishes an operation started with `mm_modem_list_bearers()`.

#### Parameters

self | A MMModem. |
res | The GAsyncResult obtained from the GAsyncReadyCallback passed to `mm_modem_list_bearers()`. |
error | Return location for error or `NULL`. |

#### Returns

The list of MMBearer objects, or `NULL` if either none found or if `error` is set.

[transfer full][element-type ModemManager.Bearer]

Since: 1.0

### mm_modem_list_bearers_sync ()

    GList *
    mm_modem_list_bearers_sync (MMModem *self,
                                GCancellable *cancellable,
                                GError **error);

Synchronously lists the packet data bearers in the MMModem.

The calling thread is blocked until a reply is received. See `mm_modem_list_bearers()` for the asynchronous version of this method.

#### Parameters

self | A MMModem. |
cancellable | A GCancellable or `NULL`. | [allow-none]
error | Return location for error or `NULL`. |

#### Returns

The list of MMBearer objects, or `NULL` if either none found or if `error` is set.

[transfer full][element-type ModemManager.Bearer]

Since: 1.0

### mm_modem_create_bearer ()

    void
    mm_modem_create_bearer (MMModem *self,
                            MMBearerProperties *properties,
                            GCancellable *cancellable,
                            GAsyncReadyCallback callback,
                            gpointer user_data);

Asynchronously creates a new packet data bearer in the MMModem.

This request may fail if the modem does not support additional bearers, if too many bearers are already defined, or if `properties` are invalid.

See CreateBearer to check which properties may be passed.

When the operation is finished, `callback` will be invoked in the

thread-default main loop

of the thread you are calling this method from. You can then call `mm_modem_create_bearer_finish()` to get the result of the operation.

See `mm_modem_create_bearer_sync()` for the synchronous, blocking version of this method.

#### Parameters

self | A MMModem. |
properties | A MMBearerProperties object with the properties to use. |
cancellable | A GCancellable or `NULL`. | [allow-none]
callback | A GAsyncReadyCallback to call when the request is satisfied or `NULL`. |
user_data | User data to pass to `callback` . |

Since: 1.0

### mm_modem_create_bearer_finish ()

    MMBearer *
    mm_modem_create_bearer_finish (MMModem *self,
                                   GAsyncResult *res,
                                   GError **error);

Finishes an operation started with `mm_modem_create_bearer()`.

#### Parameters

self | A MMModem. |
res | The GAsyncResult obtained from the GAsyncReadyCallback passed to `mm_modem_create_bearer()`. |
error | Return location for error or `NULL`. |

#### Returns

A newly created MMBearer, or `NULL` if `error` is set.

[transfer full]

Since: 1.0

### mm_modem_create_bearer_sync ()

    MMBearer *
    mm_modem_create_bearer_sync (MMModem *self,
                                 MMBearerProperties *properties,
                                 GCancellable *cancellable,
                                 GError **error);

Synchronously creates a new packet data bearer in the MMModem.

This request may fail if the modem does not support additional bearers, if too many bearers are already defined, or if `properties` are invalid.

See CreateBearer to check which properties may be passed.

The calling thread is blocked until a reply is received. See `mm_modem_create_bearer()` for the asynchronous version of this method.

#### Parameters

self | A MMModem. |
properties | A MMBearerProperties object with the properties to use. |
cancellable | A GCancellable or `NULL`. | [allow-none]
error | Return location for error or `NULL`. |

#### Returns

A newly created MMBearer, or `NULL` if `error` is set.

[transfer full]

Since: 1.0

### mm_modem_delete_bearer ()

    void
    mm_modem_delete_bearer (MMModem *self,
                            const gchar *bearer,
                            GCancellable *cancellable,
                            GAsyncReadyCallback callback,
                            gpointer user_data);

Asynchronously deletes a given bearer from the MMModem.

When the operation is finished, `callback` will be invoked in the

thread-default main loop

of the thread you are calling this method from. You can then call `mm_modem_delete_bearer_finish()` to get the result of the operation.

See `mm_modem_delete_bearer_sync()` for the synchronous, blocking version of this method.

#### Parameters

self | A MMModem. |
bearer | Path of the bearer to delete. |
cancellable | A GCancellable or `NULL`. | [allow-none]
callback | A GAsyncReadyCallback to call when the request is satisfied or `NULL`. |
user_data | User data to pass to `callback` . |

Since: 1.0

### mm_modem_delete_bearer_finish ()

    gboolean
    mm_modem_delete_bearer_finish (MMModem *self,
                                   GAsyncResult *res,
                                   GError **error);

Finishes an operation started with `mm_modem_delete_bearer()`.

#### Parameters

self | A MMModem. |
res | The GAsyncResult obtained from the GAsyncReadyCallback passed to `mm_modem_delete_bearer()`. |
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if the bearer was deleted, `FALSE` if `error` is set.

Since: 1.0

### mm_modem_delete_bearer_sync ()

    gboolean
    mm_modem_delete_bearer_sync (MMModem *self,
                                 const gchar *bearer,
                                 GCancellable *cancellable,
                                 GError **error);

Synchronously deletes a given bearer from the MMModem.

The calling thread is blocked until a reply is received. See `mm_modem_delete_bearer()` for the asynchronous version of this method.

#### Parameters

self | A MMModem. |
bearer | Path of the bearer to delete. |
cancellable | A GCancellable or `NULL`. | [allow-none]
error | Return location for error or `NULL`. |

#### Returns

`TRUE` if the bearer was deleted, `FALSE` if `error` is set.

Since: 1.0

### mm_modem_command ()

    void
    mm_modem_command (MMModem *self,
                      const gchar *cmd,
                      guint timeout,
                      GCancellable *cancellable,
                      GAsyncReadyCallback callback,
                      gpointer user_data);

Asynchronously runs an AT command in the modem.

When the operation is finished, `callback` will be invoked in the

thread-default main loop

of the thread you are calling this method from. You can then call `mm_modem_command_finish()` to get the result of the operation.

See `mm_modem_command_sync()` for the synchronous, blocking version of this method.

#### Parameters

self | A MMModem. |
cmd | AT command to run. |
timeout | Maximum time to wait for the response, in seconds. |
cancellable | A GCancellable or `NULL`. | [allow-none]
callback | A GAsyncReadyCallback to call when the request is satisfied or `NULL`. |
user_data | User data to pass to `callback` . |

Since: 1.0

### mm_modem_command_finish ()

    gchar *
    mm_modem_command_finish (MMModem *self,
                             GAsyncResult *res,
                             GError **error);

Finishes an operation started with `mm_modem_command()`.

#### Parameters

self | A MMModem. |
res | The GAsyncResult obtained from the GAsyncReadyCallback passed to `mm_modem_command()`. |
error | Return location for error or `NULL`. |

#### Returns

A newly allocated string with the reply to the command, or NULL if `error` is set. The returned value should be freed with `g_free()`.

[transfer full]

Since: 1.0

### mm_modem_command_sync ()

    gchar *
    mm_modem_command_sync (MMModem *self,
                           const gchar *cmd,
                           guint timeout,
                           GCancellable *cancellable,
                           GError **error);

Synchronously runs an AT command in the modem.

The calling thread is blocked until a reply is received. See `mm_modem_command()` for the asynchronous version of this method.

#### Parameters

self | A MMModem. |
cmd | AT command to run. |
timeout | Maximum time to wait for the response, in seconds. |
cancellable | A GCancellable or `NULL`. | [allow-none]
error | Return location for error or `NULL`. |

#### Returns

A newly allocated string with the reply to the command, or NULL if `error` is set. The returned value should be freed with `g_free()`.

[transfer full]

Since: 1.0

### mm_modem_port_info_array_free ()

    void
    mm_modem_port_info_array_free (MMModemPortInfo *array,
                                   guint array_size);

Frees an array of MMModemPortInfo values.

#### Parameters

array | an array of MMModemPortInfo values. |
array_size | length of `array` . |

Since: 1.0

## Types and Values

### struct MMModem

    struct MMModem;

The MMModem structure contains private data and should only be accessed using the provided API.

### struct MMModemModeCombination

    struct MMModemModeCombination {
        MMModemMode allowed;
        MMModemMode preferred;
    };

MMModemModeCombination is a simple struct holding a pair of MMModemMode values.

#### Members

MMModemMode `allowed`; | Mask of MMModemMode values specifying allowed modes. |
MMModemMode `preferred`; | A single MMModemMode value specifying the preferred mode. |

Since: 1.0

### struct MMModemPortInfo

    struct MMModemPortInfo {
        gchar *name;
        MMModemPortType type;
    };

Information of a given port.

#### Members

gchar *`name`; | Name of the port. |
MMModemPortType `type`; | A MMModemPortType value. |

Since: 1.0